VERSION 6		// V1 expects map checkpoint rectangles
			// V2 and above expect map checkpoint points
			// V3 and above expect splash file stuff at the end
			// V4 and above expect two sets of PIX and MAT and ped substitution entry

116.65,-6.38,94.81                                                     // Position of centre of start of grid
90										// Direction that grid faces in

// Laps, checkpoints etc

180,60,45							// Initial timer count for each skill level
3									// # laps
5000,5000,5000						// Race completed bonus (all laps raced) for each skill level
10000,10000,10000					// Race completed bonus (all peds killed) for each skill level
10000,10000,10000					// Race completed bonus (all oppos wasted) for each skill level

// Width and height of map checkpoint rectangles
9,18
11,26

0									// # checkpoints

9									// # pixelmap files to load
INDYSKY.PIX
BARRY.PIX
INDUSTA2.PIX
IHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX
INDTEX29.PIX
INDTEX30.PIX
INDTEX31.PIX

9
INDYSKY.PIX
BARRY.PIX									// # pixelmap files to load(low memory)
INDUSTA8.PIX
IHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX
INDTEX29.PIX
INDTEX30.PIX
INDTEX31.PIX

1									// # shade table files to load
DRRENDER.TAB

14									// # material files to load
INDYWIND.MAT
BARRY.MAT
URINE.MAT
RIVVY.MAT
DRAB.MAT
RIDDY.MAT
INDUSTA2.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
GANTSCRN.MAT
TUNNSCRN.MAT
ACIDSCRN.MAT
SKIDMARK.MAT

14									// # material files to load(low memory)
INDYWIND.MAT
BARRY.MAT
URINE.MAT
RIVVY.MAT
DRAB.MAT
RIDDY.MAT
INDUSTA8.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
GANTSCRN.MAT
TUNNSCRN.MAT
ACIDSCRN.MAT
SKIDMARK.MAT

1									// # model files to load
NETINDA.DAT

1									// # model files to load
NETINDA8.DAT

NETINDA.ACT                                                    // Track actor
NETINDA8.ACT                                                    // Track actor

INDUSTX.ACT							// Additional actor

// HORIZON STUFF

IHORIZN.PIX						// Name of sky texture pixelmap (or "none")
5									// Horizontal repetitions of sky texture
24									// Vertical size of sky texture (degrees)
83									// Position of horizon (pixels below top)
dark								// Depth cue mode ("none", "dark" or "fog")
7,0									// Degree of fog/darkness

// DEFAULT ENGINE NOISE

0

// SPECIAL EFFECTS VOLUMES

12									// # special effects volumes

DEFAULT WATER
0.2									// gravity multiplier
50									// viscosity multiplier
0									// Car damage per millisecond
0.002								// Pedestrian damage per millisecond
0									// camera effect index
1									// Sky colour
URINE.MAT								// Windscreen material to use
5100								// Sound ID of entry noise
5100								// Sound ID of exit noise
2									// Engine noise index
0									// material index


//------------------------ 0 -----------------------------------------
NEW IMPROVED!
-0.059, -0.003, -2.073
0.003, 1.200, -0.002
1.808, -0.005, -0.052
129.995, -4.116, 94.844
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 1 -----------------------------------------
NEW IMPROVED!
-0.039, 0.000, -2.986
-0.001, 0.833, 0.000
7.429, 0.006, -0.096
100.145, 0.271, 14.817
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 2 -----------------------------------------
NEW IMPROVED!
0.010, 0.002, 1.000
0.000, 1.000, -0.002
-4.680, 0.000, 0.047
124.928, -4.640, 19.399
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIVVY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 3 -----------------------------------------
NEW IMPROVED!
0.002, 0.002, 1.000
0.000, 1.000, -0.002
-4.095, 0.000, 0.009
124.127, -4.660, 14.664
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIVVY.MAT			// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 4 -----------------------------------------
NEW IMPROVED!
-0.001, 0.002, 1.000
0.000, 1.000, -0.002
-4.148, 0.000, -0.006
124.241, -4.600, 10.052
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIVVY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 5 -----------------------------------------
NEW IMPROVED!
-0.034, 0.001, -2.091
-0.002, 1.000, 0.000
7.447, 0.019, -1.082
45.792, -0.839, 127.248
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

//------------------------ 6 -----------------------------------------
NEW IMPROVED!
2.165, -0.001, -1.226
0.001, 1.000, 0.001
5.273, -0.008, 9.310
36.041, -0.518, 125.615
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 7 -----------------------------------------
NEW IMPROVED!
-2.986, 0.000, 0.032
0.000, 1.000, 0.000
-0.022, 0.000, -2.073
28.756, -0.837, 116.283
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 8 -----------------------------------------
NEW IMPROVED!
-7.430, 0.000, 0.037
0.000, 1.728, 0.000
-0.016, 0.000, -3.305
25.154, -3.137, 103.812
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 9 -----------------------------------------
NEW IMPROVED!
0.043, -0.001, 1.727
0.010, 4.300, 0.003
-10.117, 0.024, 0.254
42.168, -3.558, 86.838
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
DRAB.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 10 -----------------------------------------
NEW IMPROVED!
6.183, -0.003, 0.321
0.002, 2.986, -0.007
-0.385, 0.018, 7.420
118.839, -5.178, 57.802
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
BARRY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

 
// REFLECTIVE WINDSCREEN SPECIFICATIONS

INDYWIND.MAT							// Material to use for default screens
BARRY.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT							// Material to use for default screens during fog

6									// # areas with different screens
111.3,50,125.6,52					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,53.7,125.6,55.7				// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,58,125.6,60					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,61,125.6,63					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,65,125.6,67					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
67.9,76.6,111.7,96.5				// x-min, z-min, x-max, z-max rectangle describing area
TUNNSCRN.MAT						// Material to use instead

// MAP DETAILS

NINDAMAP.PIX						// Map pixelmap name

1.38,	0,		0					// World->map transformation matrix
0,		0,		0
0,		1.38,	0
37.3,	14.2,	0

// ****** START OF FUNK AND GROOVE STUFF ******

START OF FUNK

INDFAN01.MAT
distance
piss off
no fucking lighting bastards
frames
approximate
continuous
12
3
INDTEX29.PIX
INDTEX30.PIX
INDTEX31.PIX

NEXT FUNK

LIQUID.MAT
constant
roll
continuous
0,0.1
no fucking lighting
no animation you cunt

NEXT FUNK

!LIQUID.MAT
constant
throb
harmonic
0.13,0.09
5,5
50,50
no fucking lighting
no animation you cunt

NEXT FUNK

ACIDSCRN.MAT
constant
throb
harmonic
0.13,0.09
5,5
50,50
no fucking lighting
no animation you cunt

END OF FUNK

START OF GROOVE

&RCH0026.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0014.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0013.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0017.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0008.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0007.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0002.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&MNO0005.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
harmonic								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.1								// Cycles per second
1.5,0,0								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&MNO0003.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
harmonic								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.1								// Cycles per second
1.5,0,0								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&MNO0009.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
harmonic								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.1								// Cycles per second
1.5,0,0								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&CBO0012.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
no fucking path you cuuuuuuunt		// Does not move on a path
rock								// Object itself rocks
linear								// Motion is linear (i.e. direction changes instantly)
0.12								// Cycles per second
0,0,0								// Centre of movement
y									// Axis to rock in
90									// Angle to rock (each way)

NEXT GROOVE

&CAR0012.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,-0.1							// Centre of movement
0.2									// Cycles per second
0,0,0.15							// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&CBO0001.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
no fucking path you cuuuuuuunt		// Does not move on a path
rock								// Object itself rocks
linear								// Motion is linear (i.e. direction changes instantly)
0.12								// Cycles per second
0,0,0								// Centre of movement
y									// Axis to rock in
90									// Angle to rock (each way)

NEXT GROOVE

&CAR0001.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,-0.1							// Centre of movement
0.2									// Cycles per second
0,0,0.15							// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

END OF GROOVE


// ****** START OF PEDESTRIAN STUFF ******

9				// Ped subs table index

630				// Number of pedestrians

// Pedestrian number 1

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	5.259,-9.343,-4.543
	point
	5.259,-9.343,-4.543
	point
	4.451,996.000,-6.772
	point
	-3.686,996.000,-5.729
	point
	-7.395,996.000,-5.826
	reverse


// Pedestrian number 2

11				// Ref num
5				// Number of instructions
1				// Initial instruction

	point
	148.580,-5.177,36.716
	point
	148.238,-5.177,38.666
	point
	148.991,-5.177,44.640
	point
	136.110,-5.178,56.633
	reverse


// Pedestrian number 3

2				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	144.254,-5.116,28.687
	point
	149.087,-5.177,37.075
	point
	148.126,-5.177,43.342
	point
	148.930,-5.177,104.704
	reverse


// Pedestrian number 4

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	144.592,-5.177,39.950
	point
	147.111,-5.177,34.963
	point
	149.081,-5.177,29.866
	point
	144.220,-5.177,27.661
	reverse


// Pedestrian number 5

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	146.701,-5.177,37.813
	point
	142.899,-5.177,36.790
	point
	134.105,-5.177,32.951
	reverse


// Pedestrian number 6

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	145.705,-5.177,38.889
	point
	142.825,-5.177,37.021
	point
	140.413,-5.177,33.083
	reverse


// Pedestrian number 7

9				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	143.777,-5.177,44.822
	point
	143.469,-5.177,33.004
	reverse


// Pedestrian number 8

9				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	142.451,-5.177,39.728
	point
	148.901,-5.177,27.258
	point
	144.289,-5.177,15.066
	point
	150.267,-5.177,2.313
	point
	151.621,-5.177,-2.814
	reverse


// Pedestrian number 9

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	147.476,-5.177,-3.091
	point
	147.778,-5.177,2.357
	point
	148.948,-5.177,11.945
	point
	145.218,-5.177,39.315
	reverse


// Pedestrian number 10

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	147.245,-5.177,-2.660
	point
	147.422,-5.177,2.351
	point
	148.493,-5.177,53.797
	reverse


// Pedestrian number 11

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	143.997,-5.177,-2.967
	point
	144.348,-5.181,0.979
	point
	149.564,-5.177,7.073
	point
	144.239,-5.178,13.704
	point
	147.040,-5.171,37.454
	reverse


// Pedestrian number 12

10				// Ref num
7				// Number of instructions
5				// Initial instruction

	point
	147.804,-5.171,36.733
	point
	148.967,-5.174,19.044
	point
	144.139,-5.177,15.975
	point
	148.895,-5.176,10.141
	point
	145.006,-5.180,0.888
	point
	142.693,-5.182,-3.086
	reverse


// Pedestrian number 13

2				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	141.195,-5.171,52.129
	point
	146.447,-5.167,56.834
	point
	149.016,-5.164,67.117
	point
	143.908,-5.164,78.580
	reverse


// Pedestrian number 14

11				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	145.142,-5.170,48.666
	point
	146.040,-5.167,56.743
	point
	148.992,-5.166,59.274
	point
	148.890,-5.161,80.193
	point
	145.427,-5.162,80.697
	point
	127.017,-5.171,80.815
	reverse


// Pedestrian number 15

14				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	144.604,-5.170,48.790
	point
	144.784,-5.168,56.794
	point
	144.744,-5.163,78.635
	point
	137.363,-5.167,78.782
	point
	137.551,-5.166,80.446
	point
	138.783,-5.166,80.467
	reverse


// Pedestrian number 16

7				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	143.116,-5.170,49.918
	point
	144.329,-5.168,56.863
	point
	149.007,-5.163,72.414
	point
	149.037,-5.161,80.799
	point
	146.001,-5.161,84.185
	point
	144.329,-5.162,84.229
	point
	144.149,-5.163,82.185
	reverse


// Pedestrian number 17

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	136.226,-5.173,53.005
	point
	145.095,-5.167,60.482
	point
	148.938,-5.165,63.942
	point
	148.797,-5.163,71.161
	point
	140.826,-5.165,79.360
	reverse


// Pedestrian number 18

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	134.984,-5.170,70.103
	point
	141.940,-5.164,78.747
	point
	143.065,-5.164,80.378
	point
	144.667,-5.162,85.150
	reverse


// Pedestrian number 19

2				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	148.895,-5.162,75.639
	point
	142.329,-5.164,78.754
	point
	140.627,-5.165,80.446
	point
	137.155,-5.166,82.427
	reverse


// Pedestrian number 20

7				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	139.301,-5.165,80.480
	point
	142.204,-5.162,89.425
	point
	143.331,-5.161,91.465
	point
	143.338,-5.161,92.696
	point
	144.082,-5.160,93.146
	point
	144.619,-5.160,92.891
	reverse


// Pedestrian number 21

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	143.585,-5.160,95.289
	point
	141.933,-5.162,89.322
	point
	137.113,-5.166,82.900
	reverse


// Pedestrian number 22

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	137.987,-5.163,93.965
	point
	141.397,-5.162,89.191
	point
	145.043,-5.162,84.266
	reverse


// Pedestrian number 23

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	144.735,-5.162,84.200
	point
	141.687,-5.161,94.427
	point
	139.123,-5.162,95.934
	point
	135.867,-5.163,95.913
	point
	135.585,-5.163,99.305
	point
	136.435,-5.162,100.029
	reverse


// Pedestrian number 24

11				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	136.562,-5.166,84.824
	point
	141.822,-5.161,94.914
	point
	143.802,-5.159,97.710
	point
	145.254,-5.159,97.160
	reverse


// Pedestrian number 25

14				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	133.895,-5.163,99.849
	point
	139.094,-5.161,98.923
	point
	141.431,-5.161,94.893
	point
	145.224,-5.160,92.842
	point
	145.443,-5.159,95.319
	reverse


// Pedestrian number 26

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	139.314,-5.162,94.981
	point
	140.895,-5.161,95.065
	point
	148.889,-5.158,95.505
	point
	149.066,-5.155,104.623
	reverse


// Pedestrian number 27

9				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	138.505,-5.161,100.865
	point
	142.123,-5.159,100.773
	point
	142.040,-5.159,101.351
	point
	141.570,-5.160,101.529
	point
	135.367,-5.162,104.579
	point
	127.760,-5.166,101.406
	reverse


// Pedestrian number 28

9				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	132.306,-5.165,97.451
	point
	130.309,-5.165,99.145
	point
	132.148,-5.163,104.683
	point
	142.006,-5.159,101.402
	point
	149.021,-5.156,101.511
	reverse


// Pedestrian number 29

9				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	148.847,-5.156,104.028
	point
	139.837,-5.160,102.495
	point
	137.054,-5.162,101.941
	point
	134.853,-5.163,102.170
	point
	133.435,-5.164,98.211
	point
	131.505,-5.165,97.793
	reverse


// Pedestrian number 30

9				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	128.741,-5.172,73.167
	point
	129.923,-5.170,77.071
	point
	133.349,-5.168,78.306
	point
	134.363,-5.168,80.379
	point
	135.323,-5.166,84.533
	point
	136.281,-5.166,84.718
	reverse


// Pedestrian number 31


9				// Ref num
11				// Number of instructions
8				// Initial instruction

	point
	133.496,-5.170,71.673
	point
	131.635,-5.170,75.436
	point
	129.565,-5.171,75.515
	point
	128.102,-5.171,77.206
	point
	127.362,-5.171,80.109
	point
	132.332,-5.168,84.493
	point
	132.415,-5.167,86.629
	point
	139.540,-5.163,89.055
	point
	143.512,-5.161,93.068
	point
	144.031,-5.160,92.883
	reverse


// Pedestrian number 32

11				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	132.338,-5.164,99.011
	point
	132.235,-5.166,93.504
	point
	133.052,-5.166,90.396
	point
	132.402,-5.167,88.462
	point
	131.965,-5.169,80.072
	reverse


// Pedestrian number 33

2				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	132.262,-5.169,80.095
	point
	132.440,-5.167,88.946
	point
	132.148,-5.166,91.851
	point
	132.200,-5.165,97.168
	point
	131.129,-5.165,97.910
	reverse


// Pedestrian number 34

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	134.043,-5.165,94.001
	point
	139.604,-5.164,85.237
	point
	141.268,-5.165,79.506
	reverse


// Pedestrian number 35

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	133.401,-5.169,76.331
	point
	143.135,-5.166,70.197
	point
	148.826,-5.164,65.294
	point
	148.688,-5.177,1.481
	reverse


// Pedestrian number 36

9				// Ref num
8				// Number of instructions
5				// Initial instruction

	point
	149.009,-5.158,91.468
	point
	145.331,-5.161,89.047
	point
	145.377,-5.161,87.921
	point
	144.451,-5.162,86.963
	point
	136.559,-5.166,85.144
	point
	130.178,-5.169,83.124
	point
	127.489,-5.171,78.971
	reverse


// Pedestrian number 37

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	127.385,-5.171,81.080
	point
	132.079,-5.168,84.515
	point
	144.877,-5.161,88.533
	point
	145.166,-5.160,91.076
	reverse


// Pedestrian number 38

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	148.883,-5.159,88.109
	point
	145.324,-5.161,88.537
	point
	139.574,-5.162,93.486
	point
	139.030,-5.162,97.971
	point
	137.332,-5.162,100.176
	reverse


// Pedestrian number 39

7				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	143.077,-5.158,104.353
	point
	143.215,-5.160,97.599
	point
	144.354,-5.159,97.175
	point
	148.411,-5.157,98.481
	point
	148.988,-5.156,100.421
	point
	149.072,-5.156,103.392
	reverse


// Pedestrian number 40

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	139.858,-5.165,80.508
	point
	139.359,-5.163,88.792
	point
	138.815,-5.163,94.093
	reverse


// Pedestrian number 41

9				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	119.024,-5.193,-3.031
	point
	116.029,-5.193,4.572
	point
	116.080,-5.191,12.202
	point
	116.251,-5.188,24.406
	point
	117.389,-5.187,26.036
	reverse


// Pedestrian number 42

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	127.315,995.095,19.390
	point
	119.579,995.097,19.700
	point
	117.659,-5.097,21.913
	point
	116.390,995.107,23.348
	point
	112.473,993.665,24.532
	reverse


// Pedestrian number 43

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	117.436,-5.082,22.170
	point
	117.161,-5.111,12.516
	point
	116.275,-5.133,4.946
	point
	114.589,-5.177,-0.757
	reverse


// Pedestrian number 44

3				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	120.162,995.093,19.023
	point
	118.457,995.101,21.789
	point
	118.437,-5.096,22.805
	point
	116.600,-5.091,24.526
	point
	118.285,-5.086,26.308
	point
	117.745,-5.082,27.581
	point
	115.877,-5.075,30.135
	reverse


// Pedestrian number 45

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	118.225,-5.170,-2.976
	point
	114.526,995.050,4.151
	point
	113.986,994.246,5.729
	point
	112.309,993.695,16.303
	point
	108.810,992.246,18.753
	reverse


// Pedestrian number 46

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	111.988,-5.177,-3.004
	point
	113.429,995.024,3.929
	point
	110.864,993.039,7.128
	point
	119.692,995.023,7.898
	reverse


// Pedestrian number 47

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	110.798,-5.177,-2.889
	point
	110.473,995.023,4.146
	point
	109.567,992.539,6.684
	reverse


// Pedestrian number 48

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	109.453,-5.177,-2.846
	point
	107.556,995.023,4.284
	point
	106.814,991.933,7.184
	reverse


// Pedestrian number 49

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	107.201,-5.177,-2.890
	point
	104.780,995.023,4.253
	point
	103.732,991.933,7.748
	reverse


// Pedestrian number 50

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	119.780,-5.176,2.549
	point
	108.799,-5.177,1.129
	point
	104.653,-5.176,-1.010
	point
	104.148,-5.176,-3.052
	reverse


// Pedestrian number 51

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	119.733,-5.176,4.367
	point
	105.943,-5.176,-1.176
	point
	105.716,-5.176,-2.196
	reverse


// Pedestrian number 52

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	121.117,-5.177,-3.057
	point
	119.999,-5.177,0.192
	point
	116.464,-5.177,9.356
	point
	116.778,-5.177,28.088
	point
	117.441,-5.177,27.075
	reverse


// Pedestrian number 53

9				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	118.110,-5.177,36.445
	point
	119.144,-5.177,35.158
	point
	117.680,-5.177,29.237
	point
	116.412,-5.177,25.790
	point
	117.301,-5.177,25.110
	reverse


// Pedestrian number 54

10				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	100.303,-5.172,33.273
	point
	115.404,-5.171,32.720
	point
	115.892,-5.173,33.532
	point
	116.171,-5.183,38.176
	point
	117.564,-5.184,38.351
	point
	129.654,-5.203,46.534
	reverse


// Pedestrian number 55

2				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	100.326,-5.172,33.581
	point
	115.218,-5.179,36.451
	point
	119.682,-5.196,43.729
	point
	124.372,-5.207,48.684
	point
	124.423,-5.211,50.454
	point
	122.925,-5.213,51.052
	reverse


// Pedestrian number 56

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	125.070,-5.176,37.249
	point
	129.272,-5.176,33.309
	point
	137.805,-5.176,33.126
	point
	144.347,-5.176,40.159
	reverse


// Pedestrian number 57

10				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	124.559,-5.176,33.013
	point
	131.781,-5.176,41.633
	point
	132.745,-5.176,44.494
	point
	136.346,-5.176,47.987
	point
	139.698,-5.176,47.964
	point
	143.251,-5.176,44.404
	point
	143.736,-5.176,32.905
	reverse


// Pedestrian number 58

14				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	138.775,-5.176,33.119
	point
	143.216,-5.176,40.474
	point
	143.406,-5.176,45.027
	point
	138.809,-5.176,48.599
	point
	138.092,-5.176,47.941
	point
	135.662,-5.176,48.187
	reverse


// Pedestrian number 59

7				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	122.559,-5.176,50.575
	point
	118.410,-5.176,53.316
	point
	113.382,-5.176,56.633
	point
	113.469,-5.176,58.088
	point
	124.512,-5.176,64.455
	reverse


// Pedestrian number 60

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	115.311,-5.176,50.997
	point
	118.376,-5.176,55.256
	point
	124.442,-5.176,59.450
	reverse


// Pedestrian number 61

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	113.158,-5.176,59.141
	point
	119.060,-5.176,62.251
	point
	124.407,-5.176,66.067
	point
	123.867,-5.176,68.751
	reverse


// Pedestrian number 62

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	113.132,-5.176,52.420
	point
	117.606,-5.176,55.493
	point
	124.733,-5.176,58.484
	point
	124.733,-5.176,58.484
	reverse


// Pedestrian number 63

11				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	124.700,-5.176,51.872
	point
	118.164,-5.176,56.960
	point
	113.138,-5.176,62.609
	point
	114.397,-5.176,68.663
	point
	110.901,-5.176,72.749
	reverse


// Pedestrian number 64

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	113.011,-5.176,65.366
	point
	119.585,-5.176,61.064
	point
	124.619,-5.176,56.935
	reverse


// Pedestrian number 65

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	124.628,-5.176,61.948
	point
	120.149,-5.176,58.724
	point
	114.592,-5.176,50.970
	reverse


// Pedestrian number 66

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	128.732,-5.176,71.806
	point
	120.664,-5.176,69.986
	point
	117.618,-5.176,68.368
	reverse


// Pedestrian number 67

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	113.209,-5.176,66.188
	point
	117.588,-5.176,67.880
	point
	120.157,-5.176,70.183
	point
	125.738,-5.176,72.899
	point
	128.000,-5.176,72.440
	reverse


// Pedestrian number 68

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	108.920,-5.176,71.631
	point
	114.841,-5.176,67.518
	point
	124.567,-5.176,62.353
	reverse


// Pedestrian number 69

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	129.526,-5.176,70.963
	point
	119.960,-5.176,71.689
	point
	114.000,-5.176,74.105
	reverse


// Pedestrian number 70

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	122.026,-6.382,89.475
	point
	120.021,993.818,87.119
	point
	116.228,995.023,69.827
	reverse


// Pedestrian number 71

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	128.171,995.023,86.499
	point
	120.359,993.818,86.653
	point
	116.437,993.818,88.197
	point
	112.245,994.949,90.212
	reverse


// Pedestrian number 72

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	119.288,-6.382,91.387
	point
	120.609,-6.382,96.806
	point
	117.862,994.949,100.570
	reverse


// Pedestrian number 73

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	115.297,-5.170,69.804
	point
	114.288,-5.170,77.636
	point
	114.030,-5.170,80.207
	reverse


// Pedestrian number 74

9				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	125.467,-5.227,99.186
	point
	123.345,-6.382,96.769
	point
	120.113,-6.381,91.023
	point
	121.179,-6.381,90.091
	point
	122.357,-6.381,87.676
	reverse


// Pedestrian number 75

9				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	123.492,-6.381,86.978
	point
	123.411,-6.381,88.038
	point
	121.015,-6.381,88.401
	point
	119.947,994.019,91.017
	point
	114.912,994.983,98.949
	reverse


// Pedestrian number 76

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	122.982,-6.382,91.586
	point
	122.538,-6.382,93.147
	point
	119.463,994.018,93.398
	point
	112.210,994.957,96.609
	reverse


// Pedestrian number 77

10				// Ref num
9				// Number of instructions
3				// Initial instruction

	point
	112.226,994.954,96.076
	point
	111.997,995.023,94.950
	point
	106.584,995.023,95.373
	point
	90.790,-5.177,92.778
	point
	89.136,-5.177,81.603
	point
	83.739,-5.177,78.080
	point
	67.711,-5.177,79.431
	point
	63.282,-5.177,84.520
	reverse


// Pedestrian number 78

10				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	131.752,-5.177,67.911
	point
	125.398,-5.177,68.475
	point
	122.933,-5.177,67.370
	point
	120.620,-5.177,67.346
	point
	113.046,-5.177,64.949
	reverse


// Pedestrian number 79

9				// Ref num
8				// Number of instructions
6				// Initial instruction

	point
	121.546,-5.177,50.222
	point
	118.110,-5.177,53.598
	point
	120.149,-5.177,56.144
	point
	117.521,-5.177,59.421
	point
	119.876,-5.177,62.558
	point
	118.420,-5.177,65.240
	point
	119.560,-5.177,68.893
	reverse


// Pedestrian number 80

11				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	122.432,993.818,85.069
	point
	122.068,995.023,80.262
	point
	120.716,-5.177,73.782
	point
	116.852,-5.177,69.607
	reverse


// Pedestrian number 81

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	122.980,-6.381,91.687
	point
	119.917,-6.381,91.526
	point
	119.795,993.819,90.534
	point
	112.324,995.023,67.628
	reverse


// Pedestrian number 82

11				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	126.058,-5.217,98.627
	point
	123.958,-6.382,96.814
	point
	121.246,-6.382,91.276
	point
	121.651,-6.382,88.330
	point
	122.603,-6.382,88.239
	point
	123.649,-6.382,87.614
	point
	123.586,-6.382,85.714
	reverse


// Pedestrian number 83

10				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	113.119,-5.268,82.952
	point
	116.026,-6.382,84.841
	point
	120.052,-6.381,90.173
	point
	121.437,-6.381,91.649
	point
	123.992,-6.382,92.084
	point
	127.794,-5.239,90.855
	reverse


// Pedestrian number 84

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	127.969,-5.192,87.350
	point
	124.019,-6.382,88.134
	point
	121.359,-6.382,88.150
	point
	116.036,-6.382,89.314
	point
	112.342,994.918,90.169
	reverse


// Pedestrian number 85

14				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	114.454,994.934,98.980
	point
	116.092,-6.382,96.812
	point
	118.838,-6.382,91.108
	point
	122.473,-6.382,87.723
	reverse


// Pedestrian number 86

11				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	118.306,-5.209,100.727
	point
	118.172,-6.382,96.783
	point
	118.651,-6.382,93.229
	point
	118.875,-6.382,87.943
	point
	122.059,-6.382,86.082
	reverse


// Pedestrian number 87

11				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	112.174,-5.230,96.330
	point
	116.018,-6.382,95.693
	point
	116.477,-6.382,93.154
	point
	122.543,-6.382,91.641
	reverse


// Pedestrian number 88

13				// Ref num
9				// Number of instructions
3				// Initial instruction

	point
	127.180,995.023,95.266
	point
	111.063,995.023,94.203
	point
	93.734,-5.177,94.565
	point
	90.272,-5.177,92.227
	point
	87.969,-5.177,82.370
	point
	85.290,-5.177,77.520
	point
	66.593,-5.176,77.832
	point
	65.473,-5.198,75.430
	reverse


// Pedestrian number 89

9				// Ref num
10				// Number of instructions
5				// Initial instruction

	point
	113.206,995.023,97.521
	point
	111.964,995.023,95.583
	point
	103.291,-5.177,95.236
	point
	97.658,-5.177,94.914
	point
	89.785,-5.177,91.127
	point
	87.673,-5.177,81.046
	point
	85.439,-5.177,79.180
	point
	83.682,-5.177,79.021
	point
	57.049,-5.211,78.595
	reverse


// Pedestrian number 90

16				// Ref num
10				// Number of instructions
5				// Initial instruction

	point
	94.053,-5.177,94.640
	point
	93.146,-5.177,92.682
	point
	91.697,-5.177,91.466
	point
	91.000,-5.177,90.030

	point
	90.280,-5.177,86.453
	point
	88.652,-5.177,80.217
	point
	84.779,-5.177,79.140
	point
	71.990,-5.177,77.805
	point
	53.657,-5.212,83.482
	reverse


// Pedestrian number 91

16				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	63.342,-5.207,75.371
	point
	64.873,-5.177,79.716
	point
	67.857,-5.177,84.533
	reverse


// Pedestrian number 92

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	67.196,-5.177,84.563
	point
	67.694,-5.177,79.828
	point
	67.862,-5.176,77.835
	reverse


// Pedestrian number 93

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	53.551,-5.179,85.812
	point
	64.881,-5.177,80.167
	point
	81.326,-5.177,77.343
	reverse


// Pedestrian number 94

11				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	10.699,-5.177,88.485
	point
	12.438,-5.177,88.487
	point
	12.483,-5.177,87.845
	point
	19.147,-5.177,87.228
	point
	19.861,-5.177,88.429
	reverse


// Pedestrian number 95

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	10.550,-5.177,87.229
	point
	18.856,-5.177,86.839
	point
	19.162,-5.177,88.085
	point
	18.215,-5.177,92.513
	reverse


// Pedestrian number 96

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	20.981,-5.177,85.211
	point
	18.481,-5.177,87.422
	point
	10.529,-5.177,80.923
	reverse


// Pedestrian number 97

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.175,-5.177,92.576
	point
	23.174,-5.177,87.505
	point
	10.651,-5.177,82.066
	reverse


// Pedestrian number 98

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	14.412,-5.177,92.385
	point
	14.702,-5.177,90.543
	point
	15.758,-5.177,88.428
	point
	31.698,-5.177,83.717
	reverse


// Pedestrian number 99

11				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	10.616,-5.177,92.646
	point
	10.598,-5.177,90.046
	point
	12.620,-5.177,89.487
	point
	13.602,-5.177,88.352
	point
	18.961,995.023,84.937
	point
	20.767,991.481,80.133
	reverse


// Pedestrian number 100

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	18.177,-5.177,88.387
	point
	13.201,-5.177,87.795
	point
	11.902,-5.177,89.962
	point
	10.510,-5.177,89.733
	reverse


// Pedestrian number 101

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	18.759,995.023,88.292
	point
	22.617,995.912,82.605
	point
	22.421,995.023,49.442
	point
	28.094,-5.177,45.793
	reverse


// Pedestrian number 102

16				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	15.699,-5.177,46.170
	point
	21.360,995.023,50.745
	point
	21.318,995.023,86.560
	point
	20.846,-5.177,88.171
	reverse


// Pedestrian number 103

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.243,995.023,92.528
	point
	21.506,996.699,77.186
	point
	19.373,986.858,75.038
	reverse


// Pedestrian number 104

6				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.725,995.023,92.397
	point
	22.520,996.705,77.123
	point
	23.341,991.480,69.365
	reverse


// Pedestrian number 105

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	31.071,-5.177,64.052
	point
	30.458,-5.177,73.853
	point
	31.178,995.023,84.337
	point
	31.573,995.023,92.543
	reverse


// Pedestrian number 106

6				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	20.874,-5.177,52.518
	point
	21.046,-5.177,48.452
	point
	22.652,-5.177,43.328
	reverse


// Pedestrian number 107

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.234,-5.177,52.545
	point
	22.800,-5.177,47.818
	point
	19.145,-5.177,40.542
	reverse


// Pedestrian number 108

6				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	10.641,-5.177,59.783
	point
	20.460,-5.177,50.253
	point
	24.445,-5.177,43.993
	reverse


// Pedestrian number 109

16				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	10.716,-5.177,47.813
	point
	14.346,-5.177,47.825
	point
	20.462,-5.177,49.433
	point
	30.904,-5.177,47.615
	point
	35.638,-5.177,47.911
	reverse


// Pedestrian number 110

5				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	24.906,-5.177,42.026
	point
	26.079,-5.177,42.372
	point
	26.390,-5.177,43.328
	point
	25.587,-5.177,44.526
	point
	16.121,-5.177,50.262
	reverse


// Pedestrian number 111

3				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	35.474,-5.177,47.135
	point
	29.920,-5.177,47.820
	point
	22.494,-5.177,44.825
	point
	20.913,-5.177,43.099
	point
	20.741,-5.177,40.504
	point
	27.684,-5.177,41.001
	reverse


// Pedestrian number 112

10				// Ref num
5				// Number of instructions
4				// Initial instruction

	point
	133.936,-5.177,-1.453
	point
	132.525,-5.177,-1.433
	point
	132.103,-5.177,-0.853
	point
	132.315,-5.177,-0.374
	reverse


// Pedestrian number 113

134				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	146.850,-5.177,9.438
	reverse


// Pedestrian number 114

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	147.986,-5.178,13.691
	reverse


// Pedestrian number 115

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	146.724,-5.178,15.651
	reverse


// Pedestrian number 116

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.828,-5.177,22.999
	reverse


// Pedestrian number 117

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	137.937,-5.178,35.283
	reverse


// Pedestrian number 118

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	143.518,-5.177,42.189
	reverse


// Pedestrian number 119

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.858,-5.178,46.227
	reverse


// Pedestrian number 120

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.314,-5.177,48.235
	reverse


// Pedestrian number 121

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.141,-5.178,47.152
	reverse


// Pedestrian number 122

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.708,-5.178,54.174
	reverse


// Pedestrian number 123

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.343,-5.179,59.299
	reverse


// Pedestrian number 124

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.565,-5.177,65.294
	reverse


// Pedestrian number 125

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	129.180,-5.177,76.511
	reverse


// Pedestrian number 126

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	128.986,-5.178,77.055
	reverse


// Pedestrian number 127

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	128.949,-5.178,77.850
	reverse


// Pedestrian number 128

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	129.045,-5.178,78.852
	reverse


// Pedestrian number 129

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	128.169,-5.178,78.479
	reverse


// Pedestrian number 130

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	128.319,-5.177,77.301
	reverse


// Pedestrian number 131

134				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	133.663,-5.178,82.717
	reverse


// Pedestrian number 132

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.801,-5.162,94.634
	reverse


// Pedestrian number 133

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.691,-5.166,96.265
	reverse


// Pedestrian number 134

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.862,-5.170,98.456
	reverse


// Pedestrian number 135

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	134.040,-5.185,102.163
	reverse


// Pedestrian number 136

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.947,-5.152,101.586
	reverse


// Pedestrian number 137

123				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	142.165,-5.152,101.608
	reverse


// Pedestrian number 138

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.763,-5.128,97.390
	reverse


// Pedestrian number 139

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.194,-5.131,97.825
	reverse


// Pedestrian number 140

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	119.091,-5.177,26.709
	reverse


// Pedestrian number 141

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	118.693,-5.177,24.667
	reverse


// Pedestrian number 142

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.087,-5.177,88.244
	reverse


// Pedestrian number 143

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	127.042,-5.177,19.680
	reverse


// Pedestrian number 144

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	126.807,-5.177,14.509
	reverse


// Pedestrian number 145

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	126.122,-5.177,14.503
	reverse


// Pedestrian number 146

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	125.473,-5.177,14.498
	reverse


// Pedestrian number 147

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	124.353,-5.177,14.488
	reverse


// Pedestrian number 148

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.956,-5.177,14.475
	reverse


// Pedestrian number 149

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	126.097,-5.177,10.081
	reverse


// Pedestrian number 150

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	125.438,-5.177,10.066
	reverse


// Pedestrian number 151

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	124.792,-5.177,10.052
	reverse


// Pedestrian number 152

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	123.752,-5.177,10.028
	reverse


// Pedestrian number 153

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.879,-5.177,-1.327
	reverse


// Pedestrian number 154

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.930,-5.177,-0.244
	reverse


// Pedestrian number 155

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.907,-5.177,-2.053
	reverse


// Pedestrian number 156

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.395,-5.177,9.981
	reverse


// Pedestrian number 157

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.433,-5.177,11.038
	reverse


// Pedestrian number 158

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.390,-5.177,11.605
	reverse


// Pedestrian number 159

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.248,-5.177,12.765
	reverse


// Pedestrian number 160

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.212,-5.177,15.593
	reverse


// Pedestrian number 161

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	89.663,-5.177,35.720
	reverse


// Pedestrian number 162

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.575,-5.177,36.837
	reverse


// Pedestrian number 163

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	92.585,-5.177,38.819
	reverse


// Pedestrian number 164

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	97.049,-5.193,38.469
	reverse


// Pedestrian number 165

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	94.077,-5.177,41.831
	reverse


// Pedestrian number 166

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	94.277,-5.177,43.916
	reverse


// Pedestrian number 167

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	95.331,-5.177,45.307
	reverse


// Pedestrian number 168

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	96.414,-5.177,46.457
	reverse


// Pedestrian number 169

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	100.811,-5.177,48.188
	reverse


// Pedestrian number 170

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.493,-5.177,45.316
	reverse


// Pedestrian number 171

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	113.191,-5.177,49.534
	reverse


// Pedestrian number 172

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	124.555,-5.177,51.183
	reverse


// Pedestrian number 173

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.611,-5.177,55.320
	reverse


// Pedestrian number 174

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	116.287,-5.177,62.184
	reverse


// Pedestrian number 175

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	108.684,-5.177,63.533
	reverse


// Pedestrian number 176

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	129.569,-5.177,58.676
	reverse


// Pedestrian number 177

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.923,-6.382,86.474
	reverse


// Pedestrian number 178

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	123.886,-6.382,90.637
	reverse


// Pedestrian number 179

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	123.855,-6.382,89.819
	reverse


// Pedestrian number 180

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.806,-5.177,69.801
	reverse


// Pedestrian number 181

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.759,-5.177,70.355
	reverse


// Pedestrian number 182

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.722,-5.177,70.900
	reverse


// Pedestrian number 183

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.700,-5.177,79.771
	reverse


// Pedestrian number 184

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.643,-5.177,78.997
	reverse


// Pedestrian number 185

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.600,-5.177,78.091
	reverse


// Pedestrian number 186

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	55.165,-5.177,80.863
	reverse


// Pedestrian number 187

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.331,-5.177,78.676
	reverse


// Pedestrian number 188

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.324,-5.177,71.843
	reverse


// Pedestrian number 189

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.380,-5.177,70.670
	reverse


// Pedestrian number 190

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.246,-5.177,63.437
	reverse


// Pedestrian number 191

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.078,-5.177,60.795
	reverse


// Pedestrian number 192

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.525,-5.177,56.545
	reverse


// Pedestrian number 193

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.978,-8.720,68.311
	reverse


// Pedestrian number 194

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.888,-8.720,68.244
	reverse


// Pedestrian number 195

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	22.233,-8.720,68.192
	reverse


// Pedestrian number 196

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	22.709,-8.720,68.618
	reverse


// Pedestrian number 197

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	22.282,-8.720,68.934
	reverse


// Pedestrian number 198

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	21.279,-8.720,69.059
	reverse


// Pedestrian number 199

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.421,-8.720,69.364
	reverse


// Pedestrian number 200

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	21.503,-8.720,68.656
	reverse


// Pedestrian number 201

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	30.387,-17.799,68.882
	reverse


// Pedestrian number 202

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.497,-5.177,47.325
	reverse


// Pedestrian number 203

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.548,-5.177,47.915
	reverse


// Pedestrian number 204

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.532,-5.177,47.610
	reverse


// Pedestrian number 205

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.521,-5.177,39.328
	reverse


// Pedestrian number 206

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.484,-5.177,29.586
	reverse


// Pedestrian number 207

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.442,-5.177,33.837
	reverse


// Pedestrian number 208

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.366,-5.177,34.520
	reverse


// Pedestrian number 209

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.209,-5.177,35.142
	reverse


// Pedestrian number 210

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.786,-5.177,35.299
	reverse


// Pedestrian number 211

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	33.397,-5.177,39.101
	reverse


// Pedestrian number 212

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.247,-5.176,37.950
	reverse


// Pedestrian number 213

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.456,-5.176,37.923
	reverse


// Pedestrian number 214

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.626,-5.176,38.032
	reverse


// Pedestrian number 215

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.743,-5.176,42.969
	reverse


// Pedestrian number 216

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.642,-5.176,43.643
	reverse


// Pedestrian number 217

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	28.982,-5.176,46.464
	reverse


// Pedestrian number 218

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.476,-5.176,48.741
	reverse


// Pedestrian number 219

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.756,-5.176,46.640
	reverse


// Pedestrian number 220

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	92.766,-0.256,16.799
	point
	98.986,-0.251,15.853
	point
	103.945,999.952,13.516
	point
	116.058,995.046,12.687
	reverse


// Pedestrian number 221

6				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	103.420,-0.249,17.419
	point
	106.542,999.954,15.193
	point
	116.467,995.203,14.901
	reverse


// Pedestrian number 222

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	95.316,-0.255,12.289
	point
	107.109,999.954,14.278
	point
	113.265,993.967,13.823
	reverse


// Pedestrian number 223

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	94.201,-0.256,12.250
	point
	105.400,999.953,15.854
	point
	109.874,992.657,15.900
	reverse


// Pedestrian number 224

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	93.615,-0.256,17.314
	point
	106.594,999.954,13.251
	point
	111.426,993.254,11.904
	reverse


// Pedestrian number 225

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	106.945,999.954,14.649
	point
	109.367,992.461,14.705
	reverse


// Pedestrian number 226

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	92.925,-0.257,12.228
	point
	106.200,999.953,16.374
	point
	113.560,994.080,16.047
	reverse


// Pedestrian number 227

6				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	96.351,-0.254,17.098
	point
	100.055,-0.251,12.710
	point
	106.389,999.954,15.829
	point
	109.290,992.431,16.114
	reverse


// Pedestrian number 228

14				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	97.163,-0.253,12.309
	point
	100.253,-0.251,17.430
	point
	104.092,999.952,16.450
	point
	110.259,992.806,13.956
	reverse


// Pedestrian number 229

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.344,-4.071,89.907
	reverse


// Pedestrian number 230

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.322,-4.071,88.807
	reverse


// Pedestrian number 231

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.306,-4.071,87.987
	reverse


// Pedestrian number 232

137				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.327,-4.071,92.553
	reverse


// Pedestrian number 233

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.059,-4.071,92.540
	reverse


// Pedestrian number 234

133				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.443,-4.071,88.813
	reverse


// Pedestrian number 235

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.291,-4.071,91.521
	reverse


// Pedestrian number 236

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.147,-4.071,90.316
	reverse


// Pedestrian number 237

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.884,-4.071,91.903
	reverse


// Pedestrian number 238

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.895,-4.071,91.277
	reverse


// Pedestrian number 239

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.903,-4.071,90.763
	reverse


// Pedestrian number 240

123				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.792,-4.071,88.930
	reverse


// Pedestrian number 241

120				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	18.566,-5.177,87.880
	reverse


// Pedestrian number 242

120				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	14.677,-5.177,92.255
	reverse


// Pedestrian number 243

122				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.350,-4.071,28.296
	reverse


// Pedestrian number 244

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.316,-4.071,29.211
	reverse


// Pedestrian number 245

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.279,-4.071,30.218
	reverse


// Pedestrian number 246

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.244,-4.071,31.147
	reverse


// Pedestrian number 247

124				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.938,-4.071,29.194
	reverse


// Pedestrian number 248

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.039,-4.071,25.283
	reverse


// Pedestrian number 249

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.970,-4.071,25.247
	reverse


// Pedestrian number 250

108				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.345,-4.071,26.272
	reverse


// Pedestrian number 251

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.934,-4.071,26.253
	reverse


// Pedestrian number 252

104				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.957,-4.071,27.000
	reverse


// Pedestrian number 253

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.731,-4.071,47.830
	reverse


// Pedestrian number 254

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.778,-4.071,48.414
	reverse


// Pedestrian number 255

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.793,-4.071,47.161
	reverse


// Pedestrian number 256

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	34.491,995.134,33.191
	point
	45.091,996.831,34.757
	point
	54.256,998.744,29.217
	point
	55.989,982.487,27.571
	reverse


// Pedestrian number 257

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	56.608,982.407,28.441
	point
	54.181,998.768,28.280
	point
	44.139,996.780,31.776
	point
	42.799,996.392,35.506
	reverse


// Pedestrian number 258

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	63.072,982.407,24.164
	point
	59.148,999.703,26.421
	point
	56.091,999.169,27.711
	reverse


// Pedestrian number 259

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	62.185,1000.259,24.345
	point
	60.206,999.864,26.420
	point
	55.903,999.143,27.522
	reverse


// Pedestrian number 260

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	30.213,-17.799,65.743
	reverse


// Pedestrian number 261

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	31.217,-17.799,60.523
	reverse


// Pedestrian number 262

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.755,-17.799,58.092
	reverse


// Pedestrian number 263

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.265,-17.799,56.054
	reverse


// Pedestrian number 264

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.573,-17.799,54.288
	reverse


// Pedestrian number 265

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	36.608,-17.799,52.892
	reverse


// Pedestrian number 266

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	38.079,-17.799,50.907
	reverse


// Pedestrian number 267

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	42.048,-17.799,45.552
	reverse


// Pedestrian number 268

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	45.800,-17.799,40.489
	reverse


// Pedestrian number 269

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	49.856,-17.799,35.014
	reverse


// Pedestrian number 270

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	63.685,-17.799,16.587
	reverse


// Pedestrian number 271

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	57.460,-17.799,24.938
	reverse


// Pedestrian number 272

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	106.342,-8.267,22.577
	reverse


// Pedestrian number 273

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	106.261,-8.267,15.779
	reverse


// Pedestrian number 274

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	106.175,-8.267,7.589
	reverse


// Pedestrian number 275

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	100.043,-8.267,7.109
	reverse


// Pedestrian number 276

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	99.130,-8.267,22.779
	reverse


// Pedestrian number 277

10				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	60.265,-1.777,93.292
	point
	58.996,-1.850,89.351
	point
	56.635,-1.850,87.113
	point
	52.649,998.350,85.886
	point
	22.832,995.021,85.745
	reverse


// Pedestrian number 278

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	49.955,998.026,85.816
	point
	52.540,998.349,86.701
	point
	53.288,998.349,89.250
	reverse


// Pedestrian number 279

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	46.554,998.349,85.642
	point
	52.486,998.349,87.261
	point
	54.698,998.350,89.155
	reverse


// Pedestrian number 280

3				// Ref num
10				// Number of instructions
2				// Initial instruction

	point
	49.246,998.349,87.512
	point
	53.132,998.349,87.979
	point
	55.317,998.350,89.195
	point
	56.714,998.350,90.569
	point
	57.456,998.350,92.244
	point
	57.730,998.350,93.925
	point
	57.854,998.351,111.901
	point
	56.691,998.351,113.039
	point
	53.419,995.252,107.879
	reverse


// Pedestrian number 281

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	31.855,995.023,92.589
	point
	30.617,995.479,87.603
	point
	27.570,995.268,78.783
	reverse


// Pedestrian number 282

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	32.156,995.584,77.851
	point
	30.655,995.481,86.632
	point
	29.205,995.607,96.044
	reverse


// Pedestrian number 283

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	28.157,995.841,97.337
	point
	30.417,995.466,87.200
	point
	31.754,995.558,84.166
	reverse


// Pedestrian number 284

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.817,996.366,100.239
	point
	29.778,995.421,86.644
	point
	31.680,995.552,81.663
	reverse


// Pedestrian number 285

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.946,995.157,80.223
	point
	29.949,995.433,87.109
	point
	31.593,995.546,90.334
	reverse


// Pedestrian number 286

7				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	25.177,996.303,99.900
	point
	24.410,996.363,100.228
	point
	24.855,997.541,106.746
	point
	24.809,997.808,108.222
	reverse


// Pedestrian number 287

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.264,997.840,108.401
	point
	25.570,997.604,107.093
	point
	27.301,997.327,106.252
	reverse


// Pedestrian number 288

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	57.296,-5.210,89.441
	point
	57.957,-5.210,89.482
	point
	60.907,-5.204,88.090
	point
	64.219,-5.197,86.580
	reverse


// Pedestrian number 289

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	57.613,-5.206,87.987
	point
	60.461,-5.205,88.332
	point
	64.057,-5.206,90.147
	point
	65.609,-5.209,91.880
	reverse


// Pedestrian number 290

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.867,-5.208,88.627
	point
	60.692,-5.211,91.021
	point
	63.600,-5.219,95.327
	reverse


// Pedestrian number 291

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	64.790,-5.205,90.078
	point
	60.245,-5.207,91.177
	point
	53.448,-5.215,95.805
	point
	53.418,-5.234,106.855
	reverse


// Pedestrian number 292

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	64.077,-5.212,98.421
	point
	59.205,-5.212,90.503
	point
	56.434,-5.212,89.225
	point
	56.472,-5.212,88.725
	point
	54.654,-5.212,81.561
	reverse


// Pedestrian number 293

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.468,-5.135,113.773
	point
	59.151,-5.133,112.094
	point
	61.601,-5.213,109.651
	reverse


// Pedestrian number 294

14				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	53.420,-5.213,104.653
	point
	56.782,-5.213,107.164
	point
	59.722,-5.213,111.644
	point
	61.165,-5.213,113.089
	point
	60.003,-5.213,113.933
	point
	57.581,-5.213,114.008
	reverse


// Pedestrian number 295

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	61.682,-5.213,108.019
	point
	59.292,-5.213,111.628
	point
	57.296,-5.213,112.821
	point
	58.546,-5.213,113.775
	point
	61.245,-5.213,114.067
	reverse


// Pedestrian number 296

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	56.992,-5.213,108.728
	point
	58.524,-5.213,111.473
	point
	61.339,-5.213,112.939
	reverse


// Pedestrian number 297

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.566,-5.213,89.381
	point
	58.898,-5.235,109.851
	point
	58.782,-5.241,113.617
	reverse


// Pedestrian number 298

10				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	53.690,-1.338,129.740
	point
	56.758,-1.338,129.097
	point
	56.541,-1.338,125.835
	point
	57.954,998.862,116.909
	point
	57.479,998.862,114.982
	reverse


// Pedestrian number 299

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	57.746,-1.338,130.085
	point
	58.358,-1.338,123.642
	point
	58.317,998.862,116.888
	point
	59.022,998.862,112.015
	point
	61.435,998.862,109.842
	reverse


// Pedestrian number 300

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	55.849,-1.338,123.646
	point
	58.783,-1.338,123.441
	point
	63.107,998.862,117.031
	point
	63.037,998.862,114.258
	point
	60.031,998.862,78.752
	reverse


// Pedestrian number 301

3				// Ref num
8				// Number of instructions
6				// Initial instruction

	point
	53.639,-1.338,128.150
	point
	53.719,-1.338,127.008
	point
	43.974,-1.338,126.116
	point
	35.133,-1.338,126.767
	point
	31.606,-1.338,121.500
	point
	29.171,998.861,114.066
	point
	28.971,998.842,110.732
	reverse


// Pedestrian number 302

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	27.416,998.839,110.192
	point
	28.238,998.861,114.027
	point
	29.358,-1.318,117.771
	point
	34.638,-1.295,121.754
	point
	40.023,-1.338,129.216
	point
	55.740,-1.338,127.150
	reverse


// Pedestrian number 303

9				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	27.749,998.862,111.285
	point
	29.752,998.861,114.033
	point
	30.472,-1.338,119.654
	point
	41.481,-1.338,128.922
	point
	53.780,-1.338,125.299
	point
	54.731,-1.338,123.653
	reverse


// Pedestrian number 304

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	27.418,997.457,109.161
	point
	26.546,997.467,107.130
	point
	25.937,996.878,103.432
	point
	12.162,995.439,95.119
	reverse


// Pedestrian number 305

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	24.344,998.020,109.498
	point
	25.321,997.416,106.807
	point
	26.751,997.125,104.981
	reverse


// Pedestrian number 306

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.413,997.269,105.880
	point
	24.109,997.511,107.401
	point
	24.927,997.822,109.354
	reverse


// Pedestrian number 307

14				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	21.554,996.679,102.176
	point
	22.157,995.352,93.835
	point
	19.712,995.023,91.018
	point
	19.177,-5.177,91.012
	point
	18.418,-5.177,88.578
	reverse


// Pedestrian number 308

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	50.414,1.529,133.325
	reverse


// Pedestrian number 309

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.075,1.529,127.907
	reverse


// Pedestrian number 310

133				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	51.803,1.529,130.399
	reverse


// Pedestrian number 311

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.039,1.529,126.439
	reverse


// Pedestrian number 312

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.122,1.529,124.904
	reverse


// Pedestrian number 313

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.078,1.529,124.011
	reverse


// Pedestrian number 314

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.047,1.529,122.953
	reverse


// Pedestrian number 315

108				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.717,1.528,129.893
	reverse


// Pedestrian number 316

119				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.815,1.520,115.841
	reverse


// Pedestrian number 317

119				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	45.264,1.519,114.500
	reverse


// Pedestrian number 318

122				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.060,1.513,107.302
	reverse


// Pedestrian number 319

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	44.263,1.530,132.595
	reverse


// Pedestrian number 320

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	47.770,1.530,132.701
	reverse


// Pedestrian number 321

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.512,1.520,118.420
	reverse


// Pedestrian number 322

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	4.612,1.513,107.198
	reverse


// Pedestrian number 323

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	5.068,1.505,94.433
	reverse


// Pedestrian number 324

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.372,1.505,93.665
	reverse


// Pedestrian number 325

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.380,1.508,98.268
	reverse


// Pedestrian number 326

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.372,1.509,100.821
	reverse


// Pedestrian number 327

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	25.589,1.529,100.856
	reverse


// Pedestrian number 328

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.311,0.856,93.642
	reverse


// Pedestrian number 329

137				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	37.774,0.996,90.692
	reverse


// Pedestrian number 330

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	75.411,1.529,79.422
	reverse


// Pedestrian number 331

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	75.676,1.529,85.317
	reverse


// Pedestrian number 332

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	75.609,1.529,95.507
	reverse


// Pedestrian number 333

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	73.004,1.451,124.541
	reverse


// Pedestrian number 334

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.258,1.451,122.539
	reverse


// Pedestrian number 335

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.246,1.451,116.437
	reverse


// Pedestrian number 336

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.294,1.451,111.914
	reverse


// Pedestrian number 337

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.275,1.513,109.040
	reverse


// Pedestrian number 338

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.652,1.529,106.207
	reverse


// Pedestrian number 339

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	62.905,1.529,74.977
	reverse


// Pedestrian number 340

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.450,1.529,70.389
	reverse


// Pedestrian number 341

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.088,1.524,86.542
	reverse


// Pedestrian number 342

123				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	50.913,1.448,104.027
	reverse


// Pedestrian number 343

122				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	49.759,1.408,103.951
	reverse


// Pedestrian number 344

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	48.074,1.374,103.921
	reverse


// Pedestrian number 345

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.345,-3.201,112.850
	reverse


// Pedestrian number 346

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	59.877,-5.213,113.348
	reverse


// Pedestrian number 347

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	58.546,-5.213,113.292
	reverse


// Pedestrian number 348

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.784,-5.213,94.482
	reverse


// Pedestrian number 349

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.844,-5.202,89.109
	reverse


// Pedestrian number 350

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	61.898,-5.193,79.494
	reverse


// Pedestrian number 351

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	63.177,-5.193,77.921
	reverse


// Pedestrian number 352

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	56.583,-5.206,88.654
	reverse


// Pedestrian number 353

110				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.369,-5.183,77.322
	reverse


// Pedestrian number 354

110				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.346,-5.181,81.038
	reverse


// Pedestrian number 355

125				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.728,-5.659,85.604
	reverse


// Pedestrian number 356

120				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.075,-5.659,85.626
	reverse


// Pedestrian number 357

137				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.820,-5.659,87.136
	reverse


// Pedestrian number 358

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.049,-5.659,87.147
	reverse


// Pedestrian number 359

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.429,-5.659,87.152
	reverse


// Pedestrian number 360

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.405,-5.659,85.663
	reverse


// Pedestrian number 361

99				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	122.035,-6.382,90.702
	point
	115.992,-6.382,94.192
	point
	115.507,-6.236,94.831
	point
	114.181,-5.834,96.797
	point
	113.689,-5.234,98.337
	reverse


// Pedestrian number 362

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	122.988,-5.177,69.448
	point
	119.292,-5.177,73.457
	point
	114.037,-5.177,78.454
	reverse


// Pedestrian number 363

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	113.932,-5.177,76.791
	point
	118.804,-5.177,73.423
	point
	121.358,-5.177,72.267
	point
	128.410,-5.177,72.159
	reverse


// Pedestrian number 364

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	128.967,-5.177,71.575
	point
	129.153,-5.177,65.426
	point
	129.976,-5.177,62.142
	point
	130.860,-5.177,52.095
	reverse


// Pedestrian number 365

4				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	128.086,-5.177,55.193
	point
	129.807,-5.177,57.482
	point
	131.775,-5.177,59.471
	reverse


// Pedestrian number 366

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	131.668,-5.177,57.329
	point
	129.833,-5.177,57.697
	point
	128.204,-5.177,58.867
	reverse


// Pedestrian number 367

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	128.222,-5.177,57.659
	point
	130.061,-5.177,58.061
	point
	131.690,-5.177,58.202
	reverse


// Pedestrian number 368

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	131.790,-5.177,60.943
	point
	130.124,-5.177,57.511
	point
	128.192,-5.177,49.356
	reverse


// Pedestrian number 369

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	128.074,-5.177,53.723
	point
	129.128,-5.177,55.335
	point
	129.895,-5.177,58.719
	point
	131.498,-5.177,62.005
	point
	131.274,-5.177,69.241
	reverse


// Pedestrian number 370

7				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	131.836,-5.177,66.619
	point
	131.802,-5.177,62.396
	point
	130.544,-5.177,59.120
	point
	130.026,-5.177,55.085
	point
	128.123,-5.177,54.356
	reverse


// Pedestrian number 371

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	128.054,-5.177,56.940
	point
	129.049,-5.177,57.553
	point
	131.772,-5.177,61.237
	reverse


// Pedestrian number 372

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	124.683,-5.177,67.054
	point
	121.172,-5.177,66.111
	point
	113.088,-5.177,64.602
	reverse


// Pedestrian number 373

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	113.111,-5.177,64.127
	point
	116.745,-5.177,64.005
	point
	124.730,-5.177,63.241
	reverse


// Pedestrian number 374

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	124.662,-5.177,65.378
	point
	119.959,-5.177,62.127
	point
	117.940,-5.177,58.963
	point
	113.119,-5.177,55.608
	reverse


// Pedestrian number 375

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	113.086,-5.177,54.904
	point
	117.238,-5.177,52.972
	point
	121.000,-5.177,50.033
	reverse


// Pedestrian number 376

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	124.750,-5.177,51.489
	point
	119.820,-5.177,50.732
	point
	116.670,-5.177,49.940
	reverse


// Pedestrian number 377

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	116.662,-5.177,50.337
	point
	118.040,-5.177,53.633
	point
	120.501,-5.177,56.408
	point
	121.320,-5.177,60.668
	point
	124.612,-5.177,60.846
	reverse


// Pedestrian number 378

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	122.291,-5.177,67.709
	point
	119.127,-5.177,62.924
	point
	118.453,-5.177,59.357
	point
	119.049,-5.177,53.213
	point
	118.780,-5.177,48.590
	point
	108.805,-5.177,47.475
	reverse


// Pedestrian number 379

4				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	110.592,-5.177,48.494
	point
	109.777,-5.177,46.838
	point
	105.068,-5.177,42.398
	reverse


// Pedestrian number 380

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	105.174,-5.177,43.314
	point
	108.625,-5.177,46.070
	point
	111.028,-5.177,48.635
	reverse


// Pedestrian number 381

7				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	109.649,-5.177,48.287
	point
	109.241,-5.177,46.535
	point
	107.831,-5.177,44.508
	point
	105.007,-5.177,43.829
	reverse


// Pedestrian number 382

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	106.650,-5.177,45.407
	point
	109.090,-5.177,45.937
	point
	111.132,-5.177,47.017
	point
	112.417,-5.177,48.696
	reverse


// Pedestrian number 383

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	111.433,-5.177,48.382
	point
	116.044,-5.177,45.245
	point
	118.468,-5.177,41.086
	point
	121.312,-5.177,37.945
	reverse


// Pedestrian number 384

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	120.824,-5.177,37.283
	point
	121.169,-5.177,36.030
	point
	124.286,-5.177,34.287
	reverse


// Pedestrian number 385

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	123.315,-5.177,34.235
	point
	120.774,-5.177,35.685
	point
	118.925,-5.177,36.503
	reverse


// Pedestrian number 386

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	119.737,-5.177,37.007
	point
	120.964,-5.177,35.305
	point
	122.237,-5.177,33.021
	reverse


// Pedestrian number 387

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	120.031,-5.177,32.947
	point
	123.402,-5.177,34.793
	point
	124.483,-5.177,36.648
	reverse


// Pedestrian number 388

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	123.832,-5.177,36.630
	point
	120.238,-5.177,34.343
	point
	115.695,-5.177,31.234
	reverse


// Pedestrian number 389

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	115.726,-5.177,30.665
	point
	118.045,-5.177,28.174
	point
	119.870,-5.176,20.382
	reverse


// Pedestrian number 390

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	117.699,-5.182,22.462
	point
	118.055,-5.183,22.794
	point
	118.747,-5.196,28.904
	point
	117.888,-5.177,36.410
	reverse


// Pedestrian number 391

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	113.807,-5.177,33.832
	point
	111.280,-5.177,39.794
	point
	108.161,-5.177,46.865
	reverse


// Pedestrian number 392

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	107.290,-5.177,46.056
	point
	112.647,-5.177,41.408
	point
	116.851,-5.177,38.429
	reverse


// Pedestrian number 393

9				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	114.520,-5.177,36.051
	point
	112.773,-5.177,41.851
	point
	111.709,-5.177,41.693
	point
	106.835,-5.177,42.837
	point
	105.086,-5.177,41.730
	reverse


// Pedestrian number 394

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	104.615,-5.177,40.553
	point
	111.666,-5.177,40.163
	point
	119.146,-5.177,38.351
	reverse


// Pedestrian number 395

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	118.232,-5.177,38.280
	point
	113.282,-5.177,41.310
	point
	108.538,-5.177,47.183
	reverse


// Pedestrian number 396

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	104.025,-5.177,39.912
	point
	109.210,-5.177,36.895
	point
	113.802,-5.177,35.202
	reverse


// Pedestrian number 397

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	113.837,-5.177,35.805
	point
	108.393,-5.177,36.992
	point
	99.798,-5.177,35.826
	reverse


// Pedestrian number 398

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	100.757,-5.177,37.350
	point
	107.796,-5.177,36.252
	point
	111.789,-5.177,35.360
	point
	113.873,-5.177,30.373
	reverse


// Pedestrian number 399

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	121.707,-5.178,67.631
	point
	120.010,-5.181,56.315
	point
	121.983,-5.181,50.313
	reverse


// Pedestrian number 400

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	121.117,-5.182,49.638
	point
	112.266,-5.185,39.471
	point
	104.704,-5.186,37.628
	point
	100.318,-5.187,34.064
	reverse


// Pedestrian number 401

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	143.520,-5.177,0.625
	point
	137.324,-5.177,-2.024
	point
	134.294,-5.177,-3.026
	reverse


// Pedestrian number 402

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	114.711,-5.177,0.683
	point
	122.689,-5.177,0.105
	point
	126.164,-5.177,-2.104
	point
	131.133,-5.177,-3.037
	reverse


// Pedestrian number 403

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	131.812,-5.177,-3.073
	point
	135.248,-5.177,-1.582
	point
	138.991,-5.177,0.648
	reverse


// Pedestrian number 404

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	139.724,-5.177,0.679
	point
	142.356,-5.177,-0.253
	point
	145.418,-5.177,-0.961
	reverse


// Pedestrian number 405

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	114.034,-5.177,80.530
	point
	117.294,-5.177,79.095
	point
	123.774,-5.177,75.470
	reverse


// Pedestrian number 406

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	123.753,-5.177,74.900
	point
	119.551,-5.177,70.736
	point
	117.766,-5.177,69.192
	reverse


// Pedestrian number 407

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	117.700,-5.177,68.915
	point
	118.364,-5.177,61.571
	point
	119.212,-5.177,58.175
	point
	124.608,-5.177,54.942
	reverse


// Pedestrian number 408

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	124.594,-5.177,54.523
	point
	121.834,-5.177,52.278
	point
	119.878,-5.177,50.157
	point
	116.797,-5.177,49.450
	reverse


// Pedestrian number 409

7				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	116.789,-5.177,49.654
	point
	119.364,-5.177,54.216
	point
	119.622,-5.177,59.461
	point
	119.660,-5.177,64.244
	point
	121.328,-5.177,67.723
	reverse


// Pedestrian number 410

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	120.990,-5.177,67.662
	point
	119.392,-5.177,66.865
	point
	113.049,-5.177,63.759
	reverse


// Pedestrian number 411

7				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	113.050,-5.177,63.326
	point
	116.927,-5.177,59.303
	point
	118.436,-5.177,58.768
	point
	124.096,-5.177,55.925
	point
	124.643,-5.177,53.504
	reverse


// Pedestrian number 412

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	124.603,-5.177,52.925
	point
	124.779,-5.177,46.682
	point
	126.336,-5.177,33.082
	reverse


// Pedestrian number 413

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	126.802,-5.177,33.095
	point
	128.380,-5.177,40.111
	point
	130.171,-5.177,46.118
	reverse


// Pedestrian number 414

4				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	132.796,-5.177,43.612
	point
	129.322,-5.177,45.109
	point
	127.477,-5.177,46.128
	point
	126.540,-5.177,48.309
	reverse


// Pedestrian number 415

7				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	126.909,-5.177,48.675
	point
	129.124,-5.177,45.342
	point
	129.881,-5.177,42.916
	point
	132.716,-5.177,41.710
	reverse


// Pedestrian number 416

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	132.794,-5.177,42.358
	point
	128.071,-5.177,45.477
	point
	125.467,-5.177,48.639
	reverse


// Pedestrian number 417

7				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	125.989,-5.177,48.555
	point
	126.350,-5.177,46.540
	point
	128.420,-5.177,45.097
	point
	132.444,-5.177,33.108
	reverse


// Pedestrian number 418

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	133.026,-5.177,33.007
	point
	135.259,-5.177,34.811
	point
	138.250,-5.177,37.423
	reverse


// Pedestrian number 419

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	138.442,-5.177,37.408
	point
	140.966,-5.177,35.647
	point
	144.020,-5.177,33.370
	point
	148.904,-5.177,32.945
	reverse


// Pedestrian number 420

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	148.886,-5.177,32.121
	point
	144.425,-5.177,34.089
	point
	140.790,-5.177,35.353
	point
	139.749,-5.177,37.323
	reverse


// Pedestrian number 421

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	139.196,-5.177,37.434
	point
	136.282,-5.177,37.009
	point
	135.103,-5.177,34.858
	point
	134.642,-5.177,32.981
	reverse


// Pedestrian number 422

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	133.407,-5.177,32.996
	point
	129.337,-5.177,35.619
	point
	125.023,-5.177,36.887
	reverse


// Pedestrian number 423

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	124.575,-5.177,36.774
	point
	117.241,-5.177,35.143
	point
	115.622,-5.177,34.698
	reverse


// Pedestrian number 424

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	115.637,-5.177,35.244
	point
	117.494,-5.177,35.344
	point
	119.783,-5.177,35.520
	point
	121.652,-5.177,36.803
	reverse


// Pedestrian number 425

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	120.757,-5.177,37.709
	point
	119.164,-5.177,42.529
	point
	116.230,-5.177,48.941
	reverse


// Pedestrian number 426

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	115.553,-5.177,48.884
	point
	109.700,-5.177,45.343
	point
	106.652,-5.177,43.338
	point
	105.278,-5.177,41.290
	reverse


// Pedestrian number 427

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	105.218,-5.177,40.846
	point
	108.831,-5.177,37.101
	point
	114.774,-5.177,25.081
	reverse


// Pedestrian number 428

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	115.278,-5.177,25.026
	point
	118.308,-5.177,29.305
	point
	119.602,-5.177,34.972
	point
	120.042,-5.177,35.535
	reverse


// Pedestrian number 429

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	114.510,-5.177,31.869
	point
	110.375,-5.177,30.584
	point
	100.321,-5.177,32.105
	reverse


// Pedestrian number 430

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	99.700,-5.177,31.613
	point
	97.618,-5.177,29.046
	point
	96.401,-5.177,26.432
	reverse


// Pedestrian number 431

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	98.225,-5.177,26.425
	point
	104.866,-5.177,31.480
	point
	111.038,-5.177,33.685
	point
	113.802,-5.177,34.675
	reverse


// Pedestrian number 432

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	113.778,-5.177,33.529
	point
	104.174,-5.177,30.136
	point
	97.710,-5.177,29.499
	reverse


// Pedestrian number 433

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	96.331,-5.177,28.469
	point
	91.894,-5.177,27.539
	point
	88.289,-5.305,26.105
	reverse


// Pedestrian number 434

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	91.889,-5.181,25.111
	point
	91.881,-5.181,26.911
	point
	92.194,-5.177,29.321
	reverse


// Pedestrian number 435

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	93.488,-5.177,28.486
	point
	91.119,-5.208,26.442
	point
	88.335,-5.298,23.645
	reverse


// Pedestrian number 436

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	88.271,-5.301,22.773
	point
	88.874,-5.269,19.423
	point
	90.493,-5.184,16.455
	reverse


// Pedestrian number 437

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	90.491,-5.184,16.201
	point
	88.950,-5.265,14.440
	point
	88.159,-5.307,11.542
	reverse


// Pedestrian number 438

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	88.190,-5.305,10.201
	point
	89.590,-5.247,8.314
	point
	91.736,-5.177,6.191
	reverse


// Pedestrian number 439

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	91.785,-5.177,5.928
	point
	91.146,-5.177,3.782
	point
	90.628,-5.225,0.707
	point
	90.780,-5.219,-0.874
	reverse


// Pedestrian number 440

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	88.270,-5.306,3.176
	point
	91.234,-5.204,3.507
	point
	95.647,-5.177,4.427
	reverse


// Pedestrian number 441

4				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	96.191,-5.177,3.289
	point
	99.038,-5.177,-0.467
	point
	100.883,-5.177,-2.932
	reverse


// Pedestrian number 442

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	101.324,-5.177,-2.827
	point
	99.117,-5.177,-1.112
	point
	98.113,-5.177,-0.748
	reverse


// Pedestrian number 443

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	97.923,-5.177,-0.332
	point
	98.826,-5.177,-1.334
	point
	99.038,-5.177,-1.986
	reverse


// Pedestrian number 444

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	99.196,-5.177,-1.933
	point
	98.266,-5.177,-1.284
	point
	95.290,-5.177,-0.356
	reverse


// Pedestrian number 445

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	95.211,-5.177,-0.929
	point
	97.339,-5.177,-1.690
	point
	98.611,-5.177,-1.310
	point
	104.297,-5.177,3.304
	reverse


// Pedestrian number 446

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	104.495,-5.177,3.605
	point
	104.011,-5.177,2.243
	point
	100.430,-5.177,0.909
	point
	95.205,-5.177,0.293
	reverse


// Pedestrian number 447

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	95.262,-5.177,-0.008
	point
	96.970,-5.177,1.138
	point
	100.828,-5.177,3.211
	reverse


// Pedestrian number 448

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	101.269,-5.177,3.256
	point
	102.263,-5.177,2.304
	point
	104.825,-5.177,0.117
	reverse


// Pedestrian number 449

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	104.835,-5.177,-0.073
	point
	103.367,-5.177,-1.492
	point
	101.853,-5.177,-2.944
	reverse


// Pedestrian number 450

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	100.466,-5.177,-3.017
	point
	97.355,-5.177,-2.389
	point
	93.940,-5.177,-1.429
	reverse


// Pedestrian number 451

9				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	95.434,-5.177,-1.195
	point
	94.866,-5.177,-1.794
	point
	93.330,-5.177,-2.465
	point
	90.776,-5.219,-2.855
	point
	88.374,-5.302,-2.805
	reverse


// Pedestrian number 452

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	88.470,-5.299,-2.447
	point
	89.930,-5.249,1.353
	point
	92.016,-5.177,3.487
	point
	95.547,-5.177,3.995
	reverse


// Pedestrian number 453

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	95.622,-5.177,3.452
	point
	95.740,-5.177,2.139
	point
	96.646,-5.177,-2.880
	reverse


// Pedestrian number 454

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	95.657,-5.177,-2.889
	point
	96.564,-5.177,0.337
	point
	98.895,-5.177,3.152
	reverse


// Pedestrian number 455

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	99.473,-5.177,3.159
	point
	106.426,-5.177,1.595
	point
	113.444,-5.177,1.623
	reverse


// Pedestrian number 456

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	112.663,-5.177,-2.990
	point
	116.499,-5.177,-1.991
	point
	120.222,-5.177,0.668
	point
	123.508,-5.177,0.697
	reverse


// Pedestrian number 457

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	123.932,-5.177,0.657
	point
	127.901,-5.177,-0.560
	point
	128.598,-5.177,-3.031
	reverse


// Pedestrian number 458

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	127.114,-5.177,-2.981
	point
	121.359,-5.177,-1.267
	point
	114.716,-5.177,0.060
	reverse


// Pedestrian number 459

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	113.875,-5.177,-0.674
	point
	118.842,-5.177,-1.958
	point
	123.318,-5.177,-2.060
	point
	123.624,-5.177,-3.007
	reverse


// Pedestrian number 460

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	125.415,-5.177,0.688
	point
	131.371,-5.177,-1.040
	point
	133.536,-5.177,-2.977
	reverse


// Pedestrian number 461

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	136.006,-5.177,-2.958
	point
	139.890,-5.177,-2.421
	point
	143.822,-5.177,-1.511
	reverse


// Pedestrian number 462

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	144.626,-5.177,-0.939
	point
	146.203,-5.177,2.221
	point
	149.682,-5.177,6.517
	reverse


// Pedestrian number 463

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	149.291,-5.177,7.946
	point
	146.081,-5.177,15.219
	point
	144.135,-5.177,20.686
	reverse


// Pedestrian number 464

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	144.103,-5.177,21.168
	point
	146.215,-5.177,23.754
	point
	148.965,-5.177,26.510
	reverse


// Pedestrian number 465

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	149.004,-5.177,26.785
	point
	146.819,-5.177,29.011
	point
	144.215,-5.177,31.903
	reverse


// Pedestrian number 466

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	144.155,-5.177,32.241
	point
	147.179,-5.177,33.984
	point
	148.963,-5.177,34.964
	reverse


// Pedestrian number 467

7				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	147.590,-5.177,36.840
	point
	147.772,-5.177,35.175
	point
	148.596,-5.177,34.239
	point
	147.799,-5.177,31.507
	point
	144.217,-5.177,26.034
	reverse


// Pedestrian number 468

7				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	144.149,-5.177,27.227
	point
	144.709,-5.177,24.182
	point
	146.015,-5.177,21.796
	point
	148.997,-5.177,18.008
	reverse


// Pedestrian number 469

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	149.017,-5.177,17.464
	point
	147.128,-5.177,14.298
	point
	144.208,-5.177,9.635
	reverse


// Pedestrian number 470

4				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	144.110,-5.177,10.351
	point
	146.126,-5.177,8.035
	point
	150.445,-5.177,4.560
	reverse


// Pedestrian number 471

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	150.580,-5.177,4.263
	point
	151.035,-5.177,0.490
	point
	150.632,-5.177,-3.024
	reverse


// Pedestrian number 472

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	151.558,-5.177,-3.062
	point
	149.513,-5.177,-2.273
	point
	147.352,-5.177,-1.488
	reverse


// Pedestrian number 473

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	148.306,-5.177,-2.961
	point
	149.163,-5.177,-1.715
	point
	149.676,-5.177,0.475
	reverse


// Pedestrian number 474

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	149.230,-5.177,0.413
	point
	148.025,-5.177,-0.670
	point
	147.322,-5.177,-1.174
	reverse


// Pedestrian number 475

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	146.904,-5.177,-0.955
	point
	145.080,-5.177,1.111
	point
	144.155,-5.177,2.626
	reverse


// Pedestrian number 476

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	144.169,-5.177,4.432
	point
	145.127,-5.177,2.203
	point
	147.957,-5.177,0.029
	point
	149.720,-5.177,-0.744
	reverse


// Pedestrian number 477

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	151.138,-5.177,-2.096
	reverse


// Pedestrian number 478

139				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	151.700,-5.177,0.870
	point
	149.297,-5.177,2.710
	point
	144.317,-5.177,6.125
	reverse


// Pedestrian number 479

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	144.303,-5.177,6.860
	point
	146.305,-5.177,11.158
	point
	148.992,-5.177,13.546
	reverse


// Pedestrian number 480

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	148.984,-5.177,10.400
	point
	146.588,-5.177,6.253
	point
	145.087,-5.177,-0.810
	reverse


// Pedestrian number 481

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	145.657,-5.177,-0.636
	point
	149.189,-5.177,-0.179
	point
	151.814,-5.177,0.140
	reverse


// Pedestrian number 482

122				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	116.798,-2.557,14.898
	reverse


// Pedestrian number 483

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	120.264,-2.560,14.908
	reverse


// Pedestrian number 484

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	114.619,-2.555,14.929
	reverse


// Pedestrian number 485

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	114.645,-2.555,15.933
	reverse


// Pedestrian number 486

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	114.578,-2.555,13.850
	reverse


// Pedestrian number 487

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	121.727,-2.584,12.933
	point
	125.109,-2.821,15.085
	point
	127.207,-2.968,17.454
	reverse


// Pedestrian number 488

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	127.605,-2.996,17.535
	point
	131.847,-3.293,15.809
	point
	134.524,-3.482,14.201
	reverse


// Pedestrian number 489

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	136.188,-3.598,14.312
	point
	137.099,-3.662,15.996
	point
	138.361,-3.750,18.492
	reverse


// Pedestrian number 490

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	137.775,-3.709,18.508
	point
	131.709,-3.284,15.990
	point
	128.917,-3.089,13.648
	reverse


// Pedestrian number 491

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	128.567,-3.064,13.630
	point
	125.106,-2.821,15.344
	point
	122.511,-2.637,16.971
	reverse


// Pedestrian number 492

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	121.261,-2.561,16.830
	point
	117.709,-2.558,14.894
	point
	116.277,-2.556,13.596
	reverse


// Pedestrian number 493

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	114.997,997.845,12.850
	point
	116.040,997.844,14.599
	point
	117.337,997.843,17.016
	reverse


// Pedestrian number 494

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	115.502,997.844,12.667
	point
	115.799,997.844,14.621
	point
	116.221,997.844,17.392
	reverse


// Pedestrian number 495

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	118.931,997.841,17.290
	point
	117.093,997.843,15.228
	point
	115.979,997.844,12.973
	reverse


// Pedestrian number 496

13				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	119.724,997.840,12.546
	point
	116.316,997.844,14.968
	point
	112.773,997.847,17.590
	reverse


// Pedestrian number 497

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	106.867,-5.177,52.116
	point
	108.135,-5.177,58.858
	point
	109.749,-5.177,63.364
	point
	109.634,-5.177,72.416
	reverse


// Pedestrian number 498

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	107.252,-5.177,69.921
	point
	106.530,-5.177,61.717
	point
	108.194,-5.177,57.920
	point
	109.625,-5.177,49.821
	reverse


// Pedestrian number 499

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	107.807,-5.177,51.310
	point
	107.625,-5.177,58.178
	point
	107.937,-5.177,64.455
	point
	109.664,-5.177,65.717
	reverse


// Pedestrian number 500

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	106.020,-5.177,67.189
	point
	106.327,-5.177,62.183
	point
	108.810,-5.177,58.355
	point
	109.743,-5.177,55.360
	reverse


// Pedestrian number 501

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	109.694,-5.177,53.892
	point
	107.899,-5.177,58.961
	point
	106.107,-5.177,61.617
	reverse


// Pedestrian number 502

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	106.097,-5.177,62.507
	point
	108.347,-5.177,59.840
	point
	109.760,-5.177,58.860
	reverse


// Pedestrian number 503

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	139.405,-3.738,74.004
	reverse


// Pedestrian number 504

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.443,-3.732,74.321
	reverse


// Pedestrian number 505

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.961,-3.735,74.436
	reverse


// Pedestrian number 506

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	139.620,-3.740,74.762
	reverse


// Pedestrian number 507

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.487,-3.732,73.809
	reverse


// Pedestrian number 508

137				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	137.320,-3.724,73.800
	reverse


// Pedestrian number 509

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	137.267,-3.724,74.710
	reverse


// Pedestrian number 510

136				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.423,-3.732,74.754
	reverse


// Pedestrian number 511

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	144.523,-3.725,72.730
	reverse


// Pedestrian number 512

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.231,-3.730,72.753
	reverse


// Pedestrian number 513

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	146.407,-3.736,72.792
	reverse


// Pedestrian number 514

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	146.903,-3.739,72.808
	reverse


// Pedestrian number 515

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.184,-3.729,73.413
	reverse


// Pedestrian number 516

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	146.434,-3.737,73.387
	reverse


// Pedestrian number 517

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	137.926,-3.732,79.037
	reverse


// Pedestrian number 518

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.536,-3.732,79.060
	reverse


// Pedestrian number 519

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	139.116,-3.732,79.035
	reverse


// Pedestrian number 520

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	140.024,-3.732,79.044
	reverse


// Pedestrian number 521

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	140.405,-3.732,79.047
	reverse


// Pedestrian number 522

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	139.175,-3.732,79.588
	reverse


// Pedestrian number 523

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.297,-3.732,79.583
	reverse


// Pedestrian number 524

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.893,-3.732,81.874
	reverse


// Pedestrian number 525

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.835,-3.732,82.335
	reverse


// Pedestrian number 526

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.824,-3.732,82.929
	reverse


// Pedestrian number 527

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.812,-3.732,84.041
	reverse


// Pedestrian number 528

4				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	111.578,-5.177,94.025
	point
	108.976,-5.177,94.807
	point
	104.881,-5.177,95.406
	reverse


// Pedestrian number 529

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	104.265,-5.177,95.323
	point
	103.035,-5.177,94.497
	point
	101.922,-5.177,93.603
	reverse


// Pedestrian number 530

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	101.610,-5.177,93.552
	point
	98.580,-5.177,94.492
	point
	95.422,-5.177,94.794
	reverse


// Pedestrian number 531

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	95.017,-5.177,94.734
	point
	94.063,-5.177,93.764
	point
	93.298,-5.177,92.692
	reverse


// Pedestrian number 532

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	93.036,-5.177,92.506
	point
	91.925,-5.177,92.414
	point
	90.707,-5.177,92.884
	reverse


// Pedestrian number 533

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	91.508,-5.177,93.541
	point
	94.748,-5.177,93.594
	point
	98.879,-5.177,93.339
	reverse


// Pedestrian number 534

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	99.520,-5.177,93.372
	point
	100.777,-5.177,94.203
	point
	102.459,-5.177,95.316
	reverse


// Pedestrian number 535

4				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	103.162,-5.177,95.313
	point
	100.788,-5.177,93.983
	point
	95.702,-5.177,93.054
	reverse


// Pedestrian number 536

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	94.560,-5.177,92.957
	point
	90.735,-5.177,92.345
	point
	89.619,-5.177,88.615
	point
	90.313,-5.177,86.698
	reverse


// Pedestrian number 537

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	90.159,-5.177,85.911
	point
	89.263,-5.177,84.460
	point
	87.248,-5.177,81.280
	reverse


// Pedestrian number 538

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	87.167,-5.177,81.018
	point
	86.946,-5.177,79.519
	point
	86.481,-5.177,78.025
	reverse


// Pedestrian number 539

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	86.088,-5.177,77.752
	point
	85.223,-5.177,78.372
	point
	83.806,-5.177,79.053
	reverse


// Pedestrian number 540

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	82.576,-5.177,79.077
	point
	79.978,-5.177,77.819
	point
	77.882,-5.177,77.489
	reverse


// Pedestrian number 541

9				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	76.896,-5.177,77.663
	point
	73.597,-5.177,78.260
	point
	72.767,-5.177,78.892
	point
	71.117,-5.177,79.509
	point
	67.135,-5.177,78.377
	point
	67.050,-5.177,77.914
	reverse


// Pedestrian number 542

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	65.244,-5.177,77.952
	point
	66.394,-5.177,78.903
	point
	67.840,-5.177,80.180
	reverse


// Pedestrian number 543

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	69.087,-5.177,79.621
	point
	72.163,-5.177,78.433
	point
	75.436,-5.177,77.607
	reverse


// Pedestrian number 544

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	76.706,-5.177,77.549
	point
	78.068,-5.177,78.285
	point
	80.326,-5.177,79.196
	reverse


// Pedestrian number 545

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	80.772,-5.177,79.197
	point
	84.587,-5.177,78.394
	point
	88.207,-5.177,79.539
	reverse


// Pedestrian number 546

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	65.476,-5.177,81.437
	point
	65.111,-5.177,84.015
	point
	64.994,-5.197,86.685
	reverse


// Pedestrian number 547

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.715,-3.759,89.627
	reverse


// Pedestrian number 548

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.723,-3.757,88.768
	reverse


// Pedestrian number 549

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.731,-3.755,87.957
	reverse


// Pedestrian number 550

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.736,-3.754,87.396
	reverse


// Pedestrian number 551

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.640,-3.765,91.952
	reverse


// Pedestrian number 552

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.668,-3.767,92.626
	reverse


// Pedestrian number 553

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.603,-3.769,93.611
	reverse


// Pedestrian number 554

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.648,-3.771,94.431
	reverse


// Pedestrian number 555

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	64.342,-5.213,98.883
	point
	60.833,-5.213,103.416
	point
	57.010,-5.213,109.632
	reverse


// Pedestrian number 556

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.080,-5.213,110.653
	point
	59.426,-5.213,107.105
	point
	65.207,-5.213,94.814
	reverse


// Pedestrian number 557

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	64.660,-5.213,94.812
	point
	60.227,-5.213,95.876
	point
	53.513,-5.213,97.675
	reverse


// Pedestrian number 558

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	53.484,-5.213,98.270
	point
	60.959,-5.213,103.746
	point
	64.986,-5.213,106.518
	reverse


// Pedestrian number 559

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	65.805,-5.213,103.803
	point
	60.988,-5.213,98.260
	point
	53.462,-5.213,86.567
	reverse


// Pedestrian number 560

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	53.388,-5.213,91.665
	point
	59.599,-5.213,103.363
	point
	61.408,-5.213,109.456
	reverse


// Pedestrian number 561

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	59.433,-5.213,113.662
	point
	60.056,-5.213,107.099
	point
	59.800,-5.213,93.323
	point
	63.898,-5.213,88.869
	reverse


// Pedestrian number 562

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.864,1.519,114.884
	reverse


// Pedestrian number 563

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.192,1.519,114.706
	reverse


// Pedestrian number 564

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.458,1.451,118.211
	reverse


// Pedestrian number 565

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.966,1.451,118.235
	reverse


// Pedestrian number 566

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.744,1.451,118.283
	reverse


// Pedestrian number 567

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	68.230,1.451,118.376
	reverse


// Pedestrian number 568

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	69.284,1.451,118.441
	reverse


// Pedestrian number 569

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	70.456,1.451,118.501
	reverse


// Pedestrian number 570

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	71.666,1.451,118.539
	reverse


// Pedestrian number 571

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	72.816,1.451,118.567
	reverse


// Pedestrian number 572

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.906,1.451,117.551
	reverse


// Pedestrian number 573

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.138,1.451,113.492
	reverse


// Pedestrian number 574

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.251,1.506,109.866
	reverse


// Pedestrian number 575

120				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.249,1.526,124.943
	reverse


// Pedestrian number 576

120				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.243,1.523,120.341
	reverse


// Pedestrian number 577

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	60.315,-1.850,115.343
	point
	59.554,998.550,112.384
	point
	57.075,998.550,108.057
	reverse


// Pedestrian number 578

9				// Ref num
4				// Number of instructions
3				// Initial instruction

	point
	56.776,998.550,108.369
	point
	58.891,998.550,105.743
	point
	61.265,998.550,98.303
	reverse


// Pedestrian number 579

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	61.163,998.550,98.203
	point
	60.003,998.550,97.060
	point
	57.155,998.550,94.252
	reverse


// Pedestrian number 580

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.151,998.550,94.249
	point
	58.885,998.550,98.408
	point
	61.509,998.550,104.700
	reverse


// Pedestrian number 581

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	61.486,998.550,105.279
	point
	59.429,998.550,110.025
	point
	56.698,998.550,112.429
	reverse


// Pedestrian number 582

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.268,998.550,111.349
	point
	58.802,998.550,109.675
	point
	61.088,998.550,102.584
	reverse


// Pedestrian number 583

4				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	61.088,998.550,102.584
	point
	59.172,998.550,97.381
	point
	56.333,998.550,93.270
	reverse


// Pedestrian number 584

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	53.703,-1.338,116.979
	point
	57.912,-1.338,121.370
	point
	60.955,-1.338,125.614
	point
	62.150,-1.338,129.870
	reverse


// Pedestrian number 585

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	61.122,-1.338,129.953
	point
	60.323,-1.338,127.108
	point
	59.525,-1.338,125.696
	point
	56.352,-1.338,123.766
	reverse


// Pedestrian number 586

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	55.679,-1.338,124.153
	point
	56.262,-1.338,125.424
	point
	57.291,-1.338,128.729
	point
	58.681,-1.338,130.073
	reverse


// Pedestrian number 587

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	59.167,-1.338,130.064
	point
	59.832,-1.338,127.412
	point
	60.492,-1.338,125.888
	reverse


// Pedestrian number 588

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	61.932,-1.338,125.324
	point
	59.314,-1.338,126.243
	point
	55.602,-1.338,128.283
	reverse


// Pedestrian number 589

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	54.285,-1.338,128.242
	point
	58.606,-1.338,126.318
	point
	61.954,-1.338,126.945
	point
	64.996,-1.338,126.736
	reverse


// Pedestrian number 590

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	65.027,-1.338,126.291
	point
	61.558,-1.338,123.047
	point
	57.501,-1.338,120.747
	point
	53.670,-1.338,119.955
	reverse


// Pedestrian number 591

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	53.558,-1.338,121.100
	point
	58.484,-1.338,124.501
	point
	60.021,-1.338,125.407
	point
	63.547,-1.338,129.163
	reverse


// Pedestrian number 592

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	53.503,-1.338,118.475
	point
	57.687,-1.338,121.637
	point
	60.321,-1.338,124.921
	point
	64.112,-1.338,128.767
	reverse


// Pedestrian number 593

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	63.177,-1.338,125.405
	point
	61.787,-1.338,125.692
	point
	61.216,-1.338,125.027
	point
	54.946,-1.338,125.453
	point
	52.243,-1.338,127.700
	reverse


// Pedestrian number 594

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	53.128,-1.338,127.464
	point
	50.470,-1.338,126.594
	point
	48.495,-1.338,125.567
	reverse


// Pedestrian number 595

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	48.032,-1.338,125.573
	point
	43.634,-1.338,127.044
	point
	38.305,-1.338,129.277
	reverse


// Pedestrian number 596

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	37.658,-1.338,129.024
	point
	35.507,-1.338,125.389
	point
	34.230,-1.338,120.876
	reverse


// Pedestrian number 597

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	33.751,-1.338,120.097
	point
	29.700,-1.338,114.536
	point
	28.269,-1.338,113.575
	reverse


// Pedestrian number 598

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	27.712,-1.338,114.581
	point
	28.739,-1.338,113.610
	point
	30.008,-1.343,113.439
	reverse


// Pedestrian number 599

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	30.182,-1.338,114.233
	point
	29.076,-1.342,113.520
	point
	27.455,-1.343,113.462
	reverse


// Pedestrian number 600

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	33.913,-1.338,120.589
	point
	34.240,-1.338,123.360
	point
	34.187,-1.338,125.778
	point
	35.996,-1.338,128.019
	reverse


// Pedestrian number 601

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	36.456,-1.338,128.314
	point
	42.193,-1.338,126.695
	point
	47.354,-1.338,126.079
	point
	49.366,-1.338,127.822
	reverse


// Pedestrian number 602

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	50.338,-1.338,125.440
	point
	43.438,-1.338,127.505
	point
	42.221,-1.338,128.878
	reverse


// Pedestrian number 603

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	41.033,-1.338,129.135
	point
	37.436,-1.338,126.785
	point
	35.956,-1.338,123.708
	reverse


// Pedestrian number 604

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	32.229,-1.338,122.170
	point
	31.438,-1.338,118.187
	point
	31.266,-1.338,116.119
	reverse


// Pedestrian number 605

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	8.998,-4.071,40.844
	point
	9.944,-4.071,36.906
	point
	10.204,-4.071,33.162
	reverse


// Pedestrian number 606

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	9.555,-4.071,30.360
	point
	10.282,-4.071,31.975
	point
	9.347,-4.071,40.758
	reverse


// Pedestrian number 607

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	10.233,-4.071,39.772
	point
	10.112,-4.071,36.340
	point
	9.463,-4.071,30.010
	reverse


// Pedestrian number 608

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	9.553,-4.071,28.782
	point
	10.151,-4.071,30.861
	point
	9.841,-4.071,35.142
	point
	6.641,-4.071,36.795
	reverse


// Pedestrian number 609

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	9.821,-4.071,40.105
	point
	9.534,-4.071,34.545
	point
	8.641,-4.071,30.233
	reverse


// Pedestrian number 610

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	8.961,-4.071,30.000
	point
	9.783,-4.071,32.694
	point
	9.990,-4.071,39.882
	reverse


// Pedestrian number 611

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	10.342,-4.071,35.181
	point
	9.679,-4.071,35.585
	point
	6.345,-4.071,37.613
	reverse


// Pedestrian number 612

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	6.514,-4.071,35.814
	point
	9.532,-4.071,34.060
	point
	10.090,-4.071,33.373
	reverse


// Pedestrian number 613

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	10.050,-4.071,33.219
	point
	9.583,-4.071,33.163
	point
	6.458,-4.071,32.786
	reverse


// Pedestrian number 614

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	6.513,-4.071,33.823
	point
	9.054,-4.071,33.753
	point
	10.023,-4.071,33.758
	reverse


// Pedestrian number 615

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	10.338,-4.071,32.907
	point
	9.635,-4.071,32.172
	point
	6.265,-4.071,28.655
	reverse


// Pedestrian number 616

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	7.373,-4.071,27.411
	point
	8.212,-4.071,30.480
	point
	10.201,-4.071,31.380
	reverse


// Pedestrian number 617

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	10.254,-4.071,30.411
	point
	9.046,-4.071,30.766
	point
	6.487,-4.071,32.095
	reverse


// Pedestrian number 618

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	6.514,-4.071,30.870
	point
	8.454,-4.071,37.311
	point
	10.038,-4.071,39.192
	reverse


// Pedestrian number 619

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.354,-4.454,87.801
	reverse


// Pedestrian number 620

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	12.120,-4.454,87.788
	reverse


// Pedestrian number 621

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.991,-5.177,78.553
	reverse


// Pedestrian number 622

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	14.000,-5.177,76.191
	reverse


// Pedestrian number 623

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.993,-5.177,71.706
	reverse


// Pedestrian number 624

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.986,-5.177,67.161
	reverse


// Pedestrian number 625

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.977,-5.177,61.582
	reverse


// Pedestrian number 626

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.970,-5.177,57.055
	reverse


// Pedestrian number 627

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.949,-5.177,58.371
	reverse


// Pedestrian number 628

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.942,-5.177,63.248
	reverse


// Pedestrian number 629

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.933,-5.177,69.590
	reverse


// Pedestrian number 630

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.930,-5.177,74.086
	reverse



START OF OPPONENT PATHS

142                             // Number of path nodes
  151.200,   -5.100,   -1.300   // Node #0
  118.800,   -5.100,   -1.200   // Node #1
  119.212,   -5.200,   34.438   // Node #2
  118.910,   -5.177,   80.406   // Node #3
  117.648,   -6.382,   93.850   // Node #4
  112.097,   -5.207,   94.852   // Node #5
   93.485,   -5.177,   93.619   // Node #6
   90.347,   -5.177,   91.290   // Node #7
   88.176,   -5.177,   81.143   // Node #8
   85.525,   -5.176,   78.332   // Node #9
   64.638,   -5.213,   79.702   // Node #10
   59.285,   -5.213,   92.354   // Node #11
   45.156,   -2.830,   86.313   // Node #12
   35.903,   -4.104,   86.874   // Node #13
   26.451,   -5.007,   87.372   // Node #14
   21.950,   -5.177,   86.983   // Node #15
   21.984,   -5.179,   49.019   // Node #16
   22.042,   -5.179,   35.833   // Node #17
   45.541,   -3.255,   34.032   // Node #18
   98.919,   -0.253,   14.679   // Node #19
  146.857,   -5.178,   34.401   // Node #20
  147.320,   -5.178,   -1.338   // Node #21
  148.616,   -5.178,   36.256   // Node #22
  148.503,   -5.177,   51.045   // Node #23
  143.492,   -5.179,   34.955   // Node #24
  143.656,   -5.179,   44.377   // Node #25
  139.598,   -5.177,   48.484   // Node #26
  136.115,   -5.179,   48.411   // Node #27
  128.495,   -5.174,   40.410   // Node #28
  119.064,   -5.177,   47.360   // Node #29
  127.917,   -5.177,   34.918   // Node #30
  118.914,   -5.191,   72.923   // Node #31
  130.037,   -5.179,   67.903   // Node #32
  130.128,   -5.171,   54.448   // Node #33
  107.733,   -5.179,   69.194   // Node #34
  107.980,   -5.181,   53.390   // Node #35
  101.765,   -5.182,   48.495   // Node #36
   97.932,   -5.189,   48.562   // Node #37
   94.151,   -5.180,   44.730   // Node #38
   88.570,   -5.300,   36.127   // Node #39
   89.526,   -5.265,   -0.057   // Node #40
  105.526,   -5.179,    1.808   // Node #41
   89.006,   -5.283,   26.003   // Node #42
   99.471,   -5.179,   28.311   // Node #43
  115.168,   -5.177,   26.276   // Node #44
  113.386,   -6.188,   14.612   // Node #45
   94.486,   -8.264,   14.629   // Node #46
   14.378,   -5.177,   89.461   // Node #47
   11.915,   -5.178,   58.629   // Node #48
   30.862,   -5.177,   81.200   // Node #49
   30.938,   -5.181,   64.558   // Node #50
   32.963,   -5.178,   59.300   // Node #51
   30.376,   -5.179,   34.814   // Node #52
   30.520,   -5.180,   26.909   // Node #53
   14.038,   -5.181,   26.732   // Node #54
   12.474,   -5.180,   33.042   // Node #55
   94.201,   -5.177,   40.212   // Node #56
   10.790,   -5.179,   68.625   // Node #57
   27.032,   -8.722,   68.953   // Node #58
   26.992,   -8.671,   78.314   // Node #59
   22.014,   -8.633,   80.283   // Node #60
   16.997,   -8.720,   78.143   // Node #61
   17.044,   -8.560,   68.490   // Node #62
   17.122,   -8.720,   58.949   // Node #63
   21.821,   -8.760,   57.272   // Node #64
   26.928,   -8.778,   58.968   // Node #65
   22.014,   -3.067,   69.154   // Node #66
   23.021,   -5.177,   89.369   // Node #67
   31.514,   -5.180,   92.633   // Node #68
  118.918,   -5.178,   14.505   // Node #69
  110.278,   -5.178,   39.295   // Node #70
  135.113,   -5.171,   34.903   // Node #71
  147.530,   -5.179,  102.714   // Node #72
  140.099,   -5.181,  103.156   // Node #73
  141.804,   -5.177,   82.817   // Node #74
  142.439,   -5.173,   54.806   // Node #75
  142.141,   -5.176,   77.376   // Node #76
  147.865,   -5.171,   50.884   // Node #77
  148.601,   -5.169,   45.123   // Node #78
  133.329,   -5.172,   36.313   // Node #79
  130.550,   -5.184,  103.892   // Node #80
  131.412,   -5.179,   98.511   // Node #81
  134.475,   -5.177,   99.108   // Node #82
  134.265,   -5.177,  103.832   // Node #83
  140.357,   -5.177,  100.321   // Node #84
  141.217,   -5.177,   90.091   // Node #85
  133.726,   -5.177,   84.785   // Node #86
  129.049,   -5.180,   80.180   // Node #87
  129.172,   -5.177,   74.453   // Node #88
  135.897,   -5.177,   73.805   // Node #89
  147.899,   -5.177,   90.025   // Node #90
  120.386,   -5.199,   34.785   // Node #91
  120.145,   -5.198,   40.249   // Node #92
  118.744,   -5.175,   60.886   // Node #93
   15.356,   -5.180,   30.887   // Node #94
  143.441,   -5.177,   35.627   // Node #95
   64.367,    0.369,   25.085   // Node #96
   84.313,   -0.319,   14.843   // Node #97
  106.964,   -0.246,   14.787   // Node #98
  115.998,   -2.595,   14.972   // Node #99
  140.718,   -4.018,   16.688   // Node #100
  147.122,   -5.178,   16.715   // Node #101
  136.768,   -5.179,   93.459   // Node #102
  131.206,   -5.176,   94.788   // Node #103
   63.365,   -5.213,  106.332   // Node #104
   63.033,   -1.333,  116.456   // Node #105
   56.313,   -1.337,  125.560   // Node #106
   40.304,   -1.337,  127.866   // Node #107
   35.937,   -1.337,  125.673   // Node #108
   28.271,   -1.338,  112.535   // Node #109
   25.611,   -2.927,  105.832   // Node #110
   22.926,   -3.804,  100.321   // Node #111
   58.334,   -1.338,  125.627   // Node #112
   59.152,   -1.338,  128.119   // Node #113
   56.697,   -1.338,  129.652   // Node #114
   54.805,   -1.338,  129.664   // Node #115
   54.441,   -1.338,  126.005   // Node #116
   54.922,   -5.213,  106.295   // Node #117
   56.951,   -1.850,   88.859   // Node #118
   55.007,   -1.850,   87.510   // Node #119
   52.586,   -1.815,   86.989   // Node #120
   59.919,   -1.338,  121.752   // Node #121
   54.721,   -1.338,  123.485   // Node #122
   53.867,   -1.338,  119.216   // Node #123
   24.202,   -5.219,  108.796   // Node #124
   12.994,   -5.216,  107.754   // Node #125
   22.886,   -3.510,  113.097   // Node #126
   42.367,   -3.614,  112.805   // Node #127
   46.498,   -5.220,  108.875   // Node #128
   54.978,   -4.450,  109.295   // Node #129
   52.962,   -3.769,  112.712   // Node #130
   29.968,   -5.222,  109.012   // Node #131
   58.801,   -1.850,  114.698   // Node #132
   54.737,   -1.333,  116.308   // Node #133
   59.119,   -1.850,   92.324   // Node #134
   59.139,   -5.213,   82.956   // Node #135
   56.425,   -5.213,   80.499   // Node #136
   59.583,   -5.213,  106.364   // Node #137
   60.105,   -5.213,  113.030   // Node #138
   58.169,   -5.213,  113.369   // Node #139
   66.750,   -5.213,   90.669   // Node #140
   65.488,   -5.213,  100.006   // Node #141

170                                           // Number of path sections
   0,  21,   0, 255,   0, 255,    1.0, 1000   // Section #0
   1,  69,   0, 255,   0, 255,    0.7,    1   // Section #1
   3,   4,   0, 255,   0, 255,    1.1,    0   // Section #2
   4,   5,   0, 255,   0, 255,    0.5,    1   // Section #3
   5,   6,   0, 255,   0, 255,    0.5,    1   // Section #4
   6,   7,   0, 255,   0, 255,    0.5,    1   // Section #5
   7,   8,   0, 255,   0, 255,    0.5,    1   // Section #6
   8,   9,   0, 255,   0, 255,    0.5,    1   // Section #7
   9,  10,   0, 255,   0, 255,    0.5,    1   // Section #8
  10,  11,   0, 255,   0, 255,    0.5,    1   // Section #9
  12,  13,   0, 255,   0, 255,    0.5,    0   // Section #10
  13,  14,   0, 255,   0, 255,    0.5,    0   // Section #11
  14,  67,   0, 255,   0, 255,    0.5,    0   // Section #12
  15,  66,   0, 255,   0, 255,    0.5,    1   // Section #13
  16,  17,   0, 255,   0, 255,    0.5,    1   // Section #14
  17,  52,   0, 255,   0, 255,    1.2,    1   // Section #15
  24,  20,   0, 255,   0, 255,    1.5,    1   // Section #16
 101,  21,   0, 255,   0, 255,    1.7,    1   // Section #17
  21,   1,   0, 255,   0, 255,    1.0,    1   // Section #18
  20,  22,   0, 255,   0, 255,    0.3,    1   // Section #19
  71,  24,   0, 255,   0, 255,    1.2,    1   // Section #20
  26,  25,   0, 255,   0, 255,    0.4,    0   // Section #21
  26,  27,   0, 255,   0, 255,    0.4,    0   // Section #22
  27,  28,   0, 255,   0, 255,    0.4,    0   // Section #23
  28,  29,   0, 255,   0, 255,    2.0,    0   // Section #24
  29,  93,   0, 255,   0, 255,    1.5,    0   // Section #25
  28,  30,   0, 255,   0, 255,    1.0,    0   // Section #26
   2,  91,   0, 255,   0, 255,    0.5,    1   // Section #27
  32,  31,   0, 255,   0, 255,    1.0,    0   // Section #28
  31,   3,   0, 255,   0,  35,    1.8,    0   // Section #29
  33,  32,   0, 255,   0, 255,    1.6, 1000   // Section #30
  34,  31,   0, 255,   0, 255,    1.6,    0   // Section #31
  35,  34,   0, 255,   0, 255,    1.3, 1000   // Section #32
  36,  70,   0, 255,   0, 255,    0.5,    0   // Section #33
  37,  36,   0, 255,   0, 255,    0.4,    0   // Section #34
  38,  37,   0, 255,   0, 255,    0.4,    0   // Section #35
  39,  56,   0, 255,   0, 255,    0.4,    0   // Section #36
  40,  41,   0, 255,   0, 255,    1.0,    0   // Section #37
  41,   1,   0, 255,   0, 255,    1.0,    0   // Section #38
  42,  43,   0, 255,   0, 255,    0.5,    0   // Section #39
  40,  42,   0, 255,   0, 255,    0.7,    0   // Section #40
  44,   2,   0, 255,   0, 255,    0.3,    0   // Section #41
  45,  69,   0, 255,   0, 255,    0.2, 1000   // Section #42
  46,  45,   0, 255,   0, 255,    4.0, 1000   // Section #43
  48,  57,   0, 255,   0, 255,    1.0, 1000   // Section #44
  49,  14,   0, 255,   0, 255,    0.5, 1000   // Section #45
  50,  49,   0, 255,   0, 255,    0.5, 1000   // Section #46
  51,  16,   0,  15,   0,  15,    0.3, 1000   // Section #47
  53,  52,   0, 255,   0, 255,    1.2,    0   // Section #48
  52,  18,   0, 255,   0, 255,    1.0,    1   // Section #49
  54,  53,   0, 255,   0, 255,    1.0,    0   // Section #50
  56,  38,   0, 255,   0, 255,    0.3,    0   // Section #51
  39,  42,   0, 255,   0, 255,    0.5,    0   // Section #52
  58,  57,   0, 255,  25, 255,    0.9, 1000   // Section #53
  57,  47,   0, 255,   0, 255,    1.0,    0   // Section #54
  59,  58,   0, 255,   0, 255,    0.2, 1000   // Section #55
  60,  59,   0, 255,   0, 255,    0.5, 1000   // Section #56
  60,  61,   0, 255,   0, 255,    0.4,    0   // Section #57
  61,  62,   0, 255,   0, 255,    0.2, 1000   // Section #58
  63,  62,   0, 255,   0, 255,    0.2, 1000   // Section #59
  64,  63,   0, 255,   0, 255,    0.4, 1000   // Section #60
  64,  65,   0, 255,   0, 255,    0.4, 1000   // Section #61
  65,  58,   0, 255,   0, 255,    0.2, 1000   // Section #62
  62,  58,   0, 255,   0, 255,    0.8, 1000   // Section #63
  66,  16,   0, 255,   0, 255,    0.5,    1   // Section #64
  67,  15,   0, 255,   0, 255,    0.5,    1   // Section #65
  47,  67,   0, 255,   0, 255,    0.6,    0   // Section #66
  68,  67,   0, 255,   0, 255,    0.5, 1000   // Section #67
  69,   2,   0, 255,   0, 255,    0.7,    1   // Section #68
  43,  44,   0, 255,   0, 255,    0.3,    0   // Section #69
  70,   2,   0, 255,   0, 255,    0.5,    0   // Section #70
  43,  70,   0, 255,   0, 255,    1.2,    0   // Section #71
  70,  29,   0, 255,   0, 255,    1.2,    0   // Section #72
  71,  79,   0, 255,   0, 255,    1.3,    0   // Section #73
  30,  71,   0, 255,   0, 255,    1.2,    1   // Section #74
  90,  23,   0, 255,   0, 255,    0.9,    0   // Section #75
  72,  73,   0, 255,   0, 255,    0.3,    0   // Section #76
  73,  84,   0, 255,   0, 255,    1.0,    1   // Section #77
  76,  74,   0, 255,   0, 255,    0.4,    1   // Section #78
  77,  75,   0, 255,   0, 255,    0.9,    1   // Section #79
  75,  76,   0, 255,   0, 255,    1.1,    1   // Section #80
  78,  77,   0, 255,   0, 255,    0.6,    1   // Section #81
  23,  77,   0, 255,   0, 255,    0.9,    0   // Section #82
  79,  28,   0, 255,   0, 255,    1.3,    0   // Section #83
  83,  73,   0, 255,   0, 255,    0.3,    0   // Section #84
  81,  80,   0, 255,   0, 255,    0.3,    0   // Section #85
  81,  82,   0, 255,   0, 255,    0.3,    0   // Section #86
  82,  83,   0, 255,   0, 255,    0.3,    0   // Section #87
  80,  83,   0, 255,   0, 255,    0.3,    0   // Section #88
  82,  84,   0, 255,   0, 255,    0.3,    0   // Section #89
  84,  85,   0, 255,   0, 255,    1.0,    0   // Section #90
  86, 102,   0, 255,   0, 255,    1.1,    0   // Section #91
  74,  85,   0, 255,   0, 255,    1.0,    1   // Section #92
  87,  86,   0, 255,   0, 255,    1.0,    0   // Section #93
  87,  88,   0, 255,   0, 255,    1.0,    0   // Section #94
  88,  89,   0, 255,   0, 255,    1.1,    0   // Section #95
  89,  76,   0, 255,   0, 255,    1.2,    0   // Section #96
  89,  75,   0, 255,   0, 255,    1.2,    0   // Section #97
  86,  89,   0, 255,   0, 255,    1.0,    0   // Section #98
  90,  85,   0, 255,   0, 255,    0.9,    0   // Section #99
  90,  72,   0, 255,   0, 255,    0.9,    0   // Section #100
  91,  92,   0, 255,   0, 255,    0.5,    0   // Section #101
  91,  30,   0, 255,   0, 255,    0.4,    1   // Section #102
  92,  29,   0, 255,   0, 255,    1.2,    0   // Section #103
  93,  31,   0, 255,   0,  45,    0.4,    0   // Section #104
  55,  16,   0, 255,   0, 255,    0.7,    0   // Section #105
  55,  94,   0, 255,   0, 255,    1.2,    0   // Section #106
  94,  52,   0, 255,   0, 255,    0.5,    0   // Section #107
  54,  94,   0, 255,   0, 255,    1.0,    0   // Section #108
  25,  95,   0, 255,   0, 255,    0.4,    0   // Section #109
  24,  95,   0, 255,   0, 255,    0.4,    0   // Section #110
  18,  96,   0, 255,   0, 255,    0.6,    1   // Section #111
  96,  97,   0, 255,   0, 255,    0.9,    1   // Section #112
  97,  19,   0, 255,   0, 255,    1.2,    1   // Section #113
  19,  98,   0, 255,   0, 255,    1.2,    1   // Section #114
  98,  99,   0, 255,   0, 255,    1.2, 1001   // Section #115
  99, 100,   0, 255,   0, 255,    1.2,    1   // Section #116
 100, 101,   0, 255,   0, 255,    1.2,    1   // Section #117
  20, 101,   0, 255,   0, 255,    1.7,    0   // Section #118
 102, 103,   0, 255,   0, 255,    0.6,    1   // Section #119
  85, 102,   0, 255,   0, 255,    1.1,    1   // Section #120
 103,   4,   0, 255,   0, 255,    0.9,    1   // Section #121
  22,  78,   0, 255,   0, 255,    0.5,    1   // Section #122
  11, 104,   0, 255,   0, 255,    0.5,    1   // Section #123
 104, 105,   0, 255,   0,  40,    0.5,    1   // Section #124
 105, 121,   0, 255,   0, 255,    0.5,    1   // Section #125
 106, 116,   0, 255,   0, 255,    0.5,    1   // Section #126
 107, 108,   0, 255,   0, 255,    0.5,    1   // Section #127
 108, 109,   0, 255,  40,  50,    0.5,    1   // Section #128
 109, 110,   0, 255,   0, 255,    0.5,    1   // Section #129
 110, 111,   0, 255,   0, 255,    0.5,    1   // Section #130
 111,  67,   0, 255,   0, 255,    0.5,    1   // Section #131
 112, 106,   0, 255,   0, 255,    0.5,    0   // Section #132
 113, 112,   0, 255,   0, 255,    0.5,    0   // Section #133
 114, 113,   0, 255,   0, 255,    0.5,    0   // Section #134
 115, 114,   0, 255,   0, 255,    0.5,    0   // Section #135
 115, 116,   0, 255,   0, 255,    0.3,    0   // Section #136
 116, 107,   0, 255,   0, 255,    0.5,    1   // Section #137
 117, 129,   0, 255,   0, 255,    0.5,    1   // Section #138
 118, 119,   0, 255,   0, 255,    0.5,    0   // Section #139
 119, 120,   0, 255,   0, 255,    0.5,    0   // Section #140
 120,  12,   0, 255,   0, 255,    0.5,    0   // Section #141
 123, 122,   0, 255,   0, 255,    0.5,    0   // Section #142
 121, 106,   0, 255,   0, 255,    0.5,    1   // Section #143
 122, 116,   0, 255,   0, 255,    0.2,    0   // Section #144
 123, 121,   0, 255,   0, 255,    0.5,    0   // Section #145
 125, 124,   0, 255,   0, 255,    0.5, 1000   // Section #146
 124, 126,   0, 255,   0, 255,    0.5,    0   // Section #147
 126, 127,   0, 255,   0, 255,    0.5,    0   // Section #148
 127, 128,   0, 255,   0, 255,    0.5,    0   // Section #149
 128, 129,   0, 255,   0, 255,    0.5, 1000   // Section #150
 129, 133,   0, 255,   0,  30,    0.5,    1   // Section #151
 124, 131,   0, 255,   0, 255,    0.5, 1000   // Section #152
 130, 128,   0, 255,   0, 255,    0.5, 1000   // Section #153
 127, 131,   0, 255,   0, 255,    0.5,    0   // Section #154
 131, 128,   0, 255,   0, 255,    0.5, 1000   // Section #155
 133, 106,   0, 255,   0, 255,    0.5,    1   // Section #156
  11, 117,   0, 255,   0, 255,    0.5,    1   // Section #157
 118, 134,   0, 255,   0, 255,    0.5,    0   // Section #158
 134, 132,   0, 255,   0, 255,    0.5,    0   // Section #159
 132, 121,   0, 255,   0, 255,    0.5,    0   // Section #160
 135,  11,   0, 255,   0, 255,    0.5,    0   // Section #161
 136, 135,   0, 255,   0, 255,    0.5, 1000   // Section #162
 104, 137,   0, 255,   0, 255,    0.5,    0   // Section #163
 138, 137,   0, 255,   0, 255,    0.5, 1000   // Section #164
 137, 117,   0, 255,   0, 255,    0.5,    0   // Section #165
 139, 137,   0, 255,   0, 255,    0.5, 1000   // Section #166
  11, 140,   0, 255,   0, 255,    0.5,    0   // Section #167
 140, 141,   0, 255,   0, 255,    0.5,    0   // Section #168
 141, 104,   0, 255,   0, 255,    0.5,    0   // Section #169

0                                                             // Number of cop start points

END OF OPPONENT PATHS

2										// number of material modifiers

// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT							// skid mark material

//	material '0'
1.0										// car wall friction
1.0										// tyre road friction
0										// down force
0.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
1										// room for expansion
none									// room for expansion

// Non CarObjects
2										// number of non car objects
BARRIER.TXT
WRECK.TXT

0									// Number of smoke shadetables

8										// Number of network start points

129.75,-5.17,-1.22							//1
270													

146.57,-5.17,10.49							//2						
180									

117.75,-5.17,44.13							//3						
180									

93.29,-5.17,1.23							//4						
270									

107.79,-5.17,32.17						//5						
225									

107.78,-5.17,55.58							//6						
180									

120.88,-6.38,95.1							//7						
270									

141.89,-5.17,59.36							//8						
310									

1								// number of splash files
SPLSHYEL.PIX 						// name of pixelmapfile for splashes

1

NETINDA.TXT
