VERSION 5		// V1 expects map checkpoint rectangles
			// V2 and above expect map checkpoint points
			// V3 and above expect splash file stuff at the end
			// V4 and above expect two sets of PIX and MAT and ped substitution entry

-0.411,-0.247,-12.001   						// Position of centre of start of grid
181									// Direction that grid faces in

// Laps, checkpoints etc

60,30,10							// Initial timer count for each skill level
4									// # laps
5000,5000,5000						// Race completed bonus (all laps raced) for each skill level
10000,10000,10000					// Race completed bonus (all peds killed) for each skill level
10000,10000,10000					// Race completed bonus (all oppos wasted) for each skill level

// Width and height of map checkpoint rectangles
9,18
11,26

0									// # checkpoints


4									// # pixelmap files to load
DD.PIX
BIGSTAND.PIX
DRKSCRN.PIX
FOGSCRN.PIX


4									// # pixelmap files to load(low memory)
DD.PIX
BIGSTAND.PIX
DRKSCRN.PIX
FOGSCRN.PIX


2									// # shade table files to load
DRRENDER.TAB
IDENTITY.TAB

4									// # material files to load
DD.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT


4									// # material files to load(low memory)

DD.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT


1									// # model files to load
DERBY.DAT

DERBY.ACT							// Track actor
DRBYX.ACT							// Additional actor

// HORIZON STUFF

NONE						// Name of sky texture pixelmap (or "none")
5									// Horizontal repetitions of sky texture
72									// Vertical size of sky texture (degrees)
242									// Position of horizon (pixels below top)
dark								// Depth cue mode ("none", "dark" or "fog")
6,0									// Degree of fog/darkness

// DEFAULT ENGINE NOISE

0

// SPECIAL EFFECTS VOLUMES

0				// # special effects volumes


 
// REFLECTIVE WINDSCREEN SPECIFICATIONS

DARKSKY.MAT							// Material to use for default screens
DRKSCRN.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT							// Material to use for default screens during fog

0									// # areas with different screens

// MAP DETAILS

NDDMAP.PIX							// Map pixelmap name

3.153,	-3.112,		0				// World->map transformation matrix
0,		0,	   		0
2.971,	3.113,		0
159.9,	104.2,		0

// ****** START OF FUNK AND GROOVE STUFF ******

START OF FUNK

END OF FUNK



START OF GROOVE

END OF GROOVE


// ****** START OF PEDESTRIAN STUFF ******

30

146				// Number of pedestrians

// Pedestrian number 1

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-9.597,-2.071,-11.649
	reverse


// Pedestrian number 2

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-11.536,-2.071,-9.616
	reverse


// Pedestrian number 3

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-13.575,-2.071,-7.617
	reverse


// Pedestrian number 4

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-7.717,-2.071,-13.508
	reverse


// Pedestrian number 5

31				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-15.539,-2.071,-24.423
	point
	-18.114,-2.071,-24.202
	point
	-20.935,-2.071,-22.306
	reverse


// Pedestrian number 6

31				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-12.630,-2.071,-19.882
	point
	-11.985,-2.071,-21.159
	point
	-10.117,-2.071,-22.237
	reverse


// Pedestrian number 7

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-16.204,-2.071,-19.761
	point
	-17.804,-2.071,-18.596
	point
	-18.712,-2.071,-17.625
	reverse


// Pedestrian number 8

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-14.935,-2.071,-19.972
	point
	-11.467,-2.071,-21.137
	point
	-7.093,-2.071,-21.815
	reverse


// Pedestrian number 9

22				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-7.146,-2.071,-21.961
	point
	-8.299,-2.071,-22.201
	point
	-9.831,-2.071,-22.356
	reverse


// Pedestrian number 10

29				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-9.965,-2.071,-22.302
	point
	-9.677,-2.071,-21.933
	point
	-7.219,-2.071,-21.301
	point
	-4.278,-2.071,-19.712
	reverse


// Pedestrian number 11

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-5.184,-2.071,-20.823
	point
	-6.837,-2.071,-21.857
	point
	-8.236,-2.071,-22.078
	reverse


// Pedestrian number 12

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-8.726,-2.071,-22.193
	point
	-9.566,-2.071,-22.105
	point
	-10.409,-2.071,-22.141
	reverse


// Pedestrian number 13

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-10.479,-2.071,-18.979
	point
	-11.559,-2.071,-20.323
	point
	-11.140,-2.071,-21.384
	point
	-10.696,-2.071,-21.908
	reverse


// Pedestrian number 14

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-11.586,-2.071,-21.316
	point
	-10.399,-2.071,-21.672
	point
	-9.665,-2.071,-22.275
	reverse


// Pedestrian number 15

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-21.881,-2.071,-21.317
	point
	-22.230,-2.071,-18.598
	point
	-24.896,-2.071,-13.061
	reverse


// Pedestrian number 16

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-24.477,-2.071,-16.934
	point
	-23.327,-2.071,-17.162
	point
	-18.924,-2.071,-17.223
	reverse


// Pedestrian number 17

12				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-24.358,-2.071,-17.450
	point
	-23.780,-2.071,-17.378
	point
	-23.453,-2.071,-16.848
	point
	-24.035,-2.071,-14.437
	point
	-24.842,-2.071,-14.008
	reverse


// Pedestrian number 18

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-24.807,-2.071,-14.945
	point
	-23.975,-2.071,-16.508
	point
	-24.228,-2.071,-17.702
	reverse


// Pedestrian number 19

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-24.594,-2.071,-16.585
	point
	-24.441,-2.071,-17.215
	point
	-24.119,-2.071,-18.271
	reverse


// Pedestrian number 20

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-23.992,-2.071,-18.502
	point
	-22.991,-2.071,-20.350
	point
	-22.235,-2.071,-21.181
	reverse


// Pedestrian number 21

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-22.300,-2.071,-20.633
	point
	-22.094,-2.071,-19.334
	point
	-19.778,-2.071,-15.920
	reverse


// Pedestrian number 22

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-21.092,-2.071,-21.932
	point
	-19.400,-2.071,-22.325
	point
	-16.168,-2.071,-24.475
	reverse


// Pedestrian number 23

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-14.504,-2.071,-24.844
	point
	-11.845,-2.071,-23.427
	point
	-10.109,-2.071,-23.059
	point
	-7.621,-2.071,-22.793
	point
	0.038,-2.071,-20.376
	reverse


// Pedestrian number 24

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-13.333,-2.071,-2.741
	reverse


// Pedestrian number 25

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-5.889,-2.071,-2.767
	reverse


// Pedestrian number 26

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-2.785,-2.071,-4.538
	reverse


// Pedestrian number 27

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-3.542,-2.071,-18.415
	reverse


// Pedestrian number 28

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-8.602,-2.071,-17.221
	reverse


// Pedestrian number 29

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-11.570,-1.849,-25.049
	point
	-12.025,-1.849,-25.332
	point
	-13.556,-1.849,-25.527
	reverse


// Pedestrian number 30

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-15.541,-2.071,-24.712
	point
	-18.152,-2.071,-23.695
	point
	-20.166,-2.071,-23.083
	reverse


// Pedestrian number 31

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-20.020,-2.071,-22.732
	point
	-19.007,-2.071,-22.292
	point
	-9.830,-2.071,-19.506
	point
	-9.406,-2.071,-18.328
	reverse


// Pedestrian number 32

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-2.612,-2.071,-14.032
	point
	-2.957,-2.071,-15.107
	point
	-2.822,-2.071,-15.606
	point
	-3.059,-2.071,-17.203
	reverse


// Pedestrian number 33

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-3.110,-2.071,-17.371
	point
	-3.668,-2.071,-18.157
	point
	-4.629,-2.071,-20.179
	reverse


// Pedestrian number 34

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-6.074,-2.071,-21.621
	point
	-5.777,-2.071,-20.803
	point
	-4.333,-2.071,-19.870
	point
	-3.847,-2.071,-19.053
	reverse


// Pedestrian number 35

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-4.163,-2.071,-19.556
	point
	-3.816,-2.071,-18.445
	point
	-3.334,-2.071,-17.968
	reverse


// Pedestrian number 36

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-2.919,-2.071,-16.727
	point
	-3.016,-2.071,-16.989
	point
	-3.600,-2.071,-17.548
	point
	-4.616,-2.071,-19.637
	point
	-5.423,-2.071,-20.717
	reverse


// Pedestrian number 37

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-6.214,-2.071,-21.550
	point
	-5.481,-2.071,-21.151
	point
	-4.514,-2.071,-20.188
	reverse


// Pedestrian number 38

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-4.005,-2.071,-19.378
	point
	-4.012,-2.071,-18.297
	point
	-2.701,-2.071,-15.714
	reverse


// Pedestrian number 39

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-2.910,-2.071,-11.712
	point
	-2.699,-2.071,-13.639
	point
	-2.650,-2.071,-15.518
	point
	-2.819,-2.071,-16.718
	reverse


// Pedestrian number 40

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-3.629,-2.071,-17.735
	point
	-7.447,-2.071,-13.475
	point
	-8.554,-2.071,-12.621
	reverse


// Pedestrian number 41

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-8.778,-2.071,-12.432
	point
	-8.068,-2.071,-7.272
	point
	-9.590,-2.071,-2.746
	reverse


// Pedestrian number 42

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-12.195,-2.071,-2.764
	point
	-9.971,-2.071,-3.600
	point
	-3.691,-2.071,-2.954
	reverse


// Pedestrian number 43

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-9.211,-2.071,-11.346
	point
	-10.525,-2.071,-10.608
	point
	-11.354,-2.071,-9.505
	point
	-12.112,-2.071,-9.125
	reverse


// Pedestrian number 44

11				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-13.668,-2.071,-7.310
	point
	-12.320,-2.071,-8.477
	point
	-10.902,-2.071,-9.369
	point
	-10.205,-2.071,-10.567
	point
	-9.211,-2.071,-11.813
	reverse


// Pedestrian number 45

11				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-8.719,-2.071,-2.884
	point
	-7.663,-2.071,-2.796
	point
	-6.150,-2.071,-3.036
	point
	-5.113,-2.071,-2.714
	reverse


// Pedestrian number 46

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-7.820,-2.071,-16.122
	point
	-8.109,-2.071,-17.205
	point
	-9.664,-2.071,-18.486
	point
	-11.267,-2.071,-19.514
	reverse


// Pedestrian number 47

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-13.368,-2.071,-20.275
	point
	-15.571,-2.071,-19.964
	point
	-16.091,-2.071,-19.623
	point
	-22.601,-2.071,-20.619
	reverse


// Pedestrian number 48

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-19.306,-2.071,-16.726
	point
	-19.932,-2.071,-15.186
	point
	-19.997,-2.071,-13.549
	reverse


// Pedestrian number 49

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-19.261,-2.071,-10.586
	point
	-18.986,-2.071,-9.744
	point
	-18.043,-2.071,-3.353
	reverse


// Pedestrian number 50

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-17.310,-2.071,-3.116
	point
	-15.910,-2.071,-2.704
	point
	-15.102,-2.071,-2.564
	reverse


// Pedestrian number 51

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-17.811,-2.071,-3.278
	point
	-16.775,-2.071,-2.917
	point
	-15.891,-2.071,-3.014
	point
	-15.562,-2.071,-4.256
	point
	-14.092,-2.071,-7.420
	reverse


// Pedestrian number 52

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-14.054,-2.071,-2.667
	point
	-14.465,-2.071,-3.884
	point
	-15.829,-2.071,-4.027
	point
	-16.970,-2.071,-4.001
	point
	-22.383,-2.071,-0.975
	reverse


// Pedestrian number 53

1				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	-23.094,-2.071,-7.530
	point
	-23.004,-2.071,-7.105
	point
	-23.150,-2.071,-6.842
	point
	-23.548,-2.071,-6.958
	point
	-24.054,-2.071,-7.384
	point
	-24.888,-2.071,-9.270
	point
	-29.224,-2.071,-13.988
	reverse


// Pedestrian number 54

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-24.900,-2.071,-12.677
	point
	-24.772,-2.071,-11.708
	point
	-24.241,-2.071,-10.653
	point
	-24.041,-2.071,-9.254
	reverse


// Pedestrian number 55

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-17.542,-2.071,-3.459
	point
	-16.617,-2.071,-5.457
	point
	-15.640,-2.071,-6.232
	point
	-14.632,-2.071,-7.315
	reverse


// Pedestrian number 56

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-12.514,-2.071,-8.319
	point
	-8.164,-2.071,-9.923
	point
	-2.918,-2.071,-14.086
	reverse


// Pedestrian number 57

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	2.993,-2.071,-11.901
	point
	2.972,-2.071,-7.252
	point
	2.781,-2.071,-5.686
	reverse


// Pedestrian number 58

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	6.549,-2.071,-2.962
	point
	5.496,-2.071,-2.811
	point
	3.076,-2.071,-3.012
	reverse


// Pedestrian number 59

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-5.714,-2.071,-21.361
	point
	-7.189,-2.071,-21.741
	point
	-8.877,-2.071,-21.962
	point
	-10.468,-2.071,-21.909
	reverse


// Pedestrian number 60

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-9.316,-2.071,-22.183
	point
	-10.495,-2.071,-21.767
	point
	-12.073,-2.071,-19.849
	reverse


// Pedestrian number 61

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-10.309,-2.071,-19.208
	point
	-13.009,-2.071,-20.184
	point
	-14.229,-2.071,-19.992
	reverse


// Pedestrian number 62

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-4.322,-2.071,-20.001
	point
	-5.583,-2.071,-20.481
	point
	-10.446,-2.071,-19.190
	reverse


// Pedestrian number 63

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-8.868,-2.071,-22.216
	point
	-7.752,-2.071,-21.252
	point
	-7.047,-2.071,-19.518
	point
	-7.625,-2.071,-14.927
	reverse


// Pedestrian number 64

31				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-7.545,-2.071,-14.515
	point
	-7.396,-2.071,-13.068
	point
	-8.932,-2.071,-11.654
	reverse


// Pedestrian number 65

22				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-5.005,-2.071,-19.431
	point
	-6.720,-2.071,-21.328
	point
	-7.791,-2.071,-22.031
	reverse


// Pedestrian number 66

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-8.248,-2.071,-17.180
	point
	-7.565,-2.071,-18.747
	point
	-9.790,-2.071,-21.717
	point
	-10.157,-2.071,-22.229
	reverse


// Pedestrian number 67

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-13.731,-2.071,-20.041
	point
	-11.641,-2.071,-19.769
	point
	-9.340,-2.071,-21.787
	point
	-8.917,-2.071,-22.292
	reverse


// Pedestrian number 68

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-6.509,-2.071,-21.698
	point
	-7.407,-2.071,-21.262
	point
	-8.651,-2.071,-21.761
	point
	-9.879,-2.071,-22.237
	point
	-11.056,-2.071,-21.744
	reverse


// Pedestrian number 69

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-12.855,-2.071,-19.995
	point
	-16.346,-2.071,-21.184
	point
	-20.630,-2.071,-21.207
	point
	-22.448,-2.071,-20.696
	reverse


// Pedestrian number 70

12				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-21.852,-2.071,-21.639
	point
	-22.614,-2.071,-20.239
	point
	-22.070,-2.071,-19.083
	point
	-22.223,-2.071,-17.846
	point
	-24.937,-2.071,-14.450
	point
	-25.057,-2.071,-13.501
	reverse


// Pedestrian number 71

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-9.342,-2.071,-22.316
	point
	-7.476,-2.071,-20.645
	point
	-3.182,-2.071,-15.360
	reverse


// Pedestrian number 72

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-3.357,-2.071,-17.521
	point
	-2.963,-2.071,-16.946
	point
	-2.649,-2.071,-15.933
	reverse


// Pedestrian number 73

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	4.255,-2.071,-13.263
	point
	6.251,-2.071,-11.709
	point
	8.458,-2.071,-10.821
	reverse


// Pedestrian number 74

22				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	9.655,-2.071,-9.808
	point
	10.897,-2.071,-8.659
	point
	12.043,-2.071,-7.307
	reverse


// Pedestrian number 75

11				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	15.846,-2.071,-1.463
	point
	13.991,-2.071,-1.407
	point
	13.252,-2.071,-2.009
	point
	12.854,-2.071,-4.928
	reverse


// Pedestrian number 76

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	11.746,-2.071,-2.804
	point
	9.597,-2.071,-3.590
	point
	7.232,-2.071,-2.902
	reverse


// Pedestrian number 77

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	8.225,-2.071,-2.775
	point
	7.438,-2.071,-3.220
	point
	5.346,-2.071,-4.952
	point
	3.102,-2.071,-6.006
	reverse


// Pedestrian number 78

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	2.933,-2.071,-4.215
	point
	3.112,-2.071,-4.963
	point
	3.998,-2.071,-5.878
	point
	6.311,-2.071,-12.830
	reverse


// Pedestrian number 79

5				// Ref num
8				// Number of instructions
4				// Initial instruction

	point
	-5.714,-2.071,-22.174
	point
	-3.600,-2.071,-20.333
	point
	-2.694,-2.071,-18.444
	point
	-2.273,-2.071,-17.214
	point
	-0.783,-2.071,-15.358
	point
	2.735,-2.071,-13.176
	point
	3.968,-2.071,-13.363
	reverse


// Pedestrian number 80

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	2.956,-2.071,-13.321
	point
	3.361,-2.071,-12.468
	point
	2.847,-2.071,-9.261
	reverse


// Pedestrian number 81

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	2.792,-2.071,-8.566
	point
	4.672,-2.071,-7.489
	point
	12.823,-2.071,-5.964
	reverse


// Pedestrian number 82

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.066,-2.071,-11.320
	reverse


// Pedestrian number 83

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.734,-2.071,-10.153
	reverse


// Pedestrian number 84

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.744,-2.071,-7.386
	reverse


// Pedestrian number 85

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.415,-2.071,-2.920
	reverse


// Pedestrian number 86

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.205,-2.071,-2.836
	reverse


// Pedestrian number 87

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.941,-2.071,-3.311
	reverse


// Pedestrian number 88

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.887,-2.071,-3.710
	reverse


// Pedestrian number 89

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-4.407,-2.071,2.773
	reverse


// Pedestrian number 90

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-2.923,-2.071,3.295
	reverse


// Pedestrian number 91

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-2.870,-2.071,3.755
	reverse


// Pedestrian number 92

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-2.875,-2.071,4.358
	reverse


// Pedestrian number 93

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	23.083,-2.071,6.987
	point
	22.825,-2.071,7.702
	point
	23.245,-2.071,8.729
	point
	24.602,-2.071,16.417
	reverse


// Pedestrian number 94

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.821,-2.071,18.381
	point
	22.366,-2.071,20.150
	point
	21.651,-2.071,21.557
	reverse


// Pedestrian number 95

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	20.974,-2.071,22.185
	point
	20.381,-2.071,22.747
	point
	18.114,-2.071,23.828
	point
	12.634,-2.071,21.424
	reverse


// Pedestrian number 96

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	11.578,-2.071,21.380
	point
	8.768,-2.071,22.117
	point
	6.095,-2.071,21.548
	reverse


// Pedestrian number 97

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	5.706,-2.071,21.332
	point
	6.045,-2.071,20.542
	point
	7.869,-2.071,15.954
	reverse


// Pedestrian number 98

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	8.115,-2.071,16.486
	point
	9.058,-2.071,18.772
	point
	9.611,-2.071,19.214
	point
	12.218,-2.071,19.788
	reverse


// Pedestrian number 99

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	14.901,-2.071,20.148
	point
	16.852,-2.071,20.402
	point
	18.940,-2.071,17.216
	point
	19.619,-2.071,16.041
	reverse


// Pedestrian number 100

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	20.002,-2.071,15.097
	point
	20.025,-2.071,13.363
	point
	20.554,-2.071,11.717
	point
	22.750,-2.071,8.047
	reverse


// Pedestrian number 101

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	23.725,-2.071,7.092
	point
	23.455,-2.071,6.871
	point
	18.314,-2.071,4.093
	point
	15.773,-2.071,2.675
	reverse


// Pedestrian number 102

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	14.962,-2.071,2.676
	point
	13.384,-2.071,7.482
	point
	11.985,-2.070,9.074
	reverse


// Pedestrian number 103

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.535,-2.070,9.477
	reverse


// Pedestrian number 104

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.480,-2.071,7.718
	reverse


// Pedestrian number 105

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.613,-2.071,11.496
	reverse


// Pedestrian number 106

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.554,-2.071,13.456
	reverse


// Pedestrian number 107

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.998,-2.071,22.258
	reverse


// Pedestrian number 108

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.929,-2.071,25.067
	reverse


// Pedestrian number 109

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	17.795,-2.071,18.531
	reverse


// Pedestrian number 110

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	18.020,-2.070,9.156
	reverse


// Pedestrian number 111

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-5.846,-2.071,12.671
	reverse


// Pedestrian number 112

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-8.849,-2.071,9.827
	reverse


// Pedestrian number 113

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-12.665,-2.071,5.452
	point
	-11.785,-2.071,6.749
	point
	-10.712,-2.071,7.839
	point
	-3.078,-2.071,9.971
	reverse


// Pedestrian number 114

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-2.148,-2.071,13.543
	point
	-4.209,-2.071,13.036
	point
	-7.566,-2.071,11.458
	reverse


// Pedestrian number 115

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-2.779,-2.071,9.371
	point
	-3.128,-2.071,8.561
	point
	-2.763,-2.071,5.598
	reverse


// Pedestrian number 116

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-3.187,-2.071,4.970
	point
	-3.760,-2.071,4.761
	point
	-5.164,-2.071,4.685
	point
	-7.841,-2.071,2.820
	reverse


// Pedestrian number 117

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-9.765,-2.071,2.737
	point
	-11.580,-2.071,2.802
	point
	-12.484,-2.071,3.129
	point
	-13.231,-2.071,3.446
	reverse


// Pedestrian number 118

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-12.071,-2.071,2.828
	point
	-12.394,-2.071,2.765
	point
	-13.786,-2.071,1.747
	point
	-18.578,-2.071,-2.854
	point
	-22.850,-2.071,-7.479
	reverse


// Pedestrian number 119

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-23.635,-2.071,-8.512
	point
	-23.830,-2.071,-10.767
	point
	-24.730,-2.071,-14.267
	reverse


// Pedestrian number 120

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	4.125,-2.071,19.217
	point
	7.722,-2.071,19.391
	point
	14.501,-2.071,20.029
	reverse


// Pedestrian number 121

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	15.500,-2.071,19.773
	point
	17.230,-2.071,19.015
	point
	23.965,-2.071,18.004
	reverse


// Pedestrian number 122

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.351,-2.071,19.395
	point
	23.937,-2.071,16.489
	point
	24.740,-2.071,13.946
	reverse


// Pedestrian number 123

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	24.800,-2.071,12.998
	point
	22.855,-2.071,11.295
	point
	21.772,-2.071,10.941
	point
	19.249,-2.071,10.391
	reverse


// Pedestrian number 124

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	19.298,-2.071,10.781
	point
	20.091,-2.071,11.167
	point
	20.862,-2.071,11.922
	point
	20.055,-2.071,12.706
	reverse


// Pedestrian number 125

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	24.984,-2.071,13.714
	point
	23.375,-2.071,15.578
	point
	22.789,-2.071,15.945
	point
	22.658,-2.071,20.250
	reverse


// Pedestrian number 126

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	22.283,-2.071,21.002
	point
	20.644,-2.071,21.598
	point
	19.320,-2.071,21.944
	point
	17.386,-2.071,24.031
	reverse


// Pedestrian number 127

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	16.310,-2.071,24.460
	point
	14.424,-2.071,24.415
	point
	13.122,-2.071,24.764
	point
	11.554,-2.071,24.551
	reverse


// Pedestrian number 128

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	7.035,-2.071,22.613
	point
	8.099,-2.071,23.026
	point
	10.103,-2.071,23.050
	point
	10.472,-2.071,22.881
	point
	14.762,-2.071,20.238
	reverse


// Pedestrian number 129

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	18.790,-2.071,17.766
	point
	23.474,-2.071,14.885
	point
	24.353,-2.071,12.179
	reverse


// Pedestrian number 130

12				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	24.852,-2.071,13.715
	point
	23.573,-2.071,11.330
	point
	22.904,-2.071,10.679
	point
	18.937,-2.071,9.691
	point
	17.987,-2.071,8.980
	reverse


// Pedestrian number 131

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.699,-2.071,8.758
	point
	23.848,-2.071,9.317
	point
	23.613,-2.071,10.388
	reverse


// Pedestrian number 132

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	24.522,-2.071,12.146
	point
	23.257,-2.071,11.496
	point
	20.378,-2.071,11.703
	reverse


// Pedestrian number 133

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	18.792,-2.071,9.671
	point
	18.028,-2.071,8.471
	point
	16.963,-2.071,8.217
	reverse


// Pedestrian number 134

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	12.879,-2.071,8.203
	point
	9.097,-2.071,9.198
	point
	3.036,-2.071,12.455
	reverse


// Pedestrian number 135

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	2.778,-2.071,15.313
	point
	3.157,-2.071,17.333
	point
	3.562,-2.071,18.339
	reverse


// Pedestrian number 136

11				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	2.837,-2.071,13.565
	point
	2.927,-2.071,11.163
	point
	4.271,-2.071,8.500
	point
	7.141,-2.071,3.998
	point
	8.652,-2.071,2.938
	reverse


// Pedestrian number 137

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	9.986,-2.071,2.869
	point
	9.123,-2.071,4.361
	point
	6.813,-2.071,4.830
	point
	3.167,-2.071,5.559
	reverse


// Pedestrian number 138

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	4.555,-2.071,3.143
	point
	3.491,-2.071,3.831
	point
	2.946,-2.071,6.216
	point
	2.750,-2.071,7.996
	reverse


// Pedestrian number 139

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	2.749,-2.071,8.856
	point
	5.548,-2.071,11.662
	point
	7.203,-2.071,14.176
	reverse


// Pedestrian number 140

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	7.785,-2.071,13.344
	point
	7.506,-2.071,13.937
	point
	7.607,-2.071,15.205
	point
	8.628,-2.071,17.438
	reverse


// Pedestrian number 141

22				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	11.850,-2.071,21.260
	point
	10.777,-2.071,21.699
	point
	9.494,-2.071,21.211
	point
	8.721,-2.071,20.226
	point
	8.347,-2.071,18.174
	reverse


// Pedestrian number 142

22				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	13.305,-2.071,2.800
	point
	13.873,-2.071,2.686
	point
	14.071,-2.071,2.593
	point
	14.794,-2.071,2.527
	reverse


// Pedestrian number 143

31				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	16.356,-2.071,2.804
	point
	15.156,-2.071,3.079
	point
	14.311,-2.071,2.642
	point
	12.981,-2.071,3.126
	point
	12.094,-2.071,2.818
	reverse


// Pedestrian number 144

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	13.729,-2.071,7.525
	point
	16.657,-2.071,7.349
	point
	22.949,-2.071,7.499
	reverse


// Pedestrian number 145

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	18.736,-2.071,9.992
	point
	18.521,-2.071,3.094
	point
	18.150,-2.071,-0.847
	reverse


// Pedestrian number 146

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	23.324,-2.071,8.077
	point
	23.409,-2.071,8.578
	point
	22.956,-2.071,10.226
	point
	22.239,-2.071,11.397
	point
	19.903,-2.071,14.894
	reverse








START OF OPPONENT PATHS

2                              // Number of path nodes
    0.155,   -2.071,  -10.409   // Node #0
   -0.079,   -2.071,    0.005   // Node #1
   
1                                            // Number of path sections
   0,   1,   0, 255,   0, 255,    1.4,    1   // Section #0
  
0                                                             // Number of cop start points

END OF OPPONENT PATHS



10										// number of material modifiers

// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT										// room for expansion

//  material 0
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT										// room for expansion

//  material 1
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
MUD1.MAT										// room for expansion

//  material 2
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT										// room for expansion

//  material 3
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT										// room for expansion

//  material 4
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT										// room for expansion

//  material 5
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT										// room for expansion

//  material 6
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT										// room for expansion

//  material 7
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT										// room for expansion

//  material 8
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT										// room for expansion


// Non CarObjects

5									// number of non car objects
PALM2.TXT
CONE.TXT
GREENCAR.TXT
WRECK.TXT
GASPUMP.TXT


1									// Number of smoke shadetables

222, 230, 245								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"


6								// Number of network start points

9.553,-2.071,9.558
318

18.426,-2.071,19.611
115

-10.521,-2.071,7.249
246

10.082,-2.071,-8.825
199

-8.711,-2.071,-8.997
111

-16.738,-2.071,-20.209
289



1								// number of splash files
SPLSHGRN.PIX 						//  name of pixelmapfile for splashes


2 								//  yon multiplier

DD3.TXT
