VERSION 6		// V1 expects map checkpoint rectangles
			// V2 and above expect map checkpoint points
			// V3 and above expect splash file stuff at the end
			// V4 and above expect two sets of PIX and MAT and ped substitution entry

19.67,-5.17,88.19							// Position of centre of start of grid
270									// Direction that grid faces in

// Laps, checkpoints etc

60,30,10							// Initial timer count for each skill level
6									// # laps
3000,1500,500						// Race completed bonus (all laps raced) for each skill level
75000,50000,30000					// Race completed bonus (all peds killed) for each skill level
20000,10000,5000					// Race completed bonus (all oppos wasted) for each skill level

// Width and height of map checkpoint rectangles
9,18
11,26

4									// # checkpoints

// Checkpoint #1
40,15,10								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
53.15,-100,127.78							// Point #0
53.15,100,127.78							// Point #1
53.15,100,124.83							// Point #2
53.15,-100,124.83						// Point #3
107,214
182,437

// Checkpoint #2
40,15,10								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
32.62,-5.2,32.89							// Point #0
32.62,100,32.89							// Point #1
32.62,100,36.80							// Point #2
32.62,-5.2,36.80						// Point #3
80,160
57,137

// Checkpoint #3
40,15,10								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
122.76,-5.2,12.68					// Point #0
122.76,100,12.68						// Point #1
122.76,100,17.32						// Point #2
122.76,-5.2,17.32					// Point #3
204,408
30,72

// Checkpoint #4
40,15,10								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
135.109,-5.2,92.55					// Point #0
135.109,100,92.55						// Point #1
135.109,100,96.53						// Point #2
135.109,-5.2,96.53					// Point #3
221,442
140,336

9									// # pixelmap files to load
INDYSKY.PIX
BARRY.PIX
INDUSTA3.PIX
IHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX
INDTEX29.PIX
INDTEX30.PIX
INDTEX31.PIX

9
INDYSKY.PIX
BARRY.PIX									// # pixelmap files to load(low memory)
INDUST38.PIX
IHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX
INDTEX29.PIX
INDTEX30.PIX
INDTEX31.PIX

1									// # shade table files to load
DRRENDER.TAB

14									// # material files to load
INDYWIND.MAT
BARRY.MAT
URINE.MAT
RIVVY.MAT
DRAB.MAT
RIDDY.MAT
INDUSTA3.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
GANTSCRN.MAT
TUNNSCRN.MAT
ACIDSCRN.MAT
SKIDMARK.MAT

14									// # material files to load(low memory)
INDYWIND.MAT
BARRY.MAT
URINE.MAT
RIVVY.MAT
DRAB.MAT
RIDDY.MAT
INDUSTA8.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
GANTSCRN.MAT
TUNNSCRN.MAT
ACIDSCRN.MAT
SKIDMARK.MAT

1									// # model files to load
INDUSTA3.DAT

1									// # model files to load
INDA83.DAT

INDUSTA3.ACT                                          // Track actor
INDA83.ACT                                          // Track actor

INDUSTX3.ACT							// Additional actor

// HORIZON STUFF

IHORIZN.PIX						// Name of sky texture pixelmap (or "none")
5									// Horizontal repetitions of sky texture
24									// Vertical size of sky texture (degrees)
83									// Position of horizon (pixels below top)
dark								// Depth cue mode ("none", "dark" or "fog")
7,0									// Degree of fog/darkness

// DEFAULT ENGINE NOISE

0

// SPECIAL EFFECTS VOLUMES

12									// # special effects volumes

DEFAULT WATER
0.2									// gravity multiplier
50									// viscosity multiplier
0									// Car damage per millisecond
0.002								// Pedestrian damage per millisecond
0									// camera effect index
1									// Sky colour
URINE.MAT								// Windscreen material to use
5100								// Sound ID of entry noise
5100								// Sound ID of exit noise
2									// Engine noise index
0									// material index


//------------------------ 0 -----------------------------------------
NEW IMPROVED!
-0.059, -0.003, -2.073
0.003, 1.200, -0.002
1.808, -0.005, -0.052
129.995, -4.116, 94.844
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 1 -----------------------------------------
NEW IMPROVED!
-0.039, 0.000, -2.986
-0.001, 0.833, 0.000
7.429, 0.006, -0.096
100.145, 0.271, 14.817
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 2 -----------------------------------------
NEW IMPROVED!
0.010, 0.002, 1.000
0.000, 1.000, -0.002
-4.680, 0.000, 0.047
124.928, -4.640, 19.399
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIVVY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 3 -----------------------------------------
NEW IMPROVED!
0.002, 0.002, 1.000
0.000, 1.000, -0.002
-4.095, 0.000, 0.009
124.127, -4.660, 14.664
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIVVY.MAT			// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 4 -----------------------------------------
NEW IMPROVED!
-0.001, 0.002, 1.000
0.000, 1.000, -0.002
-4.148, 0.000, -0.006
124.241, -4.600, 10.052
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIVVY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 5 -----------------------------------------
NEW IMPROVED!
-0.034, 0.001, -2.091
-0.002, 1.000, 0.000
7.447, 0.019, -1.082
45.792, -0.839, 127.248
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

//------------------------ 6 -----------------------------------------
NEW IMPROVED!
2.165, -0.001, -1.226
0.001, 1.000, 0.001
5.273, -0.008, 9.310
36.041, -0.518, 125.615
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 7 -----------------------------------------
NEW IMPROVED!
-2.986, 0.000, 0.032
0.000, 1.000, 0.000
-0.022, 0.000, -2.073
28.756, -0.837, 116.283
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 8 -----------------------------------------
NEW IMPROVED!
-7.430, 0.000, 0.037
0.000, 1.728, 0.000
-0.016, 0.000, -3.305
25.154, -3.137, 103.812
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 9 -----------------------------------------
NEW IMPROVED!
0.043, -0.001, 1.727
0.010, 4.300, 0.003
-10.117, 0.024, 0.254
42.168, -3.558, 86.838
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
DRAB.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 10 -----------------------------------------
NEW IMPROVED!
6.183, -0.003, 0.321
0.002, 2.986, -0.007
-0.385, 0.018, 7.420
118.839, -5.178, 57.802
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
BARRY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

 
// REFLECTIVE WINDSCREEN SPECIFICATIONS

INDYWIND.MAT							// Material to use for default screens
BARRY.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT


6									// # areas with different screens
111.3,50,125.6,52					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,53.7,125.6,55.7				// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,58,125.6,60					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,61,125.6,63					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,65,125.6,67					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
67.9,76.6,111.7,96.5				// x-min, z-min, x-max, z-max rectangle describing area
TUNNSCRN.MAT						// Material to use instead

// MAP DETAILS

INDAMAP3.PIX						// Map pixelmap name

1.38,	0,		0					// World->map transformation matrix
0,		0,		0
0,		1.38,	0
37.3,	14.2,	0



// ****** START OF FUNK AND GROOVE STUFF ******

START OF FUNK

INDFAN01.MAT
distance
piss off
no fucking lighting bastards
frames
approximate
continuous
12
3
INDTEX29.PIX
INDTEX30.PIX
INDTEX31.PIX

NEXT FUNK

LIQUID.MAT
constant
roll
continuous
0,0.1
no fucking lighting
no animation you cunt

NEXT FUNK

CHECK.MAT
constant
roll
continuous
0.2,0
no fucking lighting
no animation you cunt

NEXT FUNK

!LIQUID.MAT
constant
throb
harmonic
0.13,0.09
5,5
50,50
no fucking lighting
no animation you cunt

NEXT FUNK

ACIDSCRN.MAT
constant
throb
harmonic
0.13,0.09
5,5
50,50
no fucking lighting
no animation you cunt

END OF FUNK

// ****** START OF GROOVY SHIT *********

START OF GROOVE

&CBO0041.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
no fucking path you cuuuuuuunt		// Does not move on a path
rock								// Object itself rocks
linear								// Motion is linear (i.e. direction changes instantly)
0.12								// Cycles per second
0,0,0								// Centre of movement
y									// Axis to rock in
90									// Angle to rock (each way)

NEXT GROOVE

&CAR0041.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,-0.1							// Centre of movement
0.2									// Cycles per second
0,0,0.15							// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&CBO0004.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
no fucking path you cuuuuuuunt		// Does not move on a path
rock								// Object itself rocks
linear								// Motion is linear (i.e. direction changes instantly)
0.12								// Cycles per second
0,0,0								// Centre of movement
y									// Axis to rock in
90									// Angle to rock (each way)

NEXT GROOVE

&CAR0004.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,-0.1							// Centre of movement
0.2									// Cycles per second
0,0,0.15							// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0040.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0026.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&MNO0005.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
harmonic								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.1								// Cycles per second
1.5,0,0								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

END OF GROOVE

// ****** START OF PEDESTRIAN STUFF ******

9				// Ped subs table index

276				// Number of pedestrians

// Pedestrian number 1

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	5.259,-9.343,-4.543
	point
	5.259,-9.343,-4.543
	point
	4.451,996.000,-6.772
	point
	-3.686,996.000,-5.729
	point
	-7.395,996.000,-5.826
	reverse


// Pedestrian number 2

11				// Ref num
5				// Number of instructions
1				// Initial instruction

	point
	148.580,-5.177,36.716
	point
	148.238,-5.177,38.666
	point
	148.991,-5.177,44.640
	point
	136.110,-5.178,56.633
	reverse


// Pedestrian number 3

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	144.254,-5.116,28.687
	point
	149.087,-5.177,37.075
	point
	148.126,-5.177,43.342
	point
	148.930,-5.177,104.704
	reverse


// Pedestrian number 4

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	144.592,-5.177,39.950
	point
	147.111,-5.177,34.963
	point
	149.081,-5.177,29.866
	point
	144.220,-5.177,27.661
	reverse


// Pedestrian number 5

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	146.701,-5.177,37.813
	point
	142.899,-5.177,36.790
	point
	136.651,-5.179,37.379
	reverse


// Pedestrian number 6

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	145.705,-5.177,38.889
	point
	142.825,-5.177,37.021
	point
	141.758,-5.177,33.093
	reverse


// Pedestrian number 7

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	144.566,-5.181,-2.960
	point
	144.348,-5.181,0.979
	point
	149.564,-5.177,7.073
	point
	144.239,-5.178,13.704
	point
	147.040,-5.171,37.454
	reverse


// Pedestrian number 8

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	141.195,-5.171,52.129
	point
	146.447,-5.167,56.834
	point
	149.016,-5.164,67.117
	point
	143.908,-5.164,78.580
	reverse


// Pedestrian number 9

11				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	145.142,-5.170,48.666
	point
	146.040,-5.167,56.743
	point
	148.992,-5.166,59.274
	point
	148.890,-5.161,80.193
	point
	145.427,-5.162,80.697
	point
	127.017,-5.171,80.815
	reverse


// Pedestrian number 10

4				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	144.604,-5.170,48.790
	point
	144.784,-5.168,56.794
	point
	144.744,-5.163,78.635
	point
	137.363,-5.167,78.782
	point
	137.551,-5.166,80.446
	point
	138.783,-5.166,80.467
	reverse


// Pedestrian number 11

16				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	143.116,-5.170,49.918
	point
	144.329,-5.168,56.863
	point
	149.007,-5.163,72.414
	point
	149.037,-5.161,80.799
	point
	146.001,-5.161,84.185
	point
	144.329,-5.162,84.229
	point
	144.149,-5.163,82.185
	reverse


// Pedestrian number 12

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	136.226,-5.173,53.005
	point
	145.095,-5.167,60.482
	point
	148.938,-5.165,63.942
	point
	148.797,-5.163,71.161
	point
	140.826,-5.165,79.360
	reverse


// Pedestrian number 13

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	134.984,-5.170,70.103
	point
	141.940,-5.164,78.747
	point
	143.065,-5.164,80.378
	point
	144.667,-5.162,85.150
	reverse


// Pedestrian number 14

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	148.895,-5.162,75.639
	point
	142.329,-5.164,78.754
	point
	140.627,-5.165,80.446
	point
	137.155,-5.166,82.427
	reverse


// Pedestrian number 15

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	137.987,-5.163,93.965
	point
	141.397,-5.162,89.191
	point
	145.043,-5.162,84.266
	reverse


// Pedestrian number 16

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	144.735,-5.162,84.200
	point
	141.687,-5.161,94.427
	point
	139.123,-5.162,95.934
	point
	135.867,-5.163,95.913
	point
	135.585,-5.163,99.305
	point
	136.435,-5.162,100.029
	reverse


// Pedestrian number 17

4				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	133.895,-5.163,99.849
	point
	139.094,-5.161,98.923
	point
	141.431,-5.161,94.893
	point
	145.224,-5.160,92.842
	point
	145.443,-5.159,95.319
	reverse


// Pedestrian number 18

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	139.314,-5.162,94.981
	point
	140.895,-5.161,95.065
	point
	148.889,-5.158,95.505
	point
	149.066,-5.155,104.623
	reverse


// Pedestrian number 19

9				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	138.505,-5.161,100.865
	point
	142.123,-5.159,100.773
	point
	142.040,-5.159,101.351
	point
	141.570,-5.160,101.529
	point
	135.367,-5.162,104.579
	point
	127.760,-5.166,101.406
	reverse


// Pedestrian number 20

9				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	132.306,-5.165,97.451
	point
	130.309,-5.165,99.145
	point
	132.148,-5.163,104.683
	point
	142.006,-5.159,101.402
	point
	149.021,-5.156,101.511
	reverse


// Pedestrian number 21

9				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	148.847,-5.156,104.028
	point
	139.837,-5.160,102.495
	point
	137.054,-5.162,101.941
	point
	134.853,-5.163,102.170
	point
	133.435,-5.164,98.211
	point
	131.505,-5.165,97.793
	reverse


// Pedestrian number 22

9				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	128.741,-5.172,73.167
	point
	129.923,-5.170,77.071
	point
	133.349,-5.168,78.306
	point
	134.363,-5.168,80.379
	point
	135.323,-5.166,84.533
	point
	136.281,-5.166,84.718
	reverse


// Pedestrian number 23

11				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	132.338,-5.164,99.011
	point
	132.235,-5.166,93.504
	point
	133.052,-5.166,90.396
	point
	132.402,-5.167,88.462
	point
	131.965,-5.169,80.072
	reverse


// Pedestrian number 24

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	132.262,-5.169,80.095
	point
	132.440,-5.167,88.946
	point
	132.148,-5.166,91.851
	point
	132.200,-5.165,97.168
	point
	131.129,-5.165,97.910
	reverse


// Pedestrian number 25

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	134.043,-5.165,94.001
	point
	139.604,-5.164,85.237
	point
	141.268,-5.165,79.506
	reverse


// Pedestrian number 26

4				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	133.401,-5.169,76.331
	point
	143.135,-5.166,70.197
	point
	148.826,-5.164,65.294
	point
	149.172,-5.175,-2.841
	reverse


// Pedestrian number 27

9				// Ref num
8				// Number of instructions
5				// Initial instruction

	point
	149.009,-5.158,91.468
	point
	145.331,-5.161,89.047
	point
	145.377,-5.161,87.921
	point
	144.451,-5.162,86.963
	point
	136.559,-5.166,85.144
	point
	130.178,-5.169,83.124
	point
	127.489,-5.171,78.971
	reverse


// Pedestrian number 28

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	127.385,-5.171,81.080
	point
	132.079,-5.168,84.515
	point
	144.877,-5.161,88.533
	point
	145.166,-5.160,91.076
	reverse


// Pedestrian number 29

9				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	148.883,-5.159,88.109
	point
	145.324,-5.161,88.537
	point
	139.574,-5.162,93.486
	point
	139.030,-5.162,97.971
	point
	137.332,-5.162,100.176
	reverse


// Pedestrian number 30

16				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	143.077,-5.158,104.353
	point
	143.215,-5.160,97.599
	point
	144.354,-5.159,97.175
	point
	148.411,-5.157,98.481
	point
	148.988,-5.156,100.421
	point
	149.072,-5.156,103.392
	reverse


// Pedestrian number 31

16				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	139.858,-5.165,80.508
	point
	139.359,-5.163,88.792
	point
	138.815,-5.163,94.093
	reverse


// Pedestrian number 32

9				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	119.024,-5.193,-3.031
	point
	116.029,-5.193,4.572
	point
	116.080,-5.191,12.202
	point
	116.251,-5.188,24.406
	point
	117.389,-5.187,26.036
	reverse


// Pedestrian number 33

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	127.315,995.095,19.390
	point
	119.579,995.097,19.700
	point
	117.659,-5.097,21.913
	point
	116.390,995.107,23.348
	point
	112.473,993.665,24.532
	reverse


// Pedestrian number 34

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	117.213,-5.171,-2.918
	point
	118.213,995.029,12.609
	point
	120.243,995.096,14.981
	point
	127.246,-5.105,14.748
	reverse


// Pedestrian number 35

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	117.436,-5.082,22.170
	point
	117.161,-5.111,12.516
	point
	116.275,-5.133,4.946
	point
	111.147,-5.156,-2.871
	reverse


// Pedestrian number 36

3				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	120.162,995.093,19.023
	point
	118.457,995.101,21.789
	point
	118.437,-5.096,22.805
	point
	116.600,-5.091,24.526
	point
	118.285,-5.086,26.308
	point
	117.745,-5.082,27.581
	point
	119.870,-5.183,31.469
	reverse


// Pedestrian number 37

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	118.225,-5.170,-2.976
	point
	114.526,995.050,4.151
	point
	113.986,994.246,5.729
	point
	112.309,993.695,16.303
	point
	108.810,992.246,18.753
	reverse


// Pedestrian number 38

4				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	112.820,-5.176,-2.894
	point
	113.429,995.024,3.929
	point
	110.864,993.039,7.128
	point
	119.692,995.023,7.898
	reverse


// Pedestrian number 39

16				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	110.798,-5.177,-2.889
	point
	110.473,995.023,4.146
	point
	109.567,992.539,6.684
	reverse


// Pedestrian number 40

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	109.453,-5.177,-2.846
	point
	107.556,995.023,4.284
	point
	106.814,991.933,7.184
	reverse


// Pedestrian number 41

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	107.201,-5.177,-2.890
	point
	104.780,995.023,4.253
	point
	103.732,991.933,7.748
	reverse


// Pedestrian number 42

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	119.780,-5.176,2.549
	point
	106.681,-5.176,-0.117
	point
	104.653,-5.176,-1.010
	point
	104.148,-5.176,-3.052
	reverse


// Pedestrian number 43

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	119.733,-5.176,4.367
	point
	105.943,-5.176,-1.176
	point
	105.716,-5.176,-2.196
	reverse


// Pedestrian number 44

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	151.657,-5.177,-0.541
	point
	117.774,-5.176,-2.963
	point
	104.987,-5.176,-2.793
	point
	104.862,-5.176,-2.229
	reverse


// Pedestrian number 45

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	121.117,-5.177,-3.057
	point
	119.999,-5.177,0.192
	point
	116.464,-5.177,9.356
	point
	116.778,-5.177,28.088
	point
	117.441,-5.177,27.075
	reverse


// Pedestrian number 46

9				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	127.591,-5.186,42.906
	point
	119.144,-5.177,35.158
	point
	117.680,-5.177,29.237
	point
	116.412,-5.177,25.790
	point
	117.301,-5.177,25.110
	reverse


// Pedestrian number 47

10				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	100.303,-5.172,33.273
	point
	115.404,-5.171,32.720
	point
	115.892,-5.173,33.532
	point
	116.171,-5.183,38.176
	point
	117.564,-5.184,38.351
	point
	132.290,-5.186,42.824
	reverse


// Pedestrian number 48

13				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	100.326,-5.172,33.581
	point
	115.218,-5.179,36.451
	point
	119.682,-5.196,43.729
	point
	124.372,-5.207,48.684
	point
	124.423,-5.211,50.454
	point
	122.925,-5.213,51.052
	reverse


// Pedestrian number 49

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	125.070,-5.176,37.249
	point
	129.272,-5.176,33.309
	point
	137.225,-5.179,35.585
	point
	144.347,-5.176,40.159
	reverse


// Pedestrian number 50

4				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	141.094,-5.177,33.090
	point
	143.216,-5.176,40.474
	point
	143.406,-5.176,45.027
	point
	138.809,-5.176,48.599
	point
	138.092,-5.176,47.941
	point
	135.662,-5.176,48.187
	reverse


// Pedestrian number 51

16				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	122.559,-5.176,50.575
	point
	118.410,-5.176,53.316
	point
	113.382,-5.176,56.633
	point
	113.469,-5.176,58.088
	point
	124.512,-5.176,64.455
	reverse


// Pedestrian number 52

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	115.311,-5.176,50.997
	point
	118.376,-5.176,55.256
	point
	124.442,-5.176,59.450
	reverse


// Pedestrian number 53

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	113.158,-5.176,59.141
	point
	119.060,-5.176,62.251
	point
	124.407,-5.176,66.067
	point
	123.867,-5.176,68.751
	reverse


// Pedestrian number 54

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	113.132,-5.176,52.420
	point
	117.606,-5.176,55.493
	point
	124.733,-5.176,58.484
	point
	124.733,-5.176,58.484
	reverse


// Pedestrian number 55

11				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	124.700,-5.176,51.872
	point
	118.164,-5.176,56.960
	point
	113.138,-5.176,62.609
	point
	114.397,-5.176,68.663
	point
	110.901,-5.176,72.749
	reverse


// Pedestrian number 56

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	113.011,-5.176,65.366
	point
	119.585,-5.176,61.064
	point
	124.619,-5.176,56.935
	reverse


// Pedestrian number 57

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	124.628,-5.176,61.948
	point
	120.149,-5.176,58.724
	point
	114.592,-5.176,50.970
	reverse


// Pedestrian number 58

4				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	128.732,-5.176,71.806
	point
	120.664,-5.176,69.986
	point
	117.618,-5.176,68.368
	reverse


// Pedestrian number 59

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	113.209,-5.176,66.188
	point
	117.588,-5.176,67.880
	point
	120.157,-5.176,70.183
	point
	125.738,-5.176,72.899
	point
	128.000,-5.176,72.440
	reverse


// Pedestrian number 60

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	108.920,-5.176,71.631
	point
	114.841,-5.176,67.518
	point
	124.567,-5.176,62.353
	reverse


// Pedestrian number 61

16				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	129.526,-5.176,70.963
	point
	119.960,-5.176,71.689
	point
	114.000,-5.176,74.105
	reverse


// Pedestrian number 62

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	122.026,-6.382,89.475
	point
	120.021,993.818,87.119
	point
	116.228,995.023,69.827
	reverse


// Pedestrian number 63

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	128.171,995.023,86.499
	point
	120.359,993.818,86.653
	point
	116.437,993.818,88.197
	point
	112.245,994.949,90.212
	reverse


// Pedestrian number 64

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	119.288,-6.382,91.387
	point
	118.514,993.818,95.990
	point
	117.862,994.949,100.570
	reverse


// Pedestrian number 65

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	115.297,-5.170,69.804
	point
	114.288,-5.170,77.636
	point
	114.030,-5.170,80.207
	reverse


// Pedestrian number 66

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	122.982,-6.382,91.586
	point
	122.538,-6.382,93.147
	point
	119.571,993.818,93.793
	point
	112.210,994.957,96.609
	reverse


// Pedestrian number 67

10				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	131.752,-5.177,67.911
	point
	125.398,-5.177,68.475
	point
	122.933,-5.177,67.370
	point
	120.620,-5.177,67.346
	point
	113.046,-5.177,64.949
	reverse


// Pedestrian number 68

9				// Ref num
8				// Number of instructions
6				// Initial instruction

	point
	121.546,-5.177,50.222
	point
	118.110,-5.177,53.598
	point
	120.149,-5.177,56.144
	point
	117.521,-5.177,59.421
	point
	119.876,-5.177,62.558
	point
	118.420,-5.177,65.240
	point
	119.560,-5.177,68.893
	reverse


// Pedestrian number 69

11				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	122.432,993.818,85.069
	point
	122.068,995.023,80.262
	point
	120.716,-5.177,73.782
	point
	116.852,-5.177,69.607
	reverse


// Pedestrian number 70

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	122.980,-6.381,91.687
	point
	119.917,-6.381,91.526
	point
	119.795,993.819,90.534
	point
	112.324,995.023,67.628
	reverse


// Pedestrian number 71

11				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	125.938,994.948,98.636
	point
	123.813,993.818,96.567
	point
	121.246,-6.382,91.276
	point
	121.651,-6.382,88.330
	point
	122.603,-6.382,88.239
	point
	123.649,-6.382,87.614
	point
	123.586,-6.382,85.714
	reverse


// Pedestrian number 72

10				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	113.229,994.867,83.191
	point
	116.622,993.819,85.147
	point
	120.052,-6.381,90.173
	point
	121.437,-6.381,91.649
	point
	123.602,993.819,91.684
	point
	127.740,994.943,90.823
	reverse


// Pedestrian number 73

4				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	114.454,994.934,98.980
	point
	116.166,993.818,96.641
	point
	118.838,-6.382,91.108
	point
	122.473,-6.382,87.723
	reverse


// Pedestrian number 74

11				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	118.236,994.942,100.553
	point
	118.538,993.818,96.413
	point
	118.717,-6.382,94.002
	point
	118.875,-6.382,87.943
	point
	122.059,-6.382,86.082
	reverse


// Pedestrian number 75

11				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	112.120,994.986,96.443
	point
	116.214,993.818,95.653
	point
	118.290,-6.382,94.553
	point
	122.543,-6.382,91.641
	reverse


// Pedestrian number 76

16				// Ref num
9				// Number of instructions
3				// Initial instruction

	point
	112.217,995.023,93.080
	point
	112.005,995.023,94.198
	point
	108.086,-5.177,94.020
	point
	93.634,-5.177,93.003
	point
	89.528,-5.177,90.805
	point
	87.840,-5.177,79.082
	point
	82.440,-5.177,78.410
	point
	56.313,-5.212,79.327
	reverse


// Pedestrian number 77

4				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.243,995.023,92.528
	point
	21.506,996.699,77.186
	point
	19.373,986.858,75.038
	reverse


// Pedestrian number 78

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.725,995.023,92.397
	point
	22.520,996.705,77.123
	point
	23.341,991.480,69.365
	reverse


// Pedestrian number 79

4				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	31.071,-5.177,64.052
	point
	30.458,-5.177,73.853
	point
	31.178,995.023,84.337
	point
	31.573,995.023,92.543
	reverse


// Pedestrian number 80

5				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	24.906,-5.177,42.026
	point
	26.079,-5.177,42.372
	point
	26.390,-5.177,43.328
	point
	25.587,-5.177,44.526
	point
	16.121,-5.177,50.262
	reverse


// Pedestrian number 81

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	143.518,-5.177,42.189
	reverse


// Pedestrian number 82

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.858,-5.178,46.227
	reverse


// Pedestrian number 83

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.314,-5.177,48.235
	reverse


// Pedestrian number 84

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.141,-5.178,47.152
	reverse


// Pedestrian number 85

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.708,-5.178,54.174
	reverse


// Pedestrian number 86

134				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	133.663,-5.178,82.717
	reverse


// Pedestrian number 87

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.691,-5.166,96.265
	reverse


// Pedestrian number 88

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.947,-5.152,101.586
	reverse


// Pedestrian number 89

123				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	142.165,-5.152,101.608
	reverse


// Pedestrian number 90

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.763,-5.128,97.390
	reverse


// Pedestrian number 91

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.194,-5.131,97.825
	reverse


// Pedestrian number 92

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	119.091,-5.177,26.709
	reverse


// Pedestrian number 93

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	118.693,-5.177,24.667
	reverse


// Pedestrian number 94

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.087,-5.177,88.244
	reverse


// Pedestrian number 95

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	127.042,-5.177,19.680
	reverse


// Pedestrian number 96

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	126.807,-5.177,14.509
	reverse


// Pedestrian number 97

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	126.122,-5.177,14.503
	reverse


// Pedestrian number 98

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	125.473,-5.177,14.498
	reverse


// Pedestrian number 99

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	124.353,-5.177,14.488
	reverse


// Pedestrian number 100

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.956,-5.177,14.475
	reverse


// Pedestrian number 101

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	126.097,-5.177,10.081
	reverse


// Pedestrian number 102

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	125.438,-5.177,10.066
	reverse


// Pedestrian number 103

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	124.792,-5.177,10.052
	reverse


// Pedestrian number 104

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	123.752,-5.177,10.028
	reverse


// Pedestrian number 105

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.879,-5.177,-1.327
	reverse


// Pedestrian number 106

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.930,-5.177,-0.244
	reverse


// Pedestrian number 107

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.907,-5.177,-2.053
	reverse


// Pedestrian number 108

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	97.049,-5.193,38.469
	reverse


// Pedestrian number 109

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	113.191,-5.177,49.534
	reverse


// Pedestrian number 110

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	124.555,-5.177,51.183
	reverse


// Pedestrian number 111

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.611,-5.177,55.320
	reverse


// Pedestrian number 112

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	116.287,-5.177,62.184
	reverse


// Pedestrian number 113

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	108.684,-5.177,63.533
	reverse


// Pedestrian number 114

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	129.569,-5.177,58.676
	reverse


// Pedestrian number 115

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	123.802,-6.382,91.499
	reverse


// Pedestrian number 116

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	123.886,-6.382,90.637
	reverse


// Pedestrian number 117

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	123.815,-6.382,89.041
	reverse


// Pedestrian number 118

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.700,-5.177,79.771
	reverse


// Pedestrian number 119

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.643,-5.177,78.997
	reverse


// Pedestrian number 120

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.331,-5.177,78.676
	reverse


// Pedestrian number 121

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.324,-5.177,71.843
	reverse


// Pedestrian number 122

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.380,-5.177,70.670
	reverse


// Pedestrian number 123

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.246,-5.177,63.437
	reverse


// Pedestrian number 124

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.078,-5.177,60.795
	reverse


// Pedestrian number 125

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.525,-5.177,56.545
	reverse


// Pedestrian number 126

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.978,-8.720,68.311
	reverse


// Pedestrian number 127

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.888,-8.720,68.244
	reverse


// Pedestrian number 128

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	22.233,-8.720,68.192
	reverse


// Pedestrian number 129

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	22.709,-8.720,68.618
	reverse


// Pedestrian number 130

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	22.282,-8.720,68.934
	reverse


// Pedestrian number 131

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	21.279,-8.720,69.059
	reverse


// Pedestrian number 132

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.421,-8.720,69.364
	reverse


// Pedestrian number 133

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	21.503,-8.720,68.656
	reverse


// Pedestrian number 134

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	30.387,-17.799,68.882
	reverse


// Pedestrian number 135

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.497,-5.177,47.325
	reverse


// Pedestrian number 136

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.548,-5.177,47.915
	reverse


// Pedestrian number 137

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.532,-5.177,47.610
	reverse


// Pedestrian number 138

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.521,-5.177,39.328
	reverse


// Pedestrian number 139

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.442,-5.177,33.837
	reverse


// Pedestrian number 140

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.366,-5.177,34.520
	reverse


// Pedestrian number 141

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.209,-5.177,35.142
	reverse


// Pedestrian number 142

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.786,-5.177,35.299
	reverse


// Pedestrian number 143

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	33.397,-5.177,39.101
	reverse


// Pedestrian number 144

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.247,-5.176,37.950
	reverse


// Pedestrian number 145

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.456,-5.176,37.923
	reverse


// Pedestrian number 146

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.626,-5.176,38.032
	reverse


// Pedestrian number 147

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.743,-5.176,42.969
	reverse


// Pedestrian number 148

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.642,-5.176,43.643
	reverse


// Pedestrian number 149

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	29.650,-5.177,47.534
	reverse


// Pedestrian number 150

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.476,-5.176,48.741
	reverse


// Pedestrian number 151

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.756,-5.176,46.640
	reverse


// Pedestrian number 152

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	101.670,-0.250,14.083
	reverse


// Pedestrian number 153

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	101.789,-0.250,15.411
	reverse


// Pedestrian number 154

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	103.420,-0.249,17.419
	point
	106.542,999.954,15.193
	point
	116.467,995.203,14.901
	reverse


// Pedestrian number 155

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	95.316,-0.255,12.289
	point
	107.109,999.954,14.278
	point
	113.265,993.967,13.823
	reverse


// Pedestrian number 156

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	97.964,-0.253,12.301
	point
	104.086,999.952,14.759
	point
	111.553,993.306,17.321
	reverse


// Pedestrian number 157

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	93.615,-0.256,17.314
	point
	106.594,999.954,13.251
	point
	111.426,993.254,11.904
	reverse


// Pedestrian number 158

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	92.925,-0.257,12.228
	point
	106.200,999.953,16.374
	point
	113.560,994.080,16.047
	reverse


// Pedestrian number 159

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	96.351,-0.254,17.098
	point
	100.055,-0.251,12.710
	point
	106.389,999.954,15.829
	point
	109.290,992.431,16.114
	reverse


// Pedestrian number 160

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.692,-4.071,27.555
	reverse


// Pedestrian number 161

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.693,-4.071,28.410
	reverse


// Pedestrian number 162

103				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.660,-4.071,29.255
	reverse


// Pedestrian number 163

104				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.617,-4.071,30.354
	reverse


// Pedestrian number 164

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.577,-4.071,31.388
	reverse


// Pedestrian number 165

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.532,-4.071,32.544
	reverse


// Pedestrian number 166

106				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.486,-4.071,33.720
	reverse


// Pedestrian number 167

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.452,-4.071,35.069
	reverse


// Pedestrian number 168

108				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.427,-4.071,36.268
	reverse


// Pedestrian number 169

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.399,-4.071,37.585
	reverse


// Pedestrian number 170

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.372,-4.071,38.866
	reverse


// Pedestrian number 171

16				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	92.840,999.943,17.370
	point
	87.337,999.905,12.885
	point
	81.092,999.852,13.819
	point
	79.309,1000.019,18.314
	reverse


// Pedestrian number 172

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	94.771,999.944,12.277
	point
	83.136,999.943,17.288
	point
	74.884,1000.021,16.655
	point
	72.600,1000.252,21.577
	reverse


// Pedestrian number 173

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	69.816,1000.426,22.940
	point
	73.438,1000.210,20.872
	point
	75.329,1000.066,18.088
	point
	78.236,999.913,14.994
	point
	81.748,999.936,16.994
	reverse


// Pedestrian number 174

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	84.963,999.885,13.343
	point
	82.617,999.899,15.806
	point
	79.067,1000.027,18.427
	point
	72.925,1000.092,17.781
	reverse


// Pedestrian number 175

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	68.771,1000.429,21.794
	point
	71.921,1000.119,18.181
	point
	78.065,1000.002,17.458
	point
	81.348,999.854,13.803
	point
	89.773,999.943,17.510
	reverse


// Pedestrian number 176

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	90.334,999.938,17.325
	point
	82.179,999.884,15.265
	point
	75.887,999.986,16.120
	reverse


// Pedestrian number 177

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	68.373,1000.332,20.156
	point
	75.554,1000.084,18.658
	point
	78.235,999.977,16.813
	point
	78.726,999.893,14.691
	reverse


// Pedestrian number 178

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	35.843,995.334,36.161
	point
	53.421,998.614,28.625
	point
	54.132,998.748,28.533
	point
	62.450,982.407,25.942
	reverse


// Pedestrian number 179

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	61.808,982.408,26.040
	point
	54.193,998.877,27.923
	point
	41.782,996.303,33.111
	point
	35.695,995.326,33.140
	reverse


// Pedestrian number 180

16				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	33.917,995.046,33.485
	point
	41.365,996.173,35.622
	point
	54.642,998.808,29.226
	point
	61.700,982.644,22.124
	reverse


// Pedestrian number 181

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	62.338,982.407,22.621
	point
	57.253,999.360,27.650
	point
	60.366,1000.042,25.468
	point
	61.993,982.407,24.215
	reverse


// Pedestrian number 182

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	62.410,982.407,23.493
	point
	57.026,999.337,26.879
	point
	64.197,982.407,21.812
	reverse


// Pedestrian number 183

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	47.863,997.397,33.395
	point
	58.998,999.627,27.612
	point
	64.888,982.407,19.482
	reverse


// Pedestrian number 184

13				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	114.902,997.905,15.451
	point
	118.922,997.640,16.331
	point
	119.276,995.021,17.808
	reverse


// Pedestrian number 185

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	111.704,993.367,13.270
	point
	115.576,997.698,14.330
	point
	119.289,995.022,11.825
	reverse


// Pedestrian number 186

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	115.034,997.663,14.901
	point
	117.607,997.606,14.922
	point
	122.627,997.553,12.976
	point
	126.218,997.301,17.345
	reverse


// Pedestrian number 187

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	112.961,993.847,16.481
	point
	117.026,997.641,15.519
	point
	122.494,997.643,17.079
	point
	126.313,997.667,14.294
	point
	149.091,995.023,14.913
	reverse


// Pedestrian number 188

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	145.626,-5.177,14.862
	point
	148.645,-5.177,17.447
	point
	144.199,-5.178,25.207
	point
	145.961,-5.178,35.385
	reverse


// Pedestrian number 189

9				// Ref num
5				// Number of instructions
1				// Initial instruction

	point
	146.999,-5.177,15.138
	point
	144.333,-5.177,20.690
	point
	148.983,-5.177,24.975
	point
	143.944,-5.177,33.324
	reverse


// Pedestrian number 190

99				// Ref num
5				// Number of instructions
1				// Initial instruction

	point
	148.622,-5.175,11.052
	point
	149.057,-5.173,14.632
	point
	147.363,-5.173,15.174
	point
	145.749,-5.174,14.791
	reverse


// Pedestrian number 191

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	111.824,-5.177,95.707
	point
	105.226,-5.177,93.810
	point
	100.746,-5.177,95.122
	point
	96.748,-5.177,93.171
	reverse


// Pedestrian number 192

13				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	111.902,-5.177,95.647
	point
	110.078,-5.177,93.988
	point
	107.648,-5.177,95.621
	reverse


// Pedestrian number 193

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	101.648,-5.177,95.301
	point
	111.502,995.023,94.233
	point
	121.758,993.818,91.308
	reverse


// Pedestrian number 194

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	108.493,-5.177,95.686
	point
	94.588,-5.177,94.664
	point
	90.427,-5.177,92.511
	reverse


// Pedestrian number 195

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	92.712,-5.177,94.194
	point
	90.752,-5.177,89.800
	point
	88.492,-5.177,79.799
	reverse


// Pedestrian number 196

16				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	19.381,-5.174,37.397
	point
	21.234,-5.175,37.520
	point
	23.169,-5.188,35.174
	point
	25.305,-5.201,32.932
	point
	25.756,-5.202,32.859
	reverse


// Pedestrian number 197

10				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	15.607,-5.177,40.454
	point
	21.040,-5.177,37.841
	point
	23.504,-5.177,35.851
	point
	24.213,-5.177,33.981
	point
	23.720,-5.177,33.083
	point
	21.459,-5.177,31.496
	point
	10.709,-5.177,31.974
	reverse


// Pedestrian number 198

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	14.889,-5.177,48.890
	point
	23.862,-5.177,36.451
	point
	26.494,-5.177,33.539
	point
	25.796,-5.177,25.060
	reverse


// Pedestrian number 199

9				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	18.150,996.115,29.610
	point
	10.590,994.999,29.361
	reverse


// Pedestrian number 200

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	18.173,996.103,29.042
	point
	10.671,995.023,25.152
	reverse


// Pedestrian number 201

3				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	18.158,996.108,30.337
	point
	10.639,995.032,35.659
	reverse


// Pedestrian number 202

10				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	60.265,-1.777,93.292
	point
	58.996,-1.850,89.351
	point
	56.635,-1.850,87.113
	point
	52.649,998.350,85.886
	point
	22.832,995.021,85.745
	reverse


// Pedestrian number 203

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	49.955,998.026,85.816
	point
	52.540,998.349,86.701
	point
	53.288,998.349,89.250
	reverse


// Pedestrian number 204

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	46.554,998.349,85.642
	point
	52.486,998.349,87.261
	point
	54.698,998.350,89.155
	reverse


// Pedestrian number 205

3				// Ref num
10				// Number of instructions
2				// Initial instruction

	point
	49.246,998.349,87.512
	point
	53.132,998.349,87.979
	point
	55.317,998.350,89.195
	point
	56.714,998.350,90.569
	point
	57.456,998.350,92.244
	point
	57.730,998.350,93.925
	point
	57.854,998.351,111.901
	point
	56.691,998.351,113.039
	point
	53.419,995.252,107.879
	reverse


// Pedestrian number 206

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	31.855,995.023,92.589
	point
	30.617,995.479,87.603
	point
	27.570,995.268,78.783
	reverse


// Pedestrian number 207

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	32.156,995.584,77.851
	point
	30.655,995.481,86.632
	point
	29.205,995.607,96.044
	reverse


// Pedestrian number 208

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	28.157,995.841,97.337
	point
	30.417,995.466,87.200
	point
	31.754,995.558,84.166
	reverse


// Pedestrian number 209

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.817,996.366,100.239
	point
	29.778,995.421,86.644
	point
	31.680,995.552,81.663
	reverse


// Pedestrian number 210

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.946,995.157,80.223
	point
	29.949,995.433,87.109
	point
	31.593,995.546,90.334
	reverse


// Pedestrian number 211

16				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	25.177,996.303,99.900
	point
	24.410,996.363,100.228
	point
	24.855,997.541,106.746
	point
	24.809,997.808,108.222
	reverse


// Pedestrian number 212

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.264,997.840,108.401
	point
	25.570,997.604,107.093
	point
	27.301,997.327,106.252
	reverse


// Pedestrian number 213

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	57.296,-5.210,89.441
	point
	57.957,-5.210,89.482
	point
	60.907,-5.204,88.090
	point
	64.219,-5.197,86.580
	reverse


// Pedestrian number 214

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	57.613,-5.206,87.987
	point
	60.461,-5.205,88.332
	point
	64.057,-5.206,90.147
	point
	65.609,-5.209,91.880
	reverse


// Pedestrian number 215

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.867,-5.208,88.627
	point
	60.692,-5.211,91.021
	point
	63.600,-5.219,95.327
	reverse


// Pedestrian number 216

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	64.790,-5.205,90.078
	point
	60.245,-5.207,91.177
	point
	53.448,-5.215,95.805
	point
	53.418,-5.234,106.855
	reverse


// Pedestrian number 217

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	64.077,-5.212,98.421
	point
	59.205,-5.212,90.503
	point
	56.434,-5.212,89.225
	point
	56.472,-5.212,88.725
	point
	54.094,-5.212,82.654
	reverse


// Pedestrian number 218

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.468,-5.135,113.773
	point
	59.151,-5.133,112.094
	point
	61.601,-5.213,109.651
	reverse


// Pedestrian number 219

4				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	53.420,-5.213,104.653
	point
	56.782,-5.213,107.164
	point
	59.722,-5.213,111.644
	point
	61.165,-5.213,113.089
	point
	60.003,-5.213,113.933
	point
	57.581,-5.213,114.008
	reverse


// Pedestrian number 220

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	61.682,-5.213,108.019
	point
	59.292,-5.213,111.628
	point
	57.296,-5.213,112.821
	point
	58.546,-5.213,113.775
	point
	61.245,-5.213,114.067
	reverse


// Pedestrian number 221

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	56.992,-5.213,108.728
	point
	58.524,-5.213,111.473
	point
	61.339,-5.213,112.939
	reverse


// Pedestrian number 222

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.566,-5.213,89.381
	point
	58.898,-5.235,109.851
	point
	58.782,-5.241,113.617
	reverse


// Pedestrian number 223

10				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	53.690,-1.338,129.740
	point
	56.758,-1.338,129.097
	point
	56.541,-1.338,125.835
	point
	57.954,998.862,116.909
	point
	57.479,998.862,114.982
	reverse


// Pedestrian number 224

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	57.746,-1.338,130.085
	point
	58.358,-1.338,123.642
	point
	58.317,998.862,116.888
	point
	59.022,998.862,112.015
	point
	61.435,998.862,109.842
	reverse


// Pedestrian number 225

9				// Ref num
6				// Number of instructions
2				// Initial instruction


	point
	55.849,-1.338,123.646
	point
	58.783,-1.338,123.441
	point
	63.107,998.862,117.031
	point
	63.037,998.862,114.258
	point
	55.793,-5.213,79.818
	reverse


// Pedestrian number 226

3				// Ref num
8				// Number of instructions
6				// Initial instruction

	point
	53.639,-1.338,128.150
	point
	53.719,-1.338,127.008
	point
	43.974,-1.338,126.116
	point
	35.133,-1.338,126.767
	point
	31.606,-1.338,121.500
	point
	29.171,998.861,114.066
	point
	28.971,998.842,110.732
	reverse


// Pedestrian number 227

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	27.416,998.839,110.192
	point
	28.238,998.861,114.027
	point
	29.358,-1.318,117.771
	point
	34.638,-1.295,121.754
	point
	40.023,-1.338,129.216
	point
	55.740,-1.338,127.150
	reverse


// Pedestrian number 228

9				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	27.749,998.862,111.285
	point
	29.752,998.861,114.033
	point
	30.472,-1.338,119.654
	point
	41.481,-1.338,128.922
	point
	53.780,-1.338,125.299
	point
	54.731,-1.338,123.653
	reverse


// Pedestrian number 229

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	27.418,997.457,109.161
	point
	26.546,997.467,107.130
	point
	25.937,996.878,103.432
	point
	12.162,995.439,95.119
	reverse


// Pedestrian number 230

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	24.344,998.020,109.498
	point
	25.321,997.416,106.807
	point
	26.751,997.125,104.981
	reverse


// Pedestrian number 231

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.413,997.269,105.880
	point
	24.109,997.511,107.401
	point
	24.927,997.822,109.354
	reverse


// Pedestrian number 232

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	12.396,-5.178,60.741
	reverse


// Pedestrian number 233

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	12.410,-5.178,60.077
	reverse


// Pedestrian number 234

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	12.430,-5.178,59.102
	reverse


// Pedestrian number 235

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.011,-5.177,58.646
	reverse


// Pedestrian number 236

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.742,-5.178,58.764
	reverse


// Pedestrian number 237

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.633,-4.071,91.950
	reverse


// Pedestrian number 238

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.473,-4.071,91.291
	reverse


// Pedestrian number 239

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.047,-4.071,90.112
	reverse


// Pedestrian number 240

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.902,-4.071,86.387
	reverse


// Pedestrian number 241

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.436,-3.985,108.640
	reverse


// Pedestrian number 242

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.429,-3.990,110.034
	reverse


// Pedestrian number 243

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	25.097,-3.985,108.619
	reverse


// Pedestrian number 244

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	25.131,-3.992,110.591
	reverse


// Pedestrian number 245

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	24.069,-3.985,108.675
	reverse


// Pedestrian number 246

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	24.066,-3.993,110.842
	reverse


// Pedestrian number 247

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.720,-5.216,107.871
	reverse


// Pedestrian number 248

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	14.934,-5.219,108.511
	reverse


// Pedestrian number 249

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	17.140,-5.224,110.116
	reverse


// Pedestrian number 250

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	58.460,-5.213,113.273
	reverse


// Pedestrian number 251

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	60.212,-5.213,113.407
	reverse


// Pedestrian number 252

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.736,-5.213,95.341
	reverse


// Pedestrian number 253

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.779,-5.213,93.374
	reverse


// Pedestrian number 254

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.852,-5.213,89.789
	reverse


// Pedestrian number 255

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.952,-5.213,84.839
	reverse


// Pedestrian number 256

121				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	56.260,-5.213,88.847
	reverse


// Pedestrian number 257

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	59.603,-1.338,126.097
	reverse


// Pedestrian number 258

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	62.919,-1.338,124.218
	reverse


// Pedestrian number 259

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	142.993,-4.454,79.341
	reverse


// Pedestrian number 260

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	143.572,-4.454,79.485
	reverse


// Pedestrian number 261

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.125,1.528,129.541
	reverse


// Pedestrian number 262

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.788,1.527,127.925
	reverse


// Pedestrian number 263

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.911,1.526,125.580
	reverse


// Pedestrian number 264

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.781,1.519,115.143
	reverse


// Pedestrian number 265

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	46.804,1.519,115.739
	reverse


// Pedestrian number 266

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.376,1.522,113.532
	reverse


// Pedestrian number 267

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.436,1.529,107.001
	reverse


// Pedestrian number 268

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	4.639,1.529,93.282
	reverse


// Pedestrian number 269

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.305,1.529,94.028
	reverse


// Pedestrian number 270

134				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.027,0.873,93.783
	reverse


// Pedestrian number 271

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	36.193,0.929,68.232
	reverse


// Pedestrian number 272

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.438,1.529,65.768
	reverse


// Pedestrian number 273

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.034,1.451,126.534
	reverse


// Pedestrian number 274

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	68.286,1.451,126.587
	reverse


// Pedestrian number 275

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	70.043,1.451,126.627
	reverse


// Pedestrian number 276

99				// Ref num
9				// Number of instructions
5				// Initial instruction

	point
	11.781,-5.177,92.461
	point
	14.829,-5.177,92.227
	point
	16.570,-5.177,89.828
	point
	20.394,-5.177,88.590
	point
	21.136,-5.177,87.672
	point
	24.312,995.223,86.576
	point
	31.108,995.223,57.602
	point
	25.325,-5.177,53.172
	reverse



START OF OPPONENT PATHS

122                             // Number of path nodes
  118.800,   -5.100,   -1.200   // Node #0
  119.212,   -5.200,   34.438   // Node #1
  118.133,   -5.177,   80.131   // Node #2
  116.068,   -6.360,   94.248   // Node #3
  112.097,   -5.207,   94.852   // Node #4
   93.485,   -5.177,   93.619   // Node #5
   90.347,   -5.177,   91.290   // Node #6
   88.176,   -5.177,   81.143   // Node #7
   85.525,   -5.176,   78.332   // Node #8
   66.676,   -5.171,   78.966   // Node #9
   34.788,   -4.341,   86.678   // Node #10
   25.707,   -5.177,   87.220   // Node #11
   21.950,   -5.177,   86.983   // Node #12
   21.984,   -5.179,   49.019   // Node #13
   22.042,   -5.179,   35.833   // Node #14
   45.541,   -3.255,   34.032   // Node #15
   98.919,   -0.253,   14.679   // Node #16
  148.440,   -5.173,   33.383   // Node #17
  147.150,   -5.177,   -1.321   // Node #18
  148.616,   -5.178,   36.256   // Node #19
  148.503,   -5.177,   51.045   // Node #20
  143.492,   -5.179,   34.955   // Node #21
  143.656,   -5.179,   44.377   // Node #22
  139.598,   -5.177,   48.484   // Node #23
  136.115,   -5.179,   48.411   // Node #24
  128.495,   -5.174,   40.410   // Node #25
  119.064,   -5.177,   47.360   // Node #26
  127.917,   -5.177,   34.918   // Node #27
  118.212,   -5.177,   73.160   // Node #28
  130.037,   -5.179,   67.903   // Node #29
  130.128,   -5.171,   54.448   // Node #30
  107.733,   -5.179,   69.194   // Node #31
  107.980,   -5.181,   53.390   // Node #32
  101.765,   -5.182,   48.495   // Node #33
   97.932,   -5.189,   48.562   // Node #34
   94.151,   -5.180,   44.730   // Node #35
   88.570,   -5.300,   36.127   // Node #36
   91.539,   -5.193,    1.880   // Node #37
  105.526,   -5.179,    1.808   // Node #38
   89.006,   -5.283,   26.003   // Node #39
   99.471,   -5.179,   28.311   // Node #40
  113.386,   -6.188,   14.612   // Node #41
   94.486,   -8.264,   14.629   // Node #42
   14.614,   -5.177,   88.841   // Node #43
   11.915,   -5.178,   58.629   // Node #44
   30.862,   -5.177,   81.200   // Node #45
   30.938,   -5.181,   64.558   // Node #46
   32.963,   -5.178,   59.300   // Node #47
   30.376,   -5.179,   34.814   // Node #48
   30.520,   -5.180,   26.909   // Node #49
   14.038,   -5.181,   26.732   // Node #50
   12.474,   -5.180,   33.042   // Node #51
   94.201,   -5.177,   40.212   // Node #52
   10.790,   -5.179,   68.625   // Node #53
   27.032,   -8.722,   68.953   // Node #54
   26.992,   -8.671,   78.314   // Node #55
   22.014,   -8.633,   80.283   // Node #56
   16.997,   -8.720,   78.143   // Node #57
   17.044,   -8.560,   68.490   // Node #58
   17.122,   -8.720,   58.949   // Node #59
   21.821,   -8.760,   57.272   // Node #60
   26.928,   -8.778,   58.968   // Node #61
   22.014,   -3.067,   69.154   // Node #62
   22.444,   -5.177,   88.452   // Node #63
   31.514,   -5.180,   92.633   // Node #64
  118.918,   -5.178,   14.505   // Node #65
  110.278,   -5.178,   39.295   // Node #66
  147.530,   -5.179,  102.714   // Node #67
  140.099,   -5.181,  103.156   // Node #68
  144.306,   -5.180,   59.574   // Node #69
  142.363,   -5.180,   77.438   // Node #70
  130.550,   -5.184,  103.892   // Node #71
  131.412,   -5.179,   98.511   // Node #72
  134.475,   -5.177,   99.108   // Node #73
  134.265,   -5.177,  103.832   // Node #74
  140.357,   -5.177,  100.321   // Node #75
  140.534,   -5.179,   90.041   // Node #76
  133.726,   -5.177,   84.785   // Node #77
  129.049,   -5.180,   80.180   // Node #78
  129.172,   -5.177,   74.453   // Node #79
  135.897,   -5.177,   73.805   // Node #80
  148.225,   -5.180,   90.045   // Node #81
  120.386,   -5.199,   34.785   // Node #82
  118.744,   -5.175,   60.886   // Node #83
   15.356,   -5.180,   30.887   // Node #84
   64.367,    0.369,   25.085   // Node #85
   84.313,   -0.319,   14.843   // Node #86
  106.964,   -0.246,   14.787   // Node #87
  115.998,   -2.595,   14.972   // Node #88
  140.718,   -4.018,   16.688   // Node #89
  147.122,   -5.178,   16.715   // Node #90
  136.244,   -5.178,   88.848   // Node #91
  135.819,   -5.180,   94.646   // Node #92
   89.707,   -5.256,    6.896   // Node #93
   88.980,   -5.281,   31.492   // Node #94
   92.137,   -5.179,   26.785   // Node #95
   61.989,   -5.188,   79.339   // Node #96
   59.576,   -5.214,   95.829   // Node #97
   63.571,   -5.231,  107.125   // Node #98
   62.212,   -1.338,  116.424   // Node #99
   58.871,   -1.338,  124.291   // Node #100
   53.331,   -1.338,  126.289   // Node #101
   38.362,   -1.338,  127.699   // Node #102
   34.534,   -1.338,  124.197   // Node #103
   27.622,   -1.338,  111.839   // Node #104
   23.166,   -3.746,  100.767   // Node #105
   52.873,   -1.851,   86.937   // Node #106
   56.785,   -1.850,   88.536   // Node #107
   58.853,   -1.850,   91.567   // Node #108
   59.309,   -1.850,   94.140   // Node #109
   59.205,   -1.850,  115.130   // Node #110
   55.047,   -5.213,  106.605   // Node #111
   55.078,   -2.764,  114.093   // Node #112
   55.265,   -1.338,  116.843   // Node #113
   14.054,   -5.216,  108.284   // Node #114
   47.109,   -5.218,  108.725   // Node #115
   53.349,   -4.091,  108.134   // Node #116
   24.243,   -3.154,  113.581   // Node #117
   45.765,   -3.517,  113.071   // Node #118
   51.864,   -4.228,  112.042   // Node #119
   80.795,   -5.173,   78.494   // Node #120
   59.092,   -5.226,  113.404   // Node #121

141                                           // Number of path sections
   2,   3,   0, 255,   0, 255,    1.1,    0   // Section #0
   3,   4,   0, 255,   0, 255,    0.5,    1   // Section #1
   4,   5,   0, 255,   0, 255,    0.5,    1   // Section #2
   5,   6,   0, 255,   0, 255,    0.5,    1   // Section #3
   6,   7,   0, 255,   0, 255,    0.5,    1   // Section #4
   7,   8,   0, 255,   0, 255,    0.5,    1   // Section #5
   8, 120,   0, 255,   0, 255,    0.5,    1   // Section #6
  11,  10,   0, 255,   0, 255,    0.5,    1   // Section #7
  63,  11,   0, 255,   0, 255,    0.5,    1   // Section #8
  12,  62,   0, 255,   0, 255,    0.5,    1   // Section #9
  13,  14,   0, 255,   0, 255,    0.5,    1   // Section #10
  14,  48,   0, 255,   0, 255,    1.2,    1   // Section #11
  21,  17,   0, 255,   0, 255,    1.5,    0   // Section #12
  18,  90,   0, 255,   0, 255,    1.2,    0   // Section #13
  17,  19,   0, 255,   0, 255,    0.3,    1   // Section #14
  19,  20,   0, 255,   0, 255,    0.4,    1   // Section #15
  23,  22,   0, 255,   0, 255,    0.4,    0   // Section #16
  23,  24,   0, 255,   0, 255,    0.4,    0   // Section #17
  24,  25,   0, 255,   0, 255,    0.4,    0   // Section #18
  25,  26,   0, 255,   0, 255,    1.7,    0   // Section #19
  26,  83,   0, 255,   0, 255,    1.5,    0   // Section #20
  25,  27,   0, 255,   0, 255,    1.0,    0   // Section #21
   1,  82,   0, 255,   0, 255,    0.5,    0   // Section #22
  29,  28,   0, 255,   0, 255,    1.0,    0   // Section #23
  28,   2,   0, 255,   0,  35,    1.8,    0   // Section #24
  30,  29,   0, 255,   0, 255,    1.6, 1000   // Section #25
  31,  28,   0, 255,   0, 255,    1.6,    0   // Section #26
  32,  31,   0, 255,   0, 255,    1.3, 1000   // Section #27
  33,  66,   0, 255,   0, 255,    0.5,    0   // Section #28
  34,  33,   0, 255,   0, 255,    0.4,    0   // Section #29
  35,  34,   0, 255,   0, 255,    0.4,    0   // Section #30
  36,  52,   0, 255,   0, 255,    0.4,    0   // Section #31
  38,  37,   0, 255,   0, 255,    1.0,    0   // Section #32
   0,  38,   0, 255,   0, 255,    1.0,    0   // Section #33
  39,  95,   0, 255,   0, 255,    0.5,    0   // Section #34
  37,  93,   0, 255,   0, 255,    0.7,    0   // Section #35
  41,  65,   0, 255,   0, 255,    0.2, 1000   // Section #36
  42,  41,   0, 255,   0, 255,    4.0, 1000   // Section #37
  44,  53,   0, 255,   0, 255,    1.0, 1000   // Section #38
  45,  11,   0, 255,   0, 255,    0.5, 1000   // Section #39
  46,  45,   0, 255,   0, 255,    0.5, 1000   // Section #40
  47,  13,   0,  15,   0,  15,    0.3, 1000   // Section #41
  49,  48,   0, 255,   0, 255,    1.2,    0   // Section #42
  48,  15,   0, 255,   0, 255,    1.0,    1   // Section #43
  50,  49,   0, 255,   0, 255,    1.0,    0   // Section #44
  52,  35,   0, 255,   0, 255,    0.3,    0   // Section #45
  36,  94,   0, 255,   0, 255,    0.5,    0   // Section #46
  54,  53,   0, 255,  25, 255,    0.9, 1000   // Section #47
  53,  43,   0, 255,   0, 255,    1.0,    0   // Section #48
  55,  54,   0, 255,   0, 255,    0.2, 1000   // Section #49
  56,  55,   0, 255,   0, 255,    0.5, 1000   // Section #50
  56,  57,   0, 255,   0, 255,    0.4,    0   // Section #51
  57,  58,   0, 255,   0, 255,    0.2, 1000   // Section #52
  59,  58,   0, 255,   0, 255,    0.2, 1000   // Section #53
  60,  59,   0, 255,   0, 255,    0.4, 1000   // Section #54
  60,  61,   0, 255,   0, 255,    0.4, 1000   // Section #55
  61,  54,   0, 255,   0, 255,    0.2, 1000   // Section #56
  58,  54,   0, 255,   0, 255,    0.8, 1000   // Section #57
  62,  13,   0, 255,   0, 255,    0.5,    1   // Section #58
  63,  12,   0, 255,   0, 255,    0.5,    1   // Section #59
  43,  63,   0, 255,   0, 255,    0.6,    1   // Section #60
  64,  63,   0, 255,   0, 255,    0.5, 1000   // Section #61
  65,   1,   0, 255,   0, 255,    0.7,    0   // Section #62
  66,   1,   0, 255,   0, 255,    0.5,    0   // Section #63
  40,  66,   0, 255,   0, 255,    1.2,    0   // Section #64
  66,  26,   0, 255,   0, 255,    1.2,    0   // Section #65
  81,  20,   0, 255,   0, 255,    0.6,    0   // Section #66
  67,  68,   0, 255,   0, 255,    0.3,    0   // Section #67
  68,  75,   0, 255,   0, 255,    1.0,    0   // Section #68
  20,  69,   0, 255,   0, 255,    0.9,    1   // Section #69
  70,  69,   0, 255,   0, 255,    1.1,    1   // Section #70
  74,  68,   0, 255,   0, 255,    0.3,    0   // Section #71
  72,  71,   0, 255,   0, 255,    0.3,    0   // Section #72
  72,  73,   0, 255,   0, 255,    0.3,    0   // Section #73
  73,  74,   0, 255,   0, 255,    0.3,    0   // Section #74
  71,  74,   0, 255,   0, 255,    0.3,    0   // Section #75
  73,  75,   0, 255,   0, 255,    0.3,    0   // Section #76
  75,  76,   0, 255,   0, 255,    1.0,    0   // Section #77
  77,  91,   0, 255,   0, 255,    1.1,    0   // Section #78
  70,  76,   0, 255,   0, 255,    1.0,    1   // Section #79
  78,  77,   0, 255,   0, 255,    1.0,    0   // Section #80
  78,  79,   0, 255,   0, 255,    1.0,    0   // Section #81
  79,  80,   0, 255,   0, 255,    1.1,    0   // Section #82
  80,  70,   0, 255,   0, 255,    1.2,    0   // Section #83
  80,  69,   0, 255,   0, 255,    1.2,    0   // Section #84
  77,  80,   0, 255,   0, 255,    1.0,    0   // Section #85
  81,  76,   0, 255,   0, 255,    0.9,    0   // Section #86
  81,  67,   0, 255,   0, 255,    0.9,    0   // Section #87
  82,  26,   0, 255,   0, 255,    1.1,    0   // Section #88
  82,  27,   0, 255,   0, 255,    0.4,    0   // Section #89
  83,  28,   0, 255,   0,  45,    0.4,    0   // Section #90
  51,  13,   0, 255,   0, 255,    0.7,    0   // Section #91
  51,  84,   0, 255,   0, 255,    1.2,    0   // Section #92
  84,  48,   0, 255,   0, 255,    0.5,    0   // Section #93
  50,  84,   0, 255,   0, 255,    1.0,    0   // Section #94
  22,  21,   0, 255,   0, 255,    0.4,    0   // Section #95
  15,  85,   0, 255,   0, 255,    0.6,    1   // Section #96
  85,  86,   0, 255,   0, 255,    0.9,    1   // Section #97
  86,  16,   0, 255,   0, 255,    1.2,    1   // Section #98
  16,  87,   0, 255,   0, 255,    1.2,    1   // Section #99
  87,  88,   0, 255,   0, 255,    1.2, 1001   // Section #100
  88,  89,   0, 255,   0, 255,    1.2,    1   // Section #101
  89,  90,   0, 255,   0, 255,    1.2,    1   // Section #102
  90,  17,   0, 255,   0, 255,    1.7,    1   // Section #103
  91,  76,   0, 255,   0, 255,    1.1,    0   // Section #104
  92,   3,   0, 255,   0, 255,    0.9,    1   // Section #105
  93,  39,   0, 255,   0, 255,    0.7,    0   // Section #106
  94,  95,   0, 255,   0, 255,    0.8,    0   // Section #107
  95,  40,   0, 255,   0, 255,    0.5,    0   // Section #108
  76,  92,   0, 255,   0, 255,    0.9,    1   // Section #109
   0,  18,   0, 255,   0, 255,    0.2,    0   // Section #110
   9,  96,   0, 255,   0, 255,    0.5,    1   // Section #111
  96,  97,   0, 255,   0, 255,    0.5,    1   // Section #112
  97,  98,   0, 255,   0, 255,    0.5,    1   // Section #113
  98,  99,   0, 255,   0, 255,    0.5,    1   // Section #114
  99, 100,   0, 255,   0, 255,    0.5,    1   // Section #115
 100, 101,   0, 255,   0, 255,    0.5,    1   // Section #116
 101, 102,   0, 255,   0, 255,    0.5,    1   // Section #117
 102, 103,   0, 255,   0, 255,    0.5,    1   // Section #118
 103, 104,   0, 255,  40,  50,    0.5,    1   // Section #119
 104, 105,   0, 255,   0, 255,    0.5,    1   // Section #120
 105,  63,   0, 255,   0, 255,    0.5,    1   // Section #121
  10, 106,   0, 255,   0, 255,    0.5,    1   // Section #122
 106, 107,   0, 255,   0, 255,    0.5,    1   // Section #123
 107, 108,   0, 255,   0, 255,    0.5,    1   // Section #124
 108, 109,   0, 255,   0, 255,    0.5,    1   // Section #125
 109, 110,   0, 255,   0, 255,    0.5,    1   // Section #126
 110, 100,   0, 255,   0, 255,    0.5,    1   // Section #127
  97, 111,   0, 255,   0, 255,    0.5,    1   // Section #128
 111, 112,   0, 255,   0, 255,    0.5,    1   // Section #129
 112, 113,   0, 255,   0, 255,    0.5,    0   // Section #130
 113, 100,   0, 255,   0, 255,    0.5,    1   // Section #131
 114, 115,   0, 255,   0, 255,    0.5, 1000   // Section #132
 115, 116,   0, 255,   0, 255,    0.5, 1000   // Section #133
 116, 111,   0, 255,   0, 255,    0.5, 1000   // Section #134
 114, 117,   0, 255,   0, 255,    0.5,    0   // Section #135
 117, 118,   0, 255,   0, 255,    0.5,    0   // Section #136
 119, 118,   0, 255,   0, 255,    0.5, 1000   // Section #137
 118, 115,   0, 255,   0, 255,    0.5,    0   // Section #138
 120,   9,   0, 255,   0, 255,    0.5,    1   // Section #139
 121,  97,   0, 255,   0, 255,    0.5, 1000   // Section #140

8                                                             // Number of cop start points
   28.577,   -5.177,   47.450,    0.000,    0.000,    0.000   // Cop start point #0
  118.235,   -5.177,   12.354,    0.000,    0.000,    0.000   // Cop start point #1
  145.467,   -5.177,   12.256,    0.000,    0.000,    0.000   // Cop start point #2
  137.645,   -5.177,   54.629,    0.000,    0.000,    0.000   // Cop start point #3
  120.966,   -6.382,   90.049,    0.000,    0.000,    0.000   // Cop start point #4
   54.284,   -5.210,   84.138,    0.000,    0.000,    0.000   // Cop start point #5
   11.198,   -5.177,   77.197,    0.000,    0.000,    0.000   // Cop start point #6
   97.734,   -0.253,   16.190,    0.000,    0.000,    0.000   // Cop start point #7

END OF OPPONENT PATHS

2										// number of material modifiers

// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT							// skid mark material

//	material '0'
1.0										// car wall friction
1.0										// tyre road friction
0										// down force
0.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
1										// room for expansion
none									// room for expansion

// Non CarObjects
2										// number of non car objects
BARRIER.TXT
WRECK.TXT

0									// Number of smoke shadetables

8										// Number of network start points

129.75,-5.17,-1.22							//1
270													

146.57,-5.17,10.49							//2						
180									

117.75,-5.17,44.13							//3						
180									

93.29,-5.17,1.23							//4						
270									

107.79,-5.17,32.17						//5						
225									

107.78,-5.17,55.58							//6						
180									

120.88,-6.38,95.1							//7						
270									

141.89,-5.17,59.36							//8						
310									

1								// number of splash files
SPLSHYEL.PIX 						// name of pixelmapfile for splashes

1

INDUSTA3.TXT
