VERSION 6							// V1 expects map checkpoint rectangles
									// V2 and above expect map checkpoint points
									// V3 and above expect splash file stuff at the end
									// V4 and above expect two sets of PIX and MAT and ped substitution entry



-256.540,-2.555,-102.5						// Position of centre of start of grid
160									// Direction that grid faces in

// Direction that grid faces in

// Laps, checkpoints etc

60,30,10							// Initial timer count for each skill level
4									// # laps
5000,5000,5000						// Race completed bonus (all laps raced) for each skill level
10000,10000,10000					// Race completed bonus (all peds killed) for each skill level
10000,10000,10000					// Race completed bonus (all oppos wasted) for each skill level

// Width and height of map checkpoint rectangles
9,18
11,26


0									// # checkpoints


6									// # pixelmap files to load
NYSKY1.PIX
C3SKY2.PIX
COASTA1.pix
NCHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX

6									// # pixelmap files to load (low memory)
NYSKY1.PIX
C3SKY2.PIX
COA8TA3.pix
NCHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX


2									// # shade table files to load
COASTA1.TAB
identity.tab

9									// # material files to load
YWW.MAT
WATTY.MAT
NYSKY1.MAT
C3SKY2.MAT
COASTA1.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT

9
YWW.MAT									// # material files to load (low memory)
WATTY.MAT
NYSKY1.MAT
C3SKY2.MAT
COA8TA3.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT


1									// # model files to load
NETCOSTA.dat

1									// # model files to load
NETCSTA8.dat


NETCOSTA.ACT							// Track actor

NETCSTA8.ACT							// Track actor

NETCSTAX.ACT							// Additional actor

// HORIZON STUFF

NCHORIZN.PIX						// Name of sky texture pixelmap (or "none")
4									// Horizontal repetitions of sky texture
66									// Vertical size of sky texture (degrees)
128									// Position of horizon (pixels below top)
dark								// Depth cue mode ("none", "dark" or "fog")
8,0									// Degree of fog/darkness

// DEFAULT ENGINE NOISE

0

// SPECIAL EFFECTS VOLUMES

11				// # special effects volumes



DEFAULT WATER
0.2									// gravity multiplier
50									// viscosity multiplier
0									// Car damage per millisecond
0.002								// Pedestrian damage per millisecond
0									// camera effect index
1									// Sky colour
WATTY.MAT								// Windscreen material to use
5100								// Sound ID of entry noise
5100								// Sound ID of exit noise
2									// Engine noise index
0									// material index




NEW IMPROVED!
8.702, -0.080, -1.941
0.031, 3.583, -0.007
12.018, 0.007, 53.882
-267.444, -15.562, -32.364
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
5.124, 0.000, 5.680
0.000, 1.000, 0.000
-40.065, 0.000, 22.294
-254.058, -16.907, -75.250
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
0.022, 0.000, 1.728
0.000, 2.074, 0.000
-3.583, 0.000, 0.046
-212.111, -17.667, -89.661
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
-0.416, 0.000, -1.677
0.003, 1.728, -0.001
1.398, -0.002, -0.347
-193.901, -17.667, -91.913
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
-0.940, 0.000, -1.848
0.000, 1.000, 0.000
1.283, 0.000, -0.653
-181.791, -16.747, -97.209
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
1.262, 0.000, 1.645
0.000, 1.728, 0.000
-1.143, 0.000, 0.876
-171.178, -16.427, -105.123
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
1.210, 0.000, 1.684
0.014, 1.440, -0.010
-0.975, 0.014, 0.700
-165.651, -14.506, -108.596
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
-0.462, 0.000, -2.022
0.000, 1.000, 0.000
1.170, 0.000, -0.267
-133.374, -12.981, -118.326
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
-0.472, 0.000, -2.019
0.013, 1.000, -0.003
1.402, -0.020, -0.328
-93.955, -12.942, -127.460
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
-0.444, 0.000, -1.831
0.000, 1.000, 0.000
9.804, 0.000, -2.379
-72.472, -13.061, -132.528
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index




 
// REFLECTIVE WINDSCREEN SPECIFICATIONS

NYSKY1.MAT							// Material to use for default screens
DRKSCRN.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT							// Material to use for default screens during fog

0									// # areas with different screens

// MAP DETAILS

NCSTAMAP.PIX						// Map pixelmap name

0.744,		0,			0			// World->map transformation matrix
0,			0,			0
0,			0.744, 		0
282.4,		114.9,		0

// ****** START OF FUNK AND GROOVE STUFF ******

START OF FUNK

!!WATER.MAT
constant
slither
harmonic
0.20,0
5,5
no fucking lighting
no animation you cunt

END OF FUNK



START OF GROOVE

&YAC0001.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
2							// max angle of rock

NEXT GROOVE

&YAC0002.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
2							// max angle of rock

NEXT GROOVE

&YAC0003.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock

NEXT GROOVE

&YAC0004.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock

NEXT GROOVE

&YAC0005.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock

NEXT GROOVE

&YAC0006.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock

NEXT GROOVE

&YAC0007.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock

NEXT GROOVE

&YAC0008.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock

NEXT GROOVE

&YAC0009.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock

NEXT GROOVE

&YAC0010.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.17							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
8							// max angle of rock

NEXT GROOVE

&YAC0011.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0012.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0013.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0014.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.16							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0015.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0016.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.17							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0017.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0018.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.9,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0018.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.1,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0019.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.12,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
11							// max angle of rock

NEXT GROOVE

&YAC0020.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.12,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0020.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock


NEXT GROOVE

&YAC0021.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0022.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0023.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.06,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0024.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0025.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0026.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.15,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
11							// max angle of rock

NEXT GROOVE

&YAC0027.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0028.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0029.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0030.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.06,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0031.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock


END OF GROOVE




// ****** START OF PEDESTRIAN STUFF ******

3

511				// Number of pedestrians

// Pedestrian number 1

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-270.099,-2.552,-90.191
	point
	-270.283,-2.552,-90.262
	point
	-270.642,-2.552,-90.240
	point
	-270.750,-2.552,-90.830
	point
	-270.106,-2.552,-94.390
	reverse


// Pedestrian number 2

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-269.542,-2.552,-93.851
	point
	-269.226,-2.552,-94.602
	point
	-268.805,-2.552,-97.226
	point
	-269.183,-2.552,-97.602
	reverse


// Pedestrian number 3

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-269.651,-2.552,-96.212
	point
	-270.692,-2.552,-96.146
	point
	-271.176,-2.552,-93.826
	point
	-270.885,-2.550,-90.653
	point
	-269.978,-2.552,-89.883
	reverse


// Pedestrian number 4

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-283.484,-2.539,-69.888
	point
	-283.344,-2.539,-70.484
	point
	-282.090,-2.547,-71.521
	point
	-281.665,-2.552,-75.949
	reverse


// Pedestrian number 5

1				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-273.553,-2.552,-71.184
	point
	-274.416,-2.552,-70.664
	point
	-276.012,-2.552,-69.593
	point
	-282.558,-2.541,-69.943
	point
	-283.671,-2.538,-70.196
	point
	-285.278,-2.538,-71.625
	reverse


// Pedestrian number 6

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-267.804,-2.552,-75.968
	point
	-269.345,-2.552,-74.693
	point
	-270.275,-2.552,-73.536
	point
	-272.513,-2.552,-72.074
	point
	-272.953,-2.552,-71.371
	reverse


// Pedestrian number 7

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-283.972,-2.540,-69.747
	point
	-285.354,-2.540,-66.865
	point
	-287.150,-2.531,-66.831
	point
	-287.955,-2.543,-68.800
	point
	-288.656,-2.544,-69.908
	reverse


// Pedestrian number 8

1				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-313.628,-11.971,-26.568
	point
	-313.384,-11.971,-24.033
	point
	-312.579,-11.971,-22.773
	point
	-312.587,-11.971,-21.316
	point
	-312.863,-11.971,-19.602
	point
	-312.938,-11.971,-18.287
	reverse


// Pedestrian number 9

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-273.343,-15.627,25.364
	point
	-272.440,-15.626,22.412
	point
	-271.392,-15.627,22.991
	point
	-270.066,-15.627,23.992
	point
	-266.453,-15.627,23.741
	reverse


// Pedestrian number 10

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-256.908,-15.622,24.732
	point
	-258.387,-15.620,25.909
	point
	-261.283,-15.627,26.499
	point
	-261.930,-15.627,25.909
	point
	-262.724,-15.627,24.242
	reverse


// Pedestrian number 11

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-259.411,-15.657,19.155
	point
	-259.250,-15.651,21.396
	point
	-258.661,-15.627,22.942
	point
	-257.584,-15.627,22.954
	point
	-254.533,-15.627,25.546
	reverse


// Pedestrian number 12

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-261.806,-15.627,23.787
	point
	-260.932,-15.627,24.492
	point
	-260.637,-15.631,25.771
	point
	-261.612,-15.627,26.439
	point
	-263.339,-15.627,27.132
	reverse


// Pedestrian number 13

8				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-259.648,-15.627,26.691
	point
	-260.517,-15.634,24.927
	point
	-260.682,-15.634,24.331
	point
	-259.094,-15.652,22.352
	point
	-259.229,-15.655,20.294
	point
	-263.211,-15.657,16.713
	reverse


// Pedestrian number 14

3				// Ref num
5				// Number of instructions
4				// Initial instruction

	point
	-258.070,-15.645,23.910
	point
	-258.197,-15.634,25.400
	point
	-258.889,-15.628,26.320
	point
	-260.490,-15.627,27.624
	reverse


// Pedestrian number 15

8				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-260.701,-15.599,47.238
	point
	-259.289,-15.606,46.406
	point
	-257.955,-15.616,46.773
	point
	-256.369,-15.627,46.363
	point
	-254.084,-15.627,46.205
	point
	-253.703,-15.666,46.495
	reverse


// Pedestrian number 16

8				// Ref num
5				// Number of instructions
5				// Initial instruction

	point
	-253.063,-15.627,45.480
	point
	-254.008,-15.627,44.645
	point
	-254.846,-15.627,44.699
	point
	-257.222,-15.627,43.235
	reverse


// Pedestrian number 17

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-255.654,-15.627,46.287
	point
	-253.574,-15.627,43.281
	point
	-246.306,-15.632,43.864
	reverse


// Pedestrian number 18

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-254.375,-15.627,42.839
	point
	-252.268,-15.627,44.870
	point
	-251.614,-15.627,45.550
	reverse


// Pedestrian number 19

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-277.839,-15.626,46.964
	point
	-278.242,-15.626,48.289
	point
	-278.639,-15.626,48.814
	point
	-279.885,-15.622,51.172
	point
	-280.454,-15.622,51.603
	reverse


// Pedestrian number 20

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-279.755,-15.627,47.717
	point
	-280.472,-15.627,48.585
	point
	-282.667,-15.627,49.018
	reverse


// Pedestrian number 21

1				// Ref num
4				// Number of instructions
3				// Initial instruction

	point
	-273.077,-15.595,49.765
	point
	-277.955,-15.626,48.609
	point
	-278.568,-15.627,47.785
	reverse


// Pedestrian number 22

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-261.550,-15.627,24.535
	point
	-259.447,-15.657,20.859
	point
	-259.724,-15.657,19.231
	point
	-260.028,-15.657,17.513
	point
	-261.038,-15.657,13.342
	point
	-264.753,-15.657,11.104


// Pedestrian number 23

8				// Ref num
9				// Number of instructions
5				// Initial instruction

	point
	-266.082,-2.553,-107.261
	point
	-264.257,-2.552,-109.714
	point
	-261.583,-2.552,-110.630
	point
	-254.872,-2.555,-114.747
	point
	-251.657,-2.553,-118.503
	point
	-250.448,-2.553,-118.685
	point
	-248.889,-2.553,-119.259
	point
	-247.098,-2.551,-119.696
	reverse


// Pedestrian number 24

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-246.091,-2.560,-122.113
	point
	-245.615,-2.566,-123.061
	point
	-245.679,-2.573,-124.489
	point
	-246.242,-2.578,-125.649
	point
	-247.503,-2.581,-126.887
	reverse


// Pedestrian number 25

1				// Ref num
8				// Number of instructions
5				// Initial instruction

	point
	-266.410,998.041,-108.087
	point
	-265.176,997.648,-109.687
	point
	-264.586,-2.552,-109.784
	point
	-263.782,-2.552,-111.050
	point
	-262.242,-2.552,-111.443
	point
	-261.234,-2.552,-111.416
	point
	-256.954,-2.552,-113.230
	reverse


// Pedestrian number 26

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-263.329,-2.552,-106.691
	point
	-264.653,-2.552,-106.833
	point
	-265.447,-2.552,-106.684
	point
	-265.923,-2.552,-106.075
	point
	-266.551,-2.552,-106.131
	reverse


// Pedestrian number 27

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-267.692,-2.552,-101.129
	point
	-265.751,-2.552,-104.003
	point
	-265.192,-2.552,-104.223
	point
	-264.814,-2.552,-104.245
	point
	-264.475,-2.552,-103.716
	reverse


// Pedestrian number 28

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-288.495,-2.544,-69.925
	point
	-287.502,-2.542,-70.409
	point
	-285.983,-2.538,-71.673
	point
	-282.791,-2.544,-71.385
	reverse


// Pedestrian number 29

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-294.143,-2.791,-66.783
	point
	-295.765,-2.911,-66.707
	point
	-298.187,996.963,-66.782
	point
	-301.141,997.563,-65.627
	reverse


// Pedestrian number 30

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-309.792,-4.048,-66.420
	point
	-310.831,-4.048,-65.068
	point
	-308.452,-4.048,-62.614
	point
	-307.596,996.743,-61.857
	reverse


// Pedestrian number 31

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-287.373,-8.005,-48.814
	point
	-286.748,-8.005,-48.424
	point
	-285.763,-8.005,-47.190
	point
	-284.516,-8.005,-44.545
	reverse


// Pedestrian number 32

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-288.702,-8.004,-37.911
	point
	-289.819,-8.005,-36.912
	point
	-291.675,-8.005,-35.896
	point
	-293.116,-8.132,-35.655
	reverse


// Pedestrian number 33

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-316.138,-11.971,-26.853
	point
	-315.844,-11.971,-24.747
	point
	-315.337,-11.971,-23.907
	point
	-314.748,-11.971,-20.162
	reverse


// Pedestrian number 34

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-280.964,-13.137,0.325
	point
	-279.881,-14.067,6.853
	point
	-279.061,-14.283,8.372
	point
	-278.439,-14.469,9.711
	reverse


// Pedestrian number 35

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-281.143,-13.637,4.305
	point
	-279.878,-13.759,4.398
	point
	-277.683,-14.024,5.166
	point
	-277.137,-14.175,6.063
	point
	-276.633,-14.232,6.556
	reverse


// Pedestrian number 36

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-279.125,-13.614,2.765
	point
	-278.599,-13.753,3.557
	point
	-278.165,-13.871,4.247
	point
	-278.714,-14.200,7.385
	point
	-279.385,-14.220,7.974
	reverse


// Pedestrian number 37

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-276.482,-14.300,7.130
	point
	-276.218,-14.378,7.742
	point
	-276.264,-14.536,9.064
	point
	-276.652,-15.143,13.609
	reverse


// Pedestrian number 38

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-275.002,-15.619,19.806
	point
	-274.496,-15.618,19.663
	point
	-268.392,-15.627,22.206
	reverse


// Pedestrian number 39

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-272.264,-15.588,17.210
	point
	-275.058,-15.622,20.682
	point
	-274.902,-15.625,21.666
	point
	-278.184,-15.627,30.167
	reverse


// Pedestrian number 40

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-277.417,-15.627,29.835
	point
	-279.133,-15.627,30.441
	point
	-280.492,-15.627,30.747
	reverse


// Pedestrian number 41

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-282.975,-15.627,28.137
	point
	-283.564,-15.627,28.642
	point
	-284.591,-15.627,31.486
	reverse


// Pedestrian number 42

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-280.448,-15.627,34.628
	point
	-282.453,-15.627,32.370
	point
	-284.006,-15.627,31.417
	point
	-284.666,-15.627,28.681
	reverse


// Pedestrian number 43

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-281.126,-15.627,31.345
	point
	-281.238,-15.627,31.978
	point
	-283.168,-15.627,35.341
	reverse


// Pedestrian number 44

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-285.095,-15.627,28.814
	point
	-286.271,-15.627,29.022
	point
	-287.036,-15.627,29.290
	point
	-287.996,-15.627,29.336
	reverse


// Pedestrian number 45

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-289.209,-15.627,30.392
	point
	-288.316,-15.627,34.406
	point
	-288.427,-15.627,35.933
	point
	-284.900,-15.627,51.411
	reverse


// Pedestrian number 46

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-288.387,-15.627,48.459
	point
	-287.352,-15.627,49.820
	point
	-276.078,-15.617,50.597
	reverse


// Pedestrian number 47

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-59.975,-14.067,-138.803
	point
	-60.505,-14.035,-138.556
	point
	-61.242,-13.918,-136.903
	point
	-62.150,-13.901,-136.874
	reverse


// Pedestrian number 48

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-62.775,-13.901,-136.216
	point
	-60.787,-13.911,-134.451
	point
	-57.955,-14.207,-135.354
	reverse


// Pedestrian number 49

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-56.289,-14.327,-137.813
	point
	-58.024,-14.202,-137.874
	point
	-60.730,-13.909,-134.134
	point
	-61.790,-13.901,-132.943
	reverse


// Pedestrian number 50

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-65.611,-13.901,-132.644
	point
	-64.250,-13.901,-133.070
	point
	-62.385,-13.901,-136.494
	point
	-62.564,-13.916,-137.158
	point
	-66.376,-13.713,-136.860
	reverse


// Pedestrian number 51

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-69.041,-13.532,-139.787
	point
	-67.521,-13.635,-139.776
	point
	-62.387,-13.925,-137.424
	point
	-62.022,-13.949,-137.335
	reverse


// Pedestrian number 52

13				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-75.245,-13.901,-133.507
	point
	-73.024,-13.906,-133.906
	point
	-71.821,-13.901,-133.901
	point
	-70.394,-13.901,-134.566
	point
	-61.138,-13.915,-136.228
	point
	-58.166,-14.192,-136.758
	reverse


// Pedestrian number 53

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-97.076,-13.901,-125.689
	point
	-99.376,-13.901,-124.838
	point
	-106.368,-13.901,-123.246
	point
	-109.898,-13.901,-125.363
	point
	-111.093,-13.901,-125.195
	reverse


// Pedestrian number 54

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-112.755,-13.901,-121.814
	point
	-111.085,-13.901,-122.181
	point
	-109.744,-13.901,-122.466
	point
	-106.911,-13.901,-125.959
	reverse


// Pedestrian number 55

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-175.042,-17.667,-100.004
	point
	-179.117,-17.667,-100.649
	point
	-181.253,-17.667,-99.148
	point
	-181.745,-17.667,-95.709
	reverse


// Pedestrian number 56

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-179.293,-17.667,-97.039
	point
	-176.732,-17.667,-98.838
	point
	-175.654,-17.667,-99.802
	point
	-174.310,-17.667,-100.624
	reverse


// Pedestrian number 57

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-170.557,-16.453,-106.909
	point
	-174.975,-17.426,-103.830
	point
	-176.094,-17.667,-102.846
	point
	-177.133,-17.667,-101.969
	point
	-178.138,-17.667,-101.345
	reverse


// Pedestrian number 58

13				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-203.787,-17.667,-91.459
	point
	-207.159,-17.667,-88.463
	point
	-209.744,-17.667,-88.486
	point
	-211.957,-17.667,-88.351
	point
	-213.212,-17.667,-88.337
	point
	-214.288,-17.667,-91.441
	reverse


// Pedestrian number 59

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-214.358,-17.667,-88.482
	point
	-212.875,-17.667,-88.949
	point
	-210.600,-17.667,-88.317
	point
	-208.806,-17.667,-89.242
	point
	-207.125,-17.667,-91.163
	reverse


// Pedestrian number 60

5				// Ref num
5				// Number of instructions
4				// Initial instruction

	point
	-244.356,-17.667,-77.863
	point
	-245.862,-17.667,-77.901
	point
	-248.054,-17.667,-78.765
	point
	-252.012,-17.667,-78.072
	reverse


// Pedestrian number 61

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-250.827,-17.667,-75.431
	point
	-250.251,-17.667,-75.935
	point
	-247.056,-17.667,-80.030
	reverse


// Pedestrian number 62

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-261.819,-17.667,-73.050
	point
	-260.784,-17.667,-73.119
	point
	-259.624,-17.667,-71.430
	point
	-257.921,-17.667,-71.828
	point
	-254.443,-17.667,-72.824
	reverse


// Pedestrian number 63

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-261.064,-17.667,-70.032
	point
	-260.448,-17.667,-70.677
	point
	-259.825,-17.667,-74.013
	reverse


// Pedestrian number 64

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-265.666,-15.657,7.363
	point
	-265.003,-15.657,8.315
	point
	-262.073,-15.657,10.449
	reverse


// Pedestrian number 65

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-264.227,-15.657,12.830
	point
	-264.807,-15.657,10.788
	point
	-262.833,-15.657,7.393
	point
	-263.603,-15.657,2.374
	reverse


// Pedestrian number 66

14				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-266.605,-15.657,0.758
	point
	-266.129,-15.657,3.554
	point
	-264.564,-15.657,9.533
	point
	-263.000,-15.657,11.069
	point
	-261.491,-15.657,11.978
	reverse


// Pedestrian number 67

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-262.447,-15.657,8.891
	point
	-262.242,-15.657,9.640
	point
	-262.573,-15.657,10.781
	point
	-263.959,-15.657,13.668
	reverse


// Pedestrian number 68

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-259.638,-15.657,18.489
	point
	-261.348,-15.657,12.474
	point
	-264.456,-15.657,10.126
	point
	-264.992,-15.657,9.778
	reverse


// Pedestrian number 69

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-263.145,-15.657,5.505
	point
	-263.338,-15.657,6.703
	point
	-262.725,-15.657,8.248
	point
	-261.501,-15.657,11.636
	reverse


// Pedestrian number 70

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-257.690,-15.632,24.742
	point
	-257.953,-15.627,26.535
	point
	-257.212,-15.627,28.230
	point
	-259.492,-15.627,31.657
	reverse


// Pedestrian number 71

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-256.166,-15.627,33.743
	point
	-256.624,-15.627,33.108
	point
	-257.324,-15.627,29.408
	point
	-257.476,-15.627,25.473
	point
	-255.290,-15.627,22.277
	reverse


// Pedestrian number 72

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-257.372,-15.627,22.881
	point
	-256.107,-15.627,22.939
	point
	-250.981,-15.627,24.575
	reverse


// Pedestrian number 73

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-252.187,-15.627,28.373
	point
	-252.575,-15.627,27.283
	point
	-251.458,-15.627,23.884
	reverse


// Pedestrian number 74

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-261.113,-15.628,25.080
	point
	-261.443,-15.630,22.852
	point
	-262.229,-15.657,20.201
	point
	-259.412,-15.657,19.456
	reverse


// Pedestrian number 75

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-245.970,-15.627,39.348
	point
	-249.793,-15.627,39.942
	point
	-250.178,-15.626,41.146
	reverse


// Pedestrian number 76

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-251.313,-15.627,42.251
	point
	-250.581,-15.627,41.983
	point
	-249.967,-15.627,41.610
	point
	-246.073,-15.632,42.138
	point
	-245.368,-15.627,39.850
	reverse


// Pedestrian number 77

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-244.877,-15.635,43.594
	point
	-247.082,-15.631,43.610
	point
	-248.305,-15.628,42.389
	point
	-251.868,-15.627,23.453
	reverse


// Pedestrian number 78

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-254.490,-15.627,41.847
	point
	-257.747,-15.627,39.460
	point
	-258.167,-15.627,37.313
	point
	-258.321,-15.654,23.099
	reverse


// Pedestrian number 79

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-261.943,-15.627,25.544
	point
	-263.120,-15.627,26.106
	point
	-267.710,-15.627,26.051
	reverse


// Pedestrian number 80

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-268.220,-15.627,25.990
	point
	-268.947,-15.627,25.494
	point
	-269.505,-15.627,20.972
	reverse


// Pedestrian number 81

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-280.302,-15.627,27.697
	point
	-281.003,-15.627,27.992
	point
	-282.525,-15.627,38.145
	reverse


// Pedestrian number 82

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-279.237,-15.627,47.436
	point
	-279.147,-15.627,46.697
	point
	-280.958,-15.627,32.440
	reverse


// Pedestrian number 83

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-283.974,-15.627,31.730
	point
	-283.756,-15.627,32.563
	point
	-283.491,-15.627,33.863
	point
	-278.829,-15.627,47.333
	reverse


// Pedestrian number 84

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-278.011,-15.627,46.284
	point
	-278.348,-15.627,45.160
	point
	-281.207,-15.627,44.482
	reverse


// Pedestrian number 85

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-278.334,-15.708,52.126
	point
	-276.456,-15.917,53.527
	point
	-276.025,-16.174,56.155
	point
	-277.909,-16.318,58.276
	reverse


// Pedestrian number 86

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-272.600,-18.908,82.287
	point
	-269.042,-18.912,86.156
	point
	-269.557,-18.914,89.312
	point
	-270.740,-18.916,92.449
	reverse


// Pedestrian number 87

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-267.411,-18.915,94.181
	point
	-269.126,-18.915,92.989
	point
	-270.514,-18.916,93.653
	point
	-274.046,-18.916,92.297
	point
	-290.575,-18.915,96.467
	reverse


// Pedestrian number 88

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-290.535,-18.915,97.563
	point
	-274.153,-18.915,94.451
	point
	-268.527,-18.915,89.919
	reverse


// Pedestrian number 89

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-267.077,-18.915,92.468
	point
	-267.702,-18.915,91.826
	point
	-268.247,-18.915,90.436
	point
	-270.731,-18.914,89.718
	reverse


// Pedestrian number 90

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-266.066,-18.913,106.289
	point
	-269.661,-18.914,94.163
	point
	-267.923,-18.915,90.522
	reverse


// Pedestrian number 91

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-246.888,-18.915,85.598
	point
	-246.557,-18.915,88.305
	point
	-246.116,-18.915,89.756
	reverse


// Pedestrian number 92

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-242.658,-18.915,100.699
	point
	-242.385,-18.915,96.290
	point
	-244.021,-18.915,89.483
	point
	-244.344,-18.914,85.812
	reverse


// Pedestrian number 93

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-224.432,-18.915,81.168
	point
	-225.555,-18.916,82.652
	point
	-228.229,-18.916,84.140
	reverse


// Pedestrian number 94

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-224.098,-18.916,82.961
	point
	-224.899,-18.916,82.519
	point
	-225.427,-18.916,82.805
	point
	-232.529,-18.916,82.657
	reverse


// Pedestrian number 95

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-224.172,-18.916,82.005
	point
	-243.623,-18.915,87.028
	point
	-244.561,-18.915,86.304
	point
	-245.521,-18.913,82.788
	point
	-248.219,-18.911,80.794
	reverse


// Pedestrian number 96

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-246.298,-18.910,78.252
	point
	-246.004,-18.911,79.590
	point
	-247.313,-18.916,88.406
	reverse


// Pedestrian number 97

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-245.505,-18.915,92.686
	point
	-245.012,-18.915,94.175
	point
	-244.207,-18.916,100.898
	reverse


// Pedestrian number 98

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-221.401,-18.916,95.766
	point
	-222.908,-18.916,95.051
	point
	-227.663,-18.916,95.340
	point
	-230.000,-18.916,96.978
	point
	-244.157,-18.915,98.220
	reverse


// Pedestrian number 99

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-238.820,-18.915,99.952
	point
	-241.360,-18.915,98.651
	point
	-244.445,-18.915,96.720
	point
	-244.997,-18.915,95.096
	reverse


// Pedestrian number 100

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-242.120,-18.915,97.469
	point
	-244.093,-18.915,98.859
	point
	-245.851,-18.916,101.360
	point
	-287.253,-18.914,110.686
	reverse


// Pedestrian number 101

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-245.032,-18.916,101.345
	point
	-244.585,-18.915,98.971
	point
	-242.312,-18.914,96.801
	reverse


// Pedestrian number 102

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-251.461,-18.916,100.610
	reverse


// Pedestrian number 103

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-253.398,-15.627,45.697
	reverse


// Pedestrian number 104

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-257.272,-15.627,42.491
	reverse


// Pedestrian number 105

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-256.284,-15.627,33.307
	reverse


// Pedestrian number 106

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-254.620,-15.627,22.531
	reverse


// Pedestrian number 107

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-250.575,-15.627,41.531
	reverse


// Pedestrian number 108

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-254.042,-17.667,-73.114
	reverse


// Pedestrian number 109

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-252.533,-17.667,-77.667
	reverse


// Pedestrian number 110

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-226.823,-17.667,-91.019
	reverse


// Pedestrian number 111

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-27.743,-15.561,-44.497
	reverse


// Pedestrian number 112

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-26.788,-15.561,-45.238
	reverse


// Pedestrian number 113

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-25.847,-15.561,-45.968
	reverse


// Pedestrian number 114

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-82.993,-13.028,-48.234
	reverse


// Pedestrian number 115

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-129.713,-18.645,-45.533
	reverse


// Pedestrian number 116

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-127.573,-18.655,-46.141
	reverse


// Pedestrian number 117

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-125.686,-18.634,-45.420
	reverse


// Pedestrian number 118

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-138.923,-18.725,-58.154
	reverse


// Pedestrian number 119

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-141.695,-18.737,-59.375
	reverse


// Pedestrian number 120

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-145.946,-18.665,-48.496
	reverse


// Pedestrian number 121

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-145.198,-18.670,-46.779
	reverse


// Pedestrian number 122

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-139.581,-16.166,-39.660
	reverse


// Pedestrian number 123

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-137.255,-14.010,-30.646
	reverse


// Pedestrian number 124

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-136.103,-13.938,-30.522
	reverse


// Pedestrian number 125

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-132.813,-9.082,-50.595
	reverse


// Pedestrian number 126

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-133.365,-9.082,-50.436
	reverse


// Pedestrian number 127

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-264.404,-2.552,-104.048
	reverse


// Pedestrian number 128

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-264.253,-2.552,-104.536
	reverse


// Pedestrian number 129

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-268.549,-2.552,-98.537
	reverse


// Pedestrian number 130

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-154.797,-8.795,-37.416
	point
	-155.758,-9.008,-39.093
	point
	-155.682,-9.077,-40.053
	point
	-146.436,-9.077,-42.540
	reverse


// Pedestrian number 131

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-146.536,-9.077,-45.589
	point
	-148.877,-9.077,-44.903
	point
	-149.937,-9.077,-44.138
	point
	-150.793,-9.077,-41.614
	reverse


// Pedestrian number 132

13				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	-144.951,-8.822,-45.084
	point
	-146.179,-9.077,-44.767
	point
	-147.609,-9.077,-45.393
	reverse


// Pedestrian number 133

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-135.266,-8.919,-46.250
	point
	-134.767,-9.089,-46.979
	point
	-132.236,-9.084,-46.497
	point
	-121.404,-9.078,-49.433
	reverse


// Pedestrian number 134

13				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-132.587,-9.081,-50.555
	point
	-132.074,-8.967,-50.100
	point
	-131.552,-9.077,-49.757
	point
	-128.024,-9.077,-49.940
	point
	-124.245,-9.078,-48.738
	point
	-122.163,-9.338,-46.182
	reverse


// Pedestrian number 135

14				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-125.546,-9.934,-40.050
	point
	-123.504,-9.673,-41.952
	point
	-124.452,-9.143,-47.802
	point
	-121.549,-9.096,-49.138
	reverse


// Pedestrian number 136

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-127.186,-9.077,-48.003
	point
	-128.893,-9.077,-48.697
	point
	-134.625,-9.081,-48.200
	point
	-136.083,-8.818,-47.566
	reverse


// Pedestrian number 137

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-134.164,-9.096,-46.011
	point
	-133.139,-9.080,-47.536
	point
	-131.164,-9.077,-48.998
	point
	-125.868,-9.078,-51.521
	reverse


// Pedestrian number 138

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-23.454,-15.561,-49.659
	point
	-25.541,-15.561,-45.735
	point
	-28.159,-15.561,-43.634
	point
	-37.209,-15.561,-46.669
	reverse


// Pedestrian number 139

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-31.746,-15.561,-44.197
	point
	-29.092,-15.561,-44.828
	point
	-23.428,-15.561,-47.823
	reverse


// Pedestrian number 140

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-23.237,-15.561,-51.567
	point
	-24.452,-15.560,-51.263
	point
	-27.403,-15.561,-49.276
	point
	-29.418,-15.561,-46.721
	point
	-28.054,-15.561,-43.551
	reverse


// Pedestrian number 141

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-24.211,-15.561,-46.619
	point
	-25.772,-15.561,-47.198
	point
	-26.246,-15.561,-49.840
	point
	-24.516,-15.561,-50.401
	reverse


// Pedestrian number 142

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-274.111,-15.600,47.219
	point
	-273.015,-15.599,47.834
	point
	-271.303,-15.599,49.503
	point
	-269.993,-15.599,49.251
	reverse


// Pedestrian number 143

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-275.307,-15.612,50.411
	point
	-274.073,-15.604,50.194
	point
	-267.833,-15.599,48.906
	reverse


// Pedestrian number 144

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-268.077,-15.599,45.919
	point
	-270.539,-15.599,46.626
	point
	-271.840,-15.599,47.562
	point
	-274.421,-15.604,47.757
	point
	-276.369,-15.619,47.718
	reverse


// Pedestrian number 145

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-266.716,-15.599,48.695
	point
	-263.974,-15.599,47.846
	point
	-261.122,-15.599,44.348
	reverse


// Pedestrian number 146

29				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-273.751,-15.599,47.079
	point
	-271.455,-15.599,47.075
	point
	-270.293,-15.599,48.141
	point
	-267.297,-15.599,47.593
	point
	-264.722,-15.599,48.203
	reverse


// Pedestrian number 147

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-262.696,-15.599,44.762
	point
	-257.263,-15.627,43.881
	point
	-253.610,-15.627,42.867
	reverse


// Pedestrian number 148

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-282.000,-15.625,51.855
	point
	-283.612,-15.627,50.231
	point
	-285.220,-15.627,48.205
	point
	-290.883,-15.627,37.644
	reverse


// Pedestrian number 149

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-269.156,-15.599,46.071
	point
	-265.497,-15.599,45.847
	point
	-263.858,-15.599,45.177
	point
	-256.357,-15.627,46.578
	reverse


// Pedestrian number 150

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-256.138,-15.649,46.817
	point
	-255.963,-15.783,47.965
	point
	-255.393,-15.998,49.747
	point
	-252.229,-16.263,52.093
	reverse


// Pedestrian number 151

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-240.193,-14.789,40.689
	point
	-237.698,-14.359,39.170
	point
	-236.859,-13.820,34.927
	reverse


// Pedestrian number 152

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-244.855,-15.619,40.005
	point
	-244.408,-15.513,39.803
	point
	-242.112,-14.883,38.503
	point
	-239.603,-14.414,36.895
	reverse


// Pedestrian number 153

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-235.848,-13.988,37.950
	point
	-232.211,-13.012,35.192
	point
	-229.563,-12.513,32.817
	reverse


// Pedestrian number 154

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-230.596,-12.208,29.479
	point
	-228.883,-11.868,28.658
	point
	-225.417,-11.308,27.739
	point
	-223.554,-11.037,25.996
	reverse


// Pedestrian number 155

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-215.914,-9.122,11.075
	point
	-215.358,-9.078,10.006
	point
	-215.350,-9.078,9.436
	point
	-217.107,-9.078,5.180
	reverse


// Pedestrian number 156

14				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-216.712,-9.078,9.149
	point
	-215.622,-9.078,5.559
	point
	-215.178,-9.078,3.462
	point
	-215.443,-9.078,2.543
	point
	-214.628,-9.078,1.286
	point
	-215.556,-9.078,-1.573
	reverse


// Pedestrian number 157

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-220.365,-9.446,14.723
	point
	-219.623,-9.293,12.993
	point
	-219.052,-9.222,12.157
	point
	-218.892,-9.163,10.928
	reverse


// Pedestrian number 158

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-217.898,-9.078,9.322
	point
	-217.505,-9.078,6.830
	point
	-216.861,-9.078,4.397
	point
	-216.390,-9.078,1.667
	reverse


// Pedestrian number 159

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-215.150,-9.078,8.818
	point
	-215.007,-9.078,7.951
	point
	-214.495,-9.078,7.136
	point
	-214.368,-9.078,6.415
	point
	-213.805,-9.078,4.554
	reverse


// Pedestrian number 160

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-218.536,-9.103,9.741
	point
	-217.609,-9.078,7.851
	point
	-216.308,-9.078,5.552
	point
	-216.740,-9.078,4.223
	reverse


// Pedestrian number 161

8				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-206.193,-8.044,-8.222
	point
	-205.343,-7.665,-8.595
	point
	-204.631,-7.562,-8.476
	point
	-204.049,-7.140,-8.757
	point
	-203.320,-6.748,-8.939
	reverse


// Pedestrian number 162

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-204.299,-7.663,-8.118
	point
	-203.816,-7.387,-8.357
	point
	-203.330,-7.145,-8.425
	point
	-202.910,-7.249,-8.038
	point
	-201.931,-7.245,-7.347
	reverse


// Pedestrian number 163

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-206.737,-8.135,-8.164
	point
	-205.643,-7.958,-7.995
	point
	-203.866,-7.672,-7.739
	point
	-203.208,-7.562,-7.607
	point
	-201.235,-7.058,-6.994
	reverse


// Pedestrian number 164

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-197.295,-5.839,-1.871
	point
	-194.701,-5.332,-0.287
	point
	-193.775,-5.328,0.480
	point
	-193.307,-5.328,0.595
	point
	-192.870,-5.328,1.078
	reverse


// Pedestrian number 165

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-188.596,-5.325,0.546
	point
	-187.717,-5.327,1.713
	point
	-186.019,-5.427,3.168
	point
	-184.273,-5.428,3.262
	reverse


// Pedestrian number 166

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-190.226,-5.270,3.747
	point
	-190.782,-4.797,3.803
	point
	-191.406,-4.735,3.288
	point
	-191.612,-5.327,2.311
	reverse


// Pedestrian number 167

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-188.997,-5.362,4.469
	point
	-186.993,-5.407,4.074
	point
	-186.415,-5.427,3.910
	point
	-183.962,-5.428,3.497
	point
	-181.176,-5.421,3.071
	reverse


// Pedestrian number 168

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-184.261,-5.428,6.319
	point
	-185.743,-5.428,5.912
	point
	-187.377,-5.421,5.567
	reverse


// Pedestrian number 169

8				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-185.924,-5.427,2.800
	point
	-185.395,-5.428,4.132
	point
	-183.905,-5.428,5.366
	point
	-181.818,-5.423,6.072
	point
	-179.124,-5.425,5.360
	reverse


// Pedestrian number 170

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-174.318,-5.442,-0.457
	point
	-174.188,-5.446,-0.956
	point
	-174.107,-5.498,-4.044
	point
	-175.052,-5.851,-7.078
	reverse


// Pedestrian number 171

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-177.642,-5.713,-5.465
	point
	-177.881,-5.840,-6.393
	point
	-178.966,-6.300,-8.660
	reverse


// Pedestrian number 172

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-177.301,-5.594,-4.567
	point
	-176.429,-5.872,-6.928
	point
	-176.337,-6.116,-8.542
	point
	-176.405,-6.376,-10.122
	reverse


// Pedestrian number 173

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-180.871,-8.504,-21.449
	point
	-180.128,-8.799,-25.143
	point
	-179.896,-8.854,-25.811
	point
	-178.526,-9.042,-27.987
	reverse


// Pedestrian number 174

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-178.132,-9.078,-28.560
	point
	-175.555,-9.078,-29.629
	point
	-173.209,-9.078,-30.268
	point
	-170.662,-9.078,-32.453
	reverse


// Pedestrian number 175

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-170.287,-9.078,-32.745
	point
	-169.972,-9.078,-34.458
	point
	-168.781,-9.078,-35.482
	point
	-164.568,-9.078,-36.741
	reverse


// Pedestrian number 176

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-166.497,-9.078,-39.067
	point
	-164.967,-9.078,-39.826
	point
	-163.602,-9.078,-40.411
	point
	-158.816,-9.078,-39.141
	reverse


// Pedestrian number 177

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-93.141,-10.699,-46.567
	point
	-90.667,-11.282,-46.195
	point
	-88.743,-11.763,-45.902
	point
	-86.841,-12.221,-46.212
	point
	-83.983,-12.934,-45.274
	reverse


// Pedestrian number 178

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-79.598,-13.281,-47.890
	point
	-76.790,-13.067,-46.072
	point
	-76.641,-13.072,-45.976
	point
	-74.152,-13.200,-44.051
	reverse


// Pedestrian number 179

5				// Ref num
7				// Number of instructions
6				// Initial instruction

	point
	-63.452,-15.005,-45.914
	point
	-59.726,-15.561,-45.200
	point
	-56.465,-15.561,-44.719
	point
	-55.502,-15.561,-44.850
	point
	-54.827,-15.561,-44.541
	point
	-54.827,-15.561,-44.541
	reverse


// Pedestrian number 180

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-50.902,-15.561,-41.216
	point
	-48.469,-15.561,-41.442
	point
	-46.856,-15.561,-41.425
	point
	-44.620,-15.561,-41.528
	reverse


// Pedestrian number 181

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-51.913,-15.561,-41.452
	point
	-54.157,-15.561,-41.768
	point
	-56.903,-15.561,-42.016
	reverse


// Pedestrian number 182

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-58.522,-15.561,-45.328
	point
	-57.228,-15.561,-44.640
	point
	-53.892,-15.561,-44.153
	point
	-52.330,-15.561,-44.363
	reverse


// Pedestrian number 183

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-60.416,-15.465,-45.270
	point
	-61.681,-15.280,-45.454
	point
	-64.002,-14.903,-45.808
	point
	-65.282,-14.658,-46.072
	reverse


// Pedestrian number 184

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-33.680,-15.561,-48.367
	point
	-29.151,-15.561,-47.717
	point
	-23.574,-15.561,-49.720
	reverse


// Pedestrian number 185

29				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-28.036,-15.561,-52.219
	point
	-29.046,-15.561,-51.305
	point
	-30.114,-15.561,-50.544
	point
	-31.076,-15.561,-50.004
	reverse


// Pedestrian number 186

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-27.654,-15.561,-47.388
	point
	-28.060,-15.561,-45.289
	point
	-28.902,-15.561,-43.269
	reverse


// Pedestrian number 187

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-18.146,-15.561,-61.368
	point
	-16.833,-15.561,-64.439
	point
	-15.727,-15.547,-68.677
	reverse


// Pedestrian number 188

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-18.611,-15.561,-60.084
	point
	-18.493,-15.561,-61.007
	point
	-15.497,-15.515,-70.280
	reverse


// Pedestrian number 189

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-18.380,-15.539,-69.591
	point
	-18.681,-15.518,-68.230
	point
	-19.311,-15.562,-66.305
	point
	-19.974,-15.561,-64.060
	point
	-20.299,-15.561,-63.560
	reverse


// Pedestrian number 190

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-18.388,-15.521,-70.426
	point
	-17.230,-15.495,-71.950
	point
	-15.033,-15.495,-73.694
	point
	-15.044,-15.495,-75.395
	reverse


// Pedestrian number 191

3				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-14.173,-14.288,-115.232
	point
	-12.458,-14.162,-117.244
	point
	-11.531,-14.109,-118.322
	point
	-11.367,-14.010,-120.702
	point
	-11.328,-14.015,-120.886
	point
	-11.564,-14.210,-121.700
	reverse


// Pedestrian number 192

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-11.554,-14.326,-114.336
	point
	-12.126,-14.253,-115.646
	point
	-13.671,-14.128,-118.100
	point
	-13.738,-14.154,-118.514
	point
	-14.235,-14.340,-120.942
	reverse


// Pedestrian number 193

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-14.431,-14.362,-114.006
	point
	-14.209,-14.161,-117.414
	point
	-14.245,-14.245,-119.162
	reverse


// Pedestrian number 194

29				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	-14.019,-14.830,-124.818
	point
	-13.509,-15.444,-127.889
	point
	-11.893,-15.631,-131.178
	point
	-12.495,-15.631,-131.975
	point
	-12.980,-15.631,-133.519
	point
	-14.167,-15.631,-134.831
	point
	-15.643,-15.631,-136.253
	reverse


// Pedestrian number 195

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-15.503,-15.631,-132.103
	point
	-11.967,-15.594,-130.452
	point
	-11.549,-15.528,-129.287
	reverse


// Pedestrian number 196

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-11.584,-15.483,-128.504
	point
	-11.700,-15.576,-130.153
	point
	-12.536,-15.631,-132.708
	reverse


// Pedestrian number 197

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-17.200,-15.631,-133.775
	point
	-19.067,-15.629,-134.677
	point
	-21.511,-15.585,-137.659
	reverse


// Pedestrian number 198

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.188,-15.562,-137.478
	point
	-33.425,-15.562,-137.417
	point
	-38.063,-15.555,-137.825
	reverse


// Pedestrian number 199

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-37.519,-15.562,-134.767
	point
	-41.532,-15.437,-137.507
	point
	-42.737,-15.345,-137.747
	reverse


// Pedestrian number 200

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-52.536,-14.601,-134.892
	point
	-54.431,-14.461,-134.946
	point
	-58.037,-14.201,-137.413
	point
	-59.248,-14.119,-138.455
	reverse


// Pedestrian number 201

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-61.996,-13.901,-136.617
	point
	-61.204,-13.916,-136.545
	point
	-58.575,-14.148,-134.805
	reverse


// Pedestrian number 202

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-61.172,-13.901,-133.827
	point
	-62.598,-13.901,-135.916
	point
	-64.597,-13.901,-135.750
	reverse


// Pedestrian number 203

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-78.384,-13.021,-140.037
	point
	-82.901,-12.812,-137.255
	point
	-86.013,-12.670,-137.159
	reverse


// Pedestrian number 204

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-89.978,-12.488,-137.208
	point
	-92.780,-12.357,-137.667
	point
	-98.558,-12.093,-137.310
	reverse


// Pedestrian number 205

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-164.897,-9.029,-141.292
	point
	-168.279,-8.767,-140.352
	point
	-169.487,-8.668,-139.876
	point
	-171.154,-8.530,-139.352
	reverse


// Pedestrian number 206

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-167.121,-8.860,-137.879
	point
	-168.014,-8.788,-137.578
	point
	-169.239,-8.690,-136.999
	reverse


// Pedestrian number 207

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-174.566,-8.230,-136.773
	point
	-175.795,-8.117,-135.328
	point
	-176.785,-8.026,-134.361
	point
	-177.411,-7.967,-133.357
	point
	-178.164,-7.895,-132.071
	reverse


// Pedestrian number 208

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-175.648,-8.132,-130.543
	point
	-176.472,-8.055,-129.160
	point
	-176.824,-8.022,-127.301
	point
	-177.463,-7.962,-123.708
	reverse


// Pedestrian number 209

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-179.881,-7.728,-118.107
	point
	-182.502,-7.468,-115.060
	point
	-183.518,-7.358,-113.824
	point
	-183.699,-6.793,-112.925
	reverse


// Pedestrian number 210

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-188.039,-6.870,-114.709
	point
	-190.069,-6.641,-113.765
	point
	-191.402,-6.484,-113.622
	point
	-193.168,-6.279,-113.335
	reverse


// Pedestrian number 211

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-199.733,-5.456,-110.360
	point
	-199.119,-5.069,-109.733
	point
	-198.364,-4.985,-109.470
	point
	-196.892,-5.166,-109.341
	point
	-195.723,-5.966,-109.956
	reverse


// Pedestrian number 212

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-201.463,-5.228,-110.850
	point
	-199.630,-5.469,-110.555
	point
	-198.233,-5.649,-110.207
	point
	-196.739,-5.838,-110.503
	point
	-196.414,-5.879,-110.232
	reverse


// Pedestrian number 213

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-195.802,-5.956,-113.173
	point
	-198.498,-5.616,-113.263
	point
	-200.035,-5.416,-113.415
	point
	-201.760,-5.191,-113.866
	point
	-203.892,-4.901,-114.969
	reverse


// Pedestrian number 214

1				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-203.170,-4.999,-111.287
	point
	-204.126,-4.867,-112.350
	point
	-205.630,-4.660,-112.790
	point
	-206.713,-4.508,-113.248
	point
	-208.206,-4.297,-114.389
	point
	-209.045,-4.174,-114.956
	reverse


// Pedestrian number 215

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-208.288,-4.285,-118.682
	point
	-209.033,-4.169,-119.281
	point
	-209.737,-4.050,-120.532
	point
	-210.064,-3.995,-121.123
	point
	-210.623,-3.889,-123.040
	reverse


// Pedestrian number 216

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-214.008,-3.465,-124.467
	point
	-213.698,-3.484,-122.753
	point
	-213.185,-3.555,-121.988
	point
	-213.022,-3.582,-121.021
	reverse


// Pedestrian number 217

29				// Ref num
9				// Number of instructions
5				// Initial instruction

	point
	-210.892,-3.885,-123.878
	point
	-212.017,-3.744,-126.687
	point
	-211.713,-3.774,-127.972
	point
	-212.090,-3.720,-128.330
	point
	-212.071,-3.717,-128.962
	point
	-211.915,-3.737,-130.228
	point
	-212.109,-3.715,-131.658
	point
	-212.803,-3.621,-134.944
	reverse


// Pedestrian number 218

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-214.005,-3.464,-137.958
	point
	-214.545,-3.400,-139.444
	point
	-215.451,-3.325,-141.219
	point
	-215.887,-3.274,-141.797
	point
	-216.623,-3.208,-143.140
	reverse


// Pedestrian number 219

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-220.808,-2.963,-142.879
	point
	-220.916,-2.427,-142.407
	point
	-220.608,-2.227,-141.860
	reverse


// Pedestrian number 220

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-217.864,-3.159,-139.088
	point
	-217.953,-2.966,-138.941
	point
	-217.926,-2.739,-138.378
	point
	-217.757,-2.537,-137.481
	reverse


// Pedestrian number 221

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-218.020,-3.154,-139.890
	point
	-218.784,-3.133,-141.209
	point
	-219.332,-3.118,-142.147
	point
	-220.767,-3.087,-143.468
	point
	-222.002,-3.059,-144.447
	reverse


// Pedestrian number 222

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-221.117,-3.071,-147.339
	point
	-221.770,-3.063,-147.743
	point
	-223.903,-3.018,-148.851
	point
	-226.591,-2.962,-150.613
	reverse


// Pedestrian number 223

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-230.681,-2.863,-152.229
	point
	-229.772,-2.879,-151.728
	point
	-228.778,-2.899,-151.598
	point
	-227.521,-2.465,-151.751
	reverse


// Pedestrian number 224

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-231.665,-2.845,-152.564
	point
	-233.043,-2.856,-152.639
	point
	-234.060,-2.806,-152.317
	reverse


// Pedestrian number 225

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-235.199,-2.734,-148.686
	point
	-235.321,-2.719,-148.387
	point
	-235.541,-2.713,-147.544
	reverse


// Pedestrian number 226

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-237.421,-2.731,-150.636
	point
	-237.956,-2.717,-150.020
	point
	-239.148,-2.700,-147.260
	reverse


// Pedestrian number 227

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-239.394,-2.695,-146.363
	point
	-238.514,-2.706,-148.017
	point
	-238.122,-2.711,-148.836
	point
	-237.989,-2.714,-149.518
	reverse


// Pedestrian number 228

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-234.193,-2.780,-149.292
	point
	-234.523,-2.762,-149.024
	point
	-235.733,-2.741,-147.978
	point
	-236.225,-2.705,-146.210
	reverse


// Pedestrian number 229

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-233.743,-2.796,-149.489
	point
	-233.018,-2.828,-149.670
	point
	-231.980,-2.846,-149.519
	reverse


// Pedestrian number 230

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-237.762,-2.682,-142.292
	point
	-238.988,-2.665,-139.503
	point
	-240.981,-2.654,-138.347
	point
	-243.640,-2.635,-136.066
	point
	-244.050,-2.630,-135.209
	reverse


// Pedestrian number 231

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-242.575,-2.650,-138.481
	point
	-241.791,-2.662,-139.986
	point
	-240.409,-2.682,-144.017
	reverse


// Pedestrian number 232

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-235.696,-2.711,-147.185
	point
	-236.687,-2.708,-146.130
	point
	-236.887,-2.693,-144.744
	point
	-237.605,-2.685,-142.872
	reverse


// Pedestrian number 233

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-237.685,-2.683,-142.634
	point
	-238.632,-2.674,-141.185
	point
	-240.579,-2.640,-135.349
	reverse


// Pedestrian number 234

29				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-241.063,-2.634,-134.364
	point
	-241.720,-2.626,-133.080
	point
	-242.694,-2.611,-130.614
	point
	-243.371,-2.601,-128.796
	reverse


// Pedestrian number 235

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-246.510,-2.595,-129.308
	point
	-246.510,-2.595,-129.308
	point
	-241.963,-2.618,-131.668
	point
	-241.075,-1.949,-132.197
	reverse


// Pedestrian number 236

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-246.760,-2.592,-128.747
	point
	-247.714,-2.576,-125.882
	point
	-248.654,-2.565,-124.034
	reverse


// Pedestrian number 237

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-250.127,-2.552,-120.536
	point
	-250.502,-2.552,-119.241
	point
	-251.703,-2.552,-118.814
	reverse


// Pedestrian number 238

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-252.670,-2.555,-115.362
	point
	-255.373,-2.552,-114.200
	point
	-256.381,-2.552,-113.722
	reverse


// Pedestrian number 239

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-257.974,-2.552,-116.086
	point
	-258.710,-2.553,-113.521
	point
	-258.878,-2.552,-111.778
	reverse


// Pedestrian number 240

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-259.951,-2.552,-111.080
	point
	-261.131,-2.552,-110.314
	point
	-262.437,-2.552,-108.285
	point
	-263.675,-2.552,-105.560
	reverse


// Pedestrian number 241

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-249.319,-2.552,-113.961
	point
	-248.765,-2.556,-115.149
	point
	-248.531,-2.556,-116.031
	reverse


// Pedestrian number 242

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-251.094,-2.553,-118.841
	point
	-251.966,-2.553,-118.639
	point
	-254.392,-2.553,-114.695
	reverse


// Pedestrian number 243

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-252.938,-2.553,-118.360
	point
	-254.900,-2.553,-117.529
	point
	-255.599,-2.553,-117.270
	point
	-256.842,-2.552,-116.703
	reverse


// Pedestrian number 244

13				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-256.254,-1.949,-118.131
	point
	-254.857,-2.538,-117.934
	point
	-254.685,-2.551,-117.868
	point
	-252.227,-2.555,-115.463
	point
	-249.649,-2.552,-113.015
	point
	-249.474,-2.375,-112.792
	reverse


// Pedestrian number 245

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-248.059,-2.552,-116.864
	point
	-253.718,-2.552,-118.154
	point
	-255.578,-2.553,-116.628
	point
	-263.178,-2.552,-112.017
	reverse


// Pedestrian number 246

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-267.119,-2.552,-105.096
	point
	-268.950,-2.552,-100.688
	point
	-268.972,-2.552,-99.885
	point
	-268.770,-2.552,-98.700
	reverse


// Pedestrian number 247

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-265.747,-2.552,-102.873
	point
	-266.213,-2.552,-102.369
	point
	-267.388,-2.552,-101.191
	point
	-268.140,-2.552,-99.290
	reverse


// Pedestrian number 248

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-268.510,-2.552,-96.082
	point
	-269.419,-2.552,-95.982
	point
	-269.996,-2.552,-96.009
	point
	-270.965,-2.552,-95.727
	reverse


// Pedestrian number 249

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-270.612,-2.552,-93.539
	point
	-272.192,-2.552,-92.011
	point
	-273.328,-2.552,-89.927
	reverse


// Pedestrian number 250

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-271.353,-2.552,-86.780
	point
	-270.768,-2.552,-88.015
	point
	-271.118,-2.552,-89.710
	point
	-271.604,-2.552,-94.356
	reverse


// Pedestrian number 251

14				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-273.074,-2.552,-90.576
	point
	-271.751,-2.552,-91.215
	point
	-270.852,-2.552,-92.071
	point
	-270.782,-2.552,-92.561
	point
	-270.966,-2.552,-93.711
	point
	-270.543,-2.552,-94.764
	reverse


// Pedestrian number 252

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-269.747,-2.552,-95.901
	point
	-269.889,-2.552,-96.406
	point
	-269.582,-2.552,-97.218
	point
	-269.587,-2.552,-99.100
	reverse


// Pedestrian number 253

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-270.059,-2.552,-97.862
	point
	-270.202,-2.552,-96.389
	point
	-269.989,-2.552,-96.204
	point
	-269.321,-2.552,-95.592
	point
	-268.932,-2.552,-95.083
	reverse


// Pedestrian number 254

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-270.161,-2.552,-95.634
	point
	-270.684,-2.552,-95.088
	point
	-271.006,-2.552,-93.934
	point
	-270.847,-2.552,-93.521
	reverse


// Pedestrian number 255

8				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-269.579,-2.552,-93.592
	point
	-270.703,-2.552,-92.680
	point
	-270.711,-2.552,-91.995
	point
	-271.785,-2.552,-89.840
	point
	-274.849,-2.552,-86.565
	reverse


// Pedestrian number 256

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-276.199,-2.552,-83.962
	point
	-275.976,-2.552,-81.561
	point
	-276.119,-2.552,-78.714
	reverse


// Pedestrian number 257

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-277.056,-2.552,-77.404
	point
	-279.163,-2.552,-76.725
	point
	-282.674,-2.552,-75.077
	reverse


// Pedestrian number 258

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-282.977,-2.552,-74.724
	point
	-283.517,-2.543,-71.793
	point
	-284.632,-2.543,-66.837
	reverse


// Pedestrian number 259

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-285.338,-2.538,-71.991
	point
	-283.194,-2.549,-72.864
	point
	-280.490,-2.558,-73.152
	reverse


// Pedestrian number 260

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-283.911,-2.549,-73.598
	point
	-283.794,-2.544,-72.309
	point
	-283.355,-2.540,-70.791
	point
	-283.430,-2.549,-66.934
	reverse


// Pedestrian number 261

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-283.092,-2.539,-70.381
	point
	-282.657,-2.547,-71.956
	point
	-281.994,-2.552,-75.766
	reverse


// Pedestrian number 262

13				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-290.901,-2.611,-66.648
	point
	-288.910,-2.545,-67.798
	point
	-285.894,-2.539,-70.891
	point
	-285.276,-2.538,-71.726
	point
	-285.246,-2.538,-72.306
	point
	-284.425,-2.536,-73.187
	reverse


// Pedestrian number 263

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-301.475,-3.692,-66.697
	point
	-302.839,-3.869,-66.676
	point
	-304.337,-3.982,-66.926
	point
	-304.980,-4.043,-66.621
	point
	-305.100,-4.048,-66.229
	reverse


// Pedestrian number 264

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-305.706,-4.048,-65.861
	point
	-307.220,-4.048,-65.232
	point
	-308.040,-4.048,-64.304
	point
	-308.729,-4.048,-62.258
	reverse


// Pedestrian number 265

12				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-303.969,-3.932,-69.400
	point
	-305.848,-4.041,-69.120
	point
	-306.448,-4.048,-68.937
	point
	-308.740,-4.048,-67.573
	point
	-309.267,-4.048,-67.093
	reverse


// Pedestrian number 266

17				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-307.891,-4.048,-64.913
	point
	-308.340,-4.048,-64.183
	point
	-309.051,-4.048,-61.428
	point
	-309.025,-4.048,-59.326
	reverse


// Pedestrian number 267

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-308.805,-4.048,-58.997
	point
	-308.080,-4.048,-57.100
	point
	-307.767,-4.048,-56.761
	point
	-307.414,-4.048,-56.369
	reverse


// Pedestrian number 268

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-309.587,-4.048,-54.168
	point
	-310.881,-4.048,-57.725
	point
	-312.007,-4.048,-60.843
	reverse


// Pedestrian number 269

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-311.804,-4.048,-61.502
	point
	-310.921,-4.048,-64.048
	point
	-310.213,-4.048,-66.074
	reverse


// Pedestrian number 270

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-308.079,-4.048,-68.005
	point
	-308.182,-4.048,-63.287
	point
	-306.977,-3.161,-62.076
	point
	-306.926,-3.032,-61.235
	reverse


// Pedestrian number 271

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-307.824,-3.507,-61.157
	point
	-308.813,-4.048,-59.570
	point
	-308.793,-4.048,-58.301
	reverse


// Pedestrian number 272

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-307.130,-4.048,-55.946
	point
	-306.899,-4.048,-55.779
	point
	-305.834,-4.096,-55.090
	reverse


// Pedestrian number 273

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-304.480,-4.189,-54.490
	point
	-301.394,-4.602,-53.573
	point
	-298.731,-5.309,-52.973
	reverse


// Pedestrian number 274

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-301.548,-4.739,-50.540
	point
	-298.747,-5.509,-49.881
	point
	-294.961,-6.758,-49.008
	reverse


// Pedestrian number 275

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-294.532,-6.654,-51.923
	point
	-291.191,-7.824,-50.756
	point
	-290.127,-7.884,-50.524
	reverse


// Pedestrian number 276

5				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-289.188,-7.940,-50.205
	point
	-287.985,-8.005,-49.575
	point
	-286.891,-8.005,-45.905
	point
	-287.160,-8.005,-42.215
	point
	-287.398,-8.005,-40.596
	reverse


// Pedestrian number 277

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-284.490,-8.005,-43.511
	point
	-284.121,-8.005,-42.692
	point
	-283.543,-7.696,-41.533
	point
	-282.199,-6.852,-41.083
	reverse


// Pedestrian number 278

1				// Ref num
9				// Number of instructions
7				// Initial instruction

	point
	-284.061,-8.005,-41.127
	point
	-284.608,-8.005,-40.453
	point
	-284.884,-8.005,-39.560
	point
	-284.993,-8.005,-37.977
	point
	-287.371,-8.005,-34.764
	point
	-287.551,-7.986,-34.585
	point
	-287.611,-7.921,-34.413
	point
	-288.716,-7.151,-32.136
	reverse


// Pedestrian number 279

29				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-289.499,-8.005,-37.279
	point
	-288.412,-8.004,-38.154
	point
	-287.520,-8.005,-38.325
	point
	-284.597,-8.005,-39.560
	reverse


// Pedestrian number 280

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-287.740,-8.005,-39.147
	point
	-284.316,-8.005,-42.046
	point
	-284.425,-8.005,-44.507
	reverse


// Pedestrian number 281

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-284.152,-7.877,-44.685
	point
	-284.000,-7.508,-45.728
	point
	-283.980,-7.130,-46.951
	point
	-283.854,-6.798,-47.763
	reverse


// Pedestrian number 282

5				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-285.223,-8.005,-46.513
	point
	-286.407,-8.005,-43.838
	point
	-286.426,-8.005,-42.530
	point
	-287.079,-8.005,-41.616
	point
	-288.226,-8.005,-38.548
	reverse


// Pedestrian number 283

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-286.337,-8.005,-35.899
	point
	-290.809,-8.008,-35.344
	point
	-293.451,-8.166,-35.358
	point
	-296.326,-8.525,-35.300
	reverse


// Pedestrian number 284

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-294.880,-8.344,-35.505
	point
	-296.654,-8.568,-35.057
	point
	-298.035,-9.013,-34.785
	point
	-299.920,-9.442,-35.244
	reverse


// Pedestrian number 285

29				// Ref num
9				// Number of instructions
4				// Initial instruction

	point
	-298.103,-9.166,-32.271
	point
	-298.430,-9.285,-32.439
	point
	-298.882,-9.455,-32.377
	point
	-299.777,-9.776,-32.361
	point
	-300.623,-9.943,-32.472
	point
	-301.872,-10.077,-33.420
	point
	-303.143,-10.477,-33.677
	point
	-304.486,-10.909,-34.832
	reverse


// Pedestrian number 286

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-307.012,-11.793,-31.538
	point
	-309.669,-11.971,-32.758
	point
	-311.882,-11.971,-33.109
	point
	-313.365,-11.971,-32.132
	reverse


// Pedestrian number 287

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-312.356,-11.971,-32.852
	point
	-313.862,-11.971,-31.535
	point
	-315.467,-11.971,-29.014
	reverse


// Pedestrian number 288

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-312.483,-11.971,-28.242
	point
	-313.842,-11.971,-28.279
	point
	-315.790,-11.970,-27.237
	point
	-316.223,-11.971,-25.335
	reverse


// Pedestrian number 289

29				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-310.193,-11.971,-30.589
	point
	-311.153,-11.971,-30.196
	point
	-312.376,-11.970,-28.775
	point
	-313.233,-11.971,-26.534
	point
	-313.226,-11.971,-25.457
	reverse


// Pedestrian number 290

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-315.747,-11.971,-28.199
	point
	-316.031,-11.971,-26.501
	point
	-316.089,-11.970,-24.197
	point
	-314.094,-11.971,-19.618
	reverse


// Pedestrian number 291

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-311.120,-11.971,-20.670
	point
	-315.798,-11.970,-23.028
	point
	-316.008,-11.970,-23.627
	reverse


// Pedestrian number 292

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-315.036,-11.971,-21.178
	point
	-313.307,-11.971,-25.137
	point
	-312.906,-11.971,-28.068
	point
	-312.947,-11.971,-32.545
	reverse


// Pedestrian number 293

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-311.320,-11.971,-33.469
	point
	-309.793,-11.956,-33.640
	point
	-308.575,-11.841,-34.222
	point
	-307.413,-11.808,-34.660
	reverse


// Pedestrian number 294

12				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-310.494,-11.971,-33.931
	point
	-312.101,-11.970,-28.817
	point
	-313.131,-11.971,-26.533
	point
	-313.080,-11.971,-24.407
	point
	-312.879,-11.971,-23.506
	reverse


// Pedestrian number 295

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-309.599,-12.052,-19.766
	point
	-307.176,-12.105,-18.568
	point
	-304.902,-12.106,-18.046
	reverse


// Pedestrian number 296

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-303.618,-12.106,-17.323
	point
	-297.948,-12.106,-11.354
	point
	-295.342,-12.106,-9.547
	reverse


// Pedestrian number 297

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-294.592,-12.106,-12.659
	point
	-293.640,-12.106,-11.881
	point
	-290.160,-12.119,-9.516
	reverse


// Pedestrian number 298

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-293.474,-12.106,-8.167
	point
	-292.018,-12.119,-7.229
	point
	-291.375,-12.134,-6.629
	point
	-290.872,-12.106,-6.118
	reverse


// Pedestrian number 299

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-287.163,-12.203,-7.032
	point
	-286.617,-11.939,-7.076
	point
	-285.686,-11.252,-7.410
	reverse


// Pedestrian number 300

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-285.871,-12.313,-5.671
	point
	-283.815,-12.540,-3.074
	point
	-283.024,-12.625,-2.703
	point
	-282.159,-12.592,-2.212
	reverse


// Pedestrian number 301

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-275.947,-15.455,15.963
	point
	-274.709,-15.615,18.590
	point
	-268.921,-15.627,21.687
	reverse


// Pedestrian number 302

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-269.260,-15.627,21.154
	point
	-269.260,-15.627,21.154
	point
	-274.742,-15.616,19.025
	point
	-274.987,-15.613,18.556
	reverse


// Pedestrian number 303

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-275.048,-15.617,19.181
	point
	-275.296,-15.626,21.891
	point
	-274.156,-15.627,26.848
	point
	-275.075,-15.627,28.241
	reverse


// Pedestrian number 304

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-276.114,-15.627,28.865
	point
	-276.806,-15.627,28.757
	point
	-276.806,-15.627,28.757
	point
	-278.927,-15.627,27.563
	point
	-279.874,-15.627,27.672
	reverse


// Pedestrian number 305

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-275.915,-15.627,28.331
	point
	-274.419,-15.627,26.937
	point
	-273.867,-15.627,26.357
	reverse


// Pedestrian number 306

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-275.798,-15.627,23.631
	point
	-275.376,-15.627,22.759
	point
	-269.842,-15.625,20.327
	point
	-269.526,-15.626,20.538
	reverse


// Pedestrian number 307

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-269.464,-15.627,20.822
	point
	-271.195,-15.627,21.548
	point
	-273.283,-15.622,20.901
	point
	-275.121,-15.621,20.428
	reverse


// Pedestrian number 308

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-271.521,-15.627,23.166
	point
	-270.772,-15.627,23.565
	point
	-267.721,-15.627,22.818
	reverse


// Pedestrian number 309

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-264.867,-15.627,23.968
	point
	-266.649,-15.627,23.637
	point
	-269.462,-15.627,22.086
	point
	-275.319,-15.623,21.089
	reverse


// Pedestrian number 310

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-270.668,-15.621,19.419
	point
	-269.911,-15.627,20.721
	point
	-270.254,-15.629,22.299
	point
	-270.389,-15.627,23.600
	point
	-269.725,-15.627,24.812
	reverse


// Pedestrian number 311

14				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-272.612,-15.627,23.147
	point
	-273.271,-15.627,24.415
	point
	-273.594,-15.627,24.889
	point
	-273.671,-15.627,25.698
	point
	-275.341,-15.627,26.548
	point
	-278.109,-15.627,26.682
	reverse


// Pedestrian number 312

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-280.589,-15.627,33.937
	point
	-280.646,-15.627,35.766
	point
	-279.847,-15.627,37.526
	reverse


// Pedestrian number 313

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-282.105,-15.627,40.554
	point
	-281.144,-15.627,41.464
	point
	-280.896,-15.627,45.967
	reverse


// Pedestrian number 314

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-275.261,-16.364,57.993
	point
	-275.306,-16.591,59.619
	point
	-274.518,-16.875,61.463
	reverse


// Pedestrian number 315

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-274.434,-16.902,61.736
	point
	-275.504,-17.083,63.476
	point
	-276.184,-17.419,66.389
	point
	-275.677,-17.638,68.356
	reverse


// Pedestrian number 316

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-276.525,-17.276,65.334
	point
	-276.656,-17.120,64.043
	point
	-277.100,-16.921,62.514
	reverse


// Pedestrian number 317

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-274.600,-16.823,61.127
	point
	-277.527,-16.613,60.288
	point
	-277.928,-16.431,59.083
	reverse


// Pedestrian number 318

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-277.329,-16.783,61.450
	point
	-274.153,-17.132,63.567
	point
	-273.629,-17.375,65.448
	reverse


// Pedestrian number 319

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-272.091,-18.286,72.098
	point
	-273.900,-18.648,76.202
	point
	-273.648,-18.772,77.788
	reverse


// Pedestrian number 320

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-273.480,-18.815,78.534
	point
	-272.702,-18.907,81.642
	point
	-272.380,-18.909,83.736
	reverse


// Pedestrian number 321

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-272.125,-18.910,84.419
	point
	-268.699,-18.913,87.433
	point
	-268.551,-18.914,88.454
	reverse


// Pedestrian number 322

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-267.860,-18.915,90.476
	point
	-267.589,-18.915,92.464
	point
	-267.190,-18.917,93.251
	reverse


// Pedestrian number 323

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-267.361,-18.915,93.750
	point
	-267.103,-18.915,94.906
	point
	-266.904,-18.915,96.369
	reverse


// Pedestrian number 324

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-266.662,-18.915,97.291
	point
	-265.214,-18.915,103.269
	point
	-263.493,-18.915,105.492
	reverse


// Pedestrian number 325

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-264.258,-18.915,103.497
	point
	-262.888,-18.915,103.594
	point
	-259.906,-18.916,102.546
	point
	-258.473,-18.916,102.074
	reverse


// Pedestrian number 326

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-260.209,-18.915,104.902
	point
	-261.442,-18.915,105.097
	point
	-262.568,-18.915,105.461
	point
	-264.052,-18.915,105.634
	reverse


// Pedestrian number 327

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-264.786,-18.914,105.968
	point
	-266.973,-18.915,105.454
	point
	-268.860,-18.916,104.565
	reverse


// Pedestrian number 328

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-265.318,-18.915,102.577
	point
	-267.780,-18.916,104.111
	point
	-271.038,-18.916,107.321
	reverse


// Pedestrian number 329

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-271.659,-18.916,107.585
	point
	-272.700,-18.916,107.682
	point
	-275.621,-18.916,108.434
	reverse


// Pedestrian number 330

12				// Ref num
7				// Number of instructions
5				// Initial instruction

	point
	-277.279,-18.916,106.409
	point
	-278.052,-18.916,106.785
	point
	-279.855,-18.916,106.897
	point
	-280.732,-18.916,107.190
	point
	-281.522,-18.916,107.353
	point
	-287.395,-18.916,108.702
	reverse


// Pedestrian number 331

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-287.781,-18.915,109.007
	point
	-287.005,-18.915,109.530
	point
	-284.483,-18.915,110.371
	reverse


// Pedestrian number 332

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-285.320,-18.915,110.565
	point
	-283.753,-18.914,110.043
	point
	-282.909,-18.914,108.214
	point
	-282.223,-18.916,107.447
	reverse


// Pedestrian number 333

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-278.529,-18.914,108.997
	point
	-276.784,-18.916,108.745
	point
	-272.298,-18.916,105.406
	reverse


// Pedestrian number 334

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-271.767,-18.916,105.116
	point
	-270.238,-18.916,105.152
	point
	-268.600,-18.916,104.356
	reverse


// Pedestrian number 335

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-257.403,-18.916,104.343
	point
	-256.166,-18.915,103.924
	point
	-253.647,-18.916,101.001
	reverse


// Pedestrian number 336

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-251.203,-18.916,100.337
	point
	-248.252,-18.916,101.620
	point
	-243.906,-18.916,101.111
	reverse


// Pedestrian number 337

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-241.962,-18.915,100.665
	point
	-239.599,-18.916,97.883
	point
	-236.994,-18.916,97.068
	point
	-236.052,-18.916,96.823
	reverse


// Pedestrian number 338

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-230.100,-18.916,95.496
	point
	-227.497,-18.916,96.367
	point
	-224.827,-18.916,96.739
	reverse


// Pedestrian number 339

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-224.247,-18.916,96.663
	point
	-223.229,-18.916,95.255
	point
	-222.475,-18.916,93.876
	reverse


// Pedestrian number 340

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-222.129,-18.916,96.112
	point
	-225.941,-18.916,95.009
	point
	-227.570,-18.916,94.916
	reverse


// Pedestrian number 341

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-230.675,-18.916,95.681
	point
	-232.337,-18.916,98.317
	point
	-234.208,-18.916,98.923
	reverse


// Pedestrian number 342

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-236.473,-18.916,99.195
	point
	-237.403,-18.916,99.547
	point
	-239.771,-18.916,99.977
	reverse


// Pedestrian number 343

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-244.636,-18.916,101.256
	point
	-243.045,-18.915,100.927
	point
	-240.603,-18.916,100.428
	reverse


// Pedestrian number 344

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-241.676,-18.916,97.872
	point
	-242.133,-18.915,99.371
	point
	-243.668,-18.916,101.059
	reverse


// Pedestrian number 345

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-258.016,-18.916,101.915
	point
	-256.635,-18.915,101.778
	point
	-251.856,-18.916,102.896
	reverse


// Pedestrian number 346

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-242.661,-18.915,94.750
	point
	-243.590,-18.915,93.460
	point
	-245.618,-18.915,91.881
	point
	-245.822,-18.915,91.091
	point
	-246.407,-18.915,89.219
	reverse


// Pedestrian number 347

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-248.346,-18.916,88.619
	point
	-248.651,-18.916,88.589
	point
	-250.594,-18.916,89.034
	point
	-253.616,-18.916,89.690
	reverse


// Pedestrian number 348

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-256.635,-18.916,90.560
	point
	-253.937,-18.916,89.438
	point
	-252.016,-18.916,89.394
	point
	-250.196,-18.916,87.138
	reverse


// Pedestrian number 349

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-248.563,-18.916,86.478
	point
	-249.387,-18.916,87.020
	point
	-253.946,-18.916,87.627
	reverse


// Pedestrian number 350

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-255.604,-18.916,87.920
	point
	-257.768,-18.915,90.792
	point
	-258.445,-18.916,90.861
	reverse


// Pedestrian number 351

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-240.526,-18.915,84.616
	point
	-239.882,-18.915,84.350
	point
	-235.910,-18.915,83.580
	reverse


// Pedestrian number 352

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-235.968,-18.916,85.765
	point
	-239.119,-18.916,86.048
	point
	-240.148,-18.916,86.797
	point
	-241.421,-18.916,86.919
	point
	-242.623,-18.916,87.273
	reverse


// Pedestrian number 353

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-243.849,-18.916,87.634
	point
	-244.802,-18.915,85.567
	point
	-245.180,-18.914,83.335
	point
	-245.664,-18.913,82.051
	point
	-245.604,-18.912,81.275
	reverse


// Pedestrian number 354

17				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-249.726,-18.892,75.676
	point
	-247.778,-18.859,74.234
	point
	-247.643,-18.786,72.308
	point
	-247.717,-18.737,71.682
	reverse


// Pedestrian number 355

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-246.677,-18.906,75.374
	point
	-248.844,-18.909,77.993
	point
	-248.383,-18.911,80.406
	reverse


// Pedestrian number 356

12				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-249.638,-18.916,89.036
	point
	-246.949,-18.915,88.290
	point
	-244.024,-18.916,87.838
	point
	-242.617,-18.915,85.084
	point
	-241.820,-18.915,84.752
	reverse


// Pedestrian number 357

29				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-230.822,-18.916,84.707
	point
	-229.908,-18.916,84.146
	point
	-228.819,-18.916,84.256
	point
	-226.632,-18.916,83.831
	point
	-224.363,-18.916,81.696
	reverse


// Pedestrian number 358

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-223.842,-18.916,82.470
	point
	-225.192,-18.916,81.939
	point
	-227.269,-18.916,81.629
	reverse


// Pedestrian number 359

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-225.378,-18.916,81.111
	point
	-227.952,-18.917,81.760
	point
	-232.958,-18.916,85.192
	reverse


// Pedestrian number 360

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-233.629,-18.916,85.244
	point
	-235.137,-18.915,85.428
	point
	-237.883,-18.916,84.002
	reverse


// Pedestrian number 361

1				// Ref num
7				// Number of instructions
5				// Initial instruction

	point
	-234.603,-18.916,83.075
	point
	-237.291,-18.916,84.277
	point
	-239.141,-18.916,84.414
	point
	-240.060,-18.916,84.651
	point
	-241.329,-18.914,84.995
	point
	-243.182,-18.916,87.368
	reverse


// Pedestrian number 362

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-243.846,-18.915,89.669
	point
	-243.772,-18.915,91.633
	point
	-242.658,-18.915,94.584
	reverse


// Pedestrian number 363

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-225.214,-18.916,96.958
	point
	-224.474,-18.916,96.468
	point
	-224.210,-18.916,95.897
	point
	-223.458,-18.916,94.270
	reverse


// Pedestrian number 364

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-289.800,-18.915,98.099
	point
	-287.528,-18.915,97.391
	point
	-286.992,-18.915,95.275
	reverse


// Pedestrian number 365

1				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-286.584,-18.916,95.062
	point
	-285.122,-18.916,94.775
	point
	-284.024,-18.916,94.553
	point
	-282.993,-18.916,94.208
	point
	-281.769,-18.916,94.357
	point
	-279.257,-18.916,93.459
	reverse


// Pedestrian number 366

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-278.403,-18.916,93.124
	point
	-276.421,-18.916,92.787
	point
	-273.351,-18.916,92.168
	reverse


// Pedestrian number 367

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-276.536,-18.916,95.028
	point
	-277.883,-18.916,95.336
	point
	-279.189,-18.916,95.195
	point
	-281.667,-18.916,96.371
	reverse


// Pedestrian number 368

17				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-280.027,-18.916,95.991
	point
	-278.853,-18.916,95.361
	point
	-277.985,-18.916,93.932
	point
	-277.008,-18.916,92.852
	reverse


// Pedestrian number 369

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-275.923,-18.916,92.597
	point
	-274.557,-18.916,92.760
	point
	-272.792,-18.916,92.171
	point
	-267.385,-18.915,90.680
	reverse


// Pedestrian number 370

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-249.956,-17.586,62.402
	point
	-253.447,-17.126,59.029
	point
	-253.663,-16.985,57.797
	reverse


// Pedestrian number 371

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-252.848,-17.401,61.382
	point
	-251.877,-16.860,56.561
	point
	-251.740,-16.522,54.063
	point
	-252.232,-16.232,51.727
	reverse


// Pedestrian number 372

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-255.093,-16.136,51.243
	point
	-255.367,-16.081,50.658
	point
	-253.478,-15.866,48.171
	reverse


// Pedestrian number 373

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-259.604,-15.627,19.171
	point
	-263.137,-15.657,16.034
	point
	-263.787,-15.657,14.920
	reverse


// Pedestrian number 374

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-266.962,-15.680,-2.238
	point
	-267.167,-15.791,-4.341
	point
	-267.122,-15.904,-6.260
	reverse


// Pedestrian number 375

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-264.090,-15.692,-2.653
	point
	-264.235,-15.791,-4.428
	point
	-264.105,-15.851,-5.513
	point
	-264.434,-16.113,-10.220
	point
	-264.228,-16.144,-10.802
	reverse


// Pedestrian number 376

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-264.208,-16.184,-11.530
	point
	-264.744,-16.682,-17.259
	point
	-265.236,-16.733,-17.799
	point
	-265.035,-16.840,-18.964
	reverse


// Pedestrian number 377

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-119.834,-13.901,-123.061
	point
	-117.564,-13.901,-123.633
	point
	-115.680,-13.901,-123.977
	reverse


// Pedestrian number 378

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-109.031,-13.901,-125.677
	point
	-105.715,-13.901,-126.182
	point
	-102.975,-13.901,-127.024
	reverse


// Pedestrian number 379

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-101.611,-13.901,-127.207
	point
	-99.451,-13.901,-127.706
	point
	-96.372,-13.901,-128.519
	point
	-93.558,-13.901,-129.240
	reverse


// Pedestrian number 380

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-91.666,-13.901,-126.863
	point
	-90.408,-13.901,-126.956
	point
	-87.817,-13.901,-127.590
	point
	-86.489,-13.901,-128.258
	point
	-85.750,-13.901,-130.193
	reverse


// Pedestrian number 381

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-84.949,-13.901,-131.149
	point
	-80.765,-13.901,-129.335
	point
	-79.234,-13.901,-129.693
	reverse


// Pedestrian number 382

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-77.973,-13.901,-129.919
	point
	-76.168,-13.900,-133.065
	point
	-73.672,-13.901,-133.667
	reverse


// Pedestrian number 383

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-83.065,-13.901,-131.665
	point
	-84.022,-13.901,-131.468
	point
	-87.263,-13.901,-130.582
	point
	-88.684,-13.901,-130.165
	point
	-89.755,-13.901,-129.999
	reverse


// Pedestrian number 384

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-91.735,-13.901,-126.627
	point
	-93.750,-13.901,-126.619
	point
	-97.768,-13.901,-125.274
	reverse


// Pedestrian number 385

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-98.194,-13.901,-125.123
	point
	-101.434,-13.901,-124.704
	point
	-103.321,-13.901,-124.105
	point
	-104.968,-13.901,-123.493
	reverse


// Pedestrian number 386

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-111.649,-13.901,-124.905
	point
	-113.716,-13.901,-122.206
	point
	-115.137,-13.901,-121.271
	point
	-116.340,-13.901,-120.804
	point
	-118.246,-13.901,-120.392
	reverse


// Pedestrian number 387

3				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-121.292,-13.901,-119.788
	point
	-123.196,-13.901,-119.728
	point
	-124.535,-13.901,-118.956
	point
	-125.394,-13.901,-118.697
	point
	-126.965,-13.901,-118.549
	point
	-128.145,-13.901,-118.237
	reverse


// Pedestrian number 388

1				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-132.275,-13.901,-119.952
	point
	-135.456,-13.817,-119.294
	point
	-137.788,-13.901,-118.554
	point
	-140.212,-13.901,-118.253
	point
	-140.870,-13.901,-117.947
	point
	-141.976,-13.977,-117.808
	reverse


// Pedestrian number 389

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-145.000,-14.111,-114.419
	point
	-147.714,-14.343,-113.757
	point
	-148.978,-14.441,-113.374
	point
	-150.077,-14.520,-113.405
	point
	-151.259,-14.618,-112.759
	reverse


// Pedestrian number 390

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-154.072,-14.744,-114.431
	point
	-156.939,-14.906,-113.855
	point
	-158.349,-14.962,-112.972
	point
	-160.074,-15.001,-112.697
	reverse


// Pedestrian number 391

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-163.051,-15.344,-108.087
	point
	-164.301,-15.485,-107.578
	point
	-166.077,-15.909,-106.568
	point
	-166.565,-16.010,-106.127
	point
	-167.904,-16.244,-105.358
	reverse


// Pedestrian number 392

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-169.241,-16.457,-104.871
	point
	-170.250,-16.652,-104.404
	point
	-172.089,-17.158,-102.408
	point
	-173.911,-17.623,-100.836
	reverse


// Pedestrian number 393

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-183.381,-17.667,-94.703
	point
	-185.582,-17.667,-93.495
	point
	-187.395,-17.667,-92.805
	point
	-188.499,-17.667,-92.221
	reverse


// Pedestrian number 394

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-189.212,-17.667,-92.062
	point
	-193.357,-17.667,-93.250
	point
	-194.419,-17.667,-93.268
	point
	-195.772,-17.667,-92.864
	point
	-196.934,-17.667,-92.532
	reverse


// Pedestrian number 395

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-200.913,-17.667,-89.040
	point
	-202.033,-17.667,-88.797
	point
	-204.014,-17.667,-88.626
	point
	-205.983,-17.667,-88.356
	reverse


// Pedestrian number 396

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-205.578,-17.667,-91.182
	point
	-207.331,-17.667,-90.489
	point
	-208.538,-17.667,-90.705
	point
	-209.648,-17.667,-91.079
	point
	-212.465,-17.667,-91.333
	reverse


// Pedestrian number 397

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-222.421,-17.667,-90.108
	point
	-225.237,-17.667,-90.657
	point
	-228.646,-17.667,-94.731
	reverse


// Pedestrian number 398

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-222.851,-17.667,-92.715
	point
	-225.380,-17.667,-93.718
	point
	-230.772,-17.667,-92.287
	reverse


// Pedestrian number 399

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-231.315,-17.667,-92.144
	point
	-236.308,-17.667,-91.844
	point
	-237.168,-17.667,-90.632
	point
	-238.428,-17.667,-88.917
	reverse


// Pedestrian number 400

14				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-234.244,-17.667,-90.010
	point
	-234.876,-17.667,-89.574
	point
	-235.287,-17.667,-88.471
	point
	-236.050,-17.667,-87.275
	point
	-237.103,-17.667,-85.875
	point
	-237.296,-17.667,-85.318
	reverse


// Pedestrian number 401

8				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-239.589,-17.667,-87.027
	point
	-238.759,-17.667,-88.124
	point
	-233.632,-17.667,-90.893
	point
	-233.018,-17.667,-91.433
	point
	-231.069,-17.667,-95.099
	reverse


// Pedestrian number 402

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-229.490,-17.667,-94.925
	point
	-232.882,-17.667,-94.231
	point
	-234.970,-17.667,-93.341
	reverse


// Pedestrian number 403

29				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-235.881,-17.667,-92.742
	point
	-237.468,-17.667,-89.190
	point
	-237.576,-17.667,-86.398
	point
	-237.810,-17.667,-84.738
	point
	-239.074,-17.667,-83.249
	reverse


// Pedestrian number 404

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-239.940,-17.667,-81.940
	point
	-241.389,-17.667,-80.509
	point
	-242.760,-17.667,-79.235
	point
	-243.512,-17.667,-78.624
	reverse


// Pedestrian number 405

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-245.986,-17.667,-80.303
	point
	-244.407,-17.667,-81.344
	point
	-243.769,-17.667,-82.153
	point
	-242.335,-17.667,-83.856
	reverse


// Pedestrian number 406

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-241.138,-17.667,-85.195
	point
	-241.675,-17.667,-83.809
	point
	-242.744,-17.667,-82.883
	point
	-243.966,-17.667,-78.255
	reverse


// Pedestrian number 407

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-245.521,-17.667,-77.607
	point
	-247.017,-17.667,-77.002
	point
	-249.465,-17.667,-76.193
	reverse


// Pedestrian number 408

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-251.893,-17.667,-74.479
	point
	-256.607,-17.667,-74.979
	point
	-259.508,-17.667,-74.238
	reverse


// Pedestrian number 409

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-264.458,-17.667,-70.671
	point
	-265.318,-17.667,-65.596
	point
	-266.224,-17.667,-63.769
	point
	-266.944,-17.667,-63.032
	point
	-267.397,-17.667,-61.949
	reverse


// Pedestrian number 410

14				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-268.182,-17.667,-60.830
	point
	-267.928,-17.667,-62.571
	point
	-266.643,-17.667,-64.806
	point
	-266.713,-17.667,-67.852
	point
	-265.824,-17.667,-68.878
	reverse


// Pedestrian number 411

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-264.989,-17.667,-69.779
	point
	-262.826,-17.667,-72.031
	point
	-262.093,-17.667,-72.685
	point
	-260.609,-17.667,-73.550
	point
	-257.839,-17.667,-74.706
	reverse


// Pedestrian number 412

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-255.378,-17.667,-75.598
	point
	-252.351,-17.667,-77.418
	point
	-250.216,-17.667,-79.156
	reverse


// Pedestrian number 413

29				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-252.969,-17.667,-73.850
	point
	-256.132,-17.667,-73.995
	point
	-258.440,-17.667,-73.304
	point
	-261.503,-17.667,-69.874
	point
	-264.039,-17.667,-66.725
	reverse


// Pedestrian number 414

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-271.027,-17.667,-61.583
	point
	-272.535,-17.667,-58.840
	point
	-274.032,-17.667,-52.526
	reverse


// Pedestrian number 415

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-271.331,-17.667,-49.860
	point
	-271.311,-17.667,-48.130
	point
	-271.297,-17.667,-46.380
	point
	-271.427,-17.667,-44.970
	point
	-271.157,-17.667,-43.681
	reverse


// Pedestrian number 416

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-268.855,-17.667,-30.778
	point
	-268.559,-17.667,-30.243
	point
	-267.896,-17.667,-29.450
	reverse


// Pedestrian number 417

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-271.924,-17.667,-32.767
	point
	-272.570,-17.667,-36.082
	point
	-272.706,-17.667,-37.178
	point
	-273.465,-17.667,-39.753
	reverse


// Pedestrian number 418

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-270.747,-17.667,-40.455
	point
	-272.866,-17.667,-36.484
	point
	-272.339,-17.667,-34.237
	reverse


// Pedestrian number 419

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-271.845,-17.667,-31.923
	point
	-269.676,-17.667,-34.570
	point
	-270.281,-17.667,-37.579
	reverse


// Pedestrian number 420

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-270.493,-17.667,-38.015
	point
	-271.410,-17.667,-36.914
	point
	-272.664,-17.667,-35.041
	point
	-272.133,-17.667,-33.504
	reverse


// Pedestrian number 421

8				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-271.174,-17.667,-31.072
	point
	-271.721,-17.667,-33.570
	point
	-272.730,-17.667,-35.622
	point
	-273.163,-17.667,-37.531
	point
	-271.921,-17.667,-39.174
	point
	-271.089,-17.667,-42.821
	reverse


// Pedestrian number 422

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-270.053,-17.667,-26.369
	point
	-269.945,-17.667,-27.000
	point
	-270.647,-17.667,-28.010
	reverse


// Pedestrian number 423

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-269.690,-17.667,-25.496
	point
	-269.842,-17.667,-25.983
	point
	-270.298,-17.667,-26.927
	point
	-270.337,-17.667,-28.194
	point
	-270.756,-17.667,-28.940
	reverse


// Pedestrian number 424

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-269.406,-17.667,-25.153
	point
	-268.996,-17.666,-24.854
	point
	-268.898,-17.355,-22.439
	reverse


// Pedestrian number 425

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-266.252,-17.443,-23.823
	point
	-265.947,-17.238,-22.254
	point
	-267.972,-16.891,-18.890
	reverse


// Pedestrian number 426

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-267.071,-17.667,-26.394
	point
	-266.334,-17.478,-24.081
	point
	-266.049,-17.349,-23.131
	reverse


// Pedestrian number 427

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-267.927,-17.000,-19.824
	point
	-268.300,-17.152,-21.026
	point
	-266.443,-17.541,-24.563
	reverse


// Pedestrian number 428

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-266.648,-17.641,-25.315
	point
	-266.742,-17.514,-24.281
	point
	-266.126,-17.317,-22.841
	point
	-265.068,-16.746,-17.961
	reverse


// Pedestrian number 429

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-269.300,-17.624,-24.315
	point
	-268.899,-17.480,-23.371
	point
	-268.473,-17.260,-21.869
	point
	-265.572,-17.078,-21.051
	reverse


// Pedestrian number 430

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-287.459,-15.627,39.118
	reverse


// Pedestrian number 431

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-287.210,-15.627,40.372
	reverse


// Pedestrian number 432

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-286.898,-15.627,41.898
	reverse


// Pedestrian number 433

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-280.139,-15.627,35.601
	reverse


// Pedestrian number 434

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-239.364,-18.916,86.650
	reverse


// Pedestrian number 435

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-271.043,-18.916,91.502
	reverse


// Pedestrian number 436

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-271.787,-18.916,91.665
	reverse


// Pedestrian number 437

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-277.022,-18.916,95.333
	reverse


// Pedestrian number 438

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-278.585,-18.916,95.637
	reverse


// Pedestrian number 439

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-287.680,-18.915,96.539
	reverse


// Pedestrian number 440

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-288.693,-18.915,96.701
	reverse


// Pedestrian number 441

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-286.898,-18.915,109.796
	reverse


// Pedestrian number 442

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-285.751,-18.915,109.419
	reverse


// Pedestrian number 443

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-275.152,-18.916,105.913
	reverse


// Pedestrian number 444

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-267.579,-18.915,103.067
	reverse


// Pedestrian number 445

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-253.508,-18.916,101.013
	reverse


// Pedestrian number 446

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-234.220,-18.916,96.708
	reverse


// Pedestrian number 447

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-233.295,-18.916,96.507
	reverse


// Pedestrian number 448

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-227.150,-18.916,97.137
	reverse


// Pedestrian number 449

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-226.593,-18.916,97.000
	reverse


// Pedestrian number 450

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-222.481,-18.916,94.977
	reverse


// Pedestrian number 451

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-221.543,-18.916,95.059
	reverse


// Pedestrian number 452

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-221.642,-18.916,94.409
	reverse


// Pedestrian number 453

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-226.181,-18.916,82.248
	reverse


// Pedestrian number 454

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-226.707,-18.916,82.354
	reverse


// Pedestrian number 455

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-274.307,-17.667,-46.446
	reverse


// Pedestrian number 456

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-274.257,-17.667,-44.535
	reverse


// Pedestrian number 457

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-274.284,-17.667,-49.706
	reverse


// Pedestrian number 458

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-259.818,-17.667,-70.806
	reverse


// Pedestrian number 459

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-259.365,-17.667,-71.060
	reverse


// Pedestrian number 460

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-260.450,-17.667,-70.372
	reverse


// Pedestrian number 461

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-134.149,-13.901,-116.744
	reverse


// Pedestrian number 462

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-133.133,-13.901,-116.986
	reverse


// Pedestrian number 463

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-94.608,-13.901,-125.770
	reverse


// Pedestrian number 464

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-93.850,-13.901,-125.954
	reverse


// Pedestrian number 465

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-55.923,-13.561,-133.129
	reverse


// Pedestrian number 466

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.012,-11.865,-136.051
	reverse


// Pedestrian number 467

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-88.779,-12.543,-137.107
	reverse


// Pedestrian number 468

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-99.301,-12.059,-137.304
	reverse


// Pedestrian number 469

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-177.768,-7.933,-122.214
	reverse


// Pedestrian number 470

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-178.348,-7.878,-120.801
	reverse


// Pedestrian number 471

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-208.762,-4.206,-119.494
	reverse


// Pedestrian number 472

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-209.185,-4.137,-120.047
	reverse


// Pedestrian number 473

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-258.207,-2.552,-100.866
	reverse


// Pedestrian number 474

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-260.159,-2.552,-96.271
	reverse


// Pedestrian number 475

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-260.816,-2.552,-94.565
	reverse


// Pedestrian number 476

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-268.781,-2.552,-98.559
	reverse


// Pedestrian number 477

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-269.871,-2.552,-90.295
	reverse


// Pedestrian number 478

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-269.961,-2.552,-90.025
	reverse


// Pedestrian number 479

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-301.068,-3.636,-66.648
	reverse


// Pedestrian number 480

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-306.901,-4.048,-65.192
	reverse


// Pedestrian number 481

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-307.481,-4.048,-64.478
	reverse


// Pedestrian number 482

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-307.952,-4.048,-63.872
	reverse


// Pedestrian number 483

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-287.591,-8.005,-40.262
	reverse


// Pedestrian number 484

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-302.234,-12.106,-16.937
	reverse


// Pedestrian number 485

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-301.804,-12.106,-16.744
	reverse


// Pedestrian number 486

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-271.668,-15.627,24.710
	reverse


// Pedestrian number 487

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-272.063,-15.627,24.805
	reverse


// Pedestrian number 488

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-271.201,-15.627,24.549
	reverse


// Pedestrian number 489

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-272.084,-15.627,23.357
	reverse


// Pedestrian number 490

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-214.152,-8.352,-7.375
	reverse


// Pedestrian number 491

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-213.866,-8.290,-7.552
	reverse


// Pedestrian number 492

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-202.868,-7.280,-4.228
	reverse


// Pedestrian number 493

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-182.746,-5.425,6.452
	reverse


// Pedestrian number 494

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-188.515,-5.380,4.779
	reverse


// Pedestrian number 495

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-179.419,-5.431,2.074
	reverse


// Pedestrian number 496

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-178.465,-5.432,1.182
	reverse


// Pedestrian number 497

125				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-146.391,-7.508,-46.202
	reverse


// Pedestrian number 498

125				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-135.465,-7.487,-49.345
	reverse


// Pedestrian number 499

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-135.327,-18.640,-34.027
	reverse


// Pedestrian number 500

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-135.395,-18.641,-34.552
	reverse


// Pedestrian number 501

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.241,-13.039,-45.299
	reverse


// Pedestrian number 502

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-82.370,-13.120,-45.117
	reverse


// Pedestrian number 503

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-23.442,-15.561,-51.867
	reverse


// Pedestrian number 504

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-19.152,-14.991,-77.396
	reverse


// Pedestrian number 505

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-19.127,-14.982,-78.241
	reverse


// Pedestrian number 506

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-14.327,-15.489,-128.504
	reverse


// Pedestrian number 507

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-16.435,-15.631,-132.987
	reverse


// Pedestrian number 508

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-43.317,-14.684,-133.268
	reverse


// Pedestrian number 509

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-42.642,-14.745,-133.291
	reverse


// Pedestrian number 510

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-61.800,-13.901,-133.221
	reverse


// Pedestrian number 511

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-62.341,-13.901,-136.832
	reverse




START OF OPPONENT PATHS

143                             // Number of path nodes
 -250.508,  -15.624,   29.209   // Node #0
 -248.031,  -15.627,   38.838   // Node #1
 -243.893,  -15.508,   41.091   // Node #2
 -229.045,  -11.606,   30.295   // Node #3
 -219.342,   -9.352,   16.413   // Node #4
 -211.405,   -8.951,   -5.008   // Node #5
 -205.429,   -7.881,   -6.354   // Node #6
 -193.708,   -5.328,   -1.252   // Node #7
 -185.485,   -5.428,    4.234   // Node #8
 -180.135,   -5.649,    4.007   // Node #9
 -176.502,   -5.435,    0.724   // Node #10
 -175.172,   -5.578,   -4.666   // Node #11
 -179.573,   -8.050,  -17.537   // Node #12
 -178.480,   -8.840,  -24.813   // Node #13
 -170.047,   -9.078,  -35.110   // Node #14
 -145.562,   -8.802,  -44.806   // Node #15
 -134.637,   -8.880,  -48.147   // Node #16
 -114.706,   -8.874,  -52.829   // Node #17
  -98.251,   -9.426,  -49.700   // Node #18
  -70.570,  -12.833,  -45.715   // Node #19
  -49.297,  -14.595,  -42.864   // Node #20
  -29.777,  -14.596,  -49.524   // Node #21
  -21.244,  -14.596,  -58.412   // Node #22
  -16.074,  -14.536,  -74.221   // Node #23
  -13.154,  -13.419, -116.560   // Node #24
  -13.090,  -14.543, -129.299   // Node #25
  -15.123,  -14.656, -134.091   // Node #26
  -18.705,  -14.657, -136.028   // Node #27
  -54.190,  -13.641, -136.953   // Node #28
 -152.848,  -13.820, -114.594   // Node #29
 -182.531,  -17.667,  -97.063   // Node #30
 -196.978,  -17.667,  -91.815   // Node #31
 -213.702,  -16.453,  -90.431   // Node #32
 -231.135,  -16.453,  -94.236   // Node #33
 -235.669,  -16.453,  -91.053   // Node #34
 -239.736,  -16.453,  -84.356   // Node #35
 -262.737,  -16.453,  -70.095   // Node #36
 -271.548,  -16.453,  -59.852   // Node #37
 -272.065,  -16.453,  -44.221   // Node #38
 -266.345,  -15.303,  -13.850   // Node #39
 -264.770,  -14.680,    3.261   // Node #40
 -254.830,  -15.627,   43.612   // Node #41
 -246.000,  -15.631,   41.796   // Node #42
 -164.508,  -15.443, -109.296   // Node #43
 -261.168,  -14.680,   17.931   // Node #44
  -42.843,  -14.595,  -43.566   // Node #45
  -61.143,  -13.907, -135.604   // Node #46
  -61.029,  -14.008, -137.895   // Node #47
  -63.087,  -13.880, -138.545   // Node #48
 -165.655,   -8.969, -139.964   // Node #49
 -169.548,   -8.663, -138.876   // Node #50
 -173.986,   -8.280, -135.278   // Node #51
 -177.553,   -7.952, -129.515   // Node #52
 -179.660,   -7.749, -122.705   // Node #53
 -182.390,   -7.474, -117.350   // Node #54
 -186.456,   -7.046, -113.764   // Node #55
 -194.200,   -6.154, -111.558   // Node #56
 -201.944,   -5.168, -112.301   // Node #57
 -207.828,   -4.353, -115.465   // Node #58
 -211.222,   -3.839, -120.541   // Node #59
 -214.289,   -3.446, -132.081   // Node #60
 -217.671,   -3.160, -141.537   // Node #61
 -222.794,   -3.040, -146.983   // Node #62
 -231.198,   -2.851, -151.002   // Node #63
 -234.592,   -2.789, -150.888   // Node #64
 -236.819,   -2.714, -148.580   // Node #65
 -248.357,   -2.552, -120.940   // Node #66
 -263.688,   -2.553,  -83.516   // Node #67
 -269.866,   -2.554,  -75.771   // Node #68
 -277.831,   -2.553,  -70.214   // Node #69
 -287.929,   -2.543,  -68.170   // Node #70
 -303.068,   -3.882,  -68.291   // Node #71
 -308.129,   -4.050,  -66.676   // Node #72
 -310.546,   -4.048,  -61.708   // Node #73
 -309.817,   -4.051,  -56.793   // Node #74
 -305.228,   -4.165,  -53.014   // Node #75
 -290.748,   -7.872,  -49.147   // Node #76
 -286.828,   -8.007,  -46.024   // Node #77
 -285.659,   -8.007,  -41.168   // Node #78
 -287.814,   -8.006,  -36.492   // Node #79
 -292.722,   -8.112,  -34.205   // Node #80
 -308.248,  -11.861,  -33.059   // Node #81
 -312.892,  -11.973,  -30.429   // Node #82
 -314.787,  -11.972,  -24.998   // Node #83
 -313.710,  -11.972,  -21.294   // Node #84
 -311.184,  -11.997,  -18.843   // Node #85
 -298.018,  -12.107,  -13.002   // Node #86
 -287.082,  -12.304,   -4.837   // Node #87
 -275.559,  -15.002,   12.043   // Node #88
 -273.364,  -15.620,   19.899   // Node #89
 -275.513,  -15.628,   26.232   // Node #90
 -279.528,  -15.628,   29.152   // Node #91
 -287.257,  -15.630,   30.917   // Node #92
 -289.703,  -15.627,   34.061   // Node #93
 -289.404,  -15.627,   37.637   // Node #94
 -287.760,  -15.627,   47.198   // Node #95
 -286.602,  -15.627,   48.854   // Node #96
 -283.707,  -15.627,   50.241   // Node #97
 -278.500,  -15.622,   50.878   // Node #98
 -259.234,  -15.607,   46.407   // Node #99
 -256.702,  -15.627,   46.017   // Node #100
 -254.571,  -15.627,   45.821   // Node #101
 -253.865,  -15.810,   47.777   // Node #102
 -243.116,  -18.915,   98.813   // Node #103
 -244.045,  -18.915,   99.848   // Node #104
 -263.285,  -18.915,  104.667   // Node #105
 -265.357,  -18.915,  103.936   // Node #106
 -266.277,  -18.915,  102.814   // Node #107
 -249.110,   -2.552, -118.924   // Node #108
 -258.219,   -2.552, -113.832   // Node #109
 -264.577,   -2.553, -106.675   // Node #110
 -272.315,   -2.552,  -88.420   // Node #111
 -281.437,   -2.552,  -74.518   // Node #112
 -251.441,  -15.623,   26.693   // Node #113
 -252.870,  -15.622,   24.867   // Node #114
 -255.388,  -15.622,   23.642   // Node #115
 -257.148,  -15.621,   23.266   // Node #116
 -259.491,  -15.621,   23.901   // Node #117
 -266.616,  -15.620,   24.606   // Node #118
 -121.550,   -9.078,  -51.179   // Node #119
 -123.816,   -9.356,  -45.510   // Node #120
 -125.287,  -10.162,  -38.526   // Node #121
 -131.912,  -13.190,  -32.790   // Node #122
 -140.261,  -13.512,  -30.740   // Node #123
 -145.006,  -12.423,  -30.887   // Node #124
 -152.848,  -10.049,  -33.455   // Node #125
 -155.717,   -8.795,  -36.452   // Node #126
 -157.728,   -9.078,  -41.463   // Node #127
 -136.791,  -14.001,  -31.257   // Node #128
 -143.569,  -18.690,  -47.648   // Node #129
 -142.298,  -18.654,  -39.284   // Node #130
 -147.869,  -18.642,  -36.886   // Node #131
 -151.331,  -18.664,  -39.018   // Node #132
 -140.591,  -18.730,  -50.247   // Node #133
 -138.024,  -18.671,  -49.664   // Node #134
 -136.208,  -18.636,  -45.375   // Node #135
 -134.454,  -18.587,  -41.220   // Node #136
 -127.194,  -18.571,  -41.632   // Node #137
 -126.725,  -18.567,  -41.644   // Node #138
 -213.557,   -9.078,    0.401   // Node #139
 -271.215,  -18.907,   81.140   // Node #140
 -248.192,  -18.907,   75.861   // Node #141
 -284.540,  -12.656,   -1.126   // Node #142

149                                           // Number of path sections
   0,   1,   0, 255,   0, 255,    1.0,    0   // Section #0
   1,   2,   0, 255,   0, 255,    1.0,    0   // Section #1
   2,   3,   0, 255,   0, 255,    1.0,    0   // Section #2
   3,   4,   0, 255,   0, 255,    1.0,    0   // Section #3
   4, 139,   0, 255,   0, 255,    1.0,    0   // Section #4
   5,   6,   0, 255,   0, 255,    1.0,    0   // Section #5
   6,   7,   0, 255,   0, 255,    1.0,    0   // Section #6
   7,   8,   0, 255,   0, 255,    1.0,    0   // Section #7
   8,   9,   0, 255,   0, 255,    1.0,    0   // Section #8
   9,  10,   0, 255,   0, 255,    1.0,    0   // Section #9
  10,  11,   0, 255,   0, 255,    1.0,    0   // Section #10
  11,  12,   0, 170,   0, 255,    1.0,    0   // Section #11
  12,  13,   0, 255,   0, 255,    1.0,    0   // Section #12
  13,  14,   0, 255,   0, 255,    1.0,    0   // Section #13
  14, 127,   0, 255,   0, 255,    1.0,    0   // Section #14
  15,  16,   0, 255,   0, 255,    1.0,    0   // Section #15
  16, 119,   0, 255,   0, 255,    1.0,    0   // Section #16
  17,  18,   0, 255,   0, 255,    1.0,    0   // Section #17
  18,  19,   0, 255,   0, 255,    1.0,    0   // Section #18
  19,  20,   0, 255,   0, 255,    1.0,    0   // Section #19
  20,  45,   0, 255,   0, 255,    1.0,    0   // Section #20
  21,  22,   0, 255,   0, 255,    1.0,    0   // Section #21
  22,  23,   0, 255,   0, 255,    1.0,    0   // Section #22
  23,  24,   0, 255,   0,  40,    1.0,    0   // Section #23
  24,  25,   0, 255,   0, 255,    1.0,    0   // Section #24
  25,  26,   0, 255,   0, 255,    1.0,    0   // Section #25
  26,  27,   0, 255,   0, 255,    1.0,    0   // Section #26
  27,  28,   0, 255,   0, 255,    1.0,    0   // Section #27
  28,  46,   0, 255,   0, 255,    1.0,    0   // Section #28
  43,  29,   0,  70,   0, 255,    1.0,    1   // Section #29
  31,  30,   0, 255,   0, 255,    1.0,    1   // Section #30
  32,  31,   0, 255,   0, 255,    1.0,    1   // Section #31
  33,  32,   0,  35,   0, 255,    1.0,    1   // Section #32
  34,  33,   0, 255,   0,  35,    1.0,    1   // Section #33
  35,  34,   0, 255,   0, 255,    1.0,    1   // Section #34
  36,  35,   0, 255,   0, 255,    0.6,    1   // Section #35
  37,  36,   0, 255,   0, 255,    0.6,    1   // Section #36
  38,  37,   0, 255,   0, 255,    0.6,    1   // Section #37
  39,  38,   0, 255,   0, 255,    0.6,    1   // Section #38
  40,  39,   0, 255,   0, 255,    0.6,    1   // Section #39
  44,  40,   0, 255,   0, 255,    1.1,    1   // Section #40
  41,  42,   0, 255,   0, 255,    1.1,    0   // Section #41
  30,  43,   0, 255,   0, 255,    1.0,    1   // Section #42
  41, 117,   0,  15,   0, 255,    1.1,    1   // Section #43
  42,   2,   0, 255,   0, 255,    1.1,    0   // Section #44
  45,  21,   0, 255,   0, 255,    1.0,    0   // Section #45
  46,  47,   0, 255,   0, 255,    1.0,    1   // Section #46
  29,  46,   0, 255,   0, 255,    1.0,    1   // Section #47
  47,  48,   0, 255,   0, 255,    1.0,    1   // Section #48
  48,  49,   0, 255,   0, 255,    1.0,    1   // Section #49
  49,  50,   0,  65,   0,  65,    1.0,    1   // Section #50
  50,  51,   0,  50,   0,  45,    1.0,    1   // Section #51
  51,  52,   0,  40,   0,  50,    1.0,    1   // Section #52
  52,  53,   0, 255,   0, 255,    1.0,    1   // Section #53
  53,  54,   0, 255,   0,  70,    1.0,    1   // Section #54
  54,  55,   0,  55,   0,  40,    1.0,    1   // Section #55
  55,  56,   0,  45,   0,  40,    1.0,    1   // Section #56
  56,  57,   0,  40,   0,  30,    1.0,    1   // Section #57
  57,  58,   0,  35,   0,  40,    1.0,    1   // Section #58
  58,  59,   0,  45,   0,  50,    1.0,    1   // Section #59
  59,  60,   0, 255,   0, 255,    1.0,    1   // Section #60
  60,  61,   0, 255,   0, 255,    1.0,    1   // Section #61
  61,  62,   0, 255,   0, 255,    1.0,    1   // Section #62
  62,  63,   0,  65,   0,  40,    1.0,    1   // Section #63
  63,  64,   0,  35,   0,  30,    1.0,    1   // Section #64
  64,  65,   0,  25,   0,  35,    1.0,    1   // Section #65
  65,  66,   0, 255,   0, 255,    1.0,    1   // Section #66
  66, 108,   0, 255,   0, 255,    1.0,    1   // Section #67
  67,  68,   0, 255,   0, 255,    1.0,    1   // Section #68
  68,  69,   0, 255,   0, 255,    1.0,    1   // Section #69
  69,  70,   0, 255,   0, 255,    1.0,    1   // Section #70
  70,  71,   0, 255,   0, 255,    1.0,    1   // Section #71
  71,  72,   0, 255,   0, 255,    1.0,    1   // Section #72
  72,  73,   0, 255,   0, 255,    1.0,    1   // Section #73
  73,  74,   0, 255,   0, 255,    1.0,    1   // Section #74
  74,  75,   0, 255,   0, 255,    1.0,    1   // Section #75
  75,  76,   0, 255,   0, 255,    1.0,    1   // Section #76
  76,  77,   0, 255,   0, 255,    1.0,    1   // Section #77
  77,  78,   0, 255,   0, 255,    1.0,    1   // Section #78
  78,  79,   0, 255,   0, 255,    1.0,    1   // Section #79
  79,  80,   0, 255,   0, 255,    1.0,    1   // Section #80
  80,  81,   0, 255,   0, 255,    1.0,    1   // Section #81
  81,  82,   0, 255,   0, 255,    1.0,    1   // Section #82
  82,  83,   0, 255,   0, 255,    1.0,    1   // Section #83
  83,  84,   0, 255,   0, 255,    1.0,    1   // Section #84
  84,  85,   0, 255,   0, 255,    1.0,    1   // Section #85
  85,  86,   0, 255,   0, 255,    1.0,    1   // Section #86
  86,  87,   0, 255,   0, 255,    1.0,    1   // Section #87
  87, 142,   0, 255,   0, 255,    1.0,    1   // Section #88
  88,  89,   0, 255,   0, 255,    1.0,    1   // Section #89
  89,  90,   0, 255,   0, 255,    1.0,    1   // Section #90
  90,  91,   0, 255,   0, 255,    1.0,    1   // Section #91
  91,  92,   0, 255,   0, 255,    1.0,    1   // Section #92
  92,  93,   0, 255,   0, 255,    1.0,    1   // Section #93
  93,  94,   0, 255,   0, 255,    1.0,    1   // Section #94
  94,  95,   0, 255,   0, 255,    1.0,    1   // Section #95
  95,  96,   0, 255,   0, 255,    1.0,    1   // Section #96
  96,  97,   0, 255,   0, 255,    1.0,    1   // Section #97
  97,  98,   0, 255,   0, 255,    1.0,    1   // Section #98
  98,  99,   0, 255,   0, 255,    1.0,    0   // Section #99
  99, 100,   0, 255,   0, 255,    1.0,    0   // Section #100
 100, 101,   0, 255,   0, 255,    1.0,    0   // Section #101
 102, 101,   0, 255,   0, 255,    1.0,    1   // Section #102
 103, 141,   0, 255,   0, 255,    1.0,    1   // Section #103
 104, 103,   0, 255,   0, 255,    1.0,    1   // Section #104
 105, 104,   0, 255,   0, 255,    1.0,    1   // Section #105
 106, 105,   0, 255,   0, 255,    1.0,    1   // Section #106
 107, 106,   0, 255,   0, 255,    1.0,    1   // Section #107
  98, 140,   0, 255,   0, 255,    1.0,    1   // Section #108
 108, 109,   0, 255,   0, 255,    1.0,    0   // Section #109
 108,  67,   0, 255,   0, 255,    1.0,    1   // Section #110
 109, 110,   0, 255,   0, 255,    1.0,    0   // Section #111
 110, 111,   0, 255,   0, 255,    1.0,    0   // Section #112
 111, 112,   0, 255,   0, 255,    1.0,    0   // Section #113
 112,  70,   0, 255,   0, 255,    1.0,    0   // Section #114
 101,  41,   0, 255,   0, 255,    1.0,    1   // Section #115
   0, 113,   0, 255,   0, 255,    1.0,    0   // Section #116
 113, 114,   0, 255,   0, 255,    1.0,    0   // Section #117
 114, 115,   0, 255,   0, 255,    0.9,    0   // Section #118
 115, 116,   0, 255,   0, 255,    0.7,    0   // Section #119
 116, 117,   0, 255,   0, 255,    0.7,    0   // Section #120
 117,  44,   0, 255,   0,  25,    1.1,    1   // Section #121
  89, 118,   0, 255,   0, 255,    0.8,    0   // Section #122
 118, 117,   0, 255,   0, 255,    0.5,    0   // Section #123
 119, 120,   0, 255,   0, 255,    1.0,    0   // Section #124
 119,  17,   0, 255,   0, 255,    1.0,    0   // Section #125
 120, 121,   0, 255,   0, 255,    1.0,    0   // Section #126
 121, 122,   0, 255,   0, 255,    1.0,    0   // Section #127
 122, 128,   0, 255,   0, 255,    1.0,    0   // Section #128
 123, 124,   0, 255,   0, 255,    1.0,    0   // Section #129
 124, 125,   0, 255,   0, 255,    1.0,    0   // Section #130
 125, 126,   0, 255,   0, 255,    1.0,    0   // Section #131
 126, 127,   0, 255,   0, 255,    1.0,    0   // Section #132
 127,  15,   0, 255,   0, 255,    1.0,    0   // Section #133
 128, 133,   0, 255,   0, 255,    1.0,    0   // Section #134
 128, 123,   0, 255,   0, 255,    1.0,    0   // Section #135
 129, 130,   0, 255,   0, 255,    1.3,    0   // Section #136
 130, 131,   0, 255,   0, 255,    1.3,    0   // Section #137
 131, 132,   0, 255,   0, 255,    1.5,    0   // Section #138
 133, 134,   0, 255,   0, 255,    1.0,    0   // Section #139
 133, 129,   0, 255,   0, 255,    1.0,    0   // Section #140
 134, 135,   0, 255,   0, 255,    1.3,    0   // Section #141
 135, 136,   0, 255,   0, 255,    1.3,    0   // Section #142
 136, 137,   0, 255,   0, 255,    1.5,    0   // Section #143
 137, 138,   0, 255,   0, 255,    1.5,    0   // Section #144
 139,   5,   0, 255,   0,  25,    1.0,    0   // Section #145
 140, 107,   0, 255,   0, 255,    1.0,    1   // Section #146
 141, 102,   0, 255,   0, 255,    1.0,    1   // Section #147
 142,  88,   0, 255,   0, 255,    1.0,    1   // Section #148

0                                                             // Number of cop start points
  

END OF OPPONENT PATHS

7										// number of material modifiers

// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT							// skid mark material

//	material '0'
1										// car wall friction
1										// tyre road friction
0.90										// down force
6.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
0										// sparkiness
3										// room for expansion
MUD2.MAT										// room for expansion

//	material '1'
1.2										// car wall friction
1.2										// tyre road friction
1.0										// down force
10.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
2.0										// sparkiness
4										// room for expansion
SAND2.MAT										// room for expansion

//	material '2'
1.2										// car wall friction
1										// tyre road friction
1.0										// down force
5										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
3										// room for expansion
MUD1.MAT										// room for expansion

//	material '3'
1.2										// car wall friction
1.00										// tyre road friction
1.0										// down force
8.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
3										// room for expansion
MUD2.MAT										// room for expansion

//	material '4'
1										// car wall friction
1										// tyre road friction
2										// down force
1										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
20										// sparkiness
1										// room for expansion
1										// room for expansion

//	material '5'
1										// car wall friction
1										// tyre road friction
2.0										// down force
4.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
1										// sparkiness
4										// room for expansion
SAND2.MAT										// room for expansion

// Non CarObjects
5										// number of non car objects

GASPUMP.TXT
GREENCAR.TXT
WRECK.TXT
PALM2.TXT
PHONE.TXT

3										// number of dust shade tables

61, 84, 33								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"

92, 51, 34							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"

117, 94, 38							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"


12										// Number of network start points

-248.296,-15.630,43.190							//1
100													

-253.514,-15.627,23.641							//2						
101									

-260.518,-15.656,20.924							//3						
189									

-274.246,-15.627,23.641							//4						
146									

-269.537,-15.627,23.339							//5						
256									

-282.704,-15.627,30.227							//6						
187									

-278.421,-15.624,49.670							//7						
280									

-271.077,-18.908,81.830							//8						
9									

-255.535,-15.627,43.903							//9						
11									

-248.102,-18.907,75.910							//10						
11									

-275.029,-15.251,13.741							//11						
198									

-281.298,-15.627,37.148							//12						
9									



1										// number of splash files
SPLSHBLU.PIX 								//  name of pixelmapfile for splashes

1

NETCOSTA.TXT

