VERSION 6							// V1 expects map checkpoint rectangles
									// V2 and above expect map checkpoint points
									// V3 and above expect splash file stuff at the end
									// V4 and above expect two sets of PIX and MAT and ped substitution entry


-136.988,-10.44,-138.850						// Position of centre of start of grid
270									// Direction that grid faces in

// Laps, checkpoints etc

60,30,10							// Initial timer count for each skill level
5									// # laps
3000,1500,500						// Race completed bonus (all laps raced) for each skill level
75000,50000,30000					// Race completed bonus (all peds killed) for each skill level
20000,10000,5000					// Race completed bonus (all oppos wasted) for each skill level

// Width and height of map checkpoint rectangles
9,18
11,26


5									// # checkpoints

// Checkpoint #1
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-15.700,-100,-103.446						// Point #0
-15.700,100,-103.446						// Point #1
-12.379,100,-103.151						// Point #2
-12.379,-100,-103.151					// Point #3
266,532
37,89

// Checkpoint #2
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-160.899,-100,-41.994						// Point #0
-160.899,100,-41.994						// Point #1
-159.935,100,-38.539						// Point #2
-159.935,-100,-38.539					// Point #3
155,310
81,194

// Checkpoint #3
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-247.979,-100,31.740						// Point #0
-247.979,100,31.740						// Point #1
-251.610,100,32.406						// Point #2
-251.610,-100,32.406					// Point #3
92,184
134,322

// Checkpoint #4
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-278.842,-100,-80.007						// Point #0
-278.842,100,-80.007						// Point #1
-276.207,100,-78.121						// Point #2
-276.207,-100,-78.121					// Point #3
70,140
52,125

// Checkpoint #5
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-148.820,-100,-137.936						// Point #0
-148.820,100,-137.936						// Point #1
-148.739,100,-141.433						// Point #2
-148.739,-100,-141.433					// Point #3
163,326
7,17

6									// # pixelmap files to load
NYSKY1.PIX
C3SKY2.PIX
COASTA2.pix
CHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX

6
NYSKY1.PIX
C3SKY2.PIX									// # pixelmap files to load (low memory)
COA8TA3.pix
NCHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX


2									// # shade table files to load
COASTA.TAB
IDENTITY.TAB

9									// # material files to load
YWW.MAT
WATTY.MAT
NYSKY1.MAT
C3SKY2.MAT
COASTA2.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT

9									// # material files to load (low memory)
YWW.MAT
WATTY.MAT
NYSKY1.MAT
C3SKY2.MAT
COA8TA3.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT


1									// # model files to load
COASTA2.dat

1									// # model files to load
COSTA82.dat

COASTA2.ACT							// Track actor

COSTA82.ACT

COASTAX.ACT							// Additional actor

// HORIZON STUFF

CHORIZN.PIX						// Name of sky texture pixelmap (or "none")
3									// Horizontal repetitions of sky texture
100									// Vertical size of sky texture (degrees)
80									// Position of horizon (pixels below top)
none								// Depth cue mode ("none", "dark" or "fog")
8,0									// Degree of fog/darkness

// DEFAULT ENGINE NOISE

0

// SPECIAL EFFECTS VOLUMES

11				// # special effects volumes



DEFAULT WATER
0.2									// gravity multiplier
50									// viscosity multiplier
0									// Car damage per millisecond
0.002								// Pedestrian damage per millisecond
0									// camera effect index
1									// Sky colour
WATTY.MAT								// Windscreen material to use
5100								// Sound ID of entry noise
5100								// Sound ID of exit noise
2									// Engine noise index
0									// material index




NEW IMPROVED!
8.702, -0.080, -1.941
0.031, 3.583, -0.007
12.018, 0.007, 53.882
-267.444, -15.562, -32.364
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
5.124, 0.000, 5.680
0.000, 1.000, 0.000
-40.065, 0.000, 22.294
-254.058, -16.907, -75.250
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
0.022, 0.000, 1.728
0.000, 2.074, 0.000
-3.583, 0.000, 0.046
-212.111, -17.667, -89.661
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
-0.416, 0.000, -1.677
0.003, 1.728, -0.001
1.398, -0.002, -0.347
-193.901, -17.667, -91.913
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
-0.940, 0.000, -1.848
0.000, 1.000, 0.000
1.283, 0.000, -0.653
-181.791, -16.747, -97.209
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
1.262, 0.000, 1.645
0.000, 1.728, 0.000
-1.143, 0.000, 0.876
-171.178, -16.427, -105.123
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
1.210, 0.000, 1.684
0.014, 1.440, -0.010
-0.975, 0.014, 0.700
-165.651, -14.506, -108.596
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
-0.462, 0.000, -2.022
0.000, 1.000, 0.000
1.170, 0.000, -0.267
-133.374, -12.981, -118.326
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
-0.472, 0.000, -2.019
0.013, 1.000, -0.003
1.402, -0.020, -0.328
-93.955, -12.942, -127.460
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

NEW IMPROVED!
-0.444, 0.000, -1.831
0.000, 1.000, 0.000
9.804, 0.000, -2.379
-72.472, -13.061, -132.528
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// REFLECTIVE WINDSCREEN SPECIFICATIONS

C3SKY2.MAT							// Material to use for default screens
DRKSCRN.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT							// Material to use for default screens during fog

0									// # areas with different screens

// MAP DETAILS

CSTAMAP2.PIX						// Map pixelmap name

0.744,		0,			0			// World->map transformation matrix
0,			0,			0
0,			0.744, 		0
282.4,		114.9,		0

// ****** START OF FUNK AND GROOVE STUFF ******

START OF FUNK

!!WATER.MAT
constant
slither
harmonic
0.20,0
5,5
no fucking lighting
no animation you cunt

NEXT FUNK

CHECK.MAT
constant
roll
continuous
0.2,0
no fucking lighting
no animation you cunt


END OF FUNK



START OF GROOVE

&YAC0001.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
2							// max angle of rock

NEXT GROOVE

&YAC0002.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
2							// max angle of rock

NEXT GROOVE

&YAC0003.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock

NEXT GROOVE

&YAC0004.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock

NEXT GROOVE

&YAC0005.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.07,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock

NEXT GROOVE

&YAC0006.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.23							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock

NEXT GROOVE

&YAC0007.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock

NEXT GROOVE

&YAC0008.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
8							// max angle of rock

NEXT GROOVE

&YAC0009.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
7							// max angle of rock

NEXT GROOVE

&YAC0010.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.08,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.17							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
8							// max angle of rock

NEXT GROOVE

&YAC0011.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0012.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0013.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0014.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.16							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0015.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0016.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.17							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0017.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.15							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0018.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.9,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0018.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.1,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0019.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.14							// Cycles per second
0,.12,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.14							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
11							// max angle of rock

NEXT GROOVE

&YAC0020.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.12,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0020.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock


NEXT GROOVE

&YAC0021.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0022.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0023.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.17							// Cycles per second
0,.06,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0024.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0025.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0026.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.15,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
11							// max angle of rock

NEXT GROOVE

&YAC0027.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.2							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0028.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0029.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.16							// Cycles per second
0,.09,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.15							// cycle speed per second
0,0,.03						// centre of rocking
z							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0030.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.06,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.18							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock

NEXT GROOVE

&YAC0031.ACT					// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance						// Only moves when in view
straight						// Moves on a straight path
harmonic						// Motion is harmonic
0,0,0							// Centre of movement
0.18							// Cycles per second
0,.05,0						// Amount of movement (each way) in each axis
rock							// object movement options
harmonic						// movement mode
0.2							// cycle speed per second
0,0,.03						// centre of rocking
x							// axis to rock in
9							// max angle of rock


END OF GROOVE

// ****** START OF PEDESTRIAN STUFF ******

17				// Ped subs table index

510				// Number of pedestrians

// Pedestrian number 1

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-270.099,-2.552,-90.191
	point
	-270.283,-2.552,-90.262
	point
	-270.642,-2.552,-90.240
	point
	-270.750,-2.552,-90.830
	point
	-270.106,-2.552,-94.390
	reverse


// Pedestrian number 2

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-269.542,-2.552,-93.851
	point
	-269.226,-2.552,-94.602
	point
	-268.805,-2.552,-97.226
	point
	-269.183,-2.552,-97.602
	reverse


// Pedestrian number 3

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-269.651,-2.552,-96.212
	point
	-270.692,-2.552,-96.146
	point
	-271.176,-2.552,-93.826
	point
	-270.885,-2.550,-90.653
	point
	-269.978,-2.552,-89.883
	reverse


// Pedestrian number 4

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-283.484,-2.539,-69.888
	point
	-283.344,-2.539,-70.484
	point
	-282.090,-2.547,-71.521
	point
	-281.665,-2.552,-75.949
	reverse


// Pedestrian number 5

1				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-273.553,-2.552,-71.184
	point
	-274.416,-2.552,-70.664
	point
	-276.012,-2.552,-69.593
	point
	-282.558,-2.541,-69.943
	point
	-283.671,-2.538,-70.196
	point
	-285.278,-2.538,-71.625
	reverse


// Pedestrian number 6

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-267.804,-2.552,-75.968
	point
	-269.345,-2.552,-74.693
	point
	-270.275,-2.552,-73.536
	point
	-272.513,-2.552,-72.074
	point
	-272.953,-2.552,-71.371
	reverse


// Pedestrian number 7

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-283.972,-2.540,-69.747
	point
	-285.354,-2.540,-66.865
	point
	-287.150,-2.531,-66.831
	point
	-287.955,-2.543,-68.800
	point
	-288.656,-2.544,-69.908
	reverse


// Pedestrian number 8

1				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-313.628,-11.971,-26.568
	point
	-313.384,-11.971,-24.033
	point
	-312.579,-11.971,-22.773
	point
	-312.587,-11.971,-21.316
	point
	-312.863,-11.971,-19.602
	point
	-312.938,-11.971,-18.287
	reverse


// Pedestrian number 9

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-273.343,-15.627,25.364
	point
	-272.440,-15.626,22.412
	point
	-271.392,-15.627,22.991
	point
	-270.066,-15.627,23.992
	point
	-266.453,-15.627,23.741
	reverse


// Pedestrian number 10

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-256.908,-15.622,24.732
	point
	-258.387,-15.620,25.909
	point
	-261.283,-15.627,26.499
	point
	-261.930,-15.627,25.909
	point
	-262.724,-15.627,24.242
	reverse


// Pedestrian number 11

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-259.411,-15.657,19.155
	point
	-259.250,-15.651,21.396
	point
	-258.661,-15.627,22.942
	point
	-257.584,-15.627,22.954
	point
	-254.533,-15.627,25.546
	reverse


// Pedestrian number 12

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-261.806,-15.627,23.787
	point
	-260.932,-15.627,24.492
	point
	-260.637,-15.631,25.771
	point
	-261.612,-15.627,26.439
	point
	-263.339,-15.627,27.132
	reverse


// Pedestrian number 13

8				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-259.648,-15.627,26.691
	point
	-260.517,-15.634,24.927
	point
	-260.682,-15.634,24.331
	point
	-259.094,-15.652,22.352
	point
	-259.229,-15.655,20.294
	point
	-263.211,-15.657,16.713
	reverse


// Pedestrian number 14

3				// Ref num
5				// Number of instructions
4				// Initial instruction

	point
	-258.070,-15.645,23.910
	point
	-258.197,-15.634,25.400
	point
	-258.889,-15.628,26.320
	point
	-260.490,-15.627,27.624
	reverse


// Pedestrian number 15

8				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-260.701,-15.599,47.238
	point
	-259.289,-15.606,46.406
	point
	-257.955,-15.616,46.773
	point
	-256.369,-15.627,46.363
	point
	-254.084,-15.627,46.205
	point
	-253.703,-15.666,46.495
	reverse


// Pedestrian number 16

8				// Ref num
5				// Number of instructions
5				// Initial instruction

	point
	-253.063,-15.627,45.480
	point
	-254.008,-15.627,44.645
	point
	-254.846,-15.627,44.699
	point
	-257.222,-15.627,43.235
	reverse


// Pedestrian number 17

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-255.654,-15.627,46.287
	point
	-253.574,-15.627,43.281
	point
	-246.855,-15.630,44.114
	reverse


// Pedestrian number 18

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-254.375,-15.627,42.839
	point
	-252.268,-15.627,44.870
	point
	-251.614,-15.627,45.550
	reverse


// Pedestrian number 19

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-277.839,-15.626,46.964
	point
	-278.242,-15.626,48.289
	point
	-278.639,-15.626,48.814
	point
	-279.885,-15.622,51.172
	point
	-280.454,-15.622,51.603
	reverse


// Pedestrian number 20

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-279.755,-15.627,47.717
	point
	-280.472,-15.627,48.585
	point
	-282.667,-15.627,49.018
	reverse


// Pedestrian number 21

1				// Ref num
4				// Number of instructions
3				// Initial instruction

	point
	-273.077,-15.595,49.765
	point
	-277.955,-15.626,48.609
	point
	-278.568,-15.627,47.785
	reverse


// Pedestrian number 22

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-261.550,-15.627,24.535
	point
	-259.447,-15.657,20.859
	point
	-259.724,-15.657,19.231
	point
	-260.028,-15.657,17.513
	point
	-261.038,-15.657,13.342
	point
	-264.753,-15.657,11.104


// Pedestrian number 23

8				// Ref num
9				// Number of instructions
5				// Initial instruction

	point
	-266.082,-2.553,-107.261
	point
	-264.257,-2.552,-109.714
	point
	-261.583,-2.552,-110.630
	point
	-254.872,-2.555,-114.747
	point
	-251.657,-2.553,-118.503
	point
	-250.448,-2.553,-118.685
	point
	-248.889,-2.553,-119.259
	point
	-247.098,-2.551,-119.696
	reverse


// Pedestrian number 24

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-246.091,-2.560,-122.113
	point
	-245.615,-2.566,-123.061
	point
	-245.679,-2.573,-124.489
	point
	-246.242,-2.578,-125.649
	point
	-247.503,-2.581,-126.887
	reverse


// Pedestrian number 25

1				// Ref num
8				// Number of instructions
5				// Initial instruction

	point
	-266.410,998.041,-108.087
	point
	-265.176,997.648,-109.687
	point
	-264.586,-2.552,-109.784
	point
	-263.782,-2.552,-111.050
	point
	-262.242,-2.552,-111.443
	point
	-261.234,-2.552,-111.416
	point
	-256.954,-2.552,-113.230
	reverse


// Pedestrian number 26

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-263.329,-2.552,-106.691
	point
	-264.653,-2.552,-106.833
	point
	-265.447,-2.552,-106.684
	point
	-265.923,-2.552,-106.075
	point
	-266.551,-2.552,-106.131
	reverse


// Pedestrian number 27

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-267.692,-2.552,-101.129
	point
	-265.751,-2.552,-104.003
	point
	-265.192,-2.552,-104.223
	point
	-264.814,-2.552,-104.245
	point
	-264.475,-2.552,-103.716
	reverse


// Pedestrian number 28

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-288.495,-2.544,-69.925
	point
	-287.502,-2.542,-70.409
	point
	-285.983,-2.538,-71.673
	point
	-282.681,-2.543,-71.064
	reverse


// Pedestrian number 29

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-294.143,-2.791,-66.783
	point
	-295.765,-2.911,-66.707
	point
	-298.187,996.963,-66.782
	point
	-301.141,997.563,-65.627
	reverse


// Pedestrian number 30

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-309.792,-4.048,-66.420
	point
	-310.831,-4.048,-65.068
	point
	-308.452,-4.048,-62.614
	point
	-307.596,996.743,-61.857
	reverse


// Pedestrian number 31

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-287.373,-8.005,-48.814
	point
	-286.748,-8.005,-48.424
	point
	-285.763,-8.005,-47.190
	point
	-284.516,-8.005,-44.545
	reverse


// Pedestrian number 32

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-288.702,-8.004,-37.911
	point
	-289.819,-8.005,-36.912
	point
	-291.675,-8.005,-35.896
	point
	-293.116,-8.132,-35.655
	reverse


// Pedestrian number 33

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-316.138,-11.971,-26.853
	point
	-315.844,-11.971,-24.747
	point
	-315.337,-11.971,-23.907
	point
	-314.748,-11.971,-20.162
	reverse


// Pedestrian number 34

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-280.964,-13.137,0.325
	point
	-279.881,-14.067,6.853
	point
	-279.061,-14.283,8.372
	point
	-278.439,-14.469,9.711
	reverse


// Pedestrian number 35

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-281.143,-13.637,4.305
	point
	-279.878,-13.759,4.398
	point
	-277.683,-14.024,5.166
	point
	-277.137,-14.175,6.063
	point
	-276.633,-14.232,6.556
	reverse


// Pedestrian number 36

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-279.125,-13.614,2.765
	point
	-278.599,-13.753,3.557
	point
	-278.165,-13.871,4.247
	point
	-278.714,-14.200,7.385
	point
	-279.385,-14.220,7.974
	reverse


// Pedestrian number 37

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-276.482,-14.300,7.130
	point
	-276.218,-14.378,7.742
	point
	-276.264,-14.536,9.064
	point
	-276.652,-15.143,13.609
	reverse


// Pedestrian number 38

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-275.002,-15.619,19.806
	point
	-274.496,-15.618,19.663
	point
	-268.392,-15.627,22.206
	reverse


// Pedestrian number 39

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-272.264,-15.588,17.210
	point
	-275.048,-15.622,20.672
	point
	-274.942,-15.624,21.368
	point
	-278.184,-15.627,30.167
	reverse


// Pedestrian number 40

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-277.417,-15.627,29.835
	point
	-279.133,-15.627,30.441
	point
	-280.492,-15.627,30.747
	reverse


// Pedestrian number 41

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-282.975,-15.627,28.137
	point
	-283.564,-15.627,28.642
	point
	-284.591,-15.627,31.486
	reverse


// Pedestrian number 42

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-280.448,-15.627,34.628
	point
	-282.453,-15.627,32.370
	point
	-284.006,-15.627,31.417
	point
	-284.666,-15.627,28.681
	reverse


// Pedestrian number 43

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-281.126,-15.627,31.345
	point
	-281.238,-15.627,31.978
	point
	-283.168,-15.627,35.341
	reverse


// Pedestrian number 44

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-285.095,-15.627,28.814
	point
	-286.271,-15.627,29.022
	point
	-287.036,-15.627,29.290
	point
	-287.996,-15.627,29.336
	reverse


// Pedestrian number 45

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-289.209,-15.627,30.392
	point
	-288.316,-15.627,34.406
	point
	-288.427,-15.627,35.933
	point
	-284.900,-15.627,51.411
	reverse


// Pedestrian number 46

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-288.387,-15.627,48.459
	point
	-287.352,-15.627,49.820
	point
	-276.078,-15.617,50.597
	reverse


// Pedestrian number 47

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-59.975,-14.067,-138.803
	point
	-60.505,-14.035,-138.556
	point
	-61.242,-13.918,-136.903
	point
	-62.150,-13.901,-136.874
	reverse


// Pedestrian number 48

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-62.775,-13.901,-136.216
	point
	-60.787,-13.911,-134.451
	point
	-57.955,-14.207,-135.354
	reverse


// Pedestrian number 49

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-56.289,-14.327,-137.813
	point
	-58.024,-14.202,-137.874
	point
	-60.730,-13.909,-134.134
	point
	-61.790,-13.901,-132.943
	reverse


// Pedestrian number 50

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-65.611,-13.901,-132.644
	point
	-63.646,-13.901,-133.128
	point
	-62.385,-13.901,-136.494
	point
	-62.564,-13.916,-137.158
	point
	-66.376,-13.713,-136.860
	reverse


// Pedestrian number 51

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-69.041,-13.532,-139.787
	point
	-67.521,-13.635,-139.776
	point
	-62.387,-13.925,-137.424
	point
	-62.022,-13.949,-137.335
	reverse


// Pedestrian number 52

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-97.076,-13.901,-125.689
	point
	-99.376,-13.901,-124.838
	point
	-106.368,-13.901,-123.246
	point
	-109.898,-13.901,-125.363
	point
	-111.093,-13.901,-125.195
	reverse


// Pedestrian number 53

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-112.755,-13.901,-121.814
	point
	-111.085,-13.901,-122.181
	point
	-109.744,-13.901,-122.466
	point
	-106.911,-13.901,-125.959
	reverse


// Pedestrian number 54

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-175.042,-17.667,-100.004
	point
	-179.117,-17.667,-100.649
	point
	-181.253,-17.667,-99.148
	point
	-181.745,-17.667,-95.709
	reverse


// Pedestrian number 55

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-179.293,-17.667,-97.039
	point
	-176.732,-17.667,-98.838
	point
	-175.654,-17.667,-99.802
	point
	-174.310,-17.667,-100.624
	reverse


// Pedestrian number 56

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-170.557,-16.453,-106.909
	point
	-174.975,-17.426,-103.830
	point
	-176.094,-17.667,-102.846
	point
	-177.133,-17.667,-101.969
	point
	-178.138,-17.667,-101.345
	reverse


// Pedestrian number 57

13				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-203.787,-17.667,-91.459
	point
	-207.159,-17.667,-88.463
	point
	-209.744,-17.667,-88.486
	point
	-211.957,-17.667,-88.351
	point
	-213.212,-17.667,-88.337
	point
	-214.288,-17.667,-91.441
	reverse


// Pedestrian number 58

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-214.358,-17.667,-88.482
	point
	-212.875,-17.667,-88.949
	point
	-210.600,-17.667,-88.317
	point
	-208.806,-17.667,-89.242
	point
	-207.125,-17.667,-91.163
	reverse


// Pedestrian number 59

5				// Ref num
5				// Number of instructions
4				// Initial instruction

	point
	-244.356,-17.667,-77.863
	point
	-245.862,-17.667,-77.901
	point
	-248.054,-17.667,-78.765
	point
	-252.012,-17.667,-78.072
	reverse


// Pedestrian number 60

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-250.827,-17.667,-75.431
	point
	-250.251,-17.667,-75.935
	point
	-247.056,-17.667,-80.030
	reverse


// Pedestrian number 61

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-261.819,-17.667,-73.050
	point
	-260.784,-17.667,-73.119
	point
	-259.624,-17.667,-71.430
	point
	-257.921,-17.667,-71.828
	point
	-254.443,-17.667,-72.824
	reverse


// Pedestrian number 62

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-261.064,-17.667,-70.032
	point
	-260.448,-17.667,-70.677
	point
	-259.825,-17.667,-74.013
	reverse


// Pedestrian number 63

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-265.666,-15.657,7.363
	point
	-265.003,-15.657,8.315
	point
	-262.073,-15.657,10.449
	reverse


// Pedestrian number 64

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-264.227,-15.657,12.830
	point
	-264.807,-15.657,10.788
	point
	-262.833,-15.657,7.393
	point
	-263.603,-15.657,2.374
	reverse


// Pedestrian number 65

14				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-266.605,-15.657,0.758
	point
	-266.129,-15.657,3.554
	point
	-264.564,-15.657,9.533
	point
	-263.000,-15.657,11.069
	point
	-261.491,-15.657,11.978
	reverse


// Pedestrian number 66

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-262.447,-15.657,8.891
	point
	-262.242,-15.657,9.640
	point
	-262.573,-15.657,10.781
	point
	-263.959,-15.657,13.668
	reverse


// Pedestrian number 67

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-259.638,-15.657,18.489
	point
	-261.348,-15.657,12.474
	point
	-264.456,-15.657,10.126
	point
	-264.992,-15.657,9.778
	reverse


// Pedestrian number 68

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-263.145,-15.657,5.505
	point
	-263.338,-15.657,6.703
	point
	-262.725,-15.657,8.248
	point
	-261.501,-15.657,11.636
	reverse


// Pedestrian number 69

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-257.690,-15.632,24.742
	point
	-257.953,-15.627,26.535
	point
	-257.212,-15.627,28.230
	point
	-259.492,-15.627,31.657
	reverse


// Pedestrian number 70

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-256.166,-15.627,33.743
	point
	-256.624,-15.627,33.108
	point
	-257.324,-15.627,29.408
	point
	-257.476,-15.627,25.473
	point
	-255.290,-15.627,22.277
	reverse


// Pedestrian number 71

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-257.372,-15.627,22.881
	point
	-256.107,-15.627,22.939
	point
	-250.981,-15.627,24.575
	reverse


// Pedestrian number 72

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-252.187,-15.627,28.373
	point
	-252.575,-15.627,27.283
	point
	-251.458,-15.627,23.884
	reverse


// Pedestrian number 73

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-261.113,-15.628,25.080
	point
	-261.443,-15.630,22.852
	point
	-262.229,-15.657,20.201
	point
	-259.412,-15.657,19.456
	reverse


// Pedestrian number 74

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-245.970,-15.627,39.348
	point
	-249.793,-15.627,39.942
	point
	-250.178,-15.626,41.146
	reverse


// Pedestrian number 75

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-251.313,-15.627,42.251
	point
	-250.725,-15.625,41.961
	point
	-249.967,-15.627,41.610
	point
	-246.365,-15.629,41.041
	point
	-245.368,-15.627,39.850
	reverse


// Pedestrian number 76

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-244.877,-15.635,43.594
	point
	-246.984,-15.653,43.465
	point
	-248.305,-15.628,42.389
	point
	-251.868,-15.627,23.453
	reverse


// Pedestrian number 77

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-254.490,-15.627,41.847
	point
	-257.747,-15.627,39.460
	point
	-258.167,-15.627,37.313
	point
	-258.198,-15.649,23.130
	reverse


// Pedestrian number 78

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-261.943,-15.627,25.544
	point
	-263.120,-15.627,26.106
	point
	-267.710,-15.627,26.051
	reverse


// Pedestrian number 79

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-268.220,-15.627,25.990
	point
	-268.947,-15.627,25.494
	point
	-269.505,-15.627,20.972
	reverse


// Pedestrian number 80

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-280.302,-15.627,27.697
	point
	-281.003,-15.627,27.992
	point
	-282.525,-15.627,38.145
	reverse


// Pedestrian number 81

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-279.237,-15.627,47.436
	point
	-279.147,-15.627,46.697
	point
	-280.958,-15.627,32.440
	reverse


// Pedestrian number 82

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-283.974,-15.627,31.730
	point
	-283.756,-15.627,32.563
	point
	-283.491,-15.627,33.863
	point
	-278.829,-15.627,47.333
	reverse


// Pedestrian number 83

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-278.011,-15.627,46.284
	point
	-278.348,-15.627,45.160
	point
	-281.207,-15.627,44.482
	reverse


// Pedestrian number 84

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-278.334,-15.708,52.126
	point
	-276.456,-15.917,53.527
	point
	-276.025,-16.174,56.155
	point
	-277.909,-16.318,58.276
	reverse


// Pedestrian number 85

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-272.600,-18.908,82.287
	point
	-269.042,-18.912,86.156
	point
	-269.557,-18.914,89.312
	point
	-270.740,-18.916,92.449
	reverse


// Pedestrian number 86

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-267.411,-18.915,94.181
	point
	-269.126,-18.915,92.989
	point
	-270.514,-18.916,93.653
	point
	-274.046,-18.916,92.297
	point
	-290.575,-18.915,96.467
	reverse


// Pedestrian number 87

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-290.535,-18.915,97.563
	point
	-274.153,-18.915,94.451
	point
	-268.527,-18.915,89.919
	reverse


// Pedestrian number 88

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-267.077,-18.915,92.468
	point
	-267.702,-18.915,91.826
	point
	-268.247,-18.915,90.436
	point
	-270.731,-18.914,89.718
	reverse


// Pedestrian number 89

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-266.066,-18.913,106.289
	point
	-269.661,-18.914,94.163
	point
	-267.923,-18.915,90.522
	reverse


// Pedestrian number 90

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-246.888,-18.915,85.598
	point
	-246.557,-18.915,88.305
	point
	-246.116,-18.915,89.756
	reverse


// Pedestrian number 91

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-242.658,-18.915,100.699
	point
	-242.385,-18.915,96.290
	point
	-244.021,-18.915,89.483
	point
	-244.344,-18.914,85.812
	reverse


// Pedestrian number 92

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-224.432,-18.915,81.168
	point
	-225.555,-18.916,82.652
	point
	-228.229,-18.916,84.140
	reverse


// Pedestrian number 93

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-224.098,-18.916,82.961
	point
	-224.899,-18.916,82.519
	point
	-225.427,-18.916,82.805
	point
	-232.529,-18.916,82.657
	reverse


// Pedestrian number 94

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-224.172,-18.916,82.005
	point
	-243.623,-18.915,87.028
	point
	-244.561,-18.915,86.304
	point
	-245.521,-18.913,82.788
	point
	-248.219,-18.911,80.794
	reverse


// Pedestrian number 95

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-246.298,-18.910,78.252
	point
	-246.004,-18.911,79.590
	point
	-247.313,-18.916,88.406
	reverse


// Pedestrian number 96

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-245.505,-18.915,92.686
	point
	-245.012,-18.915,94.175
	point
	-244.207,-18.916,100.898
	reverse


// Pedestrian number 97

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-221.401,-18.916,95.766
	point
	-222.908,-18.916,95.051
	point
	-227.663,-18.916,95.340
	point
	-230.000,-18.916,96.978
	point
	-244.157,-18.915,98.220
	reverse


// Pedestrian number 98

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-238.820,-18.915,99.952
	point
	-241.360,-18.915,98.651
	point
	-244.445,-18.915,96.720
	point
	-244.997,-18.915,95.096
	reverse


// Pedestrian number 99

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-242.120,-18.915,97.469
	point
	-244.093,-18.915,98.859
	point
	-245.851,-18.916,101.360
	point
	-287.253,-18.914,110.686
	reverse


// Pedestrian number 100

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-245.032,-18.916,101.345
	point
	-244.585,-18.915,98.971
	point
	-242.312,-18.914,96.801
	reverse


// Pedestrian number 101

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-251.461,-18.916,100.610
	reverse


// Pedestrian number 102

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-253.398,-15.627,45.697
	reverse


// Pedestrian number 103

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-257.272,-15.627,42.491
	reverse


// Pedestrian number 104

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-256.284,-15.627,33.307
	reverse


// Pedestrian number 105

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-254.620,-15.627,22.531
	reverse


// Pedestrian number 106

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-250.575,-15.627,41.531
	reverse


// Pedestrian number 107

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-254.042,-17.667,-73.114
	reverse


// Pedestrian number 108

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-252.533,-17.667,-77.667
	reverse


// Pedestrian number 109

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-226.823,-17.667,-91.019
	reverse


// Pedestrian number 110

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-27.743,-15.561,-44.497
	reverse


// Pedestrian number 111

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-26.788,-15.561,-45.238
	reverse


// Pedestrian number 112

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-25.847,-15.561,-45.968
	reverse


// Pedestrian number 113

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-82.993,-13.028,-48.234
	reverse


// Pedestrian number 114

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-129.713,-18.645,-45.533
	reverse


// Pedestrian number 115

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-127.573,-18.655,-46.141
	reverse


// Pedestrian number 116

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-125.686,-18.634,-45.420
	reverse


// Pedestrian number 117

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-138.923,-18.725,-58.154
	reverse


// Pedestrian number 118

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-141.695,-18.737,-59.375
	reverse


// Pedestrian number 119

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-145.946,-18.665,-48.496
	reverse


// Pedestrian number 120

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-145.198,-18.670,-46.779
	reverse


// Pedestrian number 121

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-139.581,-16.166,-39.660
	reverse


// Pedestrian number 122

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-137.255,-14.010,-30.646
	reverse


// Pedestrian number 123

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-136.103,-13.938,-30.522
	reverse


// Pedestrian number 124

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-132.813,-9.082,-50.595
	reverse


// Pedestrian number 125

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-133.365,-9.082,-50.436
	reverse


// Pedestrian number 126

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-264.404,-2.552,-104.048
	reverse


// Pedestrian number 127

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-264.253,-2.552,-104.536
	reverse


// Pedestrian number 128

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-268.549,-2.552,-98.537
	reverse


// Pedestrian number 129

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-154.797,-8.795,-37.416
	point
	-155.758,-9.008,-39.093
	point
	-155.682,-9.077,-40.053
	point
	-146.436,-9.077,-42.540
	reverse


// Pedestrian number 130

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-146.536,-9.077,-45.589
	point
	-148.877,-9.077,-44.903
	point
	-149.937,-9.077,-44.138
	point
	-150.793,-9.077,-41.614
	reverse


// Pedestrian number 131

13				// Ref num
4				// Number of instructions
1				// Initial instruction

	point
	-144.951,-8.822,-45.084
	point
	-146.179,-9.077,-44.767
	point
	-147.609,-9.077,-45.393
	reverse


// Pedestrian number 132

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-135.266,-8.919,-46.250
	point
	-134.767,-9.089,-46.979
	point
	-132.236,-9.084,-46.497
	point
	-121.404,-9.078,-49.433
	reverse


// Pedestrian number 133

13				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-132.587,-9.081,-50.555
	point
	-132.074,-8.967,-50.100
	point
	-131.552,-9.077,-49.757
	point
	-128.024,-9.077,-49.940
	point
	-124.245,-9.078,-48.738
	point
	-122.163,-9.338,-46.182
	reverse


// Pedestrian number 134

14				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-125.546,-9.934,-40.050
	point
	-123.504,-9.673,-41.952
	point
	-124.452,-9.143,-47.802
	point
	-121.549,-9.096,-49.138
	reverse


// Pedestrian number 135

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-127.186,-9.077,-48.003
	point
	-128.893,-9.077,-48.697
	point
	-134.625,-9.081,-48.200
	point
	-136.083,-8.818,-47.566
	reverse


// Pedestrian number 136

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-134.164,-9.096,-46.011
	point
	-133.139,-9.080,-47.536
	point
	-131.164,-9.077,-48.998
	point
	-125.868,-9.078,-51.521
	reverse


// Pedestrian number 137

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-23.454,-15.561,-49.659
	point
	-25.541,-15.561,-45.735
	point
	-28.159,-15.561,-43.634
	point
	-37.209,-15.561,-46.669
	reverse


// Pedestrian number 138

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-31.746,-15.561,-44.197
	point
	-29.092,-15.561,-44.828
	point
	-23.428,-15.561,-47.823
	reverse


// Pedestrian number 139

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-23.237,-15.561,-51.567
	point
	-24.452,-15.560,-51.263
	point
	-27.403,-15.561,-49.276
	point
	-29.418,-15.561,-46.721
	point
	-28.054,-15.561,-43.551
	reverse


// Pedestrian number 140

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-24.211,-15.561,-46.619
	point
	-25.772,-15.561,-47.198
	point
	-26.246,-15.561,-49.840
	point
	-24.516,-15.561,-50.401
	reverse


// Pedestrian number 141

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-274.111,-15.600,47.219
	point
	-273.015,-15.599,47.834
	point
	-271.303,-15.599,49.503
	point
	-269.993,-15.599,49.251
	reverse


// Pedestrian number 142

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-275.307,-15.612,50.411
	point
	-274.073,-15.604,50.194
	point
	-267.833,-15.599,48.906
	reverse


// Pedestrian number 143

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-268.077,-15.599,45.919
	point
	-270.539,-15.599,46.626
	point
	-271.840,-15.599,47.562
	point
	-274.421,-15.604,47.757
	point
	-276.369,-15.619,47.718
	reverse


// Pedestrian number 144

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-266.716,-15.599,48.695
	point
	-263.974,-15.599,47.846
	point
	-261.122,-15.599,44.348
	reverse


// Pedestrian number 145

29				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-273.751,-15.599,47.079
	point
	-271.455,-15.599,47.075
	point
	-270.293,-15.599,48.141
	point
	-267.297,-15.599,47.593
	point
	-264.722,-15.599,48.203
	reverse


// Pedestrian number 146

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-262.696,-15.599,44.762
	point
	-257.263,-15.627,43.881
	point
	-253.610,-15.627,42.867
	reverse


// Pedestrian number 147

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-282.000,-15.625,51.855
	point
	-283.612,-15.627,50.231
	point
	-285.220,-15.627,48.205
	point
	-290.883,-15.627,37.644
	reverse


// Pedestrian number 148

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-269.156,-15.599,46.071
	point
	-265.497,-15.599,45.847
	point
	-263.858,-15.599,45.177
	point
	-256.357,-15.627,46.578
	reverse


// Pedestrian number 149

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-256.138,-15.649,46.817
	point
	-255.963,-15.783,47.965
	point
	-255.393,-15.998,49.747
	point
	-252.229,-16.263,52.093
	reverse


// Pedestrian number 150

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-240.193,-14.789,40.689
	point
	-237.698,-14.359,39.170
	point
	-236.859,-13.820,34.927
	reverse


// Pedestrian number 151

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-244.855,-15.619,40.005
	point
	-244.408,-15.513,39.803
	point
	-242.112,-14.883,38.503
	point
	-239.603,-14.414,36.895
	reverse


// Pedestrian number 152

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-235.848,-13.988,37.950
	point
	-232.211,-13.012,35.192
	point
	-229.563,-12.513,32.817
	reverse


// Pedestrian number 153

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-230.596,-12.208,29.479
	point
	-228.883,-11.868,28.658
	point
	-225.417,-11.308,27.739
	point
	-223.554,-11.037,25.996
	reverse


// Pedestrian number 154

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-215.914,-9.122,11.075
	point
	-215.358,-9.078,10.006
	point
	-215.350,-9.078,9.436
	point
	-217.107,-9.078,5.180
	reverse


// Pedestrian number 155

14				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-216.712,-9.078,9.149
	point
	-215.622,-9.078,5.559
	point
	-215.178,-9.078,3.462
	point
	-215.443,-9.078,2.543
	point
	-214.628,-9.078,1.286
	point
	-215.556,-9.078,-1.573
	reverse


// Pedestrian number 156

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-220.365,-9.446,14.723
	point
	-219.623,-9.293,12.993
	point
	-219.052,-9.222,12.157
	point
	-218.892,-9.163,10.928
	reverse


// Pedestrian number 157

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-217.898,-9.078,9.322
	point
	-217.505,-9.078,6.830
	point
	-216.861,-9.078,4.397
	point
	-216.390,-9.078,1.667
	reverse


// Pedestrian number 158

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-215.150,-9.078,8.818
	point
	-215.007,-9.078,7.951
	point
	-214.495,-9.078,7.136
	point
	-214.368,-9.078,6.415
	point
	-213.805,-9.078,4.554
	reverse


// Pedestrian number 159

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-218.536,-9.103,9.741
	point
	-217.609,-9.078,7.851
	point
	-216.308,-9.078,5.552
	point
	-216.740,-9.078,4.223
	reverse


// Pedestrian number 160

8				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-206.193,-8.044,-8.222
	point
	-205.343,-7.665,-8.595
	point
	-204.631,-7.562,-8.476
	point
	-204.049,-7.140,-8.757
	point
	-203.320,-6.748,-8.939
	reverse


// Pedestrian number 161

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-204.299,-7.663,-8.118
	point
	-203.816,-7.387,-8.357
	point
	-203.330,-7.145,-8.425
	point
	-202.910,-7.249,-8.038
	point
	-201.931,-7.245,-7.347
	reverse


// Pedestrian number 162

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-206.737,-8.135,-8.164
	point
	-205.643,-7.958,-7.995
	point
	-203.866,-7.672,-7.739
	point
	-203.208,-7.562,-7.607
	point
	-201.235,-7.058,-6.994
	reverse


// Pedestrian number 163

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-197.295,-5.839,-1.871
	point
	-194.701,-5.332,-0.287
	point
	-193.775,-5.328,0.480
	point
	-193.307,-5.328,0.595
	point
	-192.870,-5.328,1.078
	reverse


// Pedestrian number 164

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-188.596,-5.325,0.546
	point
	-187.717,-5.327,1.713
	point
	-186.019,-5.427,3.168
	point
	-184.273,-5.428,3.262
	reverse


// Pedestrian number 165

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-190.226,-5.270,3.747
	point
	-190.782,-4.797,3.803
	point
	-191.406,-4.735,3.288
	point
	-191.612,-5.327,2.311
	reverse


// Pedestrian number 166

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-188.997,-5.362,4.469
	point
	-186.993,-5.407,4.074
	point
	-186.415,-5.427,3.910
	point
	-183.962,-5.428,3.497
	point
	-181.176,-5.421,3.071
	reverse


// Pedestrian number 167

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-184.261,-5.428,6.319
	point
	-185.743,-5.428,5.912
	point
	-187.377,-5.421,5.567
	reverse


// Pedestrian number 168

8				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-185.924,-5.427,2.800
	point
	-185.395,-5.428,4.132
	point
	-183.905,-5.428,5.366
	point
	-181.818,-5.423,6.072
	point
	-179.124,-5.425,5.360
	reverse


// Pedestrian number 169

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-174.318,-5.442,-0.457
	point
	-174.188,-5.446,-0.956
	point
	-174.107,-5.498,-4.044
	point
	-175.052,-5.851,-7.078
	reverse


// Pedestrian number 170

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-177.642,-5.713,-5.465
	point
	-177.881,-5.840,-6.393
	point
	-178.966,-6.300,-8.660
	reverse


// Pedestrian number 171

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-177.301,-5.594,-4.567
	point
	-176.429,-5.872,-6.928
	point
	-176.337,-6.116,-8.542
	point
	-176.405,-6.376,-10.122
	reverse


// Pedestrian number 172

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-180.871,-8.504,-21.449
	point
	-180.128,-8.799,-25.143
	point
	-179.896,-8.854,-25.811
	point
	-178.526,-9.042,-27.987
	reverse


// Pedestrian number 173

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-178.132,-9.078,-28.560
	point
	-175.555,-9.078,-29.629
	point
	-173.209,-9.078,-30.268
	point
	-170.662,-9.078,-32.453
	reverse


// Pedestrian number 174

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-170.287,-9.078,-32.745
	point
	-169.972,-9.078,-34.458
	point
	-168.781,-9.078,-35.482
	point
	-164.568,-9.078,-36.741
	reverse


// Pedestrian number 175

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-166.497,-9.078,-39.067
	point
	-164.967,-9.078,-39.826
	point
	-163.602,-9.078,-40.411
	point
	-158.816,-9.078,-39.141
	reverse


// Pedestrian number 176

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-93.141,-10.699,-46.567
	point
	-90.667,-11.282,-46.195
	point
	-88.743,-11.763,-45.902
	point
	-86.841,-12.221,-46.212
	point
	-83.983,-12.934,-45.274
	reverse


// Pedestrian number 177

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-79.598,-13.281,-47.890
	point
	-76.790,-13.067,-46.072
	point
	-76.641,-13.072,-45.976
	point
	-74.152,-13.200,-44.051
	reverse


// Pedestrian number 178

5				// Ref num
7				// Number of instructions
6				// Initial instruction

	point
	-63.452,-15.005,-45.914
	point
	-59.726,-15.561,-45.200
	point
	-56.465,-15.561,-44.719
	point
	-55.502,-15.561,-44.850
	point
	-54.827,-15.561,-44.541
	point
	-54.827,-15.561,-44.541
	reverse


// Pedestrian number 179

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-50.902,-15.561,-41.216
	point
	-48.469,-15.561,-41.442
	point
	-46.856,-15.561,-41.425
	point
	-44.620,-15.561,-41.528
	reverse


// Pedestrian number 180

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-51.913,-15.561,-41.452
	point
	-54.157,-15.561,-41.768
	point
	-56.903,-15.561,-42.016
	reverse


// Pedestrian number 181

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-58.522,-15.561,-45.328
	point
	-57.228,-15.561,-44.640
	point
	-53.892,-15.561,-44.153
	point
	-52.330,-15.561,-44.363
	reverse


// Pedestrian number 182

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-60.416,-15.465,-45.270
	point
	-61.681,-15.280,-45.454
	point
	-64.002,-14.903,-45.808
	point
	-65.282,-14.658,-46.072
	reverse


// Pedestrian number 183

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-33.680,-15.561,-48.367
	point
	-29.151,-15.561,-47.717
	point
	-23.574,-15.561,-49.720
	reverse


// Pedestrian number 184

29				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-28.036,-15.561,-52.219
	point
	-29.046,-15.561,-51.305
	point
	-30.114,-15.561,-50.544
	point
	-31.076,-15.561,-50.004
	reverse


// Pedestrian number 185

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-27.654,-15.561,-47.388
	point
	-28.060,-15.561,-45.289
	point
	-28.902,-15.561,-43.269
	reverse


// Pedestrian number 186

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-18.146,-15.561,-61.368
	point
	-16.833,-15.561,-64.439
	point
	-15.727,-15.547,-68.677
	reverse


// Pedestrian number 187

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-18.611,-15.561,-60.084
	point
	-18.493,-15.561,-61.007
	point
	-15.497,-15.515,-70.280
	reverse


// Pedestrian number 188

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-18.380,-15.539,-69.591
	point
	-18.681,-15.518,-68.230
	point
	-19.311,-15.562,-66.305
	point
	-19.974,-15.561,-64.060
	point
	-20.299,-15.561,-63.560
	reverse


// Pedestrian number 189

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-18.388,-15.521,-70.426
	point
	-17.230,-15.495,-71.950
	point
	-15.033,-15.495,-73.694
	point
	-15.044,-15.495,-75.395
	reverse


// Pedestrian number 190

3				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-14.173,-14.288,-115.232
	point
	-12.458,-14.162,-117.244
	point
	-11.531,-14.109,-118.322
	point
	-11.367,-14.010,-120.702
	point
	-11.328,-14.015,-120.886
	point
	-11.564,-14.210,-121.700
	reverse


// Pedestrian number 191

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-11.554,-14.326,-114.336
	point
	-12.126,-14.253,-115.646
	point
	-13.671,-14.128,-118.100
	point
	-13.738,-14.154,-118.514
	point
	-14.235,-14.340,-120.942
	reverse


// Pedestrian number 192

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-14.431,-14.362,-114.006
	point
	-14.209,-14.161,-117.414
	point
	-14.245,-14.245,-119.162
	reverse


// Pedestrian number 193

29				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	-14.019,-14.830,-124.818
	point
	-13.509,-15.444,-127.889
	point
	-11.893,-15.631,-131.178
	point
	-12.495,-15.631,-131.975
	point
	-12.980,-15.631,-133.519
	point
	-14.167,-15.631,-134.831
	point
	-15.643,-15.631,-136.253
	reverse


// Pedestrian number 194

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-15.503,-15.631,-132.103
	point
	-11.967,-15.594,-130.452
	point
	-11.549,-15.528,-129.287
	reverse


// Pedestrian number 195

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-11.584,-15.483,-128.504
	point
	-11.700,-15.576,-130.153
	point
	-12.536,-15.631,-132.708
	reverse


// Pedestrian number 196

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-17.200,-15.631,-133.775
	point
	-19.067,-15.629,-134.677
	point
	-21.511,-15.585,-137.659
	reverse


// Pedestrian number 197

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.188,-15.562,-137.478
	point
	-33.425,-15.562,-137.417
	point
	-38.063,-15.555,-137.825
	reverse


// Pedestrian number 198

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-37.519,-15.562,-134.767
	point
	-41.532,-15.437,-137.507
	point
	-42.737,-15.345,-137.747
	reverse


// Pedestrian number 199

13				// Ref num
5				// Number of instructions
2				// Initial instruction


	point
	-52.536,-14.601,-134.892
	point
	-54.431,-14.461,-134.946
	point
	-58.037,-14.201,-137.413
	point
	-59.248,-14.119,-138.455
	reverse


// Pedestrian number 200

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-61.996,-13.901,-136.617
	point
	-61.204,-13.916,-136.545
	point
	-58.575,-14.148,-134.805
	reverse


// Pedestrian number 201

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-61.172,-13.901,-133.827
	point
	-62.354,-13.901,-135.647
	point
	-64.597,-13.901,-135.750
	reverse


// Pedestrian number 202

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-78.384,-13.021,-140.037
	point
	-82.901,-12.812,-137.255
	point
	-86.013,-12.670,-137.159
	reverse


// Pedestrian number 203

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-89.978,-12.488,-137.208
	point
	-92.780,-12.357,-137.667
	point
	-98.558,-12.093,-137.310
	reverse


// Pedestrian number 204

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-164.897,-9.029,-141.292
	point
	-168.279,-8.767,-140.352
	point
	-169.487,-8.668,-139.876
	point
	-171.154,-8.530,-139.352
	reverse


// Pedestrian number 205

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-167.121,-8.860,-137.879
	point
	-168.014,-8.788,-137.578
	point
	-169.239,-8.690,-136.999
	reverse


// Pedestrian number 206

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-174.566,-8.230,-136.773
	point
	-175.795,-8.117,-135.328
	point
	-176.785,-8.026,-134.361
	point
	-177.411,-7.967,-133.357
	point
	-178.164,-7.895,-132.071
	reverse


// Pedestrian number 207

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-175.648,-8.132,-130.543
	point
	-176.472,-8.055,-129.160
	point
	-176.824,-8.022,-127.301
	point
	-177.463,-7.962,-123.708
	reverse


// Pedestrian number 208

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-179.881,-7.728,-118.107
	point
	-182.502,-7.468,-115.060
	point
	-183.518,-7.358,-113.824
	point
	-183.699,-6.793,-112.925
	reverse


// Pedestrian number 209

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-188.039,-6.870,-114.709
	point
	-190.069,-6.641,-113.765
	point
	-191.402,-6.484,-113.622
	point
	-193.168,-6.279,-113.335
	reverse


// Pedestrian number 210

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-199.733,-5.456,-110.360
	point
	-199.119,-5.069,-109.733
	point
	-198.364,-4.985,-109.470
	point
	-196.892,-5.166,-109.341
	point
	-195.723,-5.966,-109.956
	reverse


// Pedestrian number 211

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-201.463,-5.228,-110.850
	point
	-199.630,-5.469,-110.555
	point
	-198.233,-5.649,-110.207
	point
	-196.739,-5.838,-110.503
	point
	-196.414,-5.879,-110.232
	reverse


// Pedestrian number 212

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-195.802,-5.956,-113.173
	point
	-198.498,-5.616,-113.263
	point
	-200.035,-5.416,-113.415
	point
	-201.760,-5.191,-113.866
	point
	-203.892,-4.901,-114.969
	reverse


// Pedestrian number 213

1				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-203.170,-4.999,-111.287
	point
	-204.126,-4.867,-112.350
	point
	-205.630,-4.660,-112.790
	point
	-206.713,-4.508,-113.248
	point
	-208.206,-4.297,-114.389
	point
	-209.045,-4.174,-114.956
	reverse


// Pedestrian number 214

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-208.288,-4.285,-118.682
	point
	-209.033,-4.169,-119.281
	point
	-209.737,-4.050,-120.532
	point
	-210.064,-3.995,-121.123
	point
	-210.623,-3.889,-123.040
	reverse


// Pedestrian number 215

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-214.008,-3.465,-124.467
	point
	-213.698,-3.484,-122.753
	point
	-213.185,-3.555,-121.988
	point
	-213.022,-3.582,-121.021
	reverse


// Pedestrian number 216

29				// Ref num
9				// Number of instructions
5				// Initial instruction

	point
	-210.892,-3.885,-123.878
	point
	-212.017,-3.744,-126.687
	point
	-211.713,-3.774,-127.972
	point
	-212.090,-3.720,-128.330
	point
	-212.071,-3.717,-128.962
	point
	-211.915,-3.737,-130.228
	point
	-212.109,-3.715,-131.658
	point
	-212.803,-3.621,-134.944
	reverse


// Pedestrian number 217

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-214.005,-3.464,-137.958
	point
	-214.545,-3.400,-139.444
	point
	-215.451,-3.325,-141.219
	point
	-215.887,-3.274,-141.797
	point
	-216.623,-3.208,-143.140
	reverse


// Pedestrian number 218

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-220.808,-2.963,-142.879
	point
	-220.916,-2.427,-142.407
	point
	-220.608,-2.227,-141.860
	reverse


// Pedestrian number 219

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-217.864,-3.159,-139.088
	point
	-217.953,-2.966,-138.941
	point
	-217.926,-2.739,-138.378
	point
	-217.757,-2.537,-137.481
	reverse


// Pedestrian number 220

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-218.020,-3.154,-139.890
	point
	-218.784,-3.133,-141.209
	point
	-219.332,-3.118,-142.147
	point
	-220.767,-3.087,-143.468
	point
	-222.002,-3.059,-144.447
	reverse


// Pedestrian number 221

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-221.117,-3.071,-147.339
	point
	-221.770,-3.063,-147.743
	point
	-223.903,-3.018,-148.851
	point
	-226.591,-2.962,-150.613
	reverse


// Pedestrian number 222

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-230.681,-2.863,-152.229
	point
	-229.772,-2.879,-151.728
	point
	-228.778,-2.899,-151.598
	point
	-227.521,-2.465,-151.751
	reverse


// Pedestrian number 223

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-231.665,-2.845,-152.564
	point
	-233.043,-2.856,-152.639
	point
	-234.060,-2.806,-152.317
	reverse


// Pedestrian number 224

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-235.199,-2.734,-148.686
	point
	-235.321,-2.719,-148.387
	point
	-235.541,-2.713,-147.544
	reverse


// Pedestrian number 225

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-237.421,-2.731,-150.636
	point
	-237.956,-2.717,-150.020
	point
	-239.148,-2.700,-147.260
	reverse


// Pedestrian number 226

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-239.394,-2.695,-146.363
	point
	-238.514,-2.706,-148.017
	point
	-238.122,-2.711,-148.836
	point
	-237.989,-2.714,-149.518
	reverse


// Pedestrian number 227

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-234.193,-2.780,-149.292
	point
	-234.523,-2.762,-149.024
	point
	-235.733,-2.741,-147.978
	point
	-236.225,-2.705,-146.210
	reverse


// Pedestrian number 228

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-233.743,-2.796,-149.489
	point
	-233.018,-2.828,-149.670
	point
	-231.980,-2.846,-149.519
	reverse


// Pedestrian number 229

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-237.762,-2.682,-142.292
	point
	-238.988,-2.665,-139.503
	point
	-240.981,-2.654,-138.347
	point
	-243.640,-2.635,-136.066
	point
	-244.050,-2.630,-135.209
	reverse


// Pedestrian number 230

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-242.575,-2.650,-138.481
	point
	-241.791,-2.662,-139.986
	point
	-240.409,-2.682,-144.017
	reverse


// Pedestrian number 231

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-235.696,-2.711,-147.185
	point
	-236.687,-2.708,-146.130
	point
	-236.887,-2.693,-144.744
	point
	-237.605,-2.685,-142.872
	reverse


// Pedestrian number 232

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-237.685,-2.683,-142.634
	point
	-238.632,-2.674,-141.185
	point
	-240.579,-2.640,-135.349
	reverse


// Pedestrian number 233

29				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-241.063,-2.634,-134.364
	point
	-241.720,-2.626,-133.080
	point
	-242.694,-2.611,-130.614
	point
	-243.371,-2.601,-128.796
	reverse


// Pedestrian number 234

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-246.510,-2.595,-129.308
	point
	-246.510,-2.595,-129.308
	point
	-241.963,-2.618,-131.668
	point
	-241.075,-1.949,-132.197
	reverse


// Pedestrian number 235

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-246.760,-2.592,-128.747
	point
	-247.714,-2.576,-125.882
	point
	-248.654,-2.565,-124.034
	reverse


// Pedestrian number 236

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-250.127,-2.552,-120.536
	point
	-250.502,-2.552,-119.241
	point
	-251.703,-2.552,-118.814
	reverse


// Pedestrian number 237

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-252.670,-2.555,-115.362
	point
	-255.373,-2.552,-114.200
	point
	-256.381,-2.552,-113.722
	reverse


// Pedestrian number 238

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-257.974,-2.552,-116.086
	point
	-258.710,-2.553,-113.521
	point
	-258.878,-2.552,-111.778
	reverse


// Pedestrian number 239

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-259.951,-2.552,-111.080
	point
	-261.131,-2.552,-110.314
	point
	-262.437,-2.552,-108.285
	point
	-263.675,-2.552,-105.560
	reverse


// Pedestrian number 240

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-249.319,-2.552,-113.961
	point
	-248.765,-2.556,-115.149
	point
	-248.531,-2.556,-116.031
	reverse


// Pedestrian number 241

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-251.094,-2.553,-118.841
	point
	-251.966,-2.553,-118.639
	point
	-254.392,-2.553,-114.695
	reverse


// Pedestrian number 242

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-252.938,-2.553,-118.360
	point
	-254.900,-2.553,-117.529
	point
	-255.599,-2.553,-117.270
	point
	-256.842,-2.552,-116.703
	reverse


// Pedestrian number 243

13				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-256.254,-1.949,-118.131
	point
	-254.857,-2.538,-117.934
	point
	-254.685,-2.551,-117.868
	point
	-252.065,-2.555,-115.115
	point
	-249.649,-2.552,-113.015
	point
	-249.474,-2.375,-112.792
	reverse


// Pedestrian number 244

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-248.059,-2.552,-116.864
	point
	-253.718,-2.552,-118.154
	point
	-255.578,-2.553,-116.628
	point
	-263.178,-2.552,-112.017
	reverse


// Pedestrian number 245

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-267.119,-2.552,-105.096
	point
	-268.950,-2.552,-100.688
	point
	-268.972,-2.552,-99.885
	point
	-268.770,-2.552,-98.700
	reverse


// Pedestrian number 246

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-265.747,-2.552,-102.873
	point
	-266.213,-2.552,-102.369
	point
	-267.388,-2.552,-101.191
	point
	-268.140,-2.552,-99.290
	reverse


// Pedestrian number 247

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-268.510,-2.552,-96.082
	point
	-269.419,-2.552,-95.982
	point
	-269.996,-2.552,-96.009
	point
	-270.965,-2.552,-95.727
	reverse


// Pedestrian number 248

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-270.612,-2.552,-93.539
	point
	-272.192,-2.552,-92.011
	point
	-273.328,-2.552,-89.927
	reverse


// Pedestrian number 249

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-271.353,-2.552,-86.780
	point
	-270.768,-2.552,-88.015
	point
	-271.118,-2.552,-89.710
	point
	-271.604,-2.552,-94.356
	reverse


// Pedestrian number 250

14				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-273.074,-2.552,-90.576
	point
	-271.751,-2.552,-91.215
	point
	-270.852,-2.552,-92.071
	point
	-270.782,-2.552,-92.561
	point
	-270.966,-2.552,-93.711
	point
	-270.543,-2.552,-94.764
	reverse


// Pedestrian number 251

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-269.747,-2.552,-95.901
	point
	-269.889,-2.552,-96.406
	point
	-269.582,-2.552,-97.218
	point
	-269.587,-2.552,-99.100
	reverse


// Pedestrian number 252

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-270.059,-2.552,-97.862
	point
	-270.202,-2.552,-96.389
	point
	-269.989,-2.552,-96.204
	point
	-269.321,-2.552,-95.592
	point
	-268.932,-2.552,-95.083
	reverse


// Pedestrian number 253

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-270.161,-2.552,-95.634
	point
	-270.684,-2.552,-95.088
	point
	-271.006,-2.552,-93.934
	point
	-270.847,-2.552,-93.521
	reverse


// Pedestrian number 254

8				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-269.579,-2.552,-93.592
	point
	-270.703,-2.552,-92.680
	point
	-270.711,-2.552,-91.995
	point
	-271.785,-2.552,-89.840
	point
	-274.849,-2.552,-86.565
	reverse


// Pedestrian number 255

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-276.199,-2.552,-83.962
	point
	-277.143,-2.552,-81.787
	point
	-276.119,-2.552,-78.714
	reverse


// Pedestrian number 256

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-277.056,-2.552,-77.404
	point
	-278.316,-2.552,-76.005
	point
	-282.674,-2.552,-75.077
	reverse


// Pedestrian number 257

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-282.977,-2.552,-74.724
	point
	-282.730,-2.544,-71.327
	point
	-284.335,-2.545,-67.078
	reverse


// Pedestrian number 258

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-285.338,-2.538,-71.991
	point
	-283.427,-2.552,-73.876
	point
	-280.490,-2.558,-73.152
	reverse


// Pedestrian number 259

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-283.911,-2.549,-73.598
	point
	-284.173,-2.545,-72.714
	point
	-283.355,-2.540,-70.791
	point
	-282.854,-2.552,-67.331
	reverse


// Pedestrian number 260

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-283.092,-2.539,-70.381
	point
	-282.398,-2.547,-71.752
	point
	-281.994,-2.552,-75.766
	reverse


// Pedestrian number 261

13				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-290.901,-2.611,-66.648
	point
	-288.910,-2.545,-67.798
	point
	-285.894,-2.539,-70.891
	point
	-285.276,-2.538,-71.726
	point
	-285.246,-2.538,-72.306
	point
	-284.425,-2.536,-73.187
	reverse


// Pedestrian number 262

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-301.475,-3.692,-66.697
	point
	-302.839,-3.869,-66.676
	point
	-304.337,-3.982,-66.926
	point
	-304.980,-4.043,-66.621
	point
	-305.100,-4.048,-66.229
	reverse


// Pedestrian number 263

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-305.706,-4.048,-65.861
	point
	-307.220,-4.048,-65.232
	point
	-308.040,-4.048,-64.304
	point
	-308.729,-4.048,-62.258
	reverse


// Pedestrian number 264

12				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-303.969,-3.932,-69.400
	point
	-305.848,-4.041,-69.120
	point
	-306.448,-4.048,-68.937
	point
	-308.740,-4.048,-67.573
	point
	-309.267,-4.048,-67.093
	reverse


// Pedestrian number 265

17				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-307.891,-4.048,-64.913
	point
	-308.340,-4.048,-64.183
	point
	-309.051,-4.048,-61.428
	point
	-309.025,-4.048,-59.326
	reverse


// Pedestrian number 266

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-308.805,-4.048,-58.997
	point
	-308.080,-4.048,-57.100
	point
	-307.767,-4.048,-56.761
	point
	-307.414,-4.048,-56.369
	reverse


// Pedestrian number 267

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-309.587,-4.048,-54.168
	point
	-310.881,-4.048,-57.725
	point
	-312.007,-4.048,-60.843
	reverse


// Pedestrian number 268

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-311.804,-4.048,-61.502
	point
	-310.921,-4.048,-64.048
	point
	-310.213,-4.048,-66.074
	reverse


// Pedestrian number 269

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-308.079,-4.048,-68.005
	point
	-308.182,-4.048,-63.287
	point
	-306.977,-3.161,-62.076
	point
	-306.926,-3.032,-61.235
	reverse


// Pedestrian number 270

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-307.824,-3.507,-61.157
	point
	-308.813,-4.048,-59.570
	point
	-308.793,-4.048,-58.301
	reverse


// Pedestrian number 271

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-307.130,-4.048,-55.946
	point
	-306.899,-4.048,-55.779
	point
	-305.834,-4.096,-55.090
	reverse


// Pedestrian number 272

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-304.480,-4.189,-54.490
	point
	-301.394,-4.602,-53.573
	point
	-298.731,-5.309,-52.973
	reverse


// Pedestrian number 273

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-301.548,-4.739,-50.540
	point
	-298.747,-5.509,-49.881
	point
	-294.961,-6.758,-49.008
	reverse


// Pedestrian number 274

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-294.532,-6.654,-51.923
	point
	-291.191,-7.824,-50.756
	point
	-290.127,-7.884,-50.524
	reverse


// Pedestrian number 275

5				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-289.188,-7.940,-50.205
	point
	-287.985,-8.005,-49.575
	point
	-286.891,-8.005,-45.905
	point
	-287.160,-8.005,-42.215
	point
	-287.398,-8.005,-40.596
	reverse


// Pedestrian number 276

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-284.490,-8.005,-43.511
	point
	-284.121,-8.005,-42.692
	point
	-283.543,-7.696,-41.533
	point
	-282.199,-6.852,-41.083
	reverse


// Pedestrian number 277

1				// Ref num
9				// Number of instructions
7				// Initial instruction

	point
	-284.061,-8.005,-41.127
	point
	-284.608,-8.005,-40.453
	point
	-284.884,-8.005,-39.560
	point
	-284.993,-8.005,-37.977
	point
	-287.371,-8.005,-34.764
	point
	-287.551,-7.986,-34.585
	point
	-287.611,-7.921,-34.413
	point
	-288.716,-7.151,-32.136
	reverse


// Pedestrian number 278

29				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-289.499,-8.005,-37.279
	point
	-288.412,-8.004,-38.154
	point
	-287.520,-8.005,-38.325
	point
	-284.597,-8.005,-39.560
	reverse


// Pedestrian number 279

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-287.740,-8.005,-39.147
	point
	-284.316,-8.005,-42.046
	point
	-284.425,-8.005,-44.507
	reverse


// Pedestrian number 280

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-284.152,-7.877,-44.685
	point
	-284.000,-7.508,-45.728
	point
	-283.980,-7.130,-46.951
	point
	-283.854,-6.798,-47.763
	reverse


// Pedestrian number 281

5				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-285.223,-8.005,-46.513
	point
	-286.407,-8.005,-43.838
	point
	-286.426,-8.005,-42.530
	point
	-287.079,-8.005,-41.616
	point
	-288.226,-8.005,-38.548
	reverse


// Pedestrian number 282

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-286.337,-8.005,-35.899
	point
	-290.809,-8.008,-35.344
	point
	-293.451,-8.166,-35.358
	point
	-296.326,-8.525,-35.300
	reverse


// Pedestrian number 283

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-294.880,-8.344,-35.505
	point
	-296.654,-8.568,-35.057
	point
	-298.035,-9.013,-34.785
	point
	-299.920,-9.442,-35.244
	reverse


// Pedestrian number 284

29				// Ref num
9				// Number of instructions
4				// Initial instruction

	point
	-298.103,-9.166,-32.271
	point
	-298.430,-9.285,-32.439
	point
	-298.882,-9.455,-32.377
	point
	-299.777,-9.776,-32.361
	point
	-300.623,-9.943,-32.472
	point
	-301.872,-10.077,-33.420
	point
	-303.143,-10.477,-33.677
	point
	-304.486,-10.909,-34.832
	reverse


// Pedestrian number 285

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-307.012,-11.793,-31.538
	point
	-309.669,-11.971,-32.758
	point
	-311.882,-11.971,-33.109
	point
	-313.365,-11.971,-32.132
	reverse


// Pedestrian number 286

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-312.356,-11.971,-32.852
	point
	-313.862,-11.971,-31.535
	point
	-315.467,-11.971,-29.014
	reverse


// Pedestrian number 287

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-312.483,-11.971,-28.242
	point
	-313.842,-11.971,-28.279
	point
	-315.790,-11.970,-27.237
	point
	-316.223,-11.971,-25.335
	reverse


// Pedestrian number 288

29				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-310.193,-11.971,-30.589
	point
	-311.153,-11.971,-30.196
	point
	-312.376,-11.970,-28.775
	point
	-313.233,-11.971,-26.534
	point
	-313.226,-11.971,-25.457
	reverse


// Pedestrian number 289

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-315.747,-11.971,-28.199
	point
	-316.031,-11.971,-26.501
	point
	-316.089,-11.970,-24.197
	point
	-314.094,-11.971,-19.618
	reverse


// Pedestrian number 290

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-311.120,-11.971,-20.670
	point
	-315.798,-11.970,-23.028
	point
	-316.008,-11.970,-23.627
	reverse


// Pedestrian number 291

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-315.036,-11.971,-21.178
	point
	-313.307,-11.971,-25.137
	point
	-312.906,-11.971,-28.068
	point
	-312.947,-11.971,-32.545
	reverse


// Pedestrian number 292

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-311.320,-11.971,-33.469
	point
	-309.793,-11.956,-33.640
	point
	-308.575,-11.841,-34.222
	point
	-307.413,-11.808,-34.660
	reverse


// Pedestrian number 293

12				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-310.494,-11.971,-33.931
	point
	-312.101,-11.970,-28.817
	point
	-313.131,-11.971,-26.533
	point
	-313.080,-11.971,-24.407
	point
	-312.879,-11.971,-23.506
	reverse


// Pedestrian number 294

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-309.599,-12.052,-19.766
	point
	-307.176,-12.105,-18.568
	point
	-304.902,-12.106,-18.046
	reverse


// Pedestrian number 295

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-303.618,-12.106,-17.323
	point
	-297.948,-12.106,-11.354
	point
	-295.342,-12.106,-9.547
	reverse


// Pedestrian number 296

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-294.592,-12.106,-12.659
	point
	-293.640,-12.106,-11.881
	point
	-290.160,-12.119,-9.516
	reverse


// Pedestrian number 297

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-293.474,-12.106,-8.167
	point
	-292.018,-12.119,-7.229
	point
	-291.375,-12.134,-6.629
	point
	-290.872,-12.106,-6.118
	reverse


// Pedestrian number 298

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-287.163,-12.203,-7.032
	point
	-286.617,-11.939,-7.076
	point
	-285.686,-11.252,-7.410
	reverse


// Pedestrian number 299

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-285.871,-12.313,-5.671
	point
	-283.815,-12.540,-3.074
	point
	-283.024,-12.625,-2.703
	point
	-282.159,-12.592,-2.212
	reverse


// Pedestrian number 300

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-275.947,-15.455,15.963
	point
	-274.403,-15.615,18.459
	point
	-268.921,-15.627,21.687
	reverse


// Pedestrian number 301

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-269.260,-15.627,21.154
	point
	-269.260,-15.627,21.154
	point
	-274.763,-15.617,19.424
	point
	-274.987,-15.613,18.556
	reverse


// Pedestrian number 302

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-275.048,-15.617,19.181
	point
	-275.197,-15.625,21.645
	point
	-274.156,-15.627,26.848
	point
	-275.075,-15.627,28.241
	reverse


// Pedestrian number 303

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-276.114,-15.627,28.865
	point
	-276.806,-15.627,28.757
	point
	-276.806,-15.627,28.757
	point
	-278.927,-15.627,27.563
	point
	-279.874,-15.627,27.672
	reverse


// Pedestrian number 304

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-275.915,-15.627,28.331
	point
	-274.419,-15.627,26.937
	point
	-273.867,-15.627,26.357
	reverse


// Pedestrian number 305

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-269.464,-15.627,20.822
	point
	-272.578,-15.622,21.014
	point
	-273.043,-15.622,20.905
	point
	-275.045,-15.620,20.332
	reverse


// Pedestrian number 306

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-271.521,-15.627,23.166
	point
	-270.772,-15.627,23.565
	point
	-267.721,-15.627,22.818
	reverse


// Pedestrian number 307

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-264.867,-15.627,23.968
	point
	-266.649,-15.627,23.637
	point
	-269.492,-15.622,21.493
	point
	-275.319,-15.623,21.089
	reverse


// Pedestrian number 308

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-270.668,-15.621,19.419
	point
	-269.911,-15.627,20.721
	point
	-270.254,-15.629,22.299
	point
	-270.389,-15.627,23.600
	point
	-269.725,-15.627,24.812
	reverse


// Pedestrian number 309

14				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-272.612,-15.627,23.147
	point
	-273.271,-15.627,24.415
	point
	-273.594,-15.627,24.889
	point
	-273.671,-15.627,25.698
	point
	-275.341,-15.627,26.548
	point
	-278.109,-15.627,26.682
	reverse


// Pedestrian number 310

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-280.589,-15.627,33.937
	point
	-280.646,-15.627,35.766
	point
	-279.847,-15.627,37.526
	reverse


// Pedestrian number 311

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-282.105,-15.627,40.554
	point
	-281.144,-15.627,41.464
	point
	-280.896,-15.627,45.967
	reverse


// Pedestrian number 312

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-275.261,-16.364,57.993
	point
	-275.306,-16.591,59.619
	point
	-274.518,-16.875,61.463
	reverse


// Pedestrian number 313

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-274.434,-16.902,61.736
	point
	-275.504,-17.083,63.476
	point
	-276.184,-17.419,66.389
	point
	-275.677,-17.638,68.356
	reverse


// Pedestrian number 314

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-276.525,-17.276,65.334
	point
	-276.656,-17.120,64.043
	point
	-277.100,-16.921,62.514
	reverse


// Pedestrian number 315

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-274.600,-16.823,61.127
	point
	-277.527,-16.613,60.288
	point
	-277.928,-16.431,59.083
	reverse


// Pedestrian number 316

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-277.329,-16.783,61.450
	point
	-274.153,-17.132,63.567
	point
	-273.629,-17.375,65.448
	reverse


// Pedestrian number 317

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-272.091,-18.286,72.098
	point
	-273.900,-18.648,76.202
	point
	-273.648,-18.772,77.788
	reverse


// Pedestrian number 318

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-273.480,-18.815,78.534
	point
	-272.702,-18.907,81.642
	point
	-272.380,-18.909,83.736
	reverse


// Pedestrian number 319

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-272.125,-18.910,84.419
	point
	-268.699,-18.913,87.433
	point
	-268.551,-18.914,88.454
	reverse


// Pedestrian number 320

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-267.860,-18.915,90.476
	point
	-267.589,-18.915,92.464
	point
	-267.190,-18.917,93.251
	reverse


// Pedestrian number 321

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-267.361,-18.915,93.750
	point
	-267.103,-18.915,94.906
	point
	-266.904,-18.915,96.369
	reverse


// Pedestrian number 322

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-266.662,-18.915,97.291
	point
	-265.214,-18.915,103.269
	point
	-263.493,-18.915,105.492
	reverse


// Pedestrian number 323

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-264.258,-18.915,103.497
	point
	-262.888,-18.915,103.594
	point
	-259.906,-18.916,102.546
	point
	-258.473,-18.916,102.074
	reverse


// Pedestrian number 324

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-260.209,-18.915,104.902
	point
	-261.442,-18.915,105.097
	point
	-262.568,-18.915,105.461
	point
	-264.052,-18.915,105.634
	reverse


// Pedestrian number 325

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-264.786,-18.914,105.968
	point
	-266.973,-18.915,105.454
	point
	-268.860,-18.916,104.565
	reverse


// Pedestrian number 326

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-265.318,-18.915,102.577
	point
	-267.780,-18.916,104.111
	point
	-271.038,-18.916,107.321
	reverse


// Pedestrian number 327

14				// Ref num

4				// Number of instructions
2				// Initial instruction

	point
	-271.659,-18.916,107.585
	point
	-272.700,-18.916,107.682
	point
	-275.621,-18.916,108.434
	reverse


// Pedestrian number 328

12				// Ref num
7				// Number of instructions
5				// Initial instruction

	point
	-277.279,-18.916,106.409
	point
	-278.052,-18.916,106.785
	point
	-279.855,-18.916,106.897
	point
	-280.732,-18.916,107.190
	point
	-281.522,-18.916,107.353
	point
	-287.395,-18.916,108.702
	reverse


// Pedestrian number 329

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-287.781,-18.915,109.007
	point
	-287.005,-18.915,109.530
	point
	-284.483,-18.915,110.371
	reverse


// Pedestrian number 330

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-285.320,-18.915,110.565
	point
	-283.753,-18.914,110.043
	point
	-282.909,-18.914,108.214
	point
	-282.223,-18.916,107.447
	reverse


// Pedestrian number 331

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-278.529,-18.914,108.997
	point
	-276.784,-18.916,108.745
	point
	-272.298,-18.916,105.406
	reverse


// Pedestrian number 332

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-271.767,-18.916,105.116
	point
	-270.238,-18.916,105.152
	point
	-268.600,-18.916,104.356
	reverse


// Pedestrian number 333

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-257.403,-18.916,104.343
	point
	-256.166,-18.915,103.924
	point
	-253.647,-18.916,101.001
	reverse


// Pedestrian number 334

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-251.203,-18.916,100.337
	point
	-248.252,-18.916,101.620
	point
	-243.906,-18.916,101.111
	reverse


// Pedestrian number 335

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-241.962,-18.915,100.665
	point
	-239.599,-18.916,97.883
	point
	-236.994,-18.916,97.068
	point
	-236.052,-18.916,96.823
	reverse


// Pedestrian number 336

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-230.100,-18.916,95.496
	point
	-227.497,-18.916,96.367
	point
	-224.827,-18.916,96.739
	reverse


// Pedestrian number 337

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-224.247,-18.916,96.663
	point
	-223.229,-18.916,95.255
	point
	-222.475,-18.916,93.876
	reverse


// Pedestrian number 338

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-222.129,-18.916,96.112
	point
	-225.941,-18.916,95.009
	point
	-227.570,-18.916,94.916
	reverse


// Pedestrian number 339

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-230.675,-18.916,95.681
	point
	-232.337,-18.916,98.317
	point
	-234.208,-18.916,98.923
	reverse


// Pedestrian number 340

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-236.473,-18.916,99.195
	point
	-237.403,-18.916,99.547
	point
	-239.771,-18.916,99.977
	reverse


// Pedestrian number 341

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-244.636,-18.916,101.256
	point
	-243.045,-18.915,100.927
	point
	-240.603,-18.916,100.428
	reverse


// Pedestrian number 342

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-241.676,-18.916,97.872
	point
	-242.133,-18.915,99.371
	point
	-243.668,-18.916,101.059
	reverse


// Pedestrian number 343

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-258.016,-18.916,101.915
	point
	-256.635,-18.915,101.778
	point
	-251.856,-18.916,102.896
	reverse


// Pedestrian number 344

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point

	-242.661,-18.915,94.750
	point
	-243.590,-18.915,93.460
	point
	-245.618,-18.915,91.881
	point
	-245.822,-18.915,91.091
	point
	-246.407,-18.915,89.219
	reverse


// Pedestrian number 345

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-248.346,-18.916,88.619
	point
	-248.651,-18.916,88.589
	point
	-250.594,-18.916,89.034
	point
	-253.616,-18.916,89.690
	reverse


// Pedestrian number 346

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-256.635,-18.916,90.560
	point
	-253.937,-18.916,89.438
	point
	-252.016,-18.916,89.394
	point
	-250.196,-18.916,87.138
	reverse


// Pedestrian number 347

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-248.563,-18.916,86.478
	point
	-249.387,-18.916,87.020
	point
	-253.946,-18.916,87.627
	reverse


// Pedestrian number 348

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-255.604,-18.916,87.920
	point
	-257.768,-18.915,90.792
	point
	-258.445,-18.916,90.861
	reverse


// Pedestrian number 349

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-240.526,-18.915,84.616
	point
	-239.882,-18.915,84.350
	point
	-235.910,-18.915,83.580
	reverse


// Pedestrian number 350

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-235.968,-18.916,85.765
	point
	-239.119,-18.916,86.048
	point
	-240.148,-18.916,86.797
	point
	-241.421,-18.916,86.919
	point
	-242.623,-18.916,87.273
	reverse


// Pedestrian number 351

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-243.849,-18.916,87.634
	point
	-244.802,-18.915,85.567
	point
	-245.180,-18.914,83.335
	point
	-245.664,-18.913,82.051
	point
	-245.604,-18.912,81.275
	reverse


// Pedestrian number 352

17				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-249.726,-18.892,75.676
	point
	-247.778,-18.859,74.234
	point
	-247.643,-18.786,72.308
	point
	-247.717,-18.737,71.682
	reverse


// Pedestrian number 353

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-246.677,-18.906,75.374
	point
	-248.844,-18.909,77.993
	point
	-248.383,-18.911,80.406
	reverse


// Pedestrian number 354

12				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-249.638,-18.916,89.036
	point
	-246.949,-18.915,88.290
	point
	-244.024,-18.916,87.838
	point
	-242.617,-18.915,85.084
	point
	-241.820,-18.915,84.752
	reverse


// Pedestrian number 355

29				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-230.822,-18.916,84.707
	point
	-229.908,-18.916,84.146
	point
	-228.819,-18.916,84.256
	point
	-226.632,-18.916,83.831
	point
	-224.363,-18.916,81.696
	reverse


// Pedestrian number 356

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-223.842,-18.916,82.470
	point
	-225.192,-18.916,81.939
	point
	-227.269,-18.916,81.629
	reverse


// Pedestrian number 357

17				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-225.378,-18.916,81.111
	point
	-227.952,-18.917,81.760
	point
	-232.958,-18.916,85.192
	reverse


// Pedestrian number 358

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-233.629,-18.916,85.244
	point
	-235.137,-18.915,85.428
	point
	-237.883,-18.916,84.002
	reverse


// Pedestrian number 359

1				// Ref num
7				// Number of instructions
5				// Initial instruction

	point
	-234.603,-18.916,83.075
	point
	-237.291,-18.916,84.277
	point
	-239.141,-18.916,84.414
	point
	-240.060,-18.916,84.651
	point
	-241.329,-18.914,84.995
	point
	-243.182,-18.916,87.368
	reverse


// Pedestrian number 360

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-243.846,-18.915,89.669
	point
	-243.772,-18.915,91.633
	point
	-242.658,-18.915,94.584
	reverse


// Pedestrian number 361

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-225.214,-18.916,96.958
	point
	-224.474,-18.916,96.468
	point
	-224.210,-18.916,95.897
	point
	-223.458,-18.916,94.270
	reverse


// Pedestrian number 362

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-289.800,-18.915,98.099
	point
	-287.528,-18.915,97.391
	point
	-286.992,-18.915,95.275
	reverse


// Pedestrian number 363

1				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-286.584,-18.916,95.062
	point
	-285.122,-18.916,94.775
	point
	-284.024,-18.916,94.553
	point
	-282.993,-18.916,94.208
	point
	-281.769,-18.916,94.357
	point
	-279.257,-18.916,93.459
	reverse


// Pedestrian number 364

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-278.403,-18.916,93.124
	point
	-276.421,-18.916,92.787
	point
	-273.351,-18.916,92.168
	reverse


// Pedestrian number 365

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-276.536,-18.916,95.028
	point
	-277.883,-18.916,95.336
	point
	-279.189,-18.916,95.195
	point
	-281.667,-18.916,96.371
	reverse


// Pedestrian number 366

17				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-280.027,-18.916,95.991
	point
	-278.853,-18.916,95.361
	point
	-277.985,-18.916,93.932
	point
	-277.008,-18.916,92.852
	reverse


// Pedestrian number 367

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-275.923,-18.916,92.597
	point
	-274.557,-18.916,92.760
	point
	-272.792,-18.916,92.171
	point
	-267.385,-18.915,90.680
	reverse


// Pedestrian number 368

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-249.956,-17.586,62.402
	point
	-253.447,-17.126,59.029
	point
	-253.663,-16.985,57.797
	reverse


// Pedestrian number 369

17				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-252.848,-17.401,61.382
	point
	-251.877,-16.860,56.561
	point
	-251.740,-16.522,54.063
	point
	-252.232,-16.232,51.727
	reverse


// Pedestrian number 370

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-255.093,-16.136,51.243
	point
	-255.367,-16.081,50.658
	point
	-253.478,-15.866,48.171
	reverse


// Pedestrian number 371

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-259.604,-15.627,19.171
	point
	-263.137,-15.657,16.034
	point
	-263.787,-15.657,14.920
	reverse


// Pedestrian number 372

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-266.962,-15.680,-2.238
	point
	-267.167,-15.791,-4.341
	point
	-267.122,-15.904,-6.260
	reverse


// Pedestrian number 373

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-264.090,-15.692,-2.653
	point
	-264.235,-15.791,-4.428
	point
	-264.105,-15.851,-5.513
	point
	-264.434,-16.113,-10.220
	point
	-264.228,-16.144,-10.802
	reverse


// Pedestrian number 374

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-264.208,-16.184,-11.530
	point
	-264.744,-16.682,-17.259
	point
	-265.236,-16.733,-17.799
	point
	-265.035,-16.840,-18.964
	reverse


// Pedestrian number 375

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-119.834,-13.901,-123.061
	point
	-117.564,-13.901,-123.633
	point
	-115.680,-13.901,-123.977
	reverse


// Pedestrian number 376

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-109.031,-13.901,-125.677
	point
	-105.715,-13.901,-126.182
	point
	-102.975,-13.901,-127.024
	reverse


// Pedestrian number 377

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-101.611,-13.901,-127.207
	point
	-99.451,-13.901,-127.706
	point
	-96.372,-13.901,-128.519
	point
	-93.558,-13.901,-129.240
	reverse


// Pedestrian number 378

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-91.666,-13.901,-126.863
	point
	-90.408,-13.901,-126.956
	point
	-87.817,-13.901,-127.590
	point
	-86.489,-13.901,-128.258
	point
	-85.750,-13.901,-130.193
	reverse


// Pedestrian number 379

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-84.949,-13.901,-131.149
	point
	-80.765,-13.901,-129.335
	point
	-79.234,-13.901,-129.693
	reverse


// Pedestrian number 380

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-77.973,-13.901,-129.919
	point
	-76.168,-13.900,-133.065
	point
	-73.672,-13.901,-133.667
	reverse


// Pedestrian number 381

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-83.065,-13.901,-131.665
	point
	-84.022,-13.901,-131.468
	point
	-87.263,-13.901,-130.582
	point
	-88.684,-13.901,-130.165
	point
	-89.755,-13.901,-129.999
	reverse


// Pedestrian number 382

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-91.735,-13.901,-126.627
	point
	-93.750,-13.901,-126.619
	point
	-97.768,-13.901,-125.274
	reverse


// Pedestrian number 383

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-98.194,-13.901,-125.123
	point
	-101.434,-13.901,-124.704
	point
	-103.321,-13.901,-124.105
	point
	-104.968,-13.901,-123.493
	reverse


// Pedestrian number 384

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-111.649,-13.901,-124.905
	point
	-113.716,-13.901,-122.206
	point
	-115.137,-13.901,-121.271
	point
	-116.340,-13.901,-120.804
	point
	-118.246,-13.901,-120.392
	reverse


// Pedestrian number 385

3				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-121.292,-13.901,-119.788
	point
	-123.196,-13.901,-119.728
	point
	-124.535,-13.901,-118.956
	point
	-125.394,-13.901,-118.697
	point
	-126.965,-13.901,-118.549
	point
	-128.145,-13.901,-118.237
	reverse


// Pedestrian number 386

1				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-132.275,-13.901,-119.952
	point
	-135.456,-13.817,-119.294
	point
	-137.788,-13.901,-118.554
	point
	-140.212,-13.901,-118.253
	point
	-140.870,-13.901,-117.947
	point
	-141.976,-13.977,-117.808
	reverse


// Pedestrian number 387

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-145.000,-14.111,-114.419
	point
	-147.714,-14.343,-113.757
	point
	-148.978,-14.441,-113.374
	point
	-150.077,-14.520,-113.405
	point
	-151.259,-14.618,-112.759
	reverse


// Pedestrian number 388

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-154.072,-14.744,-114.431
	point
	-156.939,-14.906,-113.855
	point
	-158.349,-14.962,-112.972
	point
	-160.074,-15.001,-112.697
	reverse


// Pedestrian number 389

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-163.051,-15.344,-108.087
	point
	-164.301,-15.485,-107.578
	point
	-166.077,-15.909,-106.568
	point
	-166.565,-16.010,-106.127
	point
	-167.904,-16.244,-105.358
	reverse


// Pedestrian number 390

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-169.241,-16.457,-104.871
	point
	-170.250,-16.652,-104.404
	point
	-172.089,-17.158,-102.408
	point
	-173.911,-17.623,-100.836
	reverse


// Pedestrian number 391

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-183.381,-17.667,-94.703
	point
	-185.582,-17.667,-93.495
	point
	-187.395,-17.667,-92.805
	point
	-188.499,-17.667,-92.221
	reverse


// Pedestrian number 392

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-189.212,-17.667,-92.062
	point
	-193.357,-17.667,-93.250
	point
	-194.419,-17.667,-93.268
	point
	-195.772,-17.667,-92.864
	point
	-196.934,-17.667,-92.532
	reverse


// Pedestrian number 393

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-200.913,-17.667,-89.040
	point
	-202.033,-17.667,-88.797
	point
	-204.014,-17.667,-88.626
	point
	-205.983,-17.667,-88.356
	reverse


// Pedestrian number 394

1				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-205.578,-17.667,-91.182
	point
	-207.331,-17.667,-90.489
	point
	-208.538,-17.667,-90.705
	point
	-209.648,-17.667,-91.079
	point
	-212.465,-17.667,-91.333
	reverse


// Pedestrian number 395

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-222.421,-17.667,-90.108
	point
	-225.237,-17.667,-90.657
	point
	-228.646,-17.667,-94.731
	reverse


// Pedestrian number 396

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-222.851,-17.667,-92.715
	point
	-225.380,-17.667,-93.718
	point
	-230.772,-17.667,-92.287
	reverse


// Pedestrian number 397

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-231.315,-17.667,-92.144
	point
	-236.308,-17.667,-91.844
	point
	-237.168,-17.667,-90.632
	point
	-238.428,-17.667,-88.917
	reverse


// Pedestrian number 398

14				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-234.244,-17.667,-90.010
	point
	-234.876,-17.667,-89.574
	point
	-235.287,-17.667,-88.471
	point
	-236.050,-17.667,-87.275
	point
	-237.103,-17.667,-85.875
	point
	-237.296,-17.667,-85.318
	reverse


// Pedestrian number 399

8				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-239.589,-17.667,-87.027
	point
	-238.759,-17.667,-88.124
	point
	-233.632,-17.667,-90.893
	point
	-233.018,-17.667,-91.433
	point
	-231.069,-17.667,-95.099
	reverse


// Pedestrian number 400

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-229.490,-17.667,-94.925
	point
	-232.882,-17.667,-94.231
	point
	-234.970,-17.667,-93.341
	reverse


// Pedestrian number 401

29				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-235.881,-17.667,-92.742
	point
	-237.468,-17.667,-89.190
	point
	-237.576,-17.667,-86.398
	point
	-237.810,-17.667,-84.738
	point
	-239.074,-17.667,-83.249
	reverse


// Pedestrian number 402

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-239.940,-17.667,-81.940
	point
	-241.389,-17.667,-80.509
	point
	-242.760,-17.667,-79.235
	point
	-243.512,-17.667,-78.624
	reverse


// Pedestrian number 403

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-245.986,-17.667,-80.303
	point
	-244.407,-17.667,-81.344
	point
	-243.769,-17.667,-82.153
	point
	-242.335,-17.667,-83.856
	reverse


// Pedestrian number 404

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-241.138,-17.667,-85.195
	point
	-241.675,-17.667,-83.809
	point
	-242.744,-17.667,-82.883
	point
	-243.966,-17.667,-78.255
	reverse


// Pedestrian number 405

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-245.521,-17.667,-77.607
	point
	-247.017,-17.667,-77.002
	point
	-249.465,-17.667,-76.193
	reverse


// Pedestrian number 406

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-251.893,-17.667,-74.479
	point
	-256.607,-17.667,-74.979
	point
	-259.508,-17.667,-74.238
	reverse



// Pedestrian number 407

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-264.458,-17.667,-70.671
	point
	-265.318,-17.667,-65.596
	point
	-266.224,-17.667,-63.769
	point
	-266.944,-17.667,-63.032
	point
	-267.397,-17.667,-61.949
	reverse


// Pedestrian number 408

14				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-268.182,-17.667,-60.830
	point
	-267.928,-17.667,-62.571
	point
	-266.643,-17.667,-64.806
	point
	-266.713,-17.667,-67.852
	point
	-265.824,-17.667,-68.878
	reverse


// Pedestrian number 409

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-264.989,-17.667,-69.779
	point
	-262.826,-17.667,-72.031
	point
	-262.093,-17.667,-72.685
	point
	-260.609,-17.667,-73.550
	point
	-257.839,-17.667,-74.706
	reverse


// Pedestrian number 410

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-255.378,-17.667,-75.598
	point
	-252.351,-17.667,-77.418
	point
	-250.216,-17.667,-79.156
	reverse


// Pedestrian number 411

29				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-252.969,-17.667,-73.850
	point
	-256.132,-17.667,-73.995
	point
	-258.440,-17.667,-73.304
	point
	-261.503,-17.667,-69.874
	point
	-264.039,-17.667,-66.725
	reverse


// Pedestrian number 412

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-271.027,-17.667,-61.583
	point
	-272.535,-17.667,-58.840
	point
	-274.032,-17.667,-52.526
	reverse


// Pedestrian number 413

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-271.331,-17.667,-49.860
	point
	-271.311,-17.667,-48.130
	point
	-271.297,-17.667,-46.380
	point
	-271.427,-17.667,-44.970
	point
	-271.157,-17.667,-43.681
	reverse


// Pedestrian number 414

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-268.855,-17.667,-30.778
	point
	-268.559,-17.667,-30.243
	point
	-267.896,-17.667,-29.450
	reverse


// Pedestrian number 415

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-271.924,-17.667,-32.767
	point
	-272.570,-17.667,-36.082
	point
	-272.706,-17.667,-37.178
	point
	-273.465,-17.667,-39.753
	reverse


// Pedestrian number 416

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-270.747,-17.667,-40.455
	point
	-272.866,-17.667,-36.484
	point
	-272.339,-17.667,-34.237
	reverse


// Pedestrian number 417

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-271.845,-17.667,-31.923
	point
	-269.676,-17.667,-34.570
	point
	-270.281,-17.667,-37.579
	reverse


// Pedestrian number 418

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-270.493,-17.667,-38.015
	point
	-271.410,-17.667,-36.914
	point
	-272.664,-17.667,-35.041
	point
	-272.133,-17.667,-33.504
	reverse


// Pedestrian number 419

8				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-271.174,-17.667,-31.072
	point
	-271.721,-17.667,-33.570
	point
	-272.730,-17.667,-35.622
	point
	-273.163,-17.667,-37.531
	point
	-271.921,-17.667,-39.174
	point
	-271.089,-17.667,-42.821
	reverse


// Pedestrian number 420

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-270.053,-17.667,-26.369
	point
	-269.945,-17.667,-27.000
	point
	-270.647,-17.667,-28.010
	reverse


// Pedestrian number 421

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-269.690,-17.667,-25.496
	point
	-269.842,-17.667,-25.983
	point
	-270.298,-17.667,-26.927
	point
	-270.337,-17.667,-28.194
	point
	-270.756,-17.667,-28.940
	reverse


// Pedestrian number 422

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-269.406,-17.667,-25.153
	point
	-268.996,-17.666,-24.854
	point
	-268.898,-17.355,-22.439
	reverse


// Pedestrian number 423

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-266.252,-17.443,-23.823
	point
	-265.947,-17.238,-22.254
	point
	-267.972,-16.891,-18.890
	reverse


// Pedestrian number 424

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-267.071,-17.667,-26.394
	point
	-266.334,-17.478,-24.081
	point
	-266.049,-17.349,-23.131
	reverse


// Pedestrian number 425

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-267.927,-17.000,-19.824
	point
	-268.300,-17.152,-21.026
	point
	-266.443,-17.541,-24.563
	reverse


// Pedestrian number 426

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-266.648,-17.641,-25.315
	point
	-266.742,-17.514,-24.281
	point
	-266.126,-17.317,-22.841
	point
	-265.068,-16.746,-17.961
	reverse


// Pedestrian number 427

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-269.300,-17.624,-24.315
	point
	-268.899,-17.480,-23.371
	point
	-268.473,-17.260,-21.869
	point
	-265.572,-17.078,-21.051
	reverse


// Pedestrian number 428

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-287.459,-15.627,39.118
	reverse


// Pedestrian number 429

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-287.210,-15.627,40.372
	reverse


// Pedestrian number 430

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-286.898,-15.627,41.898
	reverse


// Pedestrian number 431

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-280.139,-15.627,35.601
	reverse


// Pedestrian number 432

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-239.364,-18.916,86.650
	reverse


// Pedestrian number 433

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-271.043,-18.916,91.502
	reverse


// Pedestrian number 434

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-271.787,-18.916,91.665
	reverse


// Pedestrian number 435

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-277.022,-18.916,95.333
	reverse


// Pedestrian number 436

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-278.585,-18.916,95.637
	reverse


// Pedestrian number 437

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-287.680,-18.915,96.539
	reverse


// Pedestrian number 438

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-288.693,-18.915,96.701
	reverse


// Pedestrian number 439

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-286.898,-18.915,109.796
	reverse


// Pedestrian number 440

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-285.751,-18.915,109.419
	reverse


// Pedestrian number 441

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-275.152,-18.916,105.913
	reverse


// Pedestrian number 442

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-267.579,-18.915,103.067
	reverse


// Pedestrian number 443

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-253.508,-18.916,101.013
	reverse


// Pedestrian number 444

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-234.220,-18.916,96.708
	reverse


// Pedestrian number 445

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-233.295,-18.916,96.507
	reverse


// Pedestrian number 446

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-227.150,-18.916,97.137
	reverse


// Pedestrian number 447

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-226.593,-18.916,97.000
	reverse


// Pedestrian number 448

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-222.481,-18.916,94.977
	reverse


// Pedestrian number 449

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-221.543,-18.916,95.059
	reverse


// Pedestrian number 450

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-221.642,-18.916,94.409
	reverse


// Pedestrian number 451

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-226.181,-18.916,82.248
	reverse


// Pedestrian number 452

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-226.707,-18.916,82.354
	reverse


// Pedestrian number 453

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-274.307,-17.667,-46.446
	reverse


// Pedestrian number 454

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-274.257,-17.667,-44.535
	reverse


// Pedestrian number 455

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-274.284,-17.667,-49.706
	reverse


// Pedestrian number 456

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-259.818,-17.667,-70.806
	reverse


// Pedestrian number 457

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-259.365,-17.667,-71.060
	reverse


// Pedestrian number 458

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-260.450,-17.667,-70.372
	reverse


// Pedestrian number 459

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-134.149,-13.901,-116.744
	reverse


// Pedestrian number 460

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-133.133,-13.901,-116.986
	reverse


// Pedestrian number 461

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-94.608,-13.901,-125.770
	reverse


// Pedestrian number 462

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-93.850,-13.901,-125.954
	reverse


// Pedestrian number 463

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-55.923,-13.561,-133.129
	reverse


// Pedestrian number 464

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.012,-11.865,-136.051
	reverse


// Pedestrian number 465

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-88.779,-12.543,-137.107
	reverse


// Pedestrian number 466

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-99.301,-12.059,-137.304
	reverse


// Pedestrian number 467

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-177.768,-7.933,-122.214
	reverse


// Pedestrian number 468

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-178.348,-7.878,-120.801
	reverse


// Pedestrian number 469

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-208.762,-4.206,-119.494
	reverse


// Pedestrian number 470

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-209.185,-4.137,-120.047
	reverse


// Pedestrian number 471

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-258.207,-2.552,-100.866
	reverse


// Pedestrian number 472

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-260.159,-2.552,-96.271
	reverse


// Pedestrian number 473

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-260.816,-2.552,-94.565
	reverse


// Pedestrian number 474

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-268.781,-2.552,-98.559
	reverse


// Pedestrian number 475

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-269.871,-2.552,-90.295
	reverse


// Pedestrian number 476

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-269.961,-2.552,-90.025
	reverse


// Pedestrian number 477

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-301.068,-3.636,-66.648
	reverse


// Pedestrian number 478

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-306.901,-4.048,-65.192
	reverse


// Pedestrian number 479

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-307.481,-4.048,-64.478
	reverse


// Pedestrian number 480

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-307.952,-4.048,-63.872
	reverse


// Pedestrian number 481

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-287.591,-8.005,-40.262
	reverse


// Pedestrian number 482

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-302.234,-12.106,-16.937
	reverse


// Pedestrian number 483

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-301.804,-12.106,-16.744
	reverse


// Pedestrian number 484

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-271.668,-15.627,24.710
	reverse


// Pedestrian number 485

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-272.063,-15.627,24.805
	reverse


// Pedestrian number 486

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-271.201,-15.627,24.549
	reverse


// Pedestrian number 487

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-272.084,-15.627,23.357
	reverse


// Pedestrian number 488

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-214.152,-8.352,-7.375
	reverse


// Pedestrian number 489

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-213.866,-8.290,-7.552
	reverse


// Pedestrian number 490

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-202.868,-7.280,-4.228
	reverse


// Pedestrian number 491

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-182.746,-5.425,6.452
	reverse


// Pedestrian number 492

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-188.515,-5.380,4.779
	reverse


// Pedestrian number 493

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-179.419,-5.431,2.074
	reverse


// Pedestrian number 494

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-178.465,-5.432,1.182
	reverse


// Pedestrian number 495

125				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-146.391,-7.508,-46.202
	reverse


// Pedestrian number 496

125				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-135.465,-7.487,-49.345
	reverse


// Pedestrian number 497

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-135.327,-18.640,-34.027
	reverse


// Pedestrian number 498

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-135.395,-18.641,-34.552
	reverse


// Pedestrian number 499

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.241,-13.039,-45.299
	reverse


// Pedestrian number 500

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-82.370,-13.120,-45.117
	reverse


// Pedestrian number 501

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-23.442,-15.561,-51.867
	reverse


// Pedestrian number 502

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-19.152,-14.991,-77.396
	reverse


// Pedestrian number 503

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-19.127,-14.982,-78.241
	reverse


// Pedestrian number 504

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-14.327,-15.489,-128.504
	reverse


// Pedestrian number 505

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-16.435,-15.631,-132.987
	reverse


// Pedestrian number 506

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-43.317,-14.684,-133.268
	reverse


// Pedestrian number 507

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-42.642,-14.745,-133.291
	reverse


// Pedestrian number 508

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-61.800,-13.901,-133.221
	reverse


// Pedestrian number 509

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-62.341,-13.901,-136.832
	reverse


// Pedestrian number 510

99				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-139.333,-10.219,-137.981
	point
	-135.704,-10.384,-138.290
	point
	-134.000,-10.464,-137.933
	point
	-128.739,-10.706,-137.870
	point
	-123.338,-10.946,-140.709
	reverse




// ****** START OF OPPONENT PATHS ******


START OF OPPONENT PATHS

144                             // Number of path nodes
 -249.975,  -15.603,   30.139   // Node #0
 -247.393,  -15.627,   40.526   // Node #1
 -242.474,  -15.242,   41.170   // Node #2
 -229.045,  -11.606,   30.295   // Node #3
 -219.342,   -9.352,   16.413   // Node #4
 -211.405,   -8.951,   -5.008   // Node #5
 -205.429,   -7.881,   -6.354   // Node #6
 -193.708,   -5.328,   -1.252   // Node #7
 -185.485,   -5.428,    4.234   // Node #8
 -180.135,   -5.649,    4.007   // Node #9
 -176.502,   -5.435,    0.724   // Node #10
 -175.172,   -5.578,   -4.666   // Node #11
 -179.573,   -8.050,  -17.537   // Node #12
 -178.480,   -8.840,  -24.813   // Node #13
 -170.047,   -9.078,  -35.110   // Node #14
 -145.562,   -8.802,  -44.806   // Node #15
 -134.637,   -8.880,  -48.147   // Node #16
 -114.706,   -8.874,  -52.829   // Node #17
  -98.251,   -9.426,  -49.700   // Node #18
  -70.570,  -12.833,  -45.715   // Node #19
  -49.297,  -14.595,  -42.864   // Node #20
  -29.777,  -14.596,  -49.524   // Node #21
  -21.244,  -14.596,  -58.412   // Node #22
  -16.074,  -14.536,  -74.221   // Node #23
  -13.154,  -13.419, -116.560   // Node #24
  -13.090,  -14.543, -129.299   // Node #25
  -15.123,  -14.656, -134.091   // Node #26
  -18.705,  -14.657, -136.028   // Node #27
  -53.509,  -14.529, -136.586   // Node #28
 -152.848,  -13.820, -114.594   // Node #29
 -182.531,  -17.667,  -97.063   // Node #30
 -196.978,  -17.667,  -91.815   // Node #31
 -213.702,  -16.453,  -90.431   // Node #32
 -231.135,  -16.453,  -94.236   // Node #33
 -235.669,  -16.453,  -91.053   // Node #34
 -239.736,  -16.453,  -84.356   // Node #35
 -262.737,  -16.453,  -70.095   // Node #36
 -271.548,  -16.453,  -59.852   // Node #37
 -272.065,  -16.453,  -44.221   // Node #38
 -266.345,  -15.303,  -13.850   // Node #39
 -264.770,  -14.680,    3.261   // Node #40
 -254.856,  -15.627,   43.305   // Node #41
 -248.101,  -15.630,   43.664   // Node #42
 -164.508,  -15.443, -109.296   // Node #43
 -261.168,  -14.680,   17.931   // Node #44
  -42.843,  -14.595,  -43.566   // Node #45
  -56.957,  -14.279, -137.025   // Node #46
  -61.333,  -13.989, -137.793   // Node #47
  -65.341,  -13.770, -138.421   // Node #48
 -165.655,   -8.969, -139.964   // Node #49
 -169.548,   -8.663, -138.876   // Node #50
 -173.986,   -8.280, -135.278   // Node #51
 -177.553,   -7.952, -129.515   // Node #52
 -179.660,   -7.749, -122.705   // Node #53
 -182.390,   -7.474, -117.350   // Node #54
 -186.456,   -7.046, -113.764   // Node #55
 -194.200,   -6.154, -111.558   // Node #56
 -201.944,   -5.168, -112.301   // Node #57
 -207.828,   -4.353, -115.465   // Node #58
 -211.222,   -3.839, -120.541   // Node #59
 -214.289,   -3.446, -132.081   // Node #60
 -217.671,   -3.160, -141.537   // Node #61
 -222.794,   -3.040, -146.983   // Node #62
 -231.198,   -2.851, -151.002   // Node #63
 -234.592,   -2.789, -150.888   // Node #64
 -236.819,   -2.714, -148.580   // Node #65
 -248.357,   -2.552, -120.940   // Node #66
 -263.688,   -2.553,  -83.516   // Node #67
 -269.866,   -2.554,  -75.771   // Node #68
 -277.831,   -2.553,  -70.214   // Node #69
 -287.929,   -2.543,  -68.170   // Node #70
 -303.068,   -3.882,  -68.291   // Node #71
 -308.129,   -4.050,  -66.676   // Node #72
 -310.546,   -4.048,  -61.708   // Node #73
 -309.817,   -4.051,  -56.793   // Node #74
 -305.228,   -4.165,  -53.014   // Node #75
 -290.748,   -7.872,  -49.147   // Node #76
 -286.828,   -8.007,  -46.024   // Node #77
 -285.659,   -8.007,  -41.168   // Node #78
 -287.814,   -8.006,  -36.492   // Node #79
 -292.722,   -8.112,  -34.205   // Node #80
 -308.248,  -11.861,  -33.059   // Node #81
 -312.892,  -11.973,  -30.429   // Node #82
 -314.787,  -11.972,  -24.998   // Node #83
 -313.710,  -11.972,  -21.294   // Node #84
 -311.184,  -11.997,  -18.843   // Node #85
 -298.018,  -12.107,  -13.002   // Node #86
 -287.082,  -12.304,   -4.837   // Node #87
 -275.559,  -15.002,   12.043   // Node #88
 -272.386,  -15.627,   20.075   // Node #89
 -275.513,  -15.628,   26.232   // Node #90
 -279.528,  -15.628,   29.152   // Node #91
 -287.257,  -15.630,   30.917   // Node #92
 -289.703,  -15.627,   34.061   // Node #93
 -289.404,  -15.627,   37.637   // Node #94
 -287.760,  -15.627,   47.198   // Node #95
 -286.602,  -15.627,   48.854   // Node #96
 -283.707,  -15.627,   50.241   // Node #97
 -277.724,  -15.623,   50.097   // Node #98
 -259.234,  -15.607,   46.407   // Node #99
 -256.668,  -15.627,   45.348   // Node #100
 -255.206,  -15.627,   44.437   // Node #101
 -254.146,  -15.627,   46.478   // Node #102
 -243.116,  -18.915,   98.813   // Node #103
 -244.045,  -18.915,   99.848   // Node #104
 -263.285,  -18.915,  104.667   // Node #105
 -265.357,  -18.915,  103.936   // Node #106
 -266.277,  -18.915,  102.814   // Node #107
 -250.337,   -2.553, -118.687   // Node #108
 -258.219,   -2.552, -113.832   // Node #109
 -264.039,   -2.552, -107.784   // Node #110
 -272.315,   -2.552,  -88.420   // Node #111
 -281.437,   -2.552,  -74.518   // Node #112
 -251.441,  -15.623,   26.693   // Node #113
 -252.870,  -15.622,   24.867   // Node #114
 -255.388,  -15.622,   23.642   // Node #115
 -256.944,  -15.627,   23.621   // Node #116
 -259.469,  -15.627,   24.324   // Node #117
 -265.799,  -15.627,   24.987   // Node #118
 -121.550,   -9.078,  -51.179   // Node #119
 -123.816,   -9.356,  -45.510   // Node #120
 -125.287,  -10.162,  -38.526   // Node #121
 -131.912,  -13.190,  -32.790   // Node #122
 -140.261,  -13.512,  -30.740   // Node #123
 -145.006,  -12.423,  -30.887   // Node #124
 -152.848,  -10.049,  -33.455   // Node #125
 -155.717,   -8.795,  -36.452   // Node #126
 -157.728,   -9.078,  -41.463   // Node #127
 -136.791,  -14.001,  -31.257   // Node #128
 -143.569,  -18.690,  -47.648   // Node #129
 -142.298,  -18.654,  -39.284   // Node #130
 -147.869,  -18.642,  -36.886   // Node #131
 -151.331,  -18.664,  -39.018   // Node #132
 -140.591,  -18.730,  -50.247   // Node #133
 -138.024,  -18.671,  -49.664   // Node #134
 -136.208,  -18.636,  -45.375   // Node #135
 -134.454,  -18.587,  -41.220   // Node #136
 -127.194,  -18.571,  -41.632   // Node #137
 -126.725,  -18.567,  -41.644   // Node #138
 -213.557,   -9.078,    0.401   // Node #139
 -248.839,  -15.622,   38.144   // Node #140
 -245.396,  -15.631,   41.378   // Node #141
 -274.811,  -15.627,   49.636   // Node #142
 -283.477,   -2.549,  -67.971   // Node #143

150                                           // Number of path sections
 140,   0,   0, 255,   0, 255,    1.0,    1   // Section #0
   2, 141,   0,  40,  25,  35,    1.1,    1   // Section #1
   3,   2,   0, 255,   0,  50,    1.1,    1   // Section #2
   4,   3,   0, 255,   0, 255,    1.0,    1   // Section #3
 139,   4,   0, 255,   0, 255,    1.0,    1   // Section #4
   6,   5,   0, 255,   0, 255,    1.0,    1   // Section #5
   7,   6,   0, 255,   0, 255,    1.0,    1   // Section #6
   8,   7,   0, 255,   0, 255,    1.0,    1   // Section #7
   9,   8,   0, 255,   0, 255,    1.0,    1   // Section #8
  10,   9,   0, 255,   0, 255,    1.0,    1   // Section #9
  11,  10,   0, 255,   0, 255,    1.0,    1   // Section #10
  12,  11,   0, 255,   0, 170,    1.0,    1   // Section #11
  13,  12,   0, 255,   0, 255,    1.0,    1   // Section #12
  14,  13,   0, 255,   0, 255,    1.0,    1   // Section #13
 127,  14,   0, 255,   0, 255,    1.0,    1   // Section #14
  16,  15,   0, 255,   0, 255,    1.0,    1   // Section #15
 119,  16,   0, 255,   0, 255,    1.0,    1   // Section #16
  18,  17,   0, 255,   0, 255,    1.0,    1   // Section #17
  19,  18,   0, 255,   0, 255,    1.0,    1   // Section #18
  20,  19,   0, 255,   0, 255,    1.0,    1   // Section #19
  45,  20,   0, 255,   0, 255,    1.0,    1   // Section #20
  22,  21,   0, 255,   0, 255,    1.0,    1   // Section #21
  23,  22,   0, 255,   0, 255,    1.0,    1   // Section #22
  24,  23,   0,  40,   0, 255,    1.0,    1   // Section #23
  25,  24,   0, 255,   0, 255,    1.0,    1   // Section #24
  26,  25,   0, 255,   0, 255,    1.0,    1   // Section #25
  27,  26,   0, 255,   0, 255,    1.0,    1   // Section #26
  28,  27,   0, 255,   0, 255,    1.0,    1   // Section #27
  46,  28,   0, 255,   0, 255,    1.0,    1   // Section #28
  43,  29,   0,  70,   0, 255,    1.0,    0   // Section #29
  31,  30,   0, 255,   0, 255,    1.0,    0   // Section #30
  32,  31,   0, 255,   0, 255,    1.0,    0   // Section #31
  33,  32,   0,  35,   0, 255,    1.0,    0   // Section #32
  34,  33,   0, 255,   0,  35,    1.0,    0   // Section #33
  35,  34,   0, 255,   0, 255,    1.0,    0   // Section #34
  36,  35,   0, 255,   0, 255,    0.6,    0   // Section #35
  37,  36,   0, 255,   0, 255,    0.6,    0   // Section #36
  37,  38,   0, 255,   0, 255,    0.6,    0   // Section #37
  39,  38,   0, 255,   0, 255,    0.6,    0   // Section #38
  40,  39,   0, 255,   0, 255,    0.6,    0   // Section #39
  44,  40,   0, 255,   0, 255,    1.1,    0   // Section #40
  41,  42,   0, 255,   0, 255,    1.1,    0   // Section #41
  30,  43,   0, 255,   0, 255,    1.0,    0   // Section #42
  41, 117,   0,  15,   0, 255,    1.1,    0   // Section #43
  42,   2,   0, 255,   0, 255,    1.1,    0   // Section #44
  21,  45,   0, 255,   0, 255,    1.0,    1   // Section #45
  47,  46,   0, 255,   0, 255,    1.0,    1   // Section #46
  29,  46,   0, 255,   0, 255,    1.0,    0   // Section #47
  48,  47,   0, 255,   0, 255,    1.0,    1   // Section #48
  49,  48,   0, 255,   0, 255,    1.0,    1   // Section #49
  50,  49,   0,  65,   0,  65,    1.0,    1   // Section #50
  51,  50,   0,  45,   0,  50,    1.0,    1   // Section #51
  52,  51,   0,  50,   0,  40,    1.0,    1   // Section #52
  53,  52,   0, 255,   0, 255,    1.0,    1   // Section #53
  54,  53,   0,  70,   0, 255,    1.0,    1   // Section #54
  55,  54,   0,  40,   0,  55,    1.0,    1   // Section #55
  56,  55,   0,  40,   0,  45,    1.0,    1   // Section #56
  57,  56,   0,  30,   0,  40,    1.0,    1   // Section #57
  58,  57,   0,  40,   0,  35,    1.0,    1   // Section #58
  59,  58,   0,  50,   0,  45,    1.0,    1   // Section #59
  60,  59,   0, 255,   0, 255,    1.0,    1   // Section #60
  61,  60,   0, 255,   0, 255,    1.0,    1   // Section #61
  62,  61,   0, 255,   0, 255,    1.0,    1   // Section #62
  63,  62,   0,  40,   0,  65,    1.0,    1   // Section #63
  64,  63,   0,  30,   0,  35,    1.0,    1   // Section #64
  65,  64,   0,  35,   0,  25,    1.0,    1   // Section #65
  66,  65,   0, 255,   0, 255,    1.0,    1   // Section #66
 108,  66,   0, 255,   0, 255,    1.0,    1   // Section #67
  67,  68,   0, 255,   0, 255,    1.0,    0   // Section #68
  68,  69,   0, 255,   0, 255,    0.9,    0   // Section #69
  69, 143,   0, 255,   0, 255,    0.7,    0   // Section #70
  71,  70,   0, 255,   0, 255,    1.0,    1   // Section #71
  72,  71,   0, 255,   0, 255,    1.0,    1   // Section #72
  73,  72,   0, 255,   0, 255,    1.0,    1   // Section #73
  74,  73,   0, 255,   0, 255,    1.0,    1   // Section #74
  75,  74,   0, 255,   0, 255,    1.0,    1   // Section #75
  76,  75,   0, 255,   0, 255,    1.0,    1   // Section #76
  77,  76,   0, 255,   0, 255,    1.0,    1   // Section #77
  78,  77,   0, 255,   0, 255,    1.0,    1   // Section #78
  79,  78,   0, 255,   0, 255,    1.0,    1   // Section #79
  80,  79,   0, 255,   0, 255,    1.0,    1   // Section #80
  81,  80,   0, 255,   0, 255,    1.0,    1   // Section #81
  82,  81,   0, 255,   0, 255,    1.0,    1   // Section #82
  83,  82,   0, 255,   0, 255,    1.0,    1   // Section #83
  84,  83,   0, 255,   0, 255,    1.0,    1   // Section #84
  85,  84,   0, 255,   0, 255,    1.0,    1   // Section #85
  86,  85,   0, 255,   0, 255,    1.0,    1   // Section #86
  87,  86,   0, 255,   0, 255,    1.0,    1   // Section #87
  88,  87,   0, 255,   0, 255,    1.0,    1   // Section #88
  89,  88,   0,  65,   0, 255,    1.0,    1   // Section #89
  89,  90,   0, 255,   0, 255,    1.0,    0   // Section #90
  90,  91,   0, 255,   0, 255,    1.0,    0   // Section #91
  91,  92,   0, 255,   0, 255,    1.0,    0   // Section #92
  92,  93,   0, 255,   0, 255,    1.0,    0   // Section #93
  93,  94,   0, 255,   0, 255,    1.0,    0   // Section #94
  94,  95,   0, 255,   0, 255,    1.0,    0   // Section #95
  95,  96,   0, 255,   0, 255,    1.0,    0   // Section #96
  96,  97,   0, 255,   0, 255,    1.0,    0   // Section #97
  97,  98,   0, 255,   0, 255,    1.0,    0   // Section #98
  98, 142,   0, 255,   0, 255,    1.0,    0   // Section #99
  99, 100,   0, 255,   0, 255,    1.0,    0   // Section #100
 100, 101,   0, 255,   0, 255,    1.0,    0   // Section #101
 101, 102,   0, 255,   0, 255,    1.0,    0   // Section #102
 102, 103,   0, 255,   0, 255,    1.0,    0   // Section #103
 103, 104,   0, 255,   0, 255,    1.0,    0   // Section #104
 104, 105,   0, 255,   0, 255,    1.0,    0   // Section #105
 105, 106,   0, 255,   0, 255,    1.0,    0   // Section #106
 106, 107,   0, 255,   0, 255,    1.0,    0   // Section #107
 107,  98,   0, 255,   0, 255,    1.0,    0   // Section #108
 109, 108,   0, 255,   0, 255,    0.9,    1   // Section #109
 108,  67,   0, 255,   0, 255,    1.0,    0   // Section #110
 110, 109,   0, 255,   0, 255,    0.7,    1   // Section #111
 111, 110,   0, 255,   0, 255,    0.6,    1   // Section #112
 112, 111,   0, 255,   0, 255,    0.7,    1   // Section #113
  70, 112,   0, 255,   0, 255,    0.8,    1   // Section #114
 101,  41,   0, 255,   0, 255,    1.0,    0   // Section #115
   0, 113,   0, 255,   0,  40,    1.1,    1   // Section #116
 113, 114,   0,  40,   0,  40,    1.1,    1   // Section #117
 114, 115,   0,  40,   0,  40,    1.0,    1   // Section #118
 115, 116,   0,  40,   0,  40,    1.0,    1   // Section #119
 116, 117,   0, 255,   0, 255,    0.9,    1   // Section #120
 117,  44,   0, 255,   0,  25,    1.1,    0   // Section #121
 118,  89,   0,  45,   0,  60,    1.0,    1   // Section #122
 117, 118,   0, 255,   0,  45,    0.8,    1   // Section #123
 119, 120,   0, 255,   0, 255,    1.0,    0   // Section #124
  17, 119,   0, 255,   0, 255,    1.0,    1   // Section #125
 120, 121,   0, 255,   0, 255,    1.0,    0   // Section #126
 121, 122,   0, 255,   0, 255,    1.0,    0   // Section #127
 122, 128,   0, 255,   0, 255,    1.0,    0   // Section #128
 123, 124,   0, 255,   0, 255,    1.0,    0   // Section #129
 124, 125,   0, 255,   0, 255,    1.0,    0   // Section #130
 125, 126,   0, 255,   0, 255,    1.0,    0   // Section #131
 126, 127,   0, 255,   0, 255,    1.0,    0   // Section #132
  15, 127,   0, 255,   0, 255,    1.0,    1   // Section #133
 128, 133,   0, 255,   0, 255,    1.0,    0   // Section #134
 128, 123,   0, 255,   0, 255,    1.0,    0   // Section #135
 129, 130,   0, 255,   0, 255,    1.3,    0   // Section #136
 130, 131,   0, 255,   0, 255,    1.3,    0   // Section #137
 131, 132,   0, 255,   0, 255,    1.5,    0   // Section #138
 133, 134,   0, 255,   0, 255,    1.0,    0   // Section #139
 133, 129,   0, 255,   0, 255,    1.0,    0   // Section #140
 134, 135,   0, 255,   0, 255,    1.3,    0   // Section #141
 135, 136,   0, 255,   0, 255,    1.3,    0   // Section #142
 136, 137,   0, 255,   0, 255,    1.5,    0   // Section #143
 137, 138,   0, 255,   0, 255,    1.5,    0   // Section #144
   5, 139,   0,  25,   0, 255,    1.0,    1   // Section #145
   1, 140,   0,  35,   0,  40,    1.1,    1   // Section #146
 141,   1,   0,  30,   0,  35,    1.1,    1   // Section #147
 142,  99,   0, 255,   0, 255,    1.0,    0   // Section #148
 143,  70,   0, 255,   0, 255,    0.7,    0   // Section #149

8                                                             // Number of cop start points
 -133.096,  -13.901, -118.073,    0.000,    0.000,    0.000   // Cop start point #0
 -267.099,  -18.915,  105.012,    0.000,    0.000,    0.000   // Cop start point #1
 -282.328,  -15.627,   32.606,    0.000,    0.000,    0.000   // Cop start point #2
 -273.255,   -2.552,  -74.456,    0.000,    0.000,    0.000   // Cop start point #3
  -61.503,  -13.901, -135.604,    0.000,    0.000,    0.000   // Cop start point #4
  -28.446,  -15.561,  -46.306,    0.000,    0.000,    0.000   // Cop start point #5
 -127.579,  -18.619,  -44.321,    0.000,    0.000,    0.000   // Cop start point #6
 -259.273,  -15.649,   22.857,    0.000,    0.000,    0.000   // Cop start point #7

END OF OPPONENT PATHS



7										// number of material modifiers

// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT							// skid mark material

//	material '0'
1										// car wall friction
1										// tyre road friction
0.90										// down force
6.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
0										// sparkiness
3										// room for expansion
MUD2.MAT										// room for expansion

//	material '1'
1.2										// car wall friction
1.2										// tyre road friction
1.0										// down force
10.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
2.0										// sparkiness
4										// room for expansion
SAND2.MAT										// room for expansion

//	material '2'
1.2										// car wall friction
1										// tyre road friction
1.0										// down force
5										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
3										// room for expansion
MUD1.MAT										// room for expansion

//	material '3'
1.2										// car wall friction
1.00										// tyre road friction
1.0										// down force
8.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
3										// room for expansion
MUD2.MAT										// room for expansion

//	material '4'
1										// car wall friction
1										// tyre road friction
2										// down force
1										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
20										// sparkiness
1										// room for expansion
none									// room for expansion

//	material '5'
1										// car wall friction
1										// tyre road friction
2.0										// down force
4.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
1										// sparkiness
4										// room for expansion
SAND2.MAT										// room for expansion

// Non CarObjects
6										// number of non car objects

GASPUMP.TXT
GREENCAR.TXT
WRECK.TXT
PALM2.TXT
PHONE.TXT
BARRIER.TXT

3										// number of dust shade tables

61, 84, 33								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"

92, 51, 34							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"

117, 94, 38							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"

12										// Number of network start points

-225.935,-18.923,95.733							//1
100													

-285.004,-18.921,109.366							//2						
279									

-289.563,-18.929,96.926							//3						
280									

-230.433,-18.924,83.239							//4						
101									

-250.041,15.627,31.341							//5						
189									

-289.175,-15.627,38.198							//6						
190									

-268.443,-2.552,-100.573							//7						
339									

-146.921,-9.864,-139.297							//8						
77									

-56.239,-14.331,-135.497							//9						
79									

-30.041,-15.562,-45.459							//10						
91									

-137.211,-14.009,-31.616							//11						
101									

-226.325,-17.668,-92.217							//12						
77									



1										// number of splash files
SPLSHBLU.PIX 								//  name of pixelmapfile for splashes

1

COASTA2.TXT
