VERSION 6		// V1 expects map checkpoint rectangles
			// V2 and above expect map checkpoint points
			// V3 and above expect splash file stuff at the end
			// V4 and above expect two sets of PIX and MAT and ped substitution entry

-39.433,109.502,32.932   						// Position of centre of start of grid
180									// Direction that grid faces in

// Laps, checkpoints etc

60,30,10							// Initial timer count for each skill level
4									// # laps
5000,5000,5000						// Race completed bonus (all laps raced) for each skill level
10000,10000,10000					// Race completed bonus (all peds killed) for each skill level
10000,10000,10000					// Race completed bonus (all oppos wasted) for each skill level

// Width and height of map checkpoint rectangles
9,18
11,26

0									// # checkpoints

4									// # pixelmap files to load
ARENA.PIX
SNOWDROP.PIX
DRKSCRN.PIX
FOGSCRN.PIX

4									// # pixelmap files to load(low memory)
ARENA.PIX
SNOWDROP.PIX
DRKSCRN.PIX
FOGSCRN.PIX

3									// # shade table files to load
ICE2.TAB
DRRENDER.TAB
IDENTITY.TAB

5									// # material files to load
ARENA.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
KERB01.MAT

5									// # material files to load(low memory)
ARENA.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
KERB01.MAT

1									// # model files to load
ARENA.DAT

1									// # model files to load
ARENA.DAT


ARENA.ACT							// Track actor

ARENA.ACT							// Track actor

ARNAAX.ACT							// Additional actor

// HORIZON STUFF

none						// Name of sky texture pixelmap (or "none")
3									// Horizontal repetitions of sky texture
30									// Vertical size of sky texture (degrees)
59									// Position of horizon (pixels below top)
fog								// Depth cue mode ("none", "dark" or "fog")
8,0									// Degree of fog/darkness

// DEFAULT ENGINE NOISE

0

// SPECIAL EFFECTS VOLUMES

0				// # special effects volumes



 
// REFLECTIVE WINDSCREEN SPECIFICATIONS

FOGSCRN.MAT							// Material to use for default screens
DRKSCRN.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT							// Material to use for default screens during fog

0									// # areas with different screens

// MAP DETAILS

NARENAMP.PIX						// Map pixelmap name

0.995,		0,			0			// World->map transformation matrix
0,			0,			0
0,			0.995,		0
197.8,		68.0,		0

// ****** START OF FUNK AND GROOVE STUFF ******

START OF FUNK

END OF FUNK



START OF GROOVE


END OF GROOVE


// ****** START OF PEDESTRIAN STUFF ******

9				// Ped subs table index

298				// Number of pedestrians

// Pedestrian number 1

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-56.089,111.142,20.370
	reverse


// Pedestrian number 2

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-87.697,113.471,35.261
	point
	-91.070,113.471,36.523
	point
	-96.333,113.471,40.196
	reverse


// Pedestrian number 3

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-98.085,113.471,41.071
	point
	-101.790,113.471,36.655
	point
	-104.606,113.471,29.290
	reverse


// Pedestrian number 4

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-103.218,113.471,28.371
	point
	-100.404,113.471,25.976
	point
	-96.452,113.471,22.595
	reverse


// Pedestrian number 5

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-87.921,113.471,37.719
	point
	-88.351,113.471,38.385
	point
	-88.911,113.471,38.712
	point
	-89.996,113.471,39.294
	reverse


// Pedestrian number 6

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-94.680,113.471,40.869
	point
	-94.602,113.471,42.020
	point
	-95.063,113.471,42.278
	point
	-95.852,113.471,42.194
	reverse


// Pedestrian number 7

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-97.166,113.471,42.276
	point
	-97.986,113.471,42.106
	point
	-102.214,113.471,38.247
	reverse


// Pedestrian number 8

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-106.796,113.471,36.353
	point
	-118.995,113.391,36.808
	point
	-125.834,113.337,37.165
	reverse


// Pedestrian number 9

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-125.939,113.332,40.045
	point
	-124.905,113.332,44.651
	point
	-125.524,113.332,47.745
	point
	-123.384,113.332,61.219
	reverse


// Pedestrian number 10

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-120.786,113.332,63.073
	point
	-113.868,113.332,67.414
	point
	-110.061,113.332,68.663
	point
	-104.377,113.332,70.026
	reverse


// Pedestrian number 11

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-103.325,113.332,70.371
	point
	-98.043,113.332,66.108
	point
	-95.040,113.332,64.793
	point
	-90.565,113.332,62.616
	reverse


// Pedestrian number 12

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-77.189,112.949,55.535
	point
	-78.038,112.604,52.416
	point
	-78.809,112.068,47.562
	reverse


// Pedestrian number 13

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-78.772,111.401,40.468
	point
	-78.707,111.401,36.779
	point
	-77.942,111.401,32.312
	point
	-78.783,111.401,29.711
	reverse


// Pedestrian number 14

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-78.892,111.401,28.574
	point
	-72.971,111.401,25.573
	point
	-70.066,111.401,24.088
	reverse


// Pedestrian number 15

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-69.500,111.409,23.944
	point
	-66.120,111.637,23.922
	point
	-62.911,111.856,23.675
	reverse


// Pedestrian number 16

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-62.505,111.888,39.675
	point
	-63.970,111.786,40.189
	point
	-69.291,111.423,41.018
	reverse


// Pedestrian number 17

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-63.728,111.802,38.541
	point
	-66.464,111.614,35.743
	point
	-69.680,111.401,33.491
	point
	-77.220,111.401,32.581
	reverse


// Pedestrian number 18

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-80.738,110.973,33.314
	point
	-81.274,111.081,33.345
	point
	-81.930,111.284,33.376
	point
	-83.015,111.659,33.219
	reverse


// Pedestrian number 19

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-48.727,111.401,71.291
	point
	-47.360,111.401,70.734
	point
	-45.309,111.401,71.212
	point
	-42.128,111.401,71.171
	reverse


// Pedestrian number 20

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-40.784,111.401,71.299
	point
	-37.859,111.401,71.258
	point
	-34.033,111.401,68.640
	point
	-31.398,111.401,62.403
	reverse


// Pedestrian number 21

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-31.311,111.412,61.940
	point
	-32.340,111.568,59.679
	point
	-34.342,111.683,58.012
	reverse


// Pedestrian number 22

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-45.941,111.408,62.001
	point
	-47.529,111.616,58.976
	point
	-48.711,111.779,56.612
	reverse


// Pedestrian number 23

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-48.688,111.848,55.604
	point
	-43.738,111.798,56.330
	point
	-37.899,111.741,57.167
	reverse


// Pedestrian number 24

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-16.699,111.817,41.140
	point
	-15.460,111.733,41.400
	point
	-13.249,111.584,40.142
	point
	-10.847,111.424,32.447
	point
	-10.719,111.416,24.872
	reverse


// Pedestrian number 25

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-11.569,111.472,23.993
	point
	-14.289,111.655,25.348
	point
	-15.430,111.733,26.066
	reverse


// Pedestrian number 26

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-16.539,111.810,26.464
	point
	-16.881,111.833,25.642
	point
	-17.548,111.879,24.091
	reverse


// Pedestrian number 27

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-10.138,111.401,23.756
	point
	-7.854,111.401,24.620
	point
	-1.778,111.401,31.293
	point
	-1.315,111.401,32.777
	reverse


// Pedestrian number 28

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-2.223,111.417,41.860
	point
	-2.399,111.757,44.932
	point
	-1.864,112.019,47.306
	point
	-1.190,112.316,49.997
	reverse


// Pedestrian number 29

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.328,112.484,51.513
	point
	-4.358,112.686,53.345
	point
	-8.917,112.982,56.024
	reverse


// Pedestrian number 30

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-9.644,112.784,54.234
	point
	-9.619,112.273,49.607
	point
	-10.128,112.030,47.409
	reverse


// Pedestrian number 31

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.331,112.044,17.876
	point
	-4.847,112.402,14.639
	point
	-9.674,112.839,10.690
	reverse


// Pedestrian number 32

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-17.431,112.890,2.963
	point
	-19.979,112.608,2.423
	point
	-22.121,112.372,3.091
	point
	-25.281,112.022,3.407
	reverse


// Pedestrian number 33

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-26.442,111.894,3.001
	point
	-28.273,111.692,-1.848
	point
	-30.228,111.476,-5.044
	reverse


// Pedestrian number 34

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-40.896,111.721,-6.793
	point
	-42.057,111.946,-8.777
	point
	-41.811,111.806,-10.704
	reverse


// Pedestrian number 35

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-41.476,112.878,-13.768
	point
	-40.507,112.096,-12.123
	point
	-39.978,111.605,-11.063
	point
	-39.851,111.600,-10.101
	reverse


// Pedestrian number 36

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-32.768,111.401,-5.594
	point
	-40.638,111.401,2.293
	point
	-41.696,111.401,3.353
	reverse


// Pedestrian number 37

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-49.190,111.431,3.411
	point
	-52.281,111.772,2.805
	point
	-55.277,112.103,3.374
	reverse


// Pedestrian number 38

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-59.050,112.521,3.249
	point
	-60.653,112.697,2.223
	point
	-62.992,112.956,0.744
	reverse


// Pedestrian number 39

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-59.334,112.552,-5.594
	point
	-56.929,112.286,-5.302
	point
	-50.397,111.564,-5.484
	reverse


// Pedestrian number 40

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-48.761,111.401,-5.339
	point
	-44.713,111.401,-5.495
	point
	-43.069,111.401,-5.591
	reverse


// Pedestrian number 41

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-70.113,112.798,10.875
	point
	-70.355,112.471,13.831
	point
	-69.822,112.085,17.322
	reverse


// Pedestrian number 42

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-69.925,111.470,22.887
	point
	-74.023,111.724,20.586
	point
	-78.397,111.987,18.212
	reverse


// Pedestrian number 43

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-78.765,112.060,17.547
	point
	-78.558,112.387,14.593
	point
	-78.813,112.769,11.132
	reverse


// Pedestrian number 44

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-78.305,112.668,3.223
	point
	-75.401,112.707,2.801
	point
	-74.405,112.720,-2.168
	point
	-69.987,112.774,-3.745
	reverse


// Pedestrian number 45

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-69.804,112.780,0.244
	point
	-74.950,112.712,-4.070
	point
	-76.829,112.687,-5.422
	reverse


// Pedestrian number 46

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-74.399,112.717,-5.488
	point
	-76.602,112.691,-4.358
	point
	-77.379,112.681,-3.950
	reverse


// Pedestrian number 47

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-79.072,112.722,-0.541
	point
	-80.829,112.895,-0.818
	point
	-82.236,113.033,0.224
	point
	-84.643,113.270,3.073
	reverse


// Pedestrian number 48

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-86.706,113.332,3.300
	point
	-89.243,113.332,2.888
	point
	-90.550,113.332,2.905
	point
	-93.847,113.332,3.212
	reverse


// Pedestrian number 49

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-101.972,113.332,3.564
	point
	-108.033,113.332,1.750
	point
	-119.236,113.332,2.664
	reverse


// Pedestrian number 50

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-124.889,113.332,6.489
	point
	-124.359,113.332,12.781
	point
	-124.161,113.332,19.856
	reverse


// Pedestrian number 51

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-125.863,113.337,28.894
	point
	-123.360,113.357,29.451
	point
	-117.621,113.402,28.829
	reverse


// Pedestrian number 52

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-115.249,113.421,28.690
	point
	-112.190,113.446,29.014
	point
	-109.584,113.466,28.716
	reverse


// Pedestrian number 53

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-108.428,113.471,28.231
	point
	-103.668,113.471,28.061
	point
	-102.048,113.471,28.166
	reverse


// Pedestrian number 54

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-100.798,113.471,29.124
	point
	-95.288,113.471,29.775
	point
	-93.781,113.471,29.996
	reverse


// Pedestrian number 55

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-89.880,113.471,26.336
	point
	-88.783,113.471,28.683
	point
	-87.744,113.471,30.118
	reverse


// Pedestrian number 56

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-92.889,113.471,31.496
	point
	-97.701,113.471,39.117
	point
	-100.119,113.471,43.274
	reverse


// Pedestrian number 57

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-105.678,113.507,37.105
	point
	-105.245,114.000,36.673
	point
	-104.187,113.587,35.982
	reverse


// Pedestrian number 58

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-93.326,113.514,30.110
	point
	-92.734,113.960,29.831
	point
	-92.118,113.863,29.812
	point
	-91.794,113.838,29.483
	reverse


// Pedestrian number 59

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-46.694,113.471,83.167
	point
	-42.616,113.471,80.962
	point
	-38.378,113.471,80.472
	point
	-37.950,113.471,80.495
	reverse


// Pedestrian number 60

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-34.942,113.471,80.997
	point
	-38.435,113.471,89.127
	point
	-39.929,113.471,92.811
	reverse


// Pedestrian number 61

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-37.194,113.471,91.832
	point
	-39.056,113.471,89.828
	point
	-40.146,113.471,89.140
	reverse


// Pedestrian number 62

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-42.711,113.471,89.986
	point
	-41.004,113.471,89.507
	point
	-40.402,113.471,89.123
	reverse


// Pedestrian number 63

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-35.337,113.471,90.054
	point
	-32.462,113.471,93.751
	point
	-31.734,113.471,97.462
	reverse


// Pedestrian number 64

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-33.554,113.471,97.220
	point
	-39.707,113.471,94.886
	point
	-46.054,113.471,97.719
	reverse


// Pedestrian number 65

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-47.304,113.471,98.228
	point
	-45.026,113.471,92.407
	point
	-44.406,113.471,90.454
	reverse


// Pedestrian number 66

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-44.855,113.471,89.935
	point
	-46.178,113.471,87.895
	point
	-46.634,113.471,85.909
	reverse


// Pedestrian number 67

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-48.472,113.471,86.493
	point
	-50.213,113.471,88.605
	point
	-50.288,113.471,89.994
	point
	-50.409,113.471,94.622
	reverse


// Pedestrian number 68

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-50.401,113.471,94.781
	point
	-41.172,113.471,97.474
	point
	-35.128,113.471,99.305
	reverse


// Pedestrian number 69

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	44.512,113.356,34.910
	point
	42.518,113.364,36.029
	point
	40.619,113.371,37.085
	reverse


// Pedestrian number 70

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	44.220,113.350,37.453
	point
	36.244,113.414,30.247
	point
	34.052,113.431,28.898
	reverse


// Pedestrian number 71

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	35.698,113.418,28.710
	point
	29.434,113.468,31.602
	point
	27.825,113.471,32.100
	point
	27.036,113.471,31.769
	point
	22.933,113.471,29.099
	reverse


// Pedestrian number 72

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	21.737,113.471,22.271
	point
	23.952,113.471,24.200
	point
	26.394,113.471,26.528
	reverse


// Pedestrian number 73

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	27.816,113.471,28.064
	point
	23.712,113.471,27.336
	point
	22.922,113.471,27.298
	reverse


// Pedestrian number 74

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	20.995,113.471,27.258
	point
	19.970,113.471,27.232
	point
	18.781,113.471,27.387
	point
	17.835,113.471,27.304
	reverse


// Pedestrian number 75

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	16.723,113.471,28.494
	point
	11.964,113.471,33.341
	point
	8.319,113.471,36.955
	reverse


// Pedestrian number 76

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	12.526,113.471,23.975
	point
	16.552,113.471,29.111
	point
	24.015,113.471,37.851
	reverse


// Pedestrian number 77

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	22.833,113.471,41.869
	point
	23.203,113.471,39.852
	point
	23.478,113.471,39.294
	point
	24.135,113.471,38.799
	reverse


// Pedestrian number 78

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.836,113.471,37.625
	point
	26.933,113.471,36.960
	point
	27.694,113.471,36.497
	reverse


// Pedestrian number 79

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	28.865,113.471,37.418
	point
	28.112,113.471,37.988
	point
	26.795,113.471,38.731
	point
	26.316,113.471,39.190
	reverse


// Pedestrian number 80

9				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	19.006,113.471,41.823
	point
	19.393,113.471,42.928
	point
	18.870,113.471,43.323
	point
	17.638,113.471,43.536
	point
	13.494,113.471,43.055
	reverse


// Pedestrian number 81

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	12.750,113.471,42.662
	point
	11.999,113.471,41.855
	point
	11.708,113.471,40.308
	point
	11.309,113.471,39.023
	point
	11.029,113.471,38.829
	reverse


// Pedestrian number 82

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	8.164,113.471,37.742
	point
	8.047,113.471,33.783
	point
	7.610,113.471,30.147
	reverse


// Pedestrian number 83

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	9.031,113.471,27.103
	point
	16.611,113.471,27.474
	point
	24.013,113.471,23.841
	reverse


// Pedestrian number 84

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	24.859,113.471,24.473
	point
	23.733,113.471,28.601
	point
	24.323,113.471,38.553
	reverse


// Pedestrian number 85

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	24.614,113.471,38.128
	point
	22.504,113.471,38.427
	point
	17.661,113.471,41.094
	point
	16.227,113.471,41.147
	point
	14.557,113.471,42.115
	reverse


// Pedestrian number 86

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	10.122,113.471,37.409
	point
	19.317,113.471,31.120
	point
	23.691,113.471,29.070
	point
	25.708,113.471,27.325
	reverse


// Pedestrian number 87

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	29.683,113.466,29.153
	point
	33.734,113.434,35.165
	point
	37.607,113.403,37.263
	reverse


// Pedestrian number 88

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	33.363,113.436,37.337
	point
	44.679,113.347,34.528
	point
	55.040,113.332,30.921
	reverse


// Pedestrian number 89

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	55.376,113.332,30.521
	point
	53.273,113.332,27.919
	point
	52.710,113.332,19.027
	reverse


// Pedestrian number 90

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	44.941,113.332,21.599
	point
	43.974,113.332,19.388
	point
	43.481,113.332,18.682
	point
	41.683,113.332,16.420
	reverse


// Pedestrian number 91

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	40.972,113.332,15.408
	point
	40.335,113.332,10.549
	point
	39.341,113.332,2.416
	reverse


// Pedestrian number 92

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	31.056,113.332,6.577
	point
	29.688,113.332,5.830
	point
	24.647,113.332,4.347
	reverse


// Pedestrian number 93

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	5.171,113.353,-5.591
	point
	3.005,113.688,-3.859
	point
	-0.623,114.250,-1.651
	reverse


// Pedestrian number 94

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.866,114.110,-1.193
	point
	-2.848,114.123,-1.226
	point
	-3.961,114.138,-1.257
	reverse


// Pedestrian number 95

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-5.219,114.177,-2.848
	point
	-5.673,114.161,-4.090
	point
	-6.095,114.147,-5.190
	reverse


// Pedestrian number 96

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-5.735,114.323,-6.058
	point
	-3.583,113.877,-9.402
	point
	-1.886,113.469,-12.462
	reverse


// Pedestrian number 97

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-4.818,113.372,-13.182
	point
	-5.230,113.843,-9.658
	point
	-5.088,114.291,-6.315
	reverse


// Pedestrian number 98

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.980,114.297,-6.266
	point
	-1.952,113.934,-8.985
	point
	-1.944,113.656,-11.067
	reverse


// Pedestrian number 99

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.166,114.333,-5.517
	point
	1.442,113.930,-5.452
	point
	4.232,113.498,-5.359
	reverse


// Pedestrian number 100

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.786,112.672,3.337
	point
	-5.428,112.720,0.229
	point
	-10.096,112.778,-3.744
	reverse


// Pedestrian number 101

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-10.357,112.788,-5.893
	point
	-8.228,112.949,-8.527
	point
	-6.275,113.200,-11.809
	reverse


// Pedestrian number 102

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-5.891,113.332,-14.278
	point
	-2.630,113.332,-20.943
	point
	-1.572,113.332,-26.211
	reverse


// Pedestrian number 103

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-10.568,113.332,-28.595
	point
	-12.738,113.332,-37.345
	point
	-15.466,113.332,-40.666
	reverse


// Pedestrian number 104

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-16.589,113.332,-42.354
	point
	-18.195,113.332,-44.817
	point
	-23.151,113.332,-59.047
	reverse


// Pedestrian number 105

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-23.898,113.332,-49.324
	point
	-25.995,113.332,-51.012
	point
	-30.116,113.332,-52.229
	reverse


// Pedestrian number 106

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-35.440,113.334,-53.429
	point
	-36.908,113.352,-51.085
	point
	-39.653,113.400,-45.081
	reverse


// Pedestrian number 107

9				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-40.300,113.369,-48.974
	point
	-38.705,113.383,-47.283
	point
	-36.922,113.392,-46.050
	point
	-36.305,113.412,-43.582
	point
	-35.550,113.436,-40.547
	reverse


// Pedestrian number 108

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-35.510,113.449,-38.855
	point
	-35.569,113.471,-35.761
	point
	-38.609,113.471,-30.045
	point
	-39.642,113.471,-26.920
	reverse


// Pedestrian number 109

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-40.635,113.471,-26.505
	point
	-39.590,113.471,-23.973
	point
	-34.600,113.471,-16.412
	reverse


// Pedestrian number 110

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-29.344,113.471,-23.914
	point
	-30.361,113.471,-21.981
	point
	-32.262,113.471,-18.382
	reverse


// Pedestrian number 111

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-32.848,113.471,-17.341
	point
	-37.763,113.471,-15.063
	point
	-41.180,113.471,-14.727
	point
	-48.052,113.471,-18.576
	reverse


// Pedestrian number 112

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-49.534,113.471,-19.989
	point
	-48.035,113.471,-22.494
	point
	-47.859,113.471,-24.000
	reverse


// Pedestrian number 113

11				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-48.569,113.471,-25.769
	point
	-49.904,113.471,-27.511
	point
	-50.192,113.471,-28.909
	point
	-50.159,113.471,-29.617
	reverse


// Pedestrian number 114

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-49.307,113.471,-31.067
	point
	-45.342,113.471,-32.865
	point
	-41.779,113.471,-35.785
	point
	-39.830,113.431,-41.187
	reverse


// Pedestrian number 115

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-41.050,113.425,-41.954
	point
	-42.370,113.400,-45.117
	point
	-43.875,113.382,-47.370
	reverse


// Pedestrian number 116

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-40.613,113.429,-41.434
	point
	-35.143,113.471,-33.614
	point
	-30.758,113.471,-27.611
	reverse


// Pedestrian number 117

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.324,113.471,-30.636
	point
	-30.497,113.471,-29.091
	point
	-30.462,113.471,-27.658
	reverse


// Pedestrian number 118

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-31.302,113.471,-26.857
	point
	-36.827,113.471,-24.233
	point
	-39.747,113.471,-21.177
	point
	-40.467,113.471,-19.579
	reverse


// Pedestrian number 119

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-41.294,113.471,-21.024
	point
	-41.022,113.471,-20.317
	point
	-40.184,113.471,-19.545
	reverse


// Pedestrian number 120

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-2.131,112.676,-2.610
	point
	-2.848,112.686,-3.739
	point
	-4.443,112.705,-5.188
	reverse


// Pedestrian number 121

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-4.626,112.709,-2.909
	point
	-4.132,112.703,-3.728
	point
	-3.550,112.694,-5.101
	reverse


// Pedestrian number 122

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-2.983,112.688,-2.139
	point
	-3.786,112.698,-3.442
	point
	-4.317,112.704,-4.597
	reverse


// Pedestrian number 123

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.617,112.669,-4.491
	point
	-2.647,112.683,-3.083
	point
	-3.136,112.690,-2.167
	reverse


// Pedestrian number 124

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-8.137,112.757,3.263
	point
	-9.391,112.773,1.432
	point
	-10.193,112.781,-1.467
	reverse


// Pedestrian number 125

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.820,113.471,-19.547
	point
	-39.872,113.471,-25.711
	point
	-40.953,113.471,-26.414
	reverse


// Pedestrian number 126

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-41.613,113.471,-27.591
	point
	-44.287,113.471,-32.400
	point
	-45.496,113.471,-34.445
	reverse


// Pedestrian number 127

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-45.630,113.471,82.000
	point
	-41.896,113.471,89.101
	point
	-40.199,113.471,92.147
	reverse


// Pedestrian number 128

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-36.280,113.471,89.310
	point
	-36.703,113.471,88.953
	point
	-38.666,113.471,91.210
	point
	-40.145,113.471,92.899
	reverse


// Pedestrian number 129

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-35.667,113.471,92.575
	point
	-36.255,113.471,92.861
	point
	-39.717,113.471,91.820
	point
	-42.596,113.471,90.950
	reverse


// Pedestrian number 130

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-44.170,113.471,89.295
	point
	-43.244,113.471,89.241
	point
	-37.314,113.471,91.361
	reverse


// Pedestrian number 131

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-35.826,113.471,89.236
	point
	-33.326,113.471,85.116
	point
	-32.673,113.471,83.266
	reverse


// Pedestrian number 132

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-33.833,113.471,82.482
	point
	-37.415,113.471,85.398
	point
	-39.788,113.471,87.262
	reverse


// Pedestrian number 133

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-41.839,113.471,87.785
	point
	-45.304,113.471,89.802
	point
	-50.497,113.471,92.852
	reverse


// Pedestrian number 134

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-44.124,113.471,100.001
	point
	-43.448,113.471,101.853
	point
	-43.827,113.455,103.883
	reverse


// Pedestrian number 135

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-34.550,113.471,100.107
	point
	-35.580,113.470,101.932
	point
	-38.856,113.420,108.231
	reverse


// Pedestrian number 136

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-38.830,113.414,109.068
	point
	-37.468,113.395,111.466
	point
	-35.381,113.365,115.114
	reverse


// Pedestrian number 137

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-39.677,113.393,111.695
	point
	-42.253,113.367,114.926
	point
	-44.291,113.345,117.744
	reverse


// Pedestrian number 138

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-47.938,113.332,118.396
	point
	-43.815,113.332,122.278
	point
	-34.738,113.332,128.374
	reverse


// Pedestrian number 139

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-33.424,113.332,128.029
	point
	-29.820,113.332,126.991
	point
	-22.583,113.332,124.552
	reverse


// Pedestrian number 140

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-24.003,113.332,115.094
	point
	-22.509,113.332,114.377
	point
	-21.048,113.332,112.726
	reverse


// Pedestrian number 141

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-15.280,113.332,106.292
	point
	-8.637,113.332,101.892
	point
	-2.069,113.332,95.208
	reverse


// Pedestrian number 142

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.694,113.332,89.616
	point
	-2.115,113.332,79.218
	point
	-1.797,113.547,77.579
	reverse


// Pedestrian number 143

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-5.735,113.768,75.925
	point
	-3.818,113.986,74.301
	point
	-1.837,114.311,71.875
	reverse


// Pedestrian number 144

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-5.959,114.321,71.801
	point
	-5.715,114.058,73.761
	point
	-5.822,113.495,77.962
	reverse


// Pedestrian number 145

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-6.438,113.318,78.974
	point
	-6.405,113.159,76.955
	point
	-6.419,112.887,73.522
	reverse


// Pedestrian number 146

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-6.019,112.722,71.320
	point
	-4.793,112.707,70.389
	point
	-3.614,112.693,69.381
	reverse


// Pedestrian number 147

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-5.185,112.713,69.253
	point
	-3.358,112.689,70.101
	point
	-2.238,112.675,70.851
	reverse


// Pedestrian number 148

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.879,112.670,70.885
	point
	-2.463,112.678,68.504
	point
	-1.973,112.671,62.799
	reverse


// Pedestrian number 149

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.906,112.670,62.332
	point
	-4.796,112.709,62.829
	point
	-9.669,112.774,62.471
	reverse


// Pedestrian number 150

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-10.179,112.781,62.342
	point
	-10.461,112.784,63.696
	point
	-8.470,112.756,67.201
	point
	-6.600,112.730,70.340
	reverse


// Pedestrian number 151

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-4.141,112.700,69.281
	point
	-7.280,112.739,70.162
	point
	-8.714,112.756,70.990
	point
	-9.916,112.771,71.312
	reverse


// Pedestrian number 152

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-17.618,112.894,70.681
	point
	-22.768,112.325,71.030
	point
	-28.861,111.652,71.194
	reverse


// Pedestrian number 153

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.836,111.434,62.628
	point
	-28.314,111.712,63.230
	point
	-25.573,112.015,62.372
	reverse


// Pedestrian number 154

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-22.661,112.337,62.355
	point
	-19.200,112.719,64.475
	point
	-17.183,112.942,65.713
	reverse


// Pedestrian number 155

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-10.369,112.780,66.702
	point
	-5.235,112.715,64.104
	point
	-3.454,112.691,62.800
	reverse


// Pedestrian number 156

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-0.285,112.772,62.521
	point
	2.342,112.993,64.057
	point
	5.808,113.286,66.448
	reverse


// Pedestrian number 157

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	6.483,113.332,66.797
	point
	11.016,113.332,68.348
	point
	18.857,113.332,71.033
	reverse


// Pedestrian number 158

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	6.269,113.346,71.029
	point
	3.915,113.650,70.975
	point
	-0.739,114.253,71.024
	reverse


// Pedestrian number 159

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-0.757,114.256,67.083
	point
	2.721,113.804,67.805
	point
	5.724,113.414,67.008
	reverse


// Pedestrian number 160

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	10.235,113.332,62.432
	point
	11.567,113.332,62.788
	point
	14.653,113.332,62.410
	reverse


// Pedestrian number 161

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	20.788,113.332,62.356
	point
	25.135,113.332,61.718
	point
	27.955,113.332,60.294
	point
	28.998,113.332,60.076
	reverse


// Pedestrian number 162

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	30.828,113.332,59.201
	point
	39.500,113.332,60.105
	point
	45.804,113.332,58.458
	reverse


// Pedestrian number 163

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	46.274,113.332,57.374
	point
	45.331,113.332,50.884
	point
	44.346,113.332,45.260
	reverse


// Pedestrian number 164

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	44.909,113.332,43.011
	point
	49.041,113.332,41.886
	point
	54.726,113.332,41.000
	reverse


// Pedestrian number 165

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	55.109,113.332,40.414
	point
	54.004,113.332,38.332
	point
	50.318,113.332,36.212
	point
	46.787,113.332,35.372
	reverse


// Pedestrian number 166

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	45.276,113.342,34.363
	point
	39.748,113.386,30.883
	point
	37.957,113.400,30.338
	reverse


// Pedestrian number 167

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	35.977,113.416,29.391
	point
	31.172,113.454,34.225
	point
	28.875,113.471,35.409
	reverse


// Pedestrian number 168

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	27.542,113.471,36.121
	point
	18.320,113.471,36.883
	point
	10.703,113.471,38.121
	reverse


// Pedestrian number 169

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	7.713,113.471,34.400
	point
	14.932,113.471,37.095
	point
	23.760,113.471,40.401
	reverse


// Pedestrian number 170

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	18.060,113.471,41.234
	point
	13.305,113.471,32.122
	point
	9.980,113.471,27.278
	reverse


// Pedestrian number 171

9				// Ref num
3				// Number of instructions
2				// Initial instruction

	point
	19.673,113.471,29.405
	point
	24.477,113.471,30.049
	reverse


// Pedestrian number 172

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	27.222,113.471,30.477
	point
	27.293,113.471,31.641
	point
	29.798,113.465,35.370
	reverse


// Pedestrian number 173

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	29.879,113.464,30.760
	point
	33.780,113.433,29.861
	point
	35.642,113.419,29.243
	reverse


// Pedestrian number 174

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	36.460,113.412,37.424
	point
	39.359,113.389,36.274
	point
	42.577,113.363,37.537
	reverse


// Pedestrian number 175

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	46.374,113.332,27.373
	point
	46.330,113.332,24.249
	point
	44.329,113.332,20.983
	reverse


// Pedestrian number 176

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	44.538,113.332,21.796
	point
	41.433,113.332,6.502
	point
	38.657,113.332,2.241
	point
	35.580,113.332,-0.770
	reverse


// Pedestrian number 177

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	35.842,113.332,9.848
	point
	34.161,113.332,7.031
	point
	31.780,113.332,6.666
	reverse


// Pedestrian number 178

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	22.959,113.332,4.010
	point
	12.878,113.332,-2.971
	point
	8.007,113.332,-5.327
	reverse


// Pedestrian number 179

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	4.884,113.399,-1.763
	point
	0.916,114.012,-1.401
	point
	-0.852,114.285,-1.350
	reverse


// Pedestrian number 180

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	5.798,113.332,3.307
	point
	9.738,113.332,2.552
	point
	16.076,113.332,3.545
	reverse


// Pedestrian number 181

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	17.143,113.332,3.571
	point
	26.734,113.332,-0.492
	point
	32.016,113.332,-2.221
	reverse


// Pedestrian number 182

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	28.253,113.332,-3.467
	point
	23.077,113.332,-4.479
	point
	18.481,113.332,-5.367
	reverse


// Pedestrian number 183

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	4.842,113.285,-0.966
	point
	0.765,112.875,2.392
	point
	-0.053,112.793,2.870
	point
	-0.915,112.706,3.430
	reverse


// Pedestrian number 184

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-2.422,112.680,0.113
	point
	-1.630,112.670,0.057
	point
	-1.438,112.667,-0.594
	reverse


// Pedestrian number 185

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-3.053,112.689,3.054
	point
	-4.562,112.709,2.431
	point
	-9.755,112.778,3.411
	reverse


// Pedestrian number 186

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-16.554,112.987,2.766
	point
	-21.034,112.492,-1.134
	point
	-25.459,112.003,-5.006
	reverse


// Pedestrian number 187

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-10.278,113.332,-17.783
	point
	-5.128,113.332,-30.597
	point
	-3.542,113.332,-34.683
	point
	-3.514,113.332,-35.782
	reverse


// Pedestrian number 188

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-3.857,113.332,-36.994
	point
	-5.117,113.332,-40.602
	point
	-7.097,113.332,-43.731
	reverse


// Pedestrian number 189

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-7.711,113.332,-44.784
	point
	-8.764,113.332,-46.478
	point
	-15.779,113.332,-48.428
	point
	-21.401,113.332,-48.157
	reverse


// Pedestrian number 190

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-38.949,113.332,-54.953
	point
	-34.291,113.332,-59.519
	point
	-31.603,113.332,-60.443
	point
	-28.263,113.332,-60.513
	reverse


// Pedestrian number 191

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-34.128,113.332,-62.432
	point
	-46.084,113.332,-61.967
	point
	-51.101,113.332,-60.818
	reverse


// Pedestrian number 192

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-51.447,113.332,-60.649
	point
	-53.552,113.332,-53.749
	point
	-55.144,113.332,-49.968
	reverse


// Pedestrian number 193

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-57.294,113.332,-48.227
	point
	-62.747,113.332,-45.297
	point
	-65.113,113.332,-39.827
	reverse


// Pedestrian number 194

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-66.967,113.332,-36.562
	point
	-74.685,113.332,-30.424
	point
	-78.106,113.332,-25.547
	reverse


// Pedestrian number 195

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-78.336,113.332,-23.251
	point
	-73.433,113.332,-12.470
	point
	-70.119,112.906,-7.292
	reverse


// Pedestrian number 196

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-69.479,112.780,-5.197
	point
	-75.714,112.703,-1.369
	point
	-78.106,112.671,-1.272
	reverse


// Pedestrian number 197

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-78.749,112.690,3.432
	point
	-81.588,112.969,2.656
	point
	-83.960,113.203,3.298
	reverse


// Pedestrian number 198

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-86.980,113.332,-0.974
	point
	-90.940,113.332,-2.230
	point
	-99.396,113.332,-5.102
	point
	-102.397,113.332,-4.939
	reverse


// Pedestrian number 199

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-106.687,113.332,-3.887
	point
	-114.091,113.332,-1.274
	point
	-116.273,113.332,-0.114
	reverse


// Pedestrian number 200

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-117.057,113.332,0.294
	point
	-117.461,113.332,6.256
	point
	-117.937,113.332,11.100
	reverse


// Pedestrian number 201

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-118.462,113.332,11.977
	point
	-121.538,113.332,15.900
	point
	-123.919,113.332,19.278
	reverse


// Pedestrian number 202

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-124.815,113.332,21.592
	point
	-125.729,113.332,24.295
	point
	-133.325,113.332,33.368
	point
	-134.949,113.332,36.482
	reverse


// Pedestrian number 203

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-132.560,113.332,39.819
	point
	-133.462,113.332,41.994
	point
	-133.506,113.332,44.292
	reverse


// Pedestrian number 204

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-133.259,113.332,45.321
	point
	-132.797,113.332,46.428
	point
	-130.368,113.332,48.092
	point
	-120.627,113.332,51.847
	reverse


// Pedestrian number 205

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-118.542,113.332,53.860
	point
	-117.457,113.332,55.039
	point
	-115.046,113.332,56.252
	reverse


// Pedestrian number 206

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-107.057,113.332,60.997
	point
	-101.109,113.332,62.752
	point
	-98.413,113.332,62.573
	reverse


// Pedestrian number 207

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-95.831,113.332,62.473
	point
	-88.518,113.332,70.002
	point
	-86.908,113.332,71.187
	reverse


// Pedestrian number 208

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-86.068,113.365,71.384
	point
	-82.948,113.786,69.615
	point
	-79.254,114.285,67.471
	reverse


// Pedestrian number 209

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-78.365,112.670,67.319
	point
	-77.901,112.677,69.826
	point
	-76.437,112.695,71.079
	reverse


// Pedestrian number 210

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-75.463,112.707,71.101
	point
	-72.963,112.741,67.019
	point
	-70.639,112.774,62.807
	reverse


// Pedestrian number 211

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-69.667,112.800,71.762
	point
	-72.189,113.042,74.981
	point
	-73.807,113.247,77.222
	reverse


// Pedestrian number 212

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-77.957,113.395,77.734
	point
	-78.152,113.847,74.816
	point
	-78.553,114.195,72.575
	reverse


// Pedestrian number 213

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-75.014,114.271,72.086
	point
	-74.568,113.765,75.343
	point
	-74.446,113.441,77.437
	reverse


// Pedestrian number 214

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-69.622,113.332,81.365
	point
	-70.128,113.332,83.676
	point
	-69.563,113.332,85.276
	reverse


// Pedestrian number 215

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-69.639,113.332,86.231
	point
	-73.962,113.332,93.796
	point
	-75.079,113.332,104.917
	reverse


// Pedestrian number 216

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-74.236,113.332,107.549
	point
	-68.167,113.332,107.599
	point
	-64.970,113.332,108.854
	point
	-60.783,113.332,111.267
	reverse


// Pedestrian number 217

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-56.919,113.332,114.453
	point
	-53.305,113.332,116.632
	point
	-49.770,113.332,117.876
	reverse


// Pedestrian number 218

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-42.992,113.332,128.376
	point
	-47.878,113.332,126.682
	point
	-58.458,113.332,123.909
	reverse


// Pedestrian number 219

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-60.670,113.332,121.750
	point
	-61.516,113.332,118.229
	point
	-65.679,113.332,104.553
	reverse


// Pedestrian number 220

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-66.748,113.332,102.676
	point
	-68.469,113.332,100.060
	point
	-68.791,113.332,96.257
	reverse


// Pedestrian number 221

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-67.305,113.332,101.043
	point
	-66.856,113.332,104.602
	point
	-64.417,113.332,106.684
	reverse


// Pedestrian number 222

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-57.711,113.332,114.328
	point
	-54.139,113.332,117.851
	point
	-52.694,113.332,117.410
	point
	-50.971,113.332,117.503
	reverse


// Pedestrian number 223

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-49.374,113.332,117.986
	point
	-47.054,113.332,119.920
	point
	-43.770,113.332,119.934
	point
	-43.280,113.335,118.977
	point
	-44.080,113.350,117.042
	reverse


// Pedestrian number 224

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-44.225,113.355,116.509
	point
	-43.517,113.375,113.992
	point
	-44.266,113.399,110.929
	reverse


// Pedestrian number 225

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-44.212,113.405,110.148
	point
	-43.622,113.417,108.643
	point
	-43.899,113.436,106.318
	reverse


// Pedestrian number 226

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-43.791,113.451,104.412
	point
	-39.646,113.430,107.048
	point
	-35.629,113.411,109.341
	reverse


// Pedestrian number 227

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-35.313,113.370,114.495
	point
	-36.530,113.385,112.649
	point
	-35.774,113.401,110.584
	reverse


// Pedestrian number 228

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-35.491,113.417,108.566
	point
	-36.017,113.434,106.485
	point
	-35.472,113.456,103.874
	reverse


// Pedestrian number 229

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-35.520,113.440,105.721
	point
	-37.738,113.413,109.148
	point
	-38.625,113.400,110.788
	reverse


// Pedestrian number 230

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-40.263,113.393,111.672
	point
	-37.893,113.373,114.151
	point
	-35.312,113.353,116.691
	reverse


// Pedestrian number 231

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-35.568,113.359,115.869
	point
	-36.184,113.377,113.610
	point
	-35.536,113.409,109.653
	reverse


// Pedestrian number 232

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-28.302,113.332,117.589
	point
	-20.937,113.332,120.172
	point
	-16.121,113.332,119.864
	reverse


// Pedestrian number 233

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-14.202,113.332,118.366
	point
	-12.946,113.332,115.105
	point
	-8.854,113.332,112.036
	reverse


// Pedestrian number 234

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-6.058,113.332,107.768
	point
	-10.850,113.332,108.066
	point
	-17.554,113.332,109.621
	reverse


// Pedestrian number 235

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-16.122,113.332,107.493
	point
	-18.459,113.332,111.993
	point
	-21.638,113.332,113.242
	reverse


// Pedestrian number 236

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-22.416,113.332,113.870
	point
	-11.928,113.332,112.042
	point
	-7.838,113.332,110.661
	reverse


// Pedestrian number 237

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-7.077,113.332,109.564
	point
	-6.323,113.332,105.267
	point
	-3.990,113.332,102.221
	reverse


// Pedestrian number 238

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-3.632,113.332,100.724
	point
	-6.564,113.332,94.315
	point
	-10.213,113.332,87.300
	reverse


// Pedestrian number 239

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-6.181,113.332,79.247
	point
	-7.870,113.332,81.991
	point
	-10.036,113.332,85.559
	reverse


// Pedestrian number 240

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-1.686,113.332,93.843
	point
	-3.590,113.332,96.379
	point
	-3.265,113.332,99.626
	reverse


// Pedestrian number 241

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-11.780,113.332,102.072
	point
	-13.455,113.332,103.778
	point
	-14.014,113.332,106.111
	point
	-15.425,113.332,106.845
	reverse


// Pedestrian number 242

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-11.114,113.332,115.208
	point
	-15.454,113.332,117.391
	point
	-18.596,113.332,121.578
	reverse


// Pedestrian number 243

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-20.465,113.332,123.122
	point
	-24.279,113.332,123.492
	point
	-27.491,113.332,125.971
	reverse


// Pedestrian number 244

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-28.480,113.332,126.363
	point
	-34.707,113.332,124.955
	point
	-40.844,113.332,128.205
	reverse


// Pedestrian number 245

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-42.503,113.471,81.681
	reverse


// Pedestrian number 246

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.862,113.471,32.686
	reverse


// Pedestrian number 247

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-43.504,113.471,-15.315
	reverse


// Pedestrian number 248

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.401,113.471,31.794
	reverse


// Pedestrian number 249

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-17.633,111.880,41.710
	reverse


// Pedestrian number 250

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-16.917,111.832,41.684
	reverse


// Pedestrian number 251

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-14.663,111.680,41.580
	reverse


// Pedestrian number 252

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-14.229,111.650,41.556
	reverse


// Pedestrian number 253

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-15.434,111.734,25.900
	reverse


// Pedestrian number 254

112				// Ref num
2				// Number of instructions
1				// Initial instruction


	point
	-17.026,111.843,24.003
	reverse


// Pedestrian number 255

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-15.729,111.754,24.062
	reverse


// Pedestrian number 256

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.100,111.875,10.168
	reverse


// Pedestrian number 257

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.121,111.847,9.790
	reverse


// Pedestrian number 258

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.149,111.812,9.303
	reverse


// Pedestrian number 259

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.264,111.670,7.342
	reverse


// Pedestrian number 260

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-48.430,111.627,6.757
	reverse


// Pedestrian number 261

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-48.421,111.665,7.273
	reverse


// Pedestrian number 262

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-48.372,111.760,8.552
	reverse


// Pedestrian number 263

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-48.357,111.828,9.468
	reverse


// Pedestrian number 264

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-62.574,111.879,24.185
	reverse


// Pedestrian number 265

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-63.243,111.833,24.214
	reverse


// Pedestrian number 266

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-63.914,111.787,24.275
	reverse


// Pedestrian number 267

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-64.585,111.742,24.326
	reverse


// Pedestrian number 268

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-62.997,111.854,41.096
	reverse


// Pedestrian number 269

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-63.667,111.807,41.098
	reverse


// Pedestrian number 270

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-64.345,111.760,41.099
	reverse


// Pedestrian number 271

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-64.780,111.730,41.110
	reverse


// Pedestrian number 272

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-65.189,111.702,41.120
	reverse


// Pedestrian number 273

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-65.973,111.647,41.139
	reverse


// Pedestrian number 274

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-48.926,111.877,55.175
	reverse


// Pedestrian number 275

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-48.871,111.820,56.011
	reverse


// Pedestrian number 276

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-48.861,111.785,56.522
	reverse


// Pedestrian number 277

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-48.806,111.735,57.241
	reverse


// Pedestrian number 278

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.410,111.635,58.708
	reverse


// Pedestrian number 279

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.457,111.691,57.901
	reverse


// Pedestrian number 280

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.485,111.725,57.425
	reverse


// Pedestrian number 281

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.526,111.775,56.699
	reverse


// Pedestrian number 282

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.580,111.841,55.757
	reverse


// Pedestrian number 283

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-29.145,109.614,37.285
	reverse


// Pedestrian number 284

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-29.211,109.614,28.302
	reverse


// Pedestrian number 285

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-35.589,109.614,21.944
	reverse


// Pedestrian number 286

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-44.484,109.614,22.001
	reverse


// Pedestrian number 287

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-50.435,109.614,27.974
	reverse


// Pedestrian number 288

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-50.790,109.614,36.604
	reverse


// Pedestrian number 289

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-44.956,109.614,43.032
	reverse


// Pedestrian number 290

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-35.839,109.614,43.342
	reverse


// Pedestrian number 291

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-92.291,113.332,71.272
	reverse


// Pedestrian number 292

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-78.085,113.332,80.902
	reverse


// Pedestrian number 293

134				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-1.880,113.332,82.266
	reverse


// Pedestrian number 294

134				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.809,113.332,70.772
	reverse


// Pedestrian number 295

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.051,113.332,-5.537
	reverse


// Pedestrian number 296

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-2.085,113.332,-14.603
	reverse


// Pedestrian number 297

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-78.120,113.332,-14.240
	reverse


// Pedestrian number 298

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.833,113.332,-4.930
	reverse





START OF OPPONENT PATHS



2                             // Number of path nodes
  -38.713,   -3.180,   17.325   // Node #0
  -41.760,   -3.180,   17.409   // Node #1
 
1                                          // Number of path sections
   
0,   1,   0, 255,   0, 255,    1.0,    1   // Section #0
   

0                                                             // Number of cop start points


END OF OPPONENT PATHS



9										// number of material modifiers

// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT										// room for expansion

//	material '0'
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
3										// room for expansion
SNOW2.MAT										// room for expansion

// material '1'
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
3										// room for expansion
SNOW2.MAT										// room for expansion

// material '2'
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
3										// room for expansion
SNOW2.MAT										// room for expansion

// material '3'
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
3										// room for expansion
SNOW2.MAT										// room for expansion

// material '4'
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
3										// room for expansion
SNOW2.MAT										// room for expansion

// material '5'
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
1										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
0										// sparkiness
3										// room for expansion
SNOW1.MAT										// room for expansion

// material '6'
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT										// room for expansion

// material '7'
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT										// room for expansion

// Non CarObjects

1									// number of non car objects

CONE.TXT


2									// Number of smoke shadetables

222, 230, 245								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"

219, 217, 212								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"



8								// Number of network start points

-41.024,111.142,51.233					//1						
358									

-59.020,111.142,33.125					//2						
272									

-40.294,111.142,13.761					//3						
179									

-20.959,111.142,32.442					//4						
88									

-7.632,111.401,32.890					//5						
90									

-38.849,111.401,66.423					//6						
3									

-72.671,111.401,35.141					//7						
273									

-39.308,111.401,-1.714					//8						
180									



1								// number of splash files
SPLSHGRN.PIX 						//  name of pixelmapfile for splashes


2.0								// Yon multiplier

ZEBRA.TXT
