VERSION 6		// V1 expects map checkpoint rectangles
			// V2 and above expect map checkpoint points
			// V3 and above expect splash file stuff at the end
			// V4 and above expect two sets of PIX and MAT and ped substitution entry

116.65,-6.38,94.81                                                     // Position of centre of start of grid
90										// Direction that grid faces in

// Laps, checkpoints etc

120,60,20							// Initial timer count for each skill level
4									// # laps
10000,5000,3000						// Race completed bonus (all laps raced) for each skill level
75000,50000,30000					// Race completed bonus (all peds killed) for each skill level
20000,10000,5000					// Race completed bonus (all oppos wasted) for each skill level

// Width and height of map checkpoint rectangles
9,18
11,26

4									// # checkpoints

// Checkpoint #4
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
30.23,-1.52,113.66							// Point #0
30.23,100,113.66							// Point #1
26.87,100,113.66							// Point #2
26.87,-1.52,113.66						// Point #3
215,430
140,336

// Checkpoint #1
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
92.73,-5.0,11.92					// Point #0
92.73,100,11.92						// Point #1
92.73,100,17.76						// Point #2
92.73,-5.0,17.76					// Point #3
73,146
168,403

// Checkpoint #2
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
115.60,-100,13.85						// Point #0
115.60,-3.56,13.85						// Point #1
120.27,-3.56,13.85					// Point #2
120.27,-100,13.85						// Point #3
162,324
30,72

// Checkpoint #3
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
132.02,-100,92.85					// Point #0
132.02,100,92.85						// Point #1
132.02,100,96.89						// Point #2
132.02,-100,96.89					// Point #3
195,390
23,55

9									// # pixelmap files to load
INDYSKY.PIX
BARRY.PIX
INDUSTA2.PIX
IHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX
INDTEX29.PIX
INDTEX30.PIX
INDTEX31.PIX

9
INDYSKY.PIX
BARRY.PIX									// # pixelmap files to load(low memory)
INDUSTA8.PIX
IHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX
INDTEX29.PIX
INDTEX30.PIX
INDTEX31.PIX

1									// # shade table files to load
DRRENDER.TAB

14									// # material files to load
INDYWIND.MAT
BARRY.MAT
URINE.MAT
RIVVY.MAT
DRAB.MAT
RIDDY.MAT
INDUSTA2.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
GANTSCRN.MAT
TUNNSCRN.MAT
ACIDSCRN.MAT
SKIDMARK.MAT

14									// # material files to load(low memory)
INDYWIND.MAT
BARRY.MAT
URINE.MAT
RIVVY.MAT
DRAB.MAT
RIDDY.MAT
INDUSTA8.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
GANTSCRN.MAT
TUNNSCRN.MAT
ACIDSCRN.MAT
SKIDMARK.MAT

1									// # model files to load
INDUSTA2.DAT

1									// # model files to load
INDA82.DAT

INDUSTA2.ACT                                                    // Track actor
INDA82.ACT                                                    // Track actor

INDUSTX2.ACT							// Additional actor

// HORIZON STUFF

IHORIZN.PIX						// Name of sky texture pixelmap (or "none")
5									// Horizontal repetitions of sky texture
72									// Vertical size of sky texture (degrees)
83									// Position of horizon (pixels below top)
dark								// Depth cue mode ("none", "dark" or "fog")
7,0									// Degree of fog/darkness

// DEFAULT ENGINE NOISE

0

// SPECIAL EFFECTS VOLUMES

12									// # special effects volumes

DEFAULT WATER
0.2									// gravity multiplier
50									// viscosity multiplier
0									// Car damage per millisecond
0.002								// Pedestrian damage per millisecond
0									// camera effect index
1									// Sky colour
URINE.MAT								// Windscreen material to use
5100								// Sound ID of entry noise
5100								// Sound ID of exit noise
2									// Engine noise index
0									// material index


//------------------------ 0 -----------------------------------------
NEW IMPROVED!
-0.059, -0.003, -2.073
0.003, 1.200, -0.002
1.808, -0.005, -0.052
129.995, -4.116, 94.844
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 1 -----------------------------------------
NEW IMPROVED!
-0.039, 0.000, -2.986
-0.001, 0.833, 0.000
7.429, 0.006, -0.096
100.145, 0.271, 14.817
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 2 -----------------------------------------
NEW IMPROVED!
0.010, 0.002, 1.000
0.000, 1.000, -0.002
-4.680, 0.000, 0.047
124.928, -4.640, 19.399
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIVVY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 3 -----------------------------------------
NEW IMPROVED!
0.002, 0.002, 1.000
0.000, 1.000, -0.002
-4.095, 0.000, 0.009
124.127, -4.660, 14.664
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIVVY.MAT			// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 4 -----------------------------------------
NEW IMPROVED!
-0.001, 0.002, 1.000
0.000, 1.000, -0.002
-4.148, 0.000, -0.006
124.241, -4.600, 10.052
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIVVY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 5 -----------------------------------------
NEW IMPROVED!
-0.034, 0.001, -2.091
-0.002, 1.000, 0.000
7.447, 0.019, -1.082
45.792, -0.839, 127.248
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

//------------------------ 6 -----------------------------------------
NEW IMPROVED!
2.165, -0.001, -1.226
0.001, 1.000, 0.001
5.273, -0.008, 9.310
36.041, -0.518, 125.615
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 7 -----------------------------------------
NEW IMPROVED!
-2.986, 0.000, 0.032
0.000, 1.000, 0.000
-0.022, 0.000, -2.073
28.756, -0.837, 116.283
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 8 -----------------------------------------
NEW IMPROVED!
-7.430, 0.000, 0.037
0.000, 1.728, 0.000
-0.016, 0.000, -3.305
25.154, -3.137, 103.812
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
RIDDY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 9 -----------------------------------------
NEW IMPROVED!
0.043, -0.001, 1.727
0.010, 4.300, 0.003
-10.117, 0.024, 0.254
42.168, -3.558, 86.838
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
DRAB.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


//------------------------ 10 -----------------------------------------
NEW IMPROVED!
6.183, -0.003, 0.321
0.002, 2.986, -0.007
-0.385, 0.018, 7.420
118.839, -5.178, 57.802
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// sky colour
BARRY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index

 
// REFLECTIVE WINDSCREEN SPECIFICATIONS

INDYWIND.MAT							// Material to use for default screens
BARRY.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT							// Material to use for default screens during fog

6									// # areas with different screens
111.3,50,125.6,52					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,53.7,125.6,55.7				// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,58,125.6,60					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,61,125.6,63					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
111.3,65,125.6,67					// x-min, z-min, x-max, z-max rectangle describing area
GANTSCRN.MAT						// Material to use instead
67.9,76.6,111.7,96.5				// x-min, z-min, x-max, z-max rectangle describing area
TUNNSCRN.MAT						// Material to use instead

// MAP DETAILS

INDAMAP2.PIX						// Map pixelmap name

1.38,	0,		0					// World->map transformation matrix
0,		0,		0
0,		1.38,	0
37.3,	14.2,	0

// ****** START OF FUNK AND GROOVE STUFF ******

START OF FUNK

INDFAN01.MAT
distance
piss off
no fucking lighting bastards
frames
approximate
continuous
12
3
INDTEX29.PIX
INDTEX30.PIX
INDTEX31.PIX

NEXT FUNK

LIQUID.MAT
constant
roll
continuous
0,0.1
no fucking lighting
no animation you cunt

NEXT FUNK

CHECK.MAT
constant
roll
continuous
0.2,0
no fucking lighting
no animation you cunt

NEXT FUNK

!LIQUID.MAT
constant
throb
harmonic
0.13,0.09
5,5
50,50
no fucking lighting
no animation you cunt

NEXT FUNK

ACIDSCRN.MAT
constant
throb
harmonic
0.13,0.09
5,5
50,50
no fucking lighting
no animation you cunt

END OF FUNK

START OF GROOVE

&RCH0026.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0014.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0013.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0017.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0008.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0007.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&RCH0002.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.25								// Cycles per second
0,0,0.3								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&MNO0005.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
harmonic								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.1								// Cycles per second
1.5,0,0								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&MNO0003.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
harmonic								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.1								// Cycles per second
1.5,0,0								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&MNO0009.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
harmonic								// Motion is linear (i.e. direction changes instantly)
0,0,0								// Centre of movement
0.1								// Cycles per second
1.5,0,0								// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&CBO0012.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
no fucking path you cuuuuuuunt		// Does not move on a path
rock								// Object itself rocks
linear								// Motion is linear (i.e. direction changes instantly)
0.12								// Cycles per second
0,0,0								// Centre of movement
y									// Axis to rock in
90									// Angle to rock (each way)

NEXT GROOVE

&CAR0012.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,-0.1							// Centre of movement
0.2									// Cycles per second
0,0,0.15							// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

NEXT GROOVE

&CBO0001.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
no fucking path you cuuuuuuunt		// Does not move on a path
rock								// Object itself rocks
linear								// Motion is linear (i.e. direction changes instantly)
0.12								// Cycles per second
0,0,0								// Centre of movement
y									// Axis to rock in
90									// Angle to rock (each way)

NEXT GROOVE

&CAR0001.ACT						// Actor name of moving part
not a fuckin lolliiipop				// Not a lollipop
distance							// Only moves when in view
straight							// Moves on a straight path
linear								// Motion is linear (i.e. direction changes instantly)
0,0,-0.1							// Centre of movement
0.2									// Cycles per second
0,0,0.15							// Amount of movement (each way) in each axis
no object moving cunt				// Object itself does not change orientation

END OF GROOVE


// ****** START OF PEDESTRIAN STUFF ******

9				// Ped subs table index

364				// Number of pedestrians

// Pedestrian number 1

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	5.259,-9.343,-4.543
	point
	5.259,-9.343,-4.543
	point
	4.451,996.000,-6.772
	point
	-3.686,996.000,-5.729
	point
	-7.395,996.000,-5.826
	reverse


// Pedestrian number 2

11				// Ref num
5				// Number of instructions
1				// Initial instruction

	point
	148.580,-5.177,36.716
	point
	148.238,-5.177,38.666
	point
	148.991,-5.177,44.640
	point
	136.110,-5.178,56.633
	reverse


// Pedestrian number 3

2				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	144.254,-5.116,28.687
	point
	149.087,-5.177,37.075
	point
	148.126,-5.177,43.342
	point
	148.930,-5.177,104.704
	reverse


// Pedestrian number 4

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	144.592,-5.177,39.950
	point
	147.111,-5.177,34.963
	point
	149.081,-5.177,29.866
	point
	144.220,-5.177,27.661
	reverse


// Pedestrian number 5

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	146.701,-5.177,37.813
	point
	142.899,-5.177,36.790
	point
	134.105,-5.177,32.951
	reverse


// Pedestrian number 6

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	145.705,-5.177,38.889
	point
	142.825,-5.177,37.021
	point
	140.413,-5.177,33.083
	reverse


// Pedestrian number 7

9				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	143.777,-5.177,44.822
	point
	143.469,-5.177,33.004
	reverse


// Pedestrian number 8

9				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	142.451,-5.177,39.728
	point
	148.901,-5.177,27.258
	point
	144.289,-5.177,15.066
	point
	148.267,-5.177,2.254
	point
	151.621,-5.177,-2.814
	reverse


// Pedestrian number 9

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	146.212,-5.177,-2.990
	point
	147.778,-5.177,2.357
	point
	148.948,-5.177,11.945
	point
	145.218,-5.177,39.315
	reverse


// Pedestrian number 10

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	148.053,-5.177,-3.027
	point
	147.422,-5.177,2.351
	point
	148.493,-5.177,53.797
	reverse


// Pedestrian number 11

3				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	144.566,-5.181,-2.960
	point
	144.348,-5.181,0.979
	point
	149.564,-5.177,7.073
	point
	144.239,-5.178,13.704
	point
	147.040,-5.171,37.454
	reverse


// Pedestrian number 12

10				// Ref num
7				// Number of instructions
5				// Initial instruction

	point
	147.804,-5.171,36.733
	point
	148.967,-5.174,19.044
	point
	144.139,-5.177,15.975
	point
	148.895,-5.176,10.141
	point
	145.006,-5.180,0.888
	point
	142.693,-5.182,-3.086
	reverse


// Pedestrian number 13

2				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	141.195,-5.171,52.129
	point
	146.447,-5.167,56.834
	point
	149.016,-5.164,67.117
	point
	143.908,-5.164,78.580
	reverse


// Pedestrian number 14

11				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	145.142,-5.170,48.666
	point
	146.040,-5.167,56.743
	point
	148.992,-5.166,59.274
	point
	148.890,-5.161,80.193
	point
	145.427,-5.162,80.697
	point
	127.017,-5.171,80.815
	reverse


// Pedestrian number 15

14				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	144.604,-5.170,48.790
	point
	144.784,-5.168,56.794
	point
	144.744,-5.163,78.635
	point
	137.363,-5.167,78.782
	point
	137.551,-5.166,80.446
	point
	138.783,-5.166,80.467
	reverse


// Pedestrian number 16

7				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	143.116,-5.170,49.918
	point
	144.329,-5.168,56.863
	point
	149.007,-5.163,72.414
	point
	149.037,-5.161,80.799
	point
	146.001,-5.161,84.185
	point
	144.329,-5.162,84.229
	point
	144.149,-5.163,82.185
	reverse


// Pedestrian number 17

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	136.226,-5.173,53.005
	point
	145.095,-5.167,60.482
	point
	148.938,-5.165,63.942
	point
	148.797,-5.163,71.161
	point
	140.826,-5.165,79.360
	reverse


// Pedestrian number 18

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	134.984,-5.170,70.103
	point
	141.940,-5.164,78.747
	point
	143.065,-5.164,80.378
	point
	144.667,-5.162,85.150
	reverse


// Pedestrian number 19

2				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	148.895,-5.162,75.639
	point
	142.329,-5.164,78.754
	point
	140.627,-5.165,80.446
	point
	137.155,-5.166,82.427
	reverse


// Pedestrian number 20

7				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	139.301,-5.165,80.480
	point
	142.204,-5.162,89.425
	point
	143.331,-5.161,91.465
	point
	143.338,-5.161,92.696
	point
	144.082,-5.160,93.146
	point
	144.619,-5.160,92.891
	reverse


// Pedestrian number 21

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	143.585,-5.160,95.289
	point
	141.933,-5.162,89.322
	point
	137.113,-5.166,82.900
	reverse


// Pedestrian number 22

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	137.987,-5.163,93.965
	point
	141.397,-5.162,89.191
	point
	145.043,-5.162,84.266
	reverse


// Pedestrian number 23

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	144.735,-5.162,84.200
	point
	141.687,-5.161,94.427
	point
	139.123,-5.162,95.934
	point
	135.867,-5.163,95.913
	point
	135.585,-5.163,99.305
	point
	136.435,-5.162,100.029
	reverse


// Pedestrian number 24

11				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	136.562,-5.166,84.824
	point
	141.822,-5.161,94.914
	point
	143.802,-5.159,97.710
	point
	145.254,-5.159,97.160
	reverse


// Pedestrian number 25

14				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	133.895,-5.163,99.849
	point
	139.094,-5.161,98.923
	point
	141.431,-5.161,94.893
	point
	145.224,-5.160,92.842
	point
	145.443,-5.159,95.319
	reverse


// Pedestrian number 26

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	139.314,-5.162,94.981
	point
	140.895,-5.161,95.065
	point
	148.889,-5.158,95.505
	point
	149.066,-5.155,104.623
	reverse


// Pedestrian number 27

9				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	138.505,-5.161,100.865
	point
	142.123,-5.159,100.773
	point
	142.040,-5.159,101.351
	point
	141.570,-5.160,101.529
	point
	135.367,-5.162,104.579
	point
	127.760,-5.166,101.406
	reverse


// Pedestrian number 28

9				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	132.306,-5.165,97.451
	point
	130.309,-5.165,99.145
	point
	132.148,-5.163,104.683
	point
	142.006,-5.159,101.402
	point
	149.021,-5.156,101.511
	reverse


// Pedestrian number 29

9				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	148.847,-5.156,104.028
	point
	139.837,-5.160,102.495
	point
	137.054,-5.162,101.941
	point
	134.853,-5.163,102.170
	point
	133.435,-5.164,98.211
	point
	131.505,-5.165,97.793
	reverse


// Pedestrian number 30

9				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	128.741,-5.172,73.167
	point
	129.923,-5.170,77.071
	point
	133.349,-5.168,78.306
	point
	134.363,-5.168,80.379
	point
	135.323,-5.166,84.533
	point
	136.281,-5.166,84.718
	reverse


// Pedestrian number 31


9				// Ref num
11				// Number of instructions
8				// Initial instruction

	point
	133.496,-5.170,71.673
	point
	131.635,-5.170,75.436
	point
	129.565,-5.171,75.515
	point
	128.102,-5.171,77.206
	point
	127.362,-5.171,80.109
	point
	132.332,-5.168,84.493
	point
	132.415,-5.167,86.629
	point
	139.540,-5.163,89.055
	point
	143.512,-5.161,93.068
	point
	144.031,-5.160,92.883
	reverse


// Pedestrian number 32

11				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	132.338,-5.164,99.011
	point
	132.235,-5.166,93.504
	point
	133.052,-5.166,90.396
	point
	132.402,-5.167,88.462
	point
	131.965,-5.169,80.072
	reverse


// Pedestrian number 33

2				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	132.262,-5.169,80.095
	point
	132.440,-5.167,88.946
	point
	132.148,-5.166,91.851
	point
	132.200,-5.165,97.168
	point
	131.129,-5.165,97.910
	reverse


// Pedestrian number 34

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	134.043,-5.165,94.001
	point
	139.604,-5.164,85.237
	point
	141.268,-5.165,79.506
	reverse


// Pedestrian number 35

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	133.401,-5.169,76.331
	point
	143.135,-5.166,70.197
	point
	148.826,-5.164,65.294
	point
	148.385,-5.180,-3.084
	reverse


// Pedestrian number 36

9				// Ref num
8				// Number of instructions
5				// Initial instruction

	point
	149.009,-5.158,91.468
	point
	145.331,-5.161,89.047
	point
	145.377,-5.161,87.921
	point
	144.451,-5.162,86.963
	point
	136.559,-5.166,85.144
	point
	130.178,-5.169,83.124
	point
	127.489,-5.171,78.971
	reverse


// Pedestrian number 37

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	127.385,-5.171,81.080
	point
	132.079,-5.168,84.515
	point
	144.877,-5.161,88.533
	point
	145.166,-5.160,91.076
	reverse


// Pedestrian number 38

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	148.883,-5.159,88.109
	point
	145.324,-5.161,88.537
	point
	139.574,-5.162,93.486
	point
	139.030,-5.162,97.971
	point
	137.332,-5.162,100.176
	reverse


// Pedestrian number 39

7				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	143.077,-5.158,104.353
	point
	143.215,-5.160,97.599
	point
	144.354,-5.159,97.175
	point
	148.411,-5.157,98.481
	point
	148.988,-5.156,100.421
	point
	149.072,-5.156,103.392
	reverse


// Pedestrian number 40

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	139.858,-5.165,80.508
	point
	139.359,-5.163,88.792
	point
	138.815,-5.163,94.093
	reverse


// Pedestrian number 41

9				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	119.024,-5.193,-3.031
	point
	116.029,-5.193,4.572
	point
	116.080,-5.191,12.202
	point
	116.251,-5.188,24.406
	point
	117.389,-5.187,26.036
	reverse


// Pedestrian number 42

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	127.315,995.095,19.390
	point
	119.579,995.097,19.700
	point
	117.659,-5.097,21.913
	point
	116.390,995.107,23.348
	point
	112.473,993.665,24.532
	reverse


// Pedestrian number 43

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	117.213,-5.171,-2.918
	point
	118.213,995.029,12.609
	point
	120.243,995.096,14.981
	point
	127.246,-5.105,14.748
	reverse


// Pedestrian number 44

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	117.436,-5.082,22.170
	point
	117.161,-5.111,12.516
	point
	116.275,-5.133,4.946
	point
	111.147,-5.156,-2.871
	reverse


// Pedestrian number 45

3				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	120.162,995.093,19.023
	point
	118.457,995.101,21.789
	point
	118.437,-5.096,22.805
	point
	116.600,-5.091,24.526
	point
	118.285,-5.086,26.308
	point
	117.745,-5.082,27.581
	point
	115.877,-5.075,30.135
	reverse


// Pedestrian number 46

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	118.225,-5.170,-2.976
	point
	114.526,995.050,4.151
	point
	113.986,994.246,5.729
	point
	112.309,993.695,16.303
	point
	108.810,992.246,18.753
	reverse


// Pedestrian number 47

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	112.820,-5.176,-2.894
	point
	113.429,995.024,3.929
	point
	110.864,993.039,7.128
	point
	119.692,995.023,7.898
	reverse


// Pedestrian number 48

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	110.798,-5.177,-2.889
	point
	110.473,995.023,4.146
	point
	109.567,992.539,6.684
	reverse


// Pedestrian number 49

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	109.453,-5.177,-2.846
	point
	107.556,995.023,4.284
	point
	106.814,991.933,7.184
	reverse


// Pedestrian number 50

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	107.201,-5.177,-2.890
	point
	104.780,995.023,4.253
	point
	103.732,991.933,7.748
	reverse


// Pedestrian number 51

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	119.780,-5.176,2.549
	point
	106.681,-5.176,-0.117
	point
	104.653,-5.176,-1.010
	point
	104.148,-5.176,-3.052
	reverse


// Pedestrian number 52

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	119.733,-5.176,4.367
	point
	105.943,-5.176,-1.176
	point
	105.716,-5.176,-2.196
	reverse


// Pedestrian number 53

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	151.666,-5.176,-0.848
	point
	117.774,-5.176,-2.963
	point
	104.987,-5.176,-2.793
	point
	104.862,-5.176,-2.229
	reverse


// Pedestrian number 54

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	151.684,-5.176,-1.414
	point
	117.345,-5.176,-2.604
	point
	105.824,-5.176,-2.410
	reverse


// Pedestrian number 55

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	121.117,-5.177,-3.057
	point
	119.999,-5.177,0.192
	point
	116.464,-5.177,9.356
	point
	116.778,-5.177,28.088
	point
	117.441,-5.177,27.075
	reverse


// Pedestrian number 56

9				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	118.110,-5.177,36.445
	point
	119.144,-5.177,35.158
	point
	117.680,-5.177,29.237
	point
	116.412,-5.177,25.790
	point
	117.301,-5.177,25.110
	reverse


// Pedestrian number 57

10				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	100.303,-5.172,33.273
	point
	115.404,-5.171,32.720
	point
	115.892,-5.173,33.532
	point
	116.171,-5.183,38.176
	point
	117.564,-5.184,38.351
	point
	129.654,-5.203,46.534
	reverse


// Pedestrian number 58

2				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	100.326,-5.172,33.581
	point
	115.218,-5.179,36.451
	point
	119.682,-5.196,43.729
	point
	124.372,-5.207,48.684
	point
	124.423,-5.211,50.454
	point
	122.925,-5.213,51.052
	reverse


// Pedestrian number 59

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	125.070,-5.176,37.249
	point
	129.272,-5.176,33.309
	point
	137.805,-5.176,33.126
	point
	144.347,-5.176,40.159
	reverse


// Pedestrian number 60

10				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	124.559,-5.176,33.013
	point
	131.781,-5.176,41.633
	point
	132.745,-5.176,44.494
	point
	136.346,-5.176,47.987
	point
	139.698,-5.176,47.964
	point
	143.251,-5.176,44.404
	point
	143.736,-5.176,32.905
	reverse


// Pedestrian number 61

14				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	138.775,-5.176,33.119
	point
	143.216,-5.176,40.474
	point
	143.406,-5.176,45.027
	point
	138.809,-5.176,48.599
	point
	138.092,-5.176,47.941
	point
	135.662,-5.176,48.187
	reverse


// Pedestrian number 62

7				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	122.559,-5.176,50.575
	point
	118.410,-5.176,53.316
	point
	113.382,-5.176,56.633
	point
	113.469,-5.176,58.088
	point
	124.512,-5.176,64.455
	reverse


// Pedestrian number 63

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	115.311,-5.176,50.997
	point
	118.376,-5.176,55.256
	point
	124.442,-5.176,59.450
	reverse


// Pedestrian number 64

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	113.158,-5.176,59.141
	point
	119.060,-5.176,62.251
	point
	124.407,-5.176,66.067
	point
	123.867,-5.176,68.751
	reverse


// Pedestrian number 65

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	113.132,-5.176,52.420
	point
	117.606,-5.176,55.493
	point
	124.733,-5.176,58.484
	point
	124.733,-5.176,58.484
	reverse


// Pedestrian number 66

11				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	124.700,-5.176,51.872
	point
	118.164,-5.176,56.960
	point
	113.138,-5.176,62.609
	point
	114.397,-5.176,68.663
	point
	110.901,-5.176,72.749
	reverse


// Pedestrian number 67

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	113.011,-5.176,65.366
	point
	119.585,-5.176,61.064
	point
	124.619,-5.176,56.935
	reverse


// Pedestrian number 68

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	124.628,-5.176,61.948
	point
	120.149,-5.176,58.724
	point
	114.592,-5.176,50.970
	reverse


// Pedestrian number 69

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	128.732,-5.176,71.806
	point
	120.664,-5.176,69.986
	point
	117.618,-5.176,68.368
	reverse


// Pedestrian number 70

3				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	113.209,-5.176,66.188
	point
	117.588,-5.176,67.880
	point
	120.157,-5.176,70.183
	point
	125.738,-5.176,72.899
	point
	128.000,-5.176,72.440
	reverse


// Pedestrian number 71

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	108.920,-5.176,71.631
	point
	114.841,-5.176,67.518
	point
	124.567,-5.176,62.353
	reverse


// Pedestrian number 72

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	129.526,-5.176,70.963
	point
	119.960,-5.176,71.689
	point
	114.000,-5.176,74.105
	reverse


// Pedestrian number 73

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	122.026,-6.382,89.475
	point
	120.021,993.818,87.119
	point
	116.228,995.023,69.827
	reverse


// Pedestrian number 74

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	128.171,995.023,86.499
	point
	120.359,993.818,86.653
	point
	116.437,993.818,88.197
	point
	112.245,994.949,90.212
	reverse


// Pedestrian number 75

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	119.288,-6.382,91.387
	point
	120.609,-6.382,96.806
	point
	117.862,994.949,100.570
	reverse


// Pedestrian number 76

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	115.297,-5.170,69.804
	point
	114.288,-5.170,77.636
	point
	114.030,-5.170,80.207
	reverse


// Pedestrian number 77

9				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	125.467,-5.227,99.186
	point
	123.345,-6.382,96.769
	point
	120.113,-6.381,91.023
	point
	121.179,-6.381,90.091
	point
	122.357,-6.381,87.676
	reverse


// Pedestrian number 78

9				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	123.492,-6.381,86.978
	point
	123.411,-6.381,88.038
	point
	121.015,-6.381,88.401
	point
	119.947,994.019,91.017
	point
	114.912,994.983,98.949
	reverse


// Pedestrian number 79

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	122.982,-6.382,91.586
	point
	122.538,-6.382,93.147
	point
	119.463,994.018,93.398
	point
	112.210,994.957,96.609
	reverse


// Pedestrian number 80

10				// Ref num
9				// Number of instructions
3				// Initial instruction

	point
	112.226,994.954,96.076
	point
	111.997,995.023,94.950
	point
	106.584,995.023,95.373
	point
	90.790,-5.177,92.778
	point
	89.136,-5.177,81.603
	point
	83.739,-5.177,78.080
	point
	67.711,-5.177,79.431
	point
	61.240,-5.199,86.833
	reverse


// Pedestrian number 81

10				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	131.752,-5.177,67.911
	point
	125.398,-5.177,68.475
	point
	122.933,-5.177,67.370
	point
	120.620,-5.177,67.346
	point
	113.046,-5.177,64.949
	reverse


// Pedestrian number 82

9				// Ref num
8				// Number of instructions
6				// Initial instruction

	point
	121.546,-5.177,50.222
	point
	118.110,-5.177,53.598
	point
	120.149,-5.177,56.144
	point
	117.521,-5.177,59.421
	point
	119.876,-5.177,62.558
	point
	118.420,-5.177,65.240
	point
	119.560,-5.177,68.893
	reverse


// Pedestrian number 83

11				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	122.432,993.818,85.069
	point
	122.068,995.023,80.262
	point
	120.716,-5.177,73.782
	point
	116.852,-5.177,69.607
	reverse


// Pedestrian number 84

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	122.980,-6.381,91.687
	point
	119.917,-6.381,91.526
	point
	119.795,993.819,90.534
	point
	112.324,995.023,67.628
	reverse


// Pedestrian number 85

11				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	126.058,-5.217,98.627
	point
	123.958,-6.382,96.814
	point
	121.246,-6.382,91.276
	point
	121.651,-6.382,88.330
	point
	122.603,-6.382,88.239
	point
	123.649,-6.382,87.614
	point
	123.586,-6.382,85.714
	reverse


// Pedestrian number 86

10				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	113.119,-5.268,82.952
	point
	116.026,-6.382,84.841
	point
	120.052,-6.381,90.173
	point
	121.437,-6.381,91.649
	point
	123.992,-6.382,92.084
	point
	127.794,-5.239,90.855
	reverse


// Pedestrian number 87

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	127.969,-5.192,87.350
	point
	124.019,-6.382,88.134
	point
	121.359,-6.382,88.150
	point
	116.036,-6.382,89.314
	point
	112.342,994.918,90.169
	reverse


// Pedestrian number 88

14				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	114.454,994.934,98.980
	point
	116.092,-6.382,96.812
	point
	118.838,-6.382,91.108
	point
	122.473,-6.382,87.723
	reverse


// Pedestrian number 89

11				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	118.306,-5.209,100.727
	point
	118.172,-6.382,96.783
	point
	118.651,-6.382,93.229
	point
	118.875,-6.382,87.943
	point
	122.059,-6.382,86.082
	reverse


// Pedestrian number 90

11				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	112.174,-5.230,96.330
	point
	116.018,-6.382,95.693
	point
	116.477,-6.382,93.154
	point
	122.543,-6.382,91.641
	reverse


// Pedestrian number 91

13				// Ref num
9				// Number of instructions
3				// Initial instruction

	point
	127.180,995.023,95.266
	point
	111.063,995.023,94.203
	point
	93.734,-5.177,94.565
	point
	90.272,-5.177,92.227
	point
	87.969,-5.177,82.370
	point
	85.290,-5.177,77.520
	point
	66.593,-5.176,77.832
	point
	65.473,-5.198,75.430
	reverse


// Pedestrian number 92

9				// Ref num
10				// Number of instructions
5				// Initial instruction

	point
	113.206,995.023,97.521
	point
	111.964,995.023,95.583
	point
	103.291,-5.177,95.236
	point
	97.658,-5.177,94.914
	point
	89.785,-5.177,91.127
	point
	87.673,-5.177,81.046
	point
	85.439,-5.177,79.180
	point
	83.682,-5.177,79.021
	point
	57.049,-5.211,78.595
	reverse


// Pedestrian number 93

16				// Ref num
10				// Number of instructions
5				// Initial instruction

	point
	94.053,-5.177,94.640
	point
	93.146,-5.177,92.682
	point
	91.697,-5.177,91.466
	point
	91.000,-5.177,90.030
	point
	90.280,-5.177,86.453
	point
	88.652,-5.177,80.217
	point
	84.779,-5.177,79.140
	point
	71.990,-5.177,77.805
	point
	53.657,-5.212,83.482
	reverse


// Pedestrian number 94

16				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	64.029,-5.177,75.504
	point
	63.887,-5.177,79.659
	point
	67.857,-5.177,84.533
	reverse


// Pedestrian number 95

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	67.196,-5.177,84.563
	point
	66.089,-5.177,80.105
	point
	67.862,-5.176,77.835
	reverse


// Pedestrian number 96

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	53.551,-5.179,85.812
	point
	64.881,-5.177,80.167
	point
	81.326,-5.177,77.343
	reverse


// Pedestrian number 97

11				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	10.699,-5.177,88.485
	point
	12.438,-5.177,88.487
	point
	12.483,-5.177,87.845
	point
	19.147,-5.177,87.228
	point
	19.861,-5.177,88.429
	reverse


// Pedestrian number 98

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	10.550,-5.177,87.229
	point
	18.856,-5.177,86.839
	point
	19.162,-5.177,88.085
	point
	18.215,-5.177,92.513
	reverse


// Pedestrian number 99

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	20.981,-5.177,85.211
	point
	18.481,-5.177,87.422
	point
	10.529,-5.177,80.923
	reverse


// Pedestrian number 100

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.175,-5.177,92.576
	point
	23.174,-5.177,87.505
	point
	10.651,-5.177,82.066
	reverse


// Pedestrian number 101

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	14.412,-5.177,92.385
	point
	14.702,-5.177,90.543
	point
	15.758,-5.177,88.428
	point
	31.698,-5.177,83.717
	reverse


// Pedestrian number 102

11				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	10.616,-5.177,92.646
	point
	10.598,-5.177,90.046
	point
	12.620,-5.177,89.487
	point
	13.602,-5.177,88.352
	point
	18.961,995.023,84.937
	point
	20.767,991.481,80.133
	reverse


// Pedestrian number 103

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	18.177,-5.177,88.387
	point
	13.201,-5.177,87.795
	point
	11.902,-5.177,89.962
	point
	10.510,-5.177,89.733
	reverse


// Pedestrian number 104

3				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	18.759,995.023,88.292
	point
	22.617,995.912,82.605
	point
	22.421,995.023,49.442
	point
	28.094,-5.177,45.793
	reverse


// Pedestrian number 105

16				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	15.699,-5.177,46.170
	point
	21.360,995.023,50.745
	point
	21.318,995.023,86.560
	point
	20.846,-5.177,88.171
	reverse


// Pedestrian number 106

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.243,995.023,92.528
	point
	21.506,996.699,77.186
	point
	19.373,986.858,75.038
	reverse


// Pedestrian number 107

6				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.725,995.023,92.397
	point
	22.520,996.705,77.123
	point
	23.341,991.480,69.365
	reverse


// Pedestrian number 108

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	31.071,-5.177,64.052
	point
	30.458,-5.177,73.853
	point
	31.178,995.023,84.337
	point
	31.573,995.023,92.543
	reverse


// Pedestrian number 109

6				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	20.874,-5.177,52.518
	point
	21.046,-5.177,48.452
	point
	22.652,-5.177,43.328
	reverse


// Pedestrian number 110

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.234,-5.177,52.545
	point
	22.800,-5.177,47.818
	point
	19.145,-5.177,40.542
	reverse


// Pedestrian number 111

6				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	10.641,-5.177,59.783
	point
	20.460,-5.177,50.253
	point
	24.445,-5.177,43.993
	reverse


// Pedestrian number 112

16				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	10.716,-5.177,47.813
	point
	14.346,-5.177,47.825
	point
	20.462,-5.177,49.433
	point
	30.904,-5.177,47.615
	point
	35.638,-5.177,47.911
	reverse


// Pedestrian number 113

5				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	24.906,-5.177,42.026
	point
	26.079,-5.177,42.372
	point
	26.390,-5.177,43.328
	point
	25.587,-5.177,44.526
	point
	16.121,-5.177,50.262
	reverse


// Pedestrian number 114

3				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	35.474,-5.177,47.135
	point
	29.920,-5.177,47.820
	point
	22.494,-5.177,44.825
	point
	20.913,-5.177,43.099
	point
	20.741,-5.177,40.504
	point
	27.684,-5.177,41.001
	reverse


// Pedestrian number 115

10				// Ref num
5				// Number of instructions
4				// Initial instruction

	point
	133.936,-5.177,-1.453
	point
	132.525,-5.177,-1.433
	point
	132.103,-5.177,-0.853
	point
	132.315,-5.177,-0.374
	reverse


// Pedestrian number 116

134				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	146.850,-5.177,9.438
	reverse


// Pedestrian number 117

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	147.986,-5.178,13.691
	reverse


// Pedestrian number 118

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	146.724,-5.178,15.651
	reverse


// Pedestrian number 119

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.828,-5.177,22.999
	reverse


// Pedestrian number 120

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	137.937,-5.178,35.283
	reverse


// Pedestrian number 121

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	143.518,-5.177,42.189
	reverse


// Pedestrian number 122

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.858,-5.178,46.227
	reverse


// Pedestrian number 123

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.314,-5.177,48.235
	reverse


// Pedestrian number 124

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.141,-5.178,47.152
	reverse


// Pedestrian number 125

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.708,-5.178,54.174
	reverse


// Pedestrian number 126

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.343,-5.179,59.299
	reverse


// Pedestrian number 127

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	138.565,-5.177,65.294
	reverse


// Pedestrian number 128

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	129.180,-5.177,76.511
	reverse


// Pedestrian number 129

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	128.986,-5.178,77.055
	reverse


// Pedestrian number 130

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	128.949,-5.178,77.850
	reverse


// Pedestrian number 131

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	129.045,-5.178,78.852
	reverse


// Pedestrian number 132

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	128.169,-5.178,78.479
	reverse


// Pedestrian number 133

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	128.319,-5.177,77.301
	reverse


// Pedestrian number 134

134				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	133.663,-5.178,82.717
	reverse


// Pedestrian number 135

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.801,-5.162,94.634
	reverse


// Pedestrian number 136

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.691,-5.166,96.265
	reverse


// Pedestrian number 137

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	135.862,-5.170,98.456
	reverse


// Pedestrian number 138

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	134.040,-5.185,102.163
	reverse


// Pedestrian number 139

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	141.947,-5.152,101.586
	reverse


// Pedestrian number 140

123				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	142.165,-5.152,101.608
	reverse


// Pedestrian number 141

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.763,-5.128,97.390
	reverse


// Pedestrian number 142

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.194,-5.131,97.825
	reverse


// Pedestrian number 143

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	119.091,-5.177,26.709
	reverse


// Pedestrian number 144

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	118.693,-5.177,24.667
	reverse


// Pedestrian number 145

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	145.087,-5.177,88.244
	reverse


// Pedestrian number 146

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	127.042,-5.177,19.680
	reverse


// Pedestrian number 147

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	126.807,-5.177,14.509
	reverse


// Pedestrian number 148

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	126.122,-5.177,14.503
	reverse


// Pedestrian number 149

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	125.473,-5.177,14.498
	reverse


// Pedestrian number 150

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	124.353,-5.177,14.488
	reverse


// Pedestrian number 151

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.956,-5.177,14.475
	reverse


// Pedestrian number 152

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	126.097,-5.177,10.081
	reverse


// Pedestrian number 153

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	125.438,-5.177,10.066
	reverse


// Pedestrian number 154

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	124.792,-5.177,10.052
	reverse


// Pedestrian number 155

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	123.752,-5.177,10.028
	reverse


// Pedestrian number 156

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.879,-5.177,-1.327
	reverse


// Pedestrian number 157

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.930,-5.177,-0.244
	reverse


// Pedestrian number 158

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.907,-5.177,-2.053
	reverse


// Pedestrian number 159

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.395,-5.177,9.981
	reverse


// Pedestrian number 160

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.433,-5.177,11.038
	reverse


// Pedestrian number 161

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.390,-5.177,11.605
	reverse


// Pedestrian number 162

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.248,-5.177,12.765
	reverse


// Pedestrian number 163

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.212,-5.177,15.593
	reverse


// Pedestrian number 164

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	89.663,-5.177,35.720
	reverse


// Pedestrian number 165

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	90.575,-5.177,36.837
	reverse


// Pedestrian number 166

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	92.585,-5.177,38.819
	reverse


// Pedestrian number 167

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	97.049,-5.193,38.469
	reverse


// Pedestrian number 168

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	94.077,-5.177,41.831
	reverse


// Pedestrian number 169

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	94.277,-5.177,43.916
	reverse


// Pedestrian number 170

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	95.331,-5.177,45.307
	reverse


// Pedestrian number 171

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	96.414,-5.177,46.457
	reverse


// Pedestrian number 172

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	100.811,-5.177,48.188
	reverse


// Pedestrian number 173

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	104.493,-5.177,45.316
	reverse


// Pedestrian number 174

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	113.191,-5.177,49.534
	reverse


// Pedestrian number 175

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	124.555,-5.177,51.183
	reverse


// Pedestrian number 176

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.611,-5.177,55.320
	reverse


// Pedestrian number 177

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	116.287,-5.177,62.184
	reverse


// Pedestrian number 178

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	108.684,-5.177,63.533
	reverse


// Pedestrian number 179

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	129.569,-5.177,58.676
	reverse


// Pedestrian number 180

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.923,-6.382,86.474
	reverse


// Pedestrian number 181

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	123.886,-6.382,90.637
	reverse


// Pedestrian number 182

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	123.855,-6.382,89.819
	reverse


// Pedestrian number 183

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.806,-5.177,69.801
	reverse


// Pedestrian number 184

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.759,-5.177,70.355
	reverse


// Pedestrian number 185

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.722,-5.177,70.900
	reverse


// Pedestrian number 186

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.700,-5.177,79.771
	reverse


// Pedestrian number 187

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.643,-5.177,78.997
	reverse


// Pedestrian number 188

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.600,-5.177,78.091
	reverse


// Pedestrian number 189

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	55.165,-5.177,80.863
	reverse


// Pedestrian number 190

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.331,-5.177,78.676
	reverse


// Pedestrian number 191

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.324,-5.177,71.843
	reverse


// Pedestrian number 192

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.380,-5.177,70.670
	reverse


// Pedestrian number 193

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.246,-5.177,63.437
	reverse


// Pedestrian number 194

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.078,-5.177,60.795
	reverse


// Pedestrian number 195

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.525,-5.177,56.545
	reverse


// Pedestrian number 196

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.978,-8.720,68.311
	reverse


// Pedestrian number 197

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.888,-8.720,68.244
	reverse


// Pedestrian number 198

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	22.233,-8.720,68.192
	reverse


// Pedestrian number 199

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	22.709,-8.720,68.618
	reverse


// Pedestrian number 200

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	22.282,-8.720,68.934
	reverse


// Pedestrian number 201

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	21.279,-8.720,69.059
	reverse


// Pedestrian number 202

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.421,-8.720,69.364
	reverse


// Pedestrian number 203

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	21.503,-8.720,68.656
	reverse


// Pedestrian number 204

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	30.387,-17.799,68.882
	reverse


// Pedestrian number 205

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.497,-5.177,47.325
	reverse


// Pedestrian number 206

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.548,-5.177,47.915
	reverse


// Pedestrian number 207

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.532,-5.177,47.610
	reverse


// Pedestrian number 208

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.521,-5.177,39.328
	reverse


// Pedestrian number 209

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.484,-5.177,29.586
	reverse


// Pedestrian number 210

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.442,-5.177,33.837
	reverse


// Pedestrian number 211

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.366,-5.177,34.520
	reverse


// Pedestrian number 212

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.209,-5.177,35.142
	reverse


// Pedestrian number 213

131				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.786,-5.177,35.299
	reverse


// Pedestrian number 214

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	33.397,-5.177,39.101
	reverse


// Pedestrian number 215

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.247,-5.176,37.950
	reverse


// Pedestrian number 216

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	20.456,-5.176,37.923
	reverse


// Pedestrian number 217

105				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	19.626,-5.176,38.032
	reverse


// Pedestrian number 218

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.743,-5.176,42.969
	reverse


// Pedestrian number 219

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.642,-5.176,43.643
	reverse


// Pedestrian number 220

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	28.982,-5.176,46.464
	reverse


// Pedestrian number 221

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.476,-5.176,48.741
	reverse


// Pedestrian number 222

130				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.756,-5.176,46.640
	reverse


// Pedestrian number 223

9				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	92.766,-0.256,16.799
	point
	98.986,-0.251,15.853
	point
	103.945,999.952,13.516
	point
	116.058,995.046,12.687
	reverse


// Pedestrian number 224

6				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	103.420,-0.249,17.419
	point
	106.542,999.954,15.193
	point
	116.467,995.203,14.901
	reverse


// Pedestrian number 225

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	95.316,-0.255,12.289
	point
	107.109,999.954,14.278
	point
	113.265,993.967,13.823
	reverse


// Pedestrian number 226

7				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	94.201,-0.256,12.250
	point
	105.400,999.953,15.854
	point
	109.874,992.657,15.900
	reverse


// Pedestrian number 227

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	93.615,-0.256,17.314
	point
	106.594,999.954,13.251
	point
	111.426,993.254,11.904
	reverse


// Pedestrian number 228

10				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	106.945,999.954,14.649
	point
	109.367,992.461,14.705
	reverse


// Pedestrian number 229

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	92.925,-0.257,12.228
	point
	106.200,999.953,16.374
	point
	113.560,994.080,16.047
	reverse


// Pedestrian number 230

6				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	96.351,-0.254,17.098
	point
	100.055,-0.251,12.710
	point
	106.389,999.954,15.829
	point
	109.290,992.431,16.114
	reverse


// Pedestrian number 231

14				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	97.163,-0.253,12.309
	point
	100.253,-0.251,17.430
	point
	104.092,999.952,16.450
	point
	110.259,992.806,13.956
	reverse


// Pedestrian number 232

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.344,-4.071,89.907
	reverse


// Pedestrian number 233

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.322,-4.071,88.807
	reverse


// Pedestrian number 234

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.306,-4.071,87.987
	reverse


// Pedestrian number 235

137				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.327,-4.071,92.553
	reverse


// Pedestrian number 236

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.059,-4.071,92.540
	reverse


// Pedestrian number 237

133				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.443,-4.071,88.813
	reverse


// Pedestrian number 238

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.291,-4.071,91.521
	reverse


// Pedestrian number 239

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.147,-4.071,90.316
	reverse


// Pedestrian number 240

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.884,-4.071,91.903
	reverse


// Pedestrian number 241

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.895,-4.071,91.277
	reverse


// Pedestrian number 242

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.903,-4.071,90.763
	reverse


// Pedestrian number 243

123				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.792,-4.071,88.930
	reverse


// Pedestrian number 244

120				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	18.566,-5.177,87.880
	reverse


// Pedestrian number 245

120				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	14.677,-5.177,92.255
	reverse


// Pedestrian number 246

122				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.350,-4.071,28.296
	reverse


// Pedestrian number 247

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.316,-4.071,29.211
	reverse


// Pedestrian number 248

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.279,-4.071,30.218
	reverse


// Pedestrian number 249

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.244,-4.071,31.147
	reverse


// Pedestrian number 250

124				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.938,-4.071,29.194
	reverse


// Pedestrian number 251

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.039,-4.071,25.283
	reverse


// Pedestrian number 252

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.970,-4.071,25.247
	reverse


// Pedestrian number 253

108				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.345,-4.071,26.272
	reverse


// Pedestrian number 254

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.934,-4.071,26.253
	reverse


// Pedestrian number 255

104				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.957,-4.071,27.000
	reverse


// Pedestrian number 256

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.731,-4.071,47.830
	reverse


// Pedestrian number 257

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.778,-4.071,48.414
	reverse


// Pedestrian number 258

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.793,-4.071,47.161
	reverse


// Pedestrian number 259

3				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	34.491,995.134,33.191
	point
	45.091,996.831,34.757
	point
	54.256,998.744,29.217
	point
	55.989,982.487,27.571
	reverse


// Pedestrian number 260

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	56.608,982.407,28.441
	point
	54.181,998.768,28.280
	point
	44.139,996.780,31.776
	point
	42.799,996.392,35.506
	reverse


// Pedestrian number 261

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	63.072,982.407,24.164
	point
	59.148,999.703,26.421
	point
	56.091,999.169,27.711
	reverse


// Pedestrian number 262

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	62.185,1000.259,24.345
	point
	60.206,999.864,26.420
	point
	55.903,999.143,27.522
	reverse


// Pedestrian number 263

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	30.213,-17.799,65.743
	reverse


// Pedestrian number 264

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	31.217,-17.799,60.523
	reverse


// Pedestrian number 265

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.755,-17.799,58.092
	reverse


// Pedestrian number 266

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.265,-17.799,56.054
	reverse


// Pedestrian number 267

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.573,-17.799,54.288
	reverse


// Pedestrian number 268

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	36.608,-17.799,52.892
	reverse


// Pedestrian number 269

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	38.079,-17.799,50.907
	reverse


// Pedestrian number 270

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	42.048,-17.799,45.552
	reverse


// Pedestrian number 271

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	45.800,-17.799,40.489
	reverse


// Pedestrian number 272

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	49.856,-17.799,35.014
	reverse


// Pedestrian number 273

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	63.685,-17.799,16.587
	reverse


// Pedestrian number 274

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	57.460,-17.799,24.938
	reverse


// Pedestrian number 275

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	106.342,-8.267,22.577
	reverse


// Pedestrian number 276

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	106.261,-8.267,15.779
	reverse


// Pedestrian number 277

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	106.175,-8.267,7.589
	reverse


// Pedestrian number 278

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	100.043,-8.267,7.109
	reverse


// Pedestrian number 279

111				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	99.130,-8.267,22.779
	reverse


// Pedestrian number 280

10				// Ref num
6				// Number of instructions
4				// Initial instruction


	point
	60.265,-1.777,93.292
	point
	58.996,-1.850,89.351
	point
	56.635,-1.850,87.113
	point
	52.649,998.350,85.886
	point
	22.832,995.021,85.745
	reverse


// Pedestrian number 281

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	49.955,998.026,85.816
	point
	52.540,998.349,86.701
	point
	53.288,998.349,89.250
	reverse


// Pedestrian number 282

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	46.554,998.349,85.642
	point
	52.486,998.349,87.261
	point
	54.698,998.350,89.155
	reverse


// Pedestrian number 283

3				// Ref num
10				// Number of instructions
2				// Initial instruction

	point
	49.246,998.349,87.512
	point
	53.132,998.349,87.979
	point
	55.317,998.350,89.195
	point
	56.714,998.350,90.569
	point
	57.456,998.350,92.244
	point
	57.730,998.350,93.925
	point
	57.854,998.351,111.901
	point
	56.691,998.351,113.039
	point
	53.419,995.252,107.879
	reverse


// Pedestrian number 284

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	31.855,995.023,92.589
	point
	30.617,995.479,87.603
	point
	27.570,995.268,78.783
	reverse


// Pedestrian number 285

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	32.156,995.584,77.851
	point
	30.655,995.481,86.632
	point
	29.205,995.607,96.044
	reverse


// Pedestrian number 286

11				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	28.157,995.841,97.337
	point
	30.417,995.466,87.200
	point
	31.754,995.558,84.166
	reverse


// Pedestrian number 287

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.817,996.366,100.239
	point
	29.778,995.421,86.644
	point
	31.680,995.552,81.663
	reverse


// Pedestrian number 288

14				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.946,995.157,80.223
	point
	29.949,995.433,87.109
	point
	31.593,995.546,90.334
	reverse


// Pedestrian number 289

7				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	25.177,996.303,99.900
	point
	24.410,996.363,100.228
	point
	24.855,997.541,106.746
	point
	24.809,997.808,108.222
	reverse


// Pedestrian number 290

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.264,997.840,108.401
	point
	25.570,997.604,107.093
	point
	27.301,997.327,106.252
	reverse


// Pedestrian number 291

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	57.296,-5.210,89.441
	point
	57.957,-5.210,89.482
	point
	60.702,-5.201,87.433
	point
	64.219,-5.197,86.580
	reverse


// Pedestrian number 292

9				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	57.613,-5.206,87.987
	point
	60.461,-5.205,88.332
	point
	64.057,-5.206,90.147
	point
	65.609,-5.209,91.880
	reverse


// Pedestrian number 293

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.867,-5.208,88.627
	point
	60.692,-5.211,91.021
	point
	63.600,-5.219,95.327
	reverse


// Pedestrian number 294

14				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	64.790,-5.205,90.078
	point
	60.245,-5.207,91.177
	point
	53.448,-5.215,95.805
	point
	53.418,-5.234,106.855
	reverse


// Pedestrian number 295

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	64.077,-5.212,98.421
	point
	59.205,-5.212,90.503
	point
	56.434,-5.212,89.225
	point
	56.472,-5.212,88.725
	point
	54.654,-5.212,81.561
	reverse


// Pedestrian number 296

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.468,-5.135,113.773
	point
	59.151,-5.133,112.094
	point
	61.601,-5.213,109.651
	reverse


// Pedestrian number 297

14				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	53.420,-5.213,104.653
	point
	56.782,-5.213,107.164
	point
	59.722,-5.213,111.644
	point
	61.165,-5.213,113.089
	point
	60.003,-5.213,113.933
	point
	57.581,-5.213,114.008
	reverse


// Pedestrian number 298

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	61.682,-5.213,108.019
	point
	59.292,-5.213,111.628
	point
	57.296,-5.213,112.821
	point
	58.546,-5.213,113.775
	point
	61.245,-5.213,114.067
	reverse


// Pedestrian number 299

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	56.992,-5.213,108.728
	point
	58.524,-5.213,111.473
	point
	61.339,-5.213,112.939
	reverse


// Pedestrian number 300

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.566,-5.213,89.381
	point
	58.898,-5.235,109.851
	point
	58.782,-5.241,113.617
	reverse


// Pedestrian number 301

10				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	53.690,-1.338,129.740
	point
	56.758,-1.338,129.097
	point
	56.541,-1.338,125.835
	point
	57.954,998.862,116.909
	point
	57.479,998.862,114.982
	reverse


// Pedestrian number 302

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	57.746,-1.338,130.085
	point
	58.358,-1.338,123.642
	point
	58.317,998.862,116.888
	point
	59.022,998.862,112.015
	point
	61.435,998.862,109.842
	reverse


// Pedestrian number 303

9				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	55.849,-1.338,123.646
	point
	58.783,-1.338,123.441
	point
	63.107,998.862,117.031
	point
	63.037,998.862,114.258
	point
	60.031,998.862,78.752
	reverse


// Pedestrian number 304

3				// Ref num
8				// Number of instructions
6				// Initial instruction

	point
	53.639,-1.338,128.150
	point
	53.719,-1.338,127.008
	point
	43.974,-1.338,126.116
	point
	35.133,-1.338,126.767
	point
	31.606,-1.338,121.500
	point
	29.171,998.861,114.066
	point
	28.971,998.842,110.732
	reverse


// Pedestrian number 305

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	27.416,998.839,110.192
	point
	28.238,998.861,114.027
	point
	29.358,-1.318,117.771
	point
	34.638,-1.295,121.754
	point
	40.023,-1.338,129.216
	point
	55.740,-1.338,127.150
	reverse


// Pedestrian number 306

9				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	27.749,998.862,111.285
	point
	29.752,998.861,114.033
	point
	30.472,-1.338,119.654
	point
	41.481,-1.338,128.922
	point
	53.780,-1.338,125.299
	point
	54.731,-1.338,123.653
	reverse


// Pedestrian number 307

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	27.418,997.457,109.161
	point
	26.546,997.467,107.130
	point
	25.937,996.878,103.432
	point
	12.162,995.439,95.119
	reverse


// Pedestrian number 308

9				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	24.344,998.020,109.498
	point
	25.321,997.416,106.807
	point
	26.751,997.125,104.981
	reverse


// Pedestrian number 309

3				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.413,997.269,105.880
	point
	24.109,997.511,107.401
	point
	24.927,997.822,109.354
	reverse


// Pedestrian number 310

14				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	21.554,996.679,102.176
	point
	22.157,995.352,93.835
	point
	19.712,995.023,91.018
	point
	19.177,-5.177,91.012
	point
	18.418,-5.177,88.578
	reverse


// Pedestrian number 311

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	50.414,1.529,133.325
	reverse


// Pedestrian number 312

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.075,1.529,127.907
	reverse


// Pedestrian number 313

133				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	51.803,1.529,130.399
	reverse


// Pedestrian number 314

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.039,1.529,126.439
	reverse


// Pedestrian number 315

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.122,1.529,124.904
	reverse


// Pedestrian number 316

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.078,1.529,124.011
	reverse


// Pedestrian number 317

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.047,1.529,122.953
	reverse


// Pedestrian number 318

108				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.717,1.528,129.893
	reverse


// Pedestrian number 319

119				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	52.815,1.520,115.841
	reverse


// Pedestrian number 320

119				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	45.264,1.519,114.500
	reverse


// Pedestrian number 321

122				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.060,1.513,107.302
	reverse


// Pedestrian number 322

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	44.263,1.530,132.595
	reverse


// Pedestrian number 323

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	47.770,1.530,132.701
	reverse


// Pedestrian number 324

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.512,1.520,118.420
	reverse


// Pedestrian number 325

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	4.612,1.513,107.198
	reverse


// Pedestrian number 326

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	5.068,1.505,94.433
	reverse


// Pedestrian number 327

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.372,1.505,93.665
	reverse


// Pedestrian number 328

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.380,1.508,98.268
	reverse


// Pedestrian number 329

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.372,1.509,100.821
	reverse


// Pedestrian number 330

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	25.589,1.529,100.856
	reverse


// Pedestrian number 331

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.311,0.856,93.642
	reverse


// Pedestrian number 332

137				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	37.774,0.996,90.692
	reverse


// Pedestrian number 333

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	75.411,1.529,79.422
	reverse


// Pedestrian number 334

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	75.676,1.529,85.317
	reverse


// Pedestrian number 335

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	75.609,1.529,95.507
	reverse


// Pedestrian number 336

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	73.004,1.451,124.541
	reverse


// Pedestrian number 337

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.258,1.451,122.539
	reverse


// Pedestrian number 338

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.246,1.451,116.437
	reverse


// Pedestrian number 339

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.294,1.451,111.914
	reverse


// Pedestrian number 340

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.275,1.513,109.040
	reverse


// Pedestrian number 341

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.652,1.529,106.207
	reverse


// Pedestrian number 342

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	62.905,1.529,74.977
	reverse


// Pedestrian number 343

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.450,1.529,70.389
	reverse


// Pedestrian number 344

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.088,1.524,86.542
	reverse


// Pedestrian number 345

123				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	50.913,1.448,104.027
	reverse


// Pedestrian number 346

122				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	49.759,1.408,103.951
	reverse


// Pedestrian number 347

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	48.074,1.374,103.921
	reverse


// Pedestrian number 348

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.345,-3.201,112.850
	reverse


// Pedestrian number 349

128				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	59.877,-5.213,113.348
	reverse


// Pedestrian number 350

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	58.546,-5.213,113.292
	reverse


// Pedestrian number 351

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.784,-5.213,94.482
	reverse


// Pedestrian number 352

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	65.844,-5.202,89.109
	reverse


// Pedestrian number 353

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	61.898,-5.193,79.494
	reverse


// Pedestrian number 354

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	63.177,-5.193,77.921
	reverse


// Pedestrian number 355

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	56.583,-5.206,88.654
	reverse


// Pedestrian number 356

110				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.369,-5.183,77.322
	reverse


// Pedestrian number 357

110				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.346,-5.181,81.038
	reverse


// Pedestrian number 358

125				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.728,-5.659,85.604
	reverse


// Pedestrian number 359

120				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.075,-5.659,85.626
	reverse


// Pedestrian number 360

137				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.820,-5.659,87.136
	reverse


// Pedestrian number 361

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.049,-5.659,87.147
	reverse


// Pedestrian number 362

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.429,-5.659,87.152
	reverse


// Pedestrian number 363

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	122.405,-5.659,85.663
	reverse


// Pedestrian number 364

99				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	122.035,-6.382,90.702
	point
	115.992,-6.382,94.192
	point
	115.507,-6.236,94.831
	point
	114.181,-5.834,96.797
	point
	113.689,-5.234,98.337
	reverse




START OF OPPONENT PATHS

142                             // Number of path nodes
  151.200,   -5.100,   -1.300   // Node #0
  118.800,   -5.100,   -1.200   // Node #1
  119.212,   -5.200,   34.438   // Node #2
  118.910,   -5.177,   80.406   // Node #3
  117.648,   -6.382,   93.850   // Node #4
  112.097,   -5.207,   94.852   // Node #5
   93.485,   -5.177,   93.619   // Node #6
   90.347,   -5.177,   91.290   // Node #7
   88.176,   -5.177,   81.143   // Node #8
   85.525,   -5.176,   78.332   // Node #9
   64.638,   -5.213,   79.702   // Node #10
   59.285,   -5.213,   92.354   // Node #11
   45.156,   -2.830,   86.313   // Node #12
   35.903,   -4.104,   86.874   // Node #13
   26.451,   -5.007,   87.372   // Node #14
   21.950,   -5.177,   86.983   // Node #15
   21.984,   -5.179,   49.019   // Node #16
   22.042,   -5.179,   35.833   // Node #17
   45.541,   -3.255,   34.032   // Node #18
   98.919,   -0.253,   14.679   // Node #19
  146.857,   -5.178,   34.401   // Node #20
  147.320,   -5.178,   -1.338   // Node #21
  148.616,   -5.178,   36.256   // Node #22
  148.503,   -5.177,   51.045   // Node #23
  143.492,   -5.179,   34.955   // Node #24
  143.656,   -5.179,   44.377   // Node #25
  139.598,   -5.177,   48.484   // Node #26
  136.115,   -5.179,   48.411   // Node #27
  128.495,   -5.174,   40.410   // Node #28
  119.064,   -5.177,   47.360   // Node #29
  127.917,   -5.177,   34.918   // Node #30
  118.914,   -5.191,   72.923   // Node #31
  130.037,   -5.179,   67.903   // Node #32
  130.128,   -5.171,   54.448   // Node #33
  107.733,   -5.179,   69.194   // Node #34
  107.980,   -5.181,   53.390   // Node #35
  101.765,   -5.182,   48.495   // Node #36
   97.932,   -5.189,   48.562   // Node #37
   94.151,   -5.180,   44.730   // Node #38
   88.570,   -5.300,   36.127   // Node #39
   89.526,   -5.265,   -0.057   // Node #40
  105.526,   -5.179,    1.808   // Node #41
   89.006,   -5.283,   26.003   // Node #42
   99.471,   -5.179,   28.311   // Node #43
  115.168,   -5.177,   26.276   // Node #44
  113.386,   -6.188,   14.612   // Node #45
   94.486,   -8.264,   14.629   // Node #46
   14.378,   -5.177,   89.461   // Node #47
   11.915,   -5.178,   58.629   // Node #48
   30.862,   -5.177,   81.200   // Node #49
   30.938,   -5.181,   64.558   // Node #50
   32.963,   -5.178,   59.300   // Node #51
   30.376,   -5.179,   34.814   // Node #52
   30.520,   -5.180,   26.909   // Node #53
   14.038,   -5.181,   26.732   // Node #54
   12.474,   -5.180,   33.042   // Node #55
   94.201,   -5.177,   40.212   // Node #56
   10.790,   -5.179,   68.625   // Node #57
   27.032,   -8.722,   68.953   // Node #58
   26.992,   -8.671,   78.314   // Node #59
   22.014,   -8.633,   80.283   // Node #60
   16.997,   -8.720,   78.143   // Node #61
   17.044,   -8.560,   68.490   // Node #62
   17.122,   -8.720,   58.949   // Node #63
   21.821,   -8.760,   57.272   // Node #64
   26.928,   -8.778,   58.968   // Node #65
   22.014,   -3.067,   69.154   // Node #66
   23.021,   -5.177,   89.369   // Node #67
   31.514,   -5.180,   92.633   // Node #68
  118.918,   -5.178,   14.505   // Node #69
  110.278,   -5.178,   39.295   // Node #70
  135.113,   -5.171,   34.903   // Node #71
  147.530,   -5.179,  102.714   // Node #72
  140.099,   -5.181,  103.156   // Node #73
  141.804,   -5.177,   82.817   // Node #74
  142.439,   -5.173,   54.806   // Node #75
  142.141,   -5.176,   77.376   // Node #76
  147.865,   -5.171,   50.884   // Node #77
  148.601,   -5.169,   45.123   // Node #78
  133.329,   -5.172,   36.313   // Node #79
  130.550,   -5.184,  103.892   // Node #80
  131.412,   -5.179,   98.511   // Node #81
  134.475,   -5.177,   99.108   // Node #82
  134.265,   -5.177,  103.832   // Node #83
  140.357,   -5.177,  100.321   // Node #84
  141.217,   -5.177,   90.091   // Node #85
  133.726,   -5.177,   84.785   // Node #86
  129.049,   -5.180,   80.180   // Node #87
  129.172,   -5.177,   74.453   // Node #88
  135.897,   -5.177,   73.805   // Node #89
  147.899,   -5.177,   90.025   // Node #90
  120.386,   -5.199,   34.785   // Node #91
  120.145,   -5.198,   40.249   // Node #92
  118.744,   -5.175,   60.886   // Node #93
   15.356,   -5.180,   30.887   // Node #94
  143.441,   -5.177,   35.627   // Node #95
   64.367,    0.369,   25.085   // Node #96
   84.313,   -0.319,   14.843   // Node #97
  106.964,   -0.246,   14.787   // Node #98
  115.998,   -2.595,   14.972   // Node #99
  140.718,   -4.018,   16.688   // Node #100
  147.122,   -5.178,   16.715   // Node #101
  136.768,   -5.179,   93.459   // Node #102
  131.206,   -5.176,   94.788   // Node #103
   63.365,   -5.213,  106.332   // Node #104
   63.033,   -1.333,  116.456   // Node #105
   56.313,   -1.337,  125.560   // Node #106
   40.304,   -1.337,  127.866   // Node #107
   35.937,   -1.337,  125.673   // Node #108
   28.271,   -1.338,  112.535   // Node #109
   25.611,   -2.927,  105.832   // Node #110
   22.926,   -3.804,  100.321   // Node #111
   58.334,   -1.338,  125.627   // Node #112
   59.152,   -1.338,  128.119   // Node #113
   56.697,   -1.338,  129.652   // Node #114
   54.805,   -1.338,  129.664   // Node #115
   54.441,   -1.338,  126.005   // Node #116
   54.922,   -5.213,  106.295   // Node #117
   56.951,   -1.850,   88.859   // Node #118
   55.007,   -1.850,   87.510   // Node #119
   52.586,   -1.815,   86.989   // Node #120
   59.919,   -1.338,  121.752   // Node #121
   54.721,   -1.338,  123.485   // Node #122
   53.867,   -1.338,  119.216   // Node #123
   24.202,   -5.219,  108.796   // Node #124
   12.994,   -5.216,  107.754   // Node #125
   22.886,   -3.510,  113.097   // Node #126
   42.367,   -3.614,  112.805   // Node #127
   46.498,   -5.220,  108.875   // Node #128
   54.978,   -4.450,  109.295   // Node #129
   52.962,   -3.769,  112.712   // Node #130
   29.968,   -5.222,  109.012   // Node #131
   58.801,   -1.850,  114.698   // Node #132
   54.737,   -1.333,  116.308   // Node #133
   59.119,   -1.850,   92.324   // Node #134
   59.139,   -5.213,   82.956   // Node #135
   56.425,   -5.213,   80.499   // Node #136
   59.583,   -5.213,  106.364   // Node #137
   60.105,   -5.213,  113.030   // Node #138
   58.169,   -5.213,  113.369   // Node #139
   66.750,   -5.213,   90.669   // Node #140
   65.488,   -5.213,  100.006   // Node #141

170                                           // Number of path sections
   0,  21,   0, 255,   0, 255,    1.0, 1000   // Section #0
   1,  69,   0, 255,   0, 255,    0.7,    1   // Section #1
   3,   4,   0, 255,   0, 255,    1.1,    0   // Section #2
   4,   5,   0, 255,   0, 255,    0.5,    1   // Section #3
   5,   6,   0, 255,   0, 255,    0.5,    1   // Section #4
   6,   7,   0, 255,   0, 255,    0.5,    1   // Section #5
   7,   8,   0, 255,   0, 255,    0.5,    1   // Section #6
   8,   9,   0, 255,   0, 255,    0.5,    1   // Section #7
   9,  10,   0, 255,   0, 255,    0.5,    1   // Section #8
  10,  11,   0, 255,   0, 255,    0.5,    1   // Section #9
  12,  13,   0, 255,   0, 255,    0.5,    0   // Section #10
  13,  14,   0, 255,   0, 255,    0.5,    0   // Section #11
  14,  67,   0, 255,   0, 255,    0.5,    0   // Section #12
  15,  66,   0, 255,   0, 255,    0.5,    1   // Section #13
  16,  17,   0, 255,   0, 255,    0.5,    1   // Section #14
  17,  52,   0, 255,   0, 255,    1.2,    1   // Section #15
  24,  20,   0, 255,   0, 255,    1.5,    1   // Section #16
 101,  21,   0, 255,   0, 255,    1.7,    1   // Section #17
  21,   1,   0, 255,   0, 255,    1.0,    1   // Section #18
  20,  22,   0, 255,   0, 255,    0.3,    1   // Section #19
  71,  24,   0, 255,   0, 255,    1.2,    1   // Section #20
  26,  25,   0, 255,   0, 255,    0.4,    0   // Section #21
  26,  27,   0, 255,   0, 255,    0.4,    0   // Section #22
  27,  28,   0, 255,   0, 255,    0.4,    0   // Section #23
  28,  29,   0, 255,   0, 255,    2.0,    0   // Section #24
  29,  93,   0, 255,   0, 255,    1.5,    0   // Section #25
  28,  30,   0, 255,   0, 255,    1.0,    0   // Section #26
   2,  91,   0, 255,   0, 255,    0.5,    1   // Section #27
  32,  31,   0, 255,   0, 255,    1.0,    0   // Section #28
  31,   3,   0, 255,   0,  35,    1.8,    0   // Section #29
  33,  32,   0, 255,   0, 255,    1.6, 1000   // Section #30
  34,  31,   0, 255,   0, 255,    1.6,    0   // Section #31
  35,  34,   0, 255,   0, 255,    1.3, 1000   // Section #32
  36,  70,   0, 255,   0, 255,    0.5,    0   // Section #33
  37,  36,   0, 255,   0, 255,    0.4,    0   // Section #34
  38,  37,   0, 255,   0, 255,    0.4,    0   // Section #35
  39,  56,   0, 255,   0, 255,    0.4,    0   // Section #36
  40,  41,   0, 255,   0, 255,    1.0,    0   // Section #37
  41,   1,   0, 255,   0, 255,    1.0,    0   // Section #38
  42,  43,   0, 255,   0, 255,    0.5,    0   // Section #39
  40,  42,   0, 255,   0, 255,    0.7,    0   // Section #40
  44,   2,   0, 255,   0, 255,    0.3,    0   // Section #41
  45,  69,   0, 255,   0, 255,    0.2, 1000   // Section #42
  46,  45,   0, 255,   0, 255,    4.0, 1000   // Section #43
  48,  57,   0, 255,   0, 255,    1.0, 1000   // Section #44
  49,  14,   0, 255,   0, 255,    0.5, 1000   // Section #45
  50,  49,   0, 255,   0, 255,    0.5, 1000   // Section #46
  51,  16,   0,  15,   0,  15,    0.3, 1000   // Section #47
  53,  52,   0, 255,   0, 255,    1.2,    0   // Section #48
  52,  18,   0, 255,   0, 255,    1.0,    1   // Section #49
  54,  53,   0, 255,   0, 255,    1.0,    0   // Section #50
  56,  38,   0, 255,   0, 255,    0.3,    0   // Section #51
  39,  42,   0, 255,   0, 255,    0.5,    0   // Section #52
  58,  57,   0, 255,  25, 255,    0.9, 1000   // Section #53
  57,  47,   0, 255,   0, 255,    1.0,    0   // Section #54
  59,  58,   0, 255,   0, 255,    0.2, 1000   // Section #55
  60,  59,   0, 255,   0, 255,    0.5, 1000   // Section #56
  60,  61,   0, 255,   0, 255,    0.4,    0   // Section #57
  61,  62,   0, 255,   0, 255,    0.2, 1000   // Section #58
  63,  62,   0, 255,   0, 255,    0.2, 1000   // Section #59
  64,  63,   0, 255,   0, 255,    0.4, 1000   // Section #60
  64,  65,   0, 255,   0, 255,    0.4, 1000   // Section #61
  65,  58,   0, 255,   0, 255,    0.2, 1000   // Section #62
  62,  58,   0, 255,   0, 255,    0.8, 1000   // Section #63
  66,  16,   0, 255,   0, 255,    0.5,    1   // Section #64
  67,  15,   0, 255,   0, 255,    0.5,    1   // Section #65
  47,  67,   0, 255,   0, 255,    0.6,    0   // Section #66
  68,  67,   0, 255,   0, 255,    0.5, 1000   // Section #67
  69,   2,   0, 255,   0, 255,    0.7,    1   // Section #68
  43,  44,   0, 255,   0, 255,    0.3,    0   // Section #69
  70,   2,   0, 255,   0, 255,    0.5,    0   // Section #70
  43,  70,   0, 255,   0, 255,    1.2,    0   // Section #71
  70,  29,   0, 255,   0, 255,    1.2,    0   // Section #72
  71,  79,   0, 255,   0, 255,    1.3,    0   // Section #73
  30,  71,   0, 255,   0, 255,    1.2,    1   // Section #74
  90,  23,   0, 255,   0, 255,    0.9,    0   // Section #75
  72,  73,   0, 255,   0, 255,    0.3,    0   // Section #76
  73,  84,   0, 255,   0, 255,    1.0,    0   // Section #77
  76,  74,   0, 255,   0, 255,    0.4,    1   // Section #78
  77,  75,   0, 255,   0, 255,    0.9,    1   // Section #79
  75,  76,   0, 255,   0, 255,    1.1,    1   // Section #80
  78,  77,   0, 255,   0, 255,    0.6,    1   // Section #81
  23,  77,   0, 255,   0, 255,    0.9,    0   // Section #82
  79,  28,   0, 255,   0, 255,    1.3,    0   // Section #83
  83,  73,   0, 255,   0, 255,    0.3,    0   // Section #84
  81,  80,   0, 255,   0, 255,    0.3,    0   // Section #85
  81,  82,   0, 255,   0, 255,    0.3,    0   // Section #86
  82,  83,   0, 255,   0, 255,    0.3,    0   // Section #87
  80,  83,   0, 255,   0, 255,    0.3,    0   // Section #88
  82,  84,   0, 255,   0, 255,    0.3,    0   // Section #89
  84,  85,   0, 255,   0, 255,    1.0,    0   // Section #90
  86, 102,   0, 255,   0, 255,    1.1,    0   // Section #91
  74,  85,   0, 255,   0, 255,    1.0,    1   // Section #92
  87,  86,   0, 255,   0, 255,    1.0,    0   // Section #93
  87,  88,   0, 255,   0, 255,    1.0,    0   // Section #94
  88,  89,   0, 255,   0, 255,    1.1,    0   // Section #95
  89,  76,   0, 255,   0, 255,    1.2,    0   // Section #96
  89,  75,   0, 255,   0, 255,    1.2,    0   // Section #97
  86,  89,   0, 255,   0, 255,    1.0,    0   // Section #98
  90,  85,   0, 255,   0, 255,    0.9,    0   // Section #99
  90,  72,   0, 255,   0, 255,    0.9,    0   // Section #100
  91,  92,   0, 255,   0, 255,    0.5,    0   // Section #101
  91,  30,   0, 255,   0, 255,    0.4,    1   // Section #102
  92,  29,   0, 255,   0, 255,    1.2,    0   // Section #103
  93,  31,   0, 255,   0,  45,    0.4,    0   // Section #104
  55,  16,   0, 255,   0, 255,    0.7,    0   // Section #105
  55,  94,   0, 255,   0, 255,    1.2,    0   // Section #106
  94,  52,   0, 255,   0, 255,    0.5,    0   // Section #107
  54,  94,   0, 255,   0, 255,    1.0,    0   // Section #108
  25,  95,   0, 255,   0, 255,    0.4,    0   // Section #109
  24,  95,   0, 255,   0, 255,    0.4,    0   // Section #110
  18,  96,   0, 255,   0, 255,    0.6,    1   // Section #111
  96,  97,   0, 255,   0, 255,    0.9,    1   // Section #112
  97,  19,   0, 255,   0, 255,    1.2,    1   // Section #113
  19,  98,   0, 255,   0, 255,    1.2,    1   // Section #114
  98,  99,   0, 255,   0, 255,    1.2, 1001   // Section #115
  99, 100,   0, 255,   0, 255,    1.2,    1   // Section #116
 100, 101,   0, 255,   0, 255,    1.2,    1   // Section #117
  20, 101,   0, 255,   0, 255,    1.7,    0   // Section #118
 102, 103,   0, 255,   0, 255,    0.6,    1   // Section #119
  85, 102,   0, 255,   0, 255,    1.1,    1   // Section #120
 103,   4,   0, 255,   0, 255,    0.9,    1   // Section #121
  22,  78,   0, 255,   0, 255,    0.5,    1   // Section #122
  11, 104,   0, 255,   0, 255,    0.5,    1   // Section #123
 104, 105,   0, 255,   0,  40,    0.5,    1   // Section #124
 105, 121,   0, 255,   0, 255,    0.5,    1   // Section #125
 106, 116,   0, 255,   0, 255,    0.5,    1   // Section #126
 107, 108,   0, 255,   0, 255,    0.5,    1   // Section #127
 108, 109,   0, 255,  40,  50,    0.5,    1   // Section #128
 109, 110,   0, 255,   0, 255,    0.5,    1   // Section #129
 110, 111,   0, 255,   0, 255,    0.5,    1   // Section #130
 111,  67,   0, 255,   0, 255,    0.5,    1   // Section #131
 112, 106,   0, 255,   0, 255,    0.5,    0   // Section #132
 113, 112,   0, 255,   0, 255,    0.5,    0   // Section #133
 114, 113,   0, 255,   0, 255,    0.5,    0   // Section #134
 115, 114,   0, 255,   0, 255,    0.5,    0   // Section #135
 115, 116,   0, 255,   0, 255,    0.3,    0   // Section #136
 116, 107,   0, 255,   0, 255,    0.5,    1   // Section #137
 117, 129,   0, 255,   0, 255,    0.5,    1   // Section #138
 118, 119,   0, 255,   0, 255,    0.5,    0   // Section #139
 119, 120,   0, 255,   0, 255,    0.5,    0   // Section #140
 120,  12,   0, 255,   0, 255,    0.5,    0   // Section #141
 123, 122,   0, 255,   0, 255,    0.5,    0   // Section #142
 121, 106,   0, 255,   0, 255,    0.5,    1   // Section #143
 122, 116,   0, 255,   0, 255,    0.2,    0   // Section #144
 123, 121,   0, 255,   0, 255,    0.5,    0   // Section #145
 125, 124,   0, 255,   0, 255,    0.5, 1000   // Section #146
 124, 126,   0, 255,   0, 255,    0.5,    0   // Section #147
 126, 127,   0, 255,   0, 255,    0.5,    0   // Section #148
 127, 128,   0, 255,   0, 255,    0.5,    0   // Section #149
 128, 129,   0, 255,   0, 255,    0.5, 1000   // Section #150
 129, 133,   0, 255,   0,  30,    0.5,    1   // Section #151
 124, 131,   0, 255,   0, 255,    0.5, 1000   // Section #152
 130, 128,   0, 255,   0, 255,    0.5, 1000   // Section #153
 127, 131,   0, 255,   0, 255,    0.5,    0   // Section #154
 131, 128,   0, 255,   0, 255,    0.5, 1000   // Section #155
 133, 106,   0, 255,   0, 255,    0.5,    1   // Section #156
  11, 117,   0, 255,   0, 255,    0.5,    1   // Section #157
 118, 134,   0, 255,   0, 255,    0.5,    0   // Section #158
 134, 132,   0, 255,   0, 255,    0.5,    0   // Section #159
 132, 121,   0, 255,   0, 255,    0.5,    0   // Section #160
 135,  11,   0, 255,   0, 255,    0.5,    0   // Section #161
 136, 135,   0, 255,   0, 255,    0.5, 1000   // Section #162
 104, 137,   0, 255,   0, 255,    0.5,    0   // Section #163
 138, 137,   0, 255,   0, 255,    0.5, 1000   // Section #164
 137, 117,   0, 255,   0, 255,    0.5,    0   // Section #165
 139, 137,   0, 255,   0, 255,    0.5, 1000   // Section #166
  11, 140,   0, 255,   0, 255,    0.5,    0   // Section #167
 140, 141,   0, 255,   0, 255,    0.5,    0   // Section #168
 141, 104,   0, 255,   0, 255,    0.5,    0   // Section #169

7                                                             // Number of cop start points
  115.314,   -5.178,   63.804,    0.000,    0.000,    0.000   // Cop start point #0
  107.005,   -5.177,   -2.222,    0.000,    0.000,    0.000   // Cop start point #1
  146.777,   -5.177,  103.513,    0.000,    0.000,    0.000   // Cop start point #2
  128.928,   -5.177,   80.695,    0.000,    0.000,    0.000   // Cop start point #3
   21.293,   -5.177,  108.560,    0.000,    0.000,    0.000   // Cop start point #4
   12.338,   -5.177,   85.469,    0.000,    0.000,    0.000   // Cop start point #5
   28.552,   -5.177,   47.591,    0.000,    0.000,    0.000   // Cop start point #6

END OF OPPONENT PATHS

2										// number of material modifiers

// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
SKIDMARK.MAT							// skid mark material

//	material '0'
1.0										// car wall friction
1.0										// tyre road friction
0										// down force
0.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
1										// room for expansion
none									// room for expansion

// Non CarObjects
2										// number of non car objects
BARRIER.TXT
WRECK.TXT

0									// Number of smoke shadetables

8										// Number of network start points

129.75,-5.17,-1.22							//1
270													

146.57,-5.17,10.49							//2						
180									

117.75,-5.17,44.13							//3						
180									

93.29,-5.17,1.23							//4						
270									

107.79,-5.17,32.17						//5						
225									

107.78,-5.17,55.58							//6						
180									

120.88,-6.38,95.1							//7						
270									

141.89,-5.17,59.36							//8						
310									

1								// number of splash files
SPLSHYEL.PIX 						// name of pixelmapfile for splashes

1

INDUSTA2.TXT
