VERSION 6		// V1 expects map checkpoint rectangles
			// V2 and above expect map checkpoint points
			// V3 and above expect splash file stuff at the end
			// V4 and above expect two sets of PIX and MAT and ped substitution entry

11.621,-5.321,64.789						// Position of centre of start of grid
90									// Direction that grid faces in

// Laps, checkpoints etc

150,75,25							// Initial timer count for each skill level
4									// # laps
10000,5000,3000						// Race completed bonus (all laps raced) for each skill level
75000,50000,30000					// Race completed bonus (all peds killed) for each skill level
20000,10000,5000					// Race completed bonus (all oppos wasted) for each skill level

// Width and height of map checkpoint rectangles
9,18
11,26

4									// # checkpoints

// Checkpoint #1
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-76.388,-100,71.972						// Point #0
-76.388,100,71.972						// Point #1
-75.950,100,75.033						// Point #2
-75.950,-100,75.033					// Point #3
82,164
22,53

// Checkpoint #2
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-79.752,-100,-77.820						// Point #0
-79.752,100,-77.820						// Point #1
-79.907,100,-81.12						// Point #2
-79.907,-100,-81.12					// Point #3
236,472
22,53

// Checkpoint #3
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-33.551,-100,-4.836						// Point #0
-33.551,100,-4.836						// Point #1
-30.577,100,-4.785						// Point #2
-30.577,-100,-4.785					// Point #3
166,332
63,151

// Checkpoint #4
20,10,5								// Timer increment for each skill level (ped mode)
60,30,10							// Timer increment for each skill level (pedless mode)
1									// # quads for this checkpoint
-20.794,-100,55.809						// Point #0
-20.794,100,55.809						// Point #1
-17.546,100,55.853						// Point #2
-17.546,-100,55.853					// Point #3
101,202
77,185	
				
5									// # pixelmap files to load
DEZSKY.PIX
DEZRACE1.PIX
NDHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX

5
DEZSKY.PIX									// # pixelmap files to load
DESERT8.PIX
NDHORIZN.PIX
DRKSCRN.PIX
FOGSCRN.PIX


2									// # shade table files to load
Deztrak3.TAB
IDENTITY.TAB

13
DEZSKY.MAT
BRP3.MAT
YWW.MAT
LITTY.MAT
STONY.MAT
GBW2.MAT
VENTY.MAT
TANTY.MAT									// # material files to load
DEZRACE1.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT

13
DEZSKY.MAT
BRP3.MAT
YWW.MAT
LITTY.MAT
STONY.MAT
GBW2.MAT
VENTY.MAT
TANTY.MAT									// # material files to load
DESERT8.MAT
DARKSKY.MAT
DRKSCRN.MAT
FOGSCRN.MAT
SKIDMARK.MAT


1									// # model files to load
DEZRACE1.DAT

1									// # model files to load
DESERT81.DAT

DEZRACE1.ACT							// Track actor

DESERT81.ACT							// Track actor

DESERT3X.ACT							// Additional actor

// HORIZON STUFF

NDHORIZN.PIX						// Name of sky texture pixelmap (or "none")
4									// Horizontal repetitions of sky texture
66									// Vertical size of sky texture (degrees)
125									// Position of horizon (pixels below top)
dark							// Depth cue mode ("none", "dark" or "fog")
7,0									// Degree of fog/darkness

// DEFAULT ENGINE NOISE

0

// SPECIAL EFFECTS VOLUMES

26				// # special effects volumes

// -------------------- 0 ---------------------------------
NEW IMPROVED!
0.021, 0.002, -3.619
-0.003, 1.440, 0.001
11.221, 0.024, 0.064
-3.808, -4.244, 64.644
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
TANTY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 1 ---------------------------------
NEW IMPROVED!
-1.000, 0.000, -0.007
0.000, 3.583, 0.000
0.138, 0.000, -18.488
-18.874, -6.999, 26.482
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
LITTY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 2 ---------------------------------
NEW IMPROVED!
0.999, 0.000, -0.053
0.000, 1.000, 0.002
0.053, -0.002, 0.999
-4.645, -7.518, -20.356
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
BRP3.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 3 ---------------------------------
NEW IMPROVED!
0.049, -0.001, -1.439
-0.003, 2.488, -0.001
15.398, 0.021, 0.528
-34.404, -5.980, 27.237
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
GBW2.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 4 ---------------------------------
NEW IMPROVED!
1.271, -0.001, 1.170
0.015, 1.200, -0.016
-4.193, 0.115, 4.555
-33.621, -7.508, 38.829
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 5 ---------------------------------
NEW IMPROVED!
-1.197, 0.001, -0.086
0.004, 0.999, -0.034
0.309, -0.146, -4.286
-31.901, -8.332, 32.643
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 6 ---------------------------------
NEW IMPROVED!
1.440, 0.000, -0.025
0.000, 2.986, 0.000
0.323, 0.000, 18.486
-31.822, -6.599, 15.068
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
STONY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 7 ---------------------------------
NEW IMPROVED!
-0.258, 0.000, 1.739
0.000, 2.488, 0.000
-15.395, 0.000, 0.549
-17.062, -6.019, 14.469
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
STONY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 8 ---------------------------------
NEW IMPROVED!
-2.986, 0.002, -3.094
-0.015, 1.200, 0.016
6.414, 0.165, -6.191
-19.435, -7.503, 5.012
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 9 ---------------------------------
NEW IMPROVED!
0.073, 0.026, -7.432
-0.073, 10.699, 0.037
7.800, 0.053, 0.023
-25.429, -8.117, 19.832
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
LITTY.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 10 ---------------------------------
NEW IMPROVED!
-0.012, 0.000, -1.728
-0.012, 1.000, 0.000
7.429, 0.090, -0.053
-25.167, -7.506, -12.864
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 11 ---------------------------------
NEW IMPROVED!
-0.392, 0.006, 2.960
0.018, 1.000, 0.000
-10.605, 0.195, -1.403
25.423, -7.485, -10.626
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 12 ---------------------------------
NEW IMPROVED!
0.889, 0.000, -6.128
0.000, 1.440, 0.000
12.706, -0.002, 1.842
32.425, -7.517, -2.288
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 13 ---------------------------------
NEW IMPROVED!
-2.985, 0.001, -0.071
0.000, 1.000, 0.010
0.170, 0.070, -7.165
12.529, -7.429, 20.961
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 14 ---------------------------------
NEW IMPROVED!
0.037, 0.001, -1.440
-0.010, 1.000, 0.000
7.398, 0.073, 0.193
-25.389, -7.505, 51.442
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 15 ---------------------------------
NEW IMPROVED!
0.058, 0.000, 0.998
-0.002, 1.000, 0.000
-0.998, -0.002, 0.058
54.447, -7.519, -23.139
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
BRP3.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 16 ---------------------------------
NEW IMPROVED!
-0.007, 0.000, 1.050
0.002, 1.000, 0.000
-1.000, 0.002, -0.006
64.424, -7.519, -4.571
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
BRP3.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 17 ---------------------------------
NEW IMPROVED!
-2.071, 0.001, -0.095
0.000, 1.200, 0.012
0.325, 0.069, -7.068
-53.860, -7.609, 20.884
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 18 ---------------------------------
NEW IMPROVED!
-1.440, 0.000, 0.006
0.000, 1.000, -0.001
-0.004, -0.001, -1.000
94.360, -6.647, 7.603
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
BRP3.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 19 ---------------------------------
NEW IMPROVED!
0.071, 0.000, -1.100
0.001, 1.000, 0.000
0.998, -0.001, 0.064
-18.953, -6.648, 109.721
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
BRP3.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 20 ---------------------------------
NEW IMPROVED!
-0.027, 0.000, 1.000
0.001, 1.000, 0.000
-1.000, 0.001, -0.027
-32.069, -6.647, -101.915
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
BRP3.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 21 ---------------------------------
NEW IMPROVED!
0.004, 0.000, -1.440
0.000, 1.000, 0.000
18.488, -0.006, 0.048
-0.603, -7.517, -43.856
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 22 ---------------------------------
NEW IMPROVED!
0.010, 0.000, -1.000
-0.002, 1.000, 0.000
1.000, 0.002, 0.010
-31.736, -7.518, -44.314
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
BRP3.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 23 ---------------------------------
NEW IMPROVED!
-0.235, 0.000, 4.293
0.000, 1.000, 0.000
-12.210, 0.000, -0.668
-7.426, -7.519, -74.978
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// -------------------- 24 ---------------------------------
NEW IMPROVED!
-0.867, 0.000, -0.830
0.000, 1.000, 0.000
1.721, 0.001, -1.798
21.451, -7.519, -32.127
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
BRP3.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index


// -------------------- 25 ---------------------------------
NEW IMPROVED!
1.200, 0.001, 0.023
-0.001, 1.000, -0.018
-0.166, 0.154, 8.598
-61.325, -7.499, -27.911
1				// gravity multiplier
1				// viscosity multiplier
0				// Car damage per millisecond
0				// Pedestrian damage per millisecond
-1					// camera effect index
-1					// depth effect index
YWW.MAT				// Windscreen material to use
-1					// Sound ID of entry noise
-1					// Sound ID of exit noise
1					// Engine noise index
0					// material index



// REFLECTIVE WINDSCREEN SPECIFICATIONS

DEZSKY.MAT							// Material to use for default screens
DRKSCRN.MAT							// Material to use for default screens during darkness
FOGSCRN.MAT							// Material to use for default screens during fog

0									// # areas with different screens

// MAP DETAILS

DEZMAP1.PIX						// Map pixelmap name

0,			0.959,		0			// World->map transformation matrix
0,			0,			0
-0.959,		0,			0
161.0,		101.0,		0

// ****** START OF FUNK AND GROOVE STUFF ******

START OF FUNK


END OF FUNK



START OF GROOVE


END OF GROOVE


// ****** START OF PEDESTRIAN STUFF ******

10				// Ped subs table index

894				// Number of pedestrians

// Pedestrian number 1

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	14.012,-5.320,63.752
	point
	10.140,-5.321,62.726
	point
	5.898,-5.319,67.252
	point
	5.324,-5.227,67.609
	point
	1.888,-5.227,67.995
	reverse


// Pedestrian number 2

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	7.804,-5.227,57.304
	point
	7.725,-5.227,61.416
	point
	-9.325,-5.227,61.302
	point
	-15.621,-5.227,61.289
	point
	-15.376,-5.227,58.210
	reverse


// Pedestrian number 3

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-17.696,-5.309,47.050
	point
	-18.185,-5.307,46.896
	point
	-19.032,-5.297,45.283
	point
	-18.159,-8.346,28.340
	reverse


// Pedestrian number 4

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-23.369,-8.399,18.554
	point
	-23.069,-8.399,20.571
	point
	-21.163,-8.399,26.634
	reverse


// Pedestrian number 5

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-18.137,-8.399,23.771
	point
	-18.867,-8.399,22.917
	point
	-20.687,-8.399,22.551
	point
	-23.181,-8.399,21.273
	point
	-25.988,-8.399,16.984
	reverse


// Pedestrian number 6

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-27.810,-8.399,13.408
	point
	-27.261,-8.399,14.370
	point
	-27.766,-8.399,16.810
	point
	-23.176,-8.399,27.683
	reverse


// Pedestrian number 7

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-21.252,-8.399,27.843
	point
	-22.764,-8.399,26.030
	point
	-24.484,-8.399,21.206
	point
	-24.143,-8.399,18.460
	reverse


// Pedestrian number 8

18				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-25.096,-8.399,13.334
	point
	-23.290,-8.399,17.112
	point
	-22.795,-8.399,19.298
	point
	-18.014,-8.399,27.295
	reverse


// Pedestrian number 9

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-18.088,-8.399,25.796
	point
	-18.541,-8.399,25.217
	point
	-21.875,-8.399,22.582
	point
	-28.026,-8.399,20.969
	reverse


// Pedestrian number 10

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-31.049,-8.312,30.797
	point
	-32.365,-8.378,28.670
	point
	-31.880,-8.399,27.049
	point
	-26.954,-8.399,22.126
	reverse


// Pedestrian number 11

29				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-18.195,-8.399,20.342
	point
	-23.002,-8.399,21.605
	point
	-25.091,-8.399,20.653
	point
	-32.598,-8.399,22.399
	reverse


// Pedestrian number 12

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-32.591,-8.399,24.086
	point
	-27.924,-8.399,23.873
	point
	-23.525,-8.399,21.791
	point
	-19.997,-8.399,21.901
	reverse


// Pedestrian number 13

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-21.375,-8.399,20.306
	point
	-23.681,-8.399,20.191
	point
	-32.543,-8.399,17.329
	reverse


// Pedestrian number 14

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-18.315,-8.354,11.767
	point
	-19.966,-8.399,15.144
	point
	-26.241,-8.399,17.897
	point
	-32.394,-8.399,15.594
	reverse


// Pedestrian number 15

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.274,-8.399,13.778
	point
	-30.907,-8.399,14.378
	point
	-32.797,-8.399,27.616
	reverse


// Pedestrian number 16

29				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-30.049,-8.399,27.794
	point
	-27.854,-8.399,22.185
	point
	-26.024,-8.399,20.083
	point
	-22.452,-8.399,18.255
	point
	-17.979,-8.399,14.448
	point
	-1.122,-5.365,14.985
	reverse


// Pedestrian number 17

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	1.063,-5.307,12.463
	point
	0.386,-5.303,13.297
	point
	-0.783,-5.294,13.746
	point
	-7.011,-6.424,13.323
	reverse


// Pedestrian number 18

5				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-1.894,-5.304,9.058
	point
	-0.350,-5.294,12.230
	point
	-0.252,-5.296,13.216
	point
	2.601,-5.305,15.754
	point
	2.929,-5.225,16.048
	point
	7.170,-5.225,16.504
	reverse


// Pedestrian number 19

18				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	17.123,-5.321,10.428
	point
	13.455,-5.319,13.244
	point
	10.759,-5.318,13.696
	point
	-0.545,-5.303,15.818
	reverse


// Pedestrian number 20

29				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-23.880,-8.399,23.374
	point
	-21.320,-8.399,24.896
	point
	-19.720,-8.399,27.932
	point
	-19.448,-5.302,45.150
	point
	-20.203,-5.303,46.980
	reverse


// Pedestrian number 21

12				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-7.473,-5.301,37.613
	point
	-17.773,-5.293,45.538
	point
	-20.046,-5.307,48.500
	point
	-20.247,-5.319,52.576
	point
	-20.737,-5.321,53.106
	reverse


// Pedestrian number 22

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-17.552,-5.321,56.743
	point
	-17.572,-5.321,53.681
	point
	-18.367,-5.321,51.240
	point
	-21.440,-5.303,45.351
	reverse


// Pedestrian number 23

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-29.494,-5.227,57.113
	point
	-28.602,-5.227,59.589
	point
	-28.827,-5.227,62.849
	point
	-28.978,-5.321,63.741
	point
	-31.162,-5.321,66.194
	reverse


// Pedestrian number 24

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-19.156,-5.321,66.553
	point
	-19.631,-5.321,66.050
	point
	-20.608,-5.321,66.293
	point
	-21.008,-5.321,66.981
	reverse


// Pedestrian number 25

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-13.986,-5.321,62.002
	point
	-15.351,-5.321,64.998
	point
	-17.136,-5.321,66.298
	reverse


// Pedestrian number 26

12				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-42.283,-5.227,62.674
	reverse


// Pedestrian number 27

29				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-42.018,-5.227,62.534
	point
	-38.953,-5.227,59.487
	point
	-38.628,-5.227,56.770
	point
	-38.094,-5.321,56.548
	point
	-35.805,-5.321,53.301
	reverse


// Pedestrian number 28

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-9.322,-1.840,61.719
	reverse


// Pedestrian number 29

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-5.649,-1.840,67.414
	reverse


// Pedestrian number 30

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-12.912,-1.840,67.295
	reverse


// Pedestrian number 31

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-2.931,-1.840,62.178
	reverse


// Pedestrian number 32

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-13.341,-1.840,64.569
	reverse


// Pedestrian number 33

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-41.643,-4.084,68.713
	reverse


// Pedestrian number 34

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-44.706,-4.084,68.910
	reverse


// Pedestrian number 35

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-42.034,-4.474,61.188
	reverse


// Pedestrian number 36

29				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-32.094,-5.321,65.994
	point
	-33.415,-5.321,65.146
	point
	-41.769,-5.321,63.522
	point
	-42.056,-5.227,63.222
	reverse


// Pedestrian number 37

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-44.591,-5.321,65.031
	point
	-46.246,-5.321,66.410
	point
	-48.160,-5.321,66.702
	point
	-50.564,-5.321,63.745
	reverse


// Pedestrian number 38

5				// Ref num
6				// Number of instructions
1				// Initial instruction

	point
	-67.648,-5.227,69.397
	point
	-68.394,-5.227,67.602
	point
	-67.555,-5.227,63.133
	point
	-67.346,-5.321,62.787
	point
	-63.812,-5.321,53.125
	reverse


// Pedestrian number 39

29				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-75.106,-5.262,74.922
	point
	-74.894,-5.321,74.644
	point
	-72.745,-5.321,73.058
	point
	-69.381,-5.321,73.289
	point
	-58.874,-5.321,68.371
	reverse


// Pedestrian number 40

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-70.448,-5.321,73.729
	point
	-72.571,-5.321,71.917
	point
	-75.422,-5.321,70.399
	point
	-77.709,-5.321,65.198
	reverse


// Pedestrian number 41

18				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-29.517,-5.227,61.133
	point
	-28.966,-5.227,62.947
	point
	-28.534,-5.321,63.497
	point
	-27.560,-5.321,63.970
	point
	-24.515,-5.321,67.051
	reverse


// Pedestrian number 42

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-76.953,-6.648,71.460
	point
	-82.272,-6.648,72.886
	point
	-85.897,-6.648,75.415
	reverse


// Pedestrian number 43

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-88.477,-6.648,72.005
	point
	-87.850,-6.648,73.675
	point
	-87.004,-6.648,74.096
	point
	-86.230,-6.648,75.277
	reverse


// Pedestrian number 44

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-78.247,-6.648,76.207
	point
	-82.786,-6.648,76.308
	point
	-85.012,-6.648,75.466
	point
	-88.219,-6.648,72.905
	reverse


// Pedestrian number 45

29				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-80.970,-6.648,79.033
	point
	-81.714,-6.648,76.012
	point
	-83.772,-6.648,74.856
	point
	-87.039,-6.648,74.348
	point
	-87.636,-6.648,73.561
	point
	-89.362,-6.648,69.407
	reverse


// Pedestrian number 46

29				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	-89.085,-6.648,71.186
	point
	-88.452,-6.648,70.950
	point
	-84.985,-6.648,73.504
	point
	-83.672,-6.648,75.832
	point
	-81.837,-6.648,76.652
	point
	-81.653,-6.648,77.503
	point
	-83.770,-6.648,77.759
	reverse


// Pedestrian number 47

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-88.279,-6.648,74.961
	reverse


// Pedestrian number 48

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-88.902,-6.648,74.066
	reverse


// Pedestrian number 49

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.004,-6.648,75.995
	reverse


// Pedestrian number 50

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.920,-5.417,26.965
	reverse


// Pedestrian number 51

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.628,-5.417,26.963
	reverse


// Pedestrian number 52

5				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-90.891,-6.648,-35.690
	point
	-90.342,-6.647,-33.875
	point
	-90.047,-6.647,-28.666
	point
	-88.543,-6.171,-26.759
	point
	-87.852,-6.628,-25.876
	point
	-82.563,-6.648,-18.997
	reverse


// Pedestrian number 53

10				// Ref num
7				// Number of instructions
5				// Initial instruction

	point
	-89.925,-6.648,-20.622
	point
	-89.546,-6.647,-19.084
	point
	-88.319,-6.258,-17.588
	point
	-87.737,-6.631,-16.966
	point
	-87.455,-6.636,-10.959
	point
	-83.230,-6.648,-2.391
	reverse


// Pedestrian number 54

8				// Ref num
11				// Number of instructions
4				// Initial instruction

	point
	-88.452,-6.648,3.354
	point
	-88.376,-6.642,2.321
	point
	-87.841,-6.431,1.195
	point
	-87.495,-6.638,-1.411
	point
	-87.913,-6.404,-2.668
	point
	-88.809,-6.647,-5.345
	point
	-89.307,-6.647,-15.314
	point
	-88.292,-6.261,-16.920
	point
	-87.660,-6.632,-17.694
	point
	-82.574,-6.648,-20.452
	reverse


// Pedestrian number 55

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-88.967,-6.637,-68.597
	point
	-90.920,-6.400,-70.141
	point
	-92.975,-6.648,-75.911
	point
	-93.653,-6.648,-78.433
	reverse


// Pedestrian number 56

18				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-86.090,-6.648,-81.646
	point
	-85.622,-6.648,-80.477
	point
	-85.080,-6.648,-80.200
	point
	-81.226,-5.492,-79.198
	point
	-79.841,-5.321,-78.922
	point
	-76.160,-5.319,-74.699
	reverse


// Pedestrian number 57

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-89.252,-6.648,-83.266
	point
	-89.475,-6.648,-81.629
	point
	-89.212,-6.648,-80.641
	point
	-87.409,-6.648,-79.368
	point
	-84.498,-6.648,-78.376
	reverse


// Pedestrian number 58

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-81.447,-6.648,-72.345
	point
	-81.755,-6.648,-70.081
	point
	-83.177,-6.648,-68.151
	point
	-90.389,-6.645,-52.910
	point
	-91.957,-6.647,-54.421
	reverse


// Pedestrian number 59

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-49.093,-5.319,-77.204
	point
	-47.154,-5.319,-77.529
	point
	-44.923,-5.319,-76.198
	point
	-44.005,-5.319,-73.460
	reverse


// Pedestrian number 60

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-47.327,-5.319,-79.094
	point
	-50.687,-5.319,-77.792
	point
	-54.044,-5.319,-73.655
	reverse


// Pedestrian number 61

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-55.344,-5.224,-74.026
	point
	-54.972,-5.224,-77.511
	point
	-54.576,-5.319,-77.750
	point
	-54.122,-5.319,-77.884
	reverse


// Pedestrian number 62

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-37.740,-5.319,-73.546
	point
	-38.758,-5.319,-74.882
	point
	-39.119,-5.319,-76.393
	point
	-44.056,-5.319,-78.759
	reverse


// Pedestrian number 63

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-43.025,-5.319,-76.245
	point
	-41.614,-5.319,-77.200
	point
	-39.345,-5.319,-78.423
	point
	-37.843,-5.319,-81.178
	reverse


// Pedestrian number 64

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-39.236,-5.319,-79.427
	reverse


// Pedestrian number 65

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-38.614,-5.319,-78.720
	reverse


// Pedestrian number 66

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-38.891,-5.319,-79.925
	reverse


// Pedestrian number 67

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-43.751,-5.319,-73.712
	reverse


// Pedestrian number 68

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-55.105,-5.224,-74.024
	reverse


// Pedestrian number 69

115				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-55.563,-5.224,-77.767
	reverse


// Pedestrian number 70

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-30.907,-5.321,-85.638
	point
	-31.574,-5.321,-86.054
	point
	-32.137,-5.320,-87.106
	point
	-31.452,-5.321,-88.482
	reverse


// Pedestrian number 71

18				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-34.904,-5.319,-74.596
	point
	-37.617,-5.319,-73.377
	point
	-42.632,-5.319,-75.825
	reverse


// Pedestrian number 72

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-38.183,-5.319,-72.798
	point
	-38.718,-5.319,-71.605
	point
	-43.589,-5.319,-62.910
	reverse


// Pedestrian number 73

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-38.178,-5.319,-75.792
	point
	-40.334,-5.319,-76.063
	point
	-43.821,-5.319,-74.561
	point
	-46.478,-5.319,-78.150
	reverse


// Pedestrian number 74

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-30.939,-5.321,-55.344
	point
	-32.309,-5.320,-52.493
	point
	-33.024,-5.320,-51.273
	point
	-34.123,-5.321,-50.775
	reverse


// Pedestrian number 75

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-33.001,-5.321,-20.667
	point
	-32.298,-5.321,-20.971
	point
	-30.495,-5.321,-25.312
	reverse


// Pedestrian number 76

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.551,-5.321,-20.395
	point
	-32.235,-5.321,-21.925
	point
	-33.110,-5.321,-23.830
	reverse


// Pedestrian number 77

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-28.252,-5.321,-19.093
	point
	-31.897,-5.321,-22.698
	point
	-32.964,-5.321,-24.484
	reverse


// Pedestrian number 78

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-32.847,-5.321,-19.296
	point
	-31.604,-5.321,-21.880
	point
	-30.388,-5.321,-23.099
	reverse


// Pedestrian number 79

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-33.246,-5.321,-34.937
	point
	-31.470,-5.321,-22.700
	point
	-32.662,-5.321,-17.085
	reverse


// Pedestrian number 80

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-31.184,-3.635,-51.529
	point
	-32.212,-3.635,-50.425
	point
	-32.647,-3.635,-49.389
	reverse


// Pedestrian number 81

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-32.733,-5.321,-38.497
	point
	-31.376,-5.321,-37.037
	point
	-29.717,-5.321,-36.045
	point
	-29.625,-5.321,-35.436
	reverse


// Pedestrian number 82

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-16.851,-5.296,-4.208
	reverse


// Pedestrian number 83

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-33.426,-5.293,-4.312
	reverse


// Pedestrian number 84

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-10.136,-7.469,-3.416
	reverse


// Pedestrian number 85

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-33.609,-5.319,-97.957
	point
	-32.853,-5.320,-98.633
	point
	-32.500,-5.320,-99.654
	point
	-32.674,-5.320,-117.515
	reverse


// Pedestrian number 86

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-37.581,-5.319,-81.980
	point
	-34.109,-5.319,-87.067
	point
	-31.974,-5.319,-92.894
	point
	-30.769,-5.321,-98.100
	reverse


// Pedestrian number 87

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-38.728,-5.319,-82.532
	point
	-37.817,-5.319,-85.014
	point
	-35.587,-5.319,-87.805
	reverse


// Pedestrian number 88

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-33.927,-5.319,-85.912
	point
	-36.495,-5.319,-86.126
	point
	-39.019,-5.319,-84.962
	point
	-41.135,-5.319,-82.860
	reverse


// Pedestrian number 89

10				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-40.113,-5.088,-89.029
	point
	-40.949,-5.088,-89.124
	point
	-41.130,-5.319,-89.021
	point
	-44.173,-5.319,-85.803
	point
	-52.253,-5.319,-84.731
	reverse


// Pedestrian number 90

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-45.334,-5.319,-86.076
	point
	-44.383,-5.319,-85.489
	point
	-41.409,-5.319,-82.847
	reverse


// Pedestrian number 91

18				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-36.317,-5.319,-87.727
	point
	-39.898,-5.319,-87.312
	point
	-44.351,-5.319,-85.084
	point
	-46.645,-5.319,-82.498
	reverse


// Pedestrian number 92

29				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-45.426,-5.319,-85.838
	point
	-44.300,-5.319,-84.685
	point
	-40.717,-5.319,-84.527
	point
	-37.134,-5.319,-88.122
	reverse


// Pedestrian number 93

29				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-31.193,-5.321,-77.841
	point
	-32.539,-5.320,-80.880
	point
	-34.091,-5.319,-82.181
	point
	-37.083,-5.319,-81.677
	reverse


// Pedestrian number 94

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-37.106,-5.319,-73.155
	point
	-34.648,-5.319,-73.732
	point
	-33.380,-5.319,-75.938
	point
	-33.311,-5.319,-83.925
	reverse


// Pedestrian number 95

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-49.597,-5.319,-85.839
	point
	-44.608,-5.319,-83.891
	point
	-43.191,-5.319,-83.940
	point
	-40.660,-5.319,-82.883
	point
	-31.528,-5.319,-83.380
	reverse


// Pedestrian number 96

18				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-31.008,-5.319,-71.208
	point
	-32.598,-5.320,-72.958
	point
	-33.214,-5.319,-75.849
	point
	-33.214,-5.319,-75.849
	point
	-31.237,-5.319,-80.950
	reverse


// Pedestrian number 97

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-36.137,-5.321,-50.784
	point
	-33.254,-5.319,-53.487
	point
	-33.687,-5.319,-63.950
	reverse


// Pedestrian number 98

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-30.820,-5.320,-49.066
	point
	-32.345,-5.320,-51.488
	point
	-34.484,-5.319,-53.789
	point
	-34.952,-5.319,-55.561
	reverse


// Pedestrian number 99

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.553,-5.321,-35.452
	point
	-32.388,-5.321,-37.288
	point
	-32.808,-5.321,-40.197
	reverse


// Pedestrian number 100

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-33.031,-5.321,-35.691
	point
	-31.212,-5.321,-38.189
	point
	-30.807,-5.319,-42.220
	reverse


// Pedestrian number 101

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-32.719,-5.311,-8.840
	point
	-31.304,-5.306,-7.145
	point
	-26.611,-5.298,-4.304
	reverse


// Pedestrian number 102

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.372,-5.321,-19.545
	point
	-31.584,-5.311,-8.705
	point
	-30.715,-5.303,-4.285
	reverse


// Pedestrian number 103

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-32.750,-5.321,-20.817
	point
	-31.320,-5.321,-21.757
	point
	-30.581,-5.321,-25.161
	reverse


// Pedestrian number 104

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-19.239,-8.399,13.849
	point
	-29.898,-8.399,20.852
	point
	-30.488,-8.399,26.197
	reverse


// Pedestrian number 105

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.243,-8.399,15.715
	point
	-31.130,-8.399,18.218
	point
	-32.888,-8.397,26.804
	reverse


// Pedestrian number 106

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-33.924,-8.347,37.231
	point
	-35.200,-8.028,40.328
	point
	-37.560,-7.534,43.643
	point
	-37.865,-7.488,45.047
	reverse


// Pedestrian number 107

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-55.360,-7.497,28.890
	point
	-54.836,-7.477,30.598
	point
	-58.002,-7.403,41.387
	reverse


// Pedestrian number 108

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-56.320,-7.487,29.840
	point
	-54.031,-7.461,31.904
	point
	-38.389,-7.470,45.549
	reverse


// Pedestrian number 109

18				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-38.877,-7.459,45.966
	point
	-40.502,-7.478,44.070
	point
	-43.110,-7.458,42.865
	point
	-44.367,-7.486,39.044
	point
	-51.609,-7.485,30.825
	point
	-52.239,-7.497,28.405
	reverse


// Pedestrian number 110

29				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-52.859,-7.500,28.229
	point
	-52.673,-7.479,30.075
	point
	-44.568,-7.437,42.954
	point
	-42.204,-7.460,43.746
	point
	-38.939,-7.514,42.841
	reverse


// Pedestrian number 111

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-53.603,-8.266,18.817
	point
	-54.205,-8.154,17.550
	point
	-54.310,-7.848,15.737
	point
	-53.576,-7.513,12.810
	point
	-51.472,-7.497,10.926
	reverse


// Pedestrian number 112

18				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-52.057,-7.472,9.743
	point
	-53.463,-7.497,11.499
	point
	-53.994,-7.516,13.019
	point
	-54.849,-7.703,14.633
	reverse


// Pedestrian number 113

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-52.603,-7.510,12.860
	point
	-54.345,-7.498,11.543
	point
	-57.119,-7.425,5.584
	reverse


// Pedestrian number 114

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-63.503,-7.515,49.931
	point
	-53.007,-7.302,45.814
	point
	-43.031,-7.510,38.558
	reverse


// Pedestrian number 115

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-48.942,-7.502,32.422
	point
	-53.221,-7.310,45.190
	point
	-54.016,-7.358,49.137
	point
	-53.294,-7.385,49.822
	reverse


// Pedestrian number 116

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-42.887,-7.510,52.955
	point
	-37.376,-7.463,50.669
	point
	-33.542,-7.510,49.028
	point
	-33.345,-7.514,47.551
	reverse


// Pedestrian number 117

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-33.344,-7.507,47.348
	point
	-40.562,-7.423,48.479
	point
	-46.938,-7.348,48.558
	point
	-51.771,-7.511,52.973
	reverse


// Pedestrian number 118

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-40.970,-7.513,53.013
	point
	-41.118,-7.415,47.584
	point
	-41.346,-7.506,40.813
	reverse


// Pedestrian number 119

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-46.660,-7.514,53.034
	point
	-50.115,-7.329,45.770
	point
	-52.728,-7.382,39.328
	point
	-63.538,-7.516,35.472
	reverse


// Pedestrian number 120

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-57.296,-7.507,29.085
	point
	-57.609,-7.500,29.621
	point
	-54.895,-7.402,37.643
	point
	-53.158,-7.336,43.100
	point
	-43.323,-7.511,52.961
	reverse


// Pedestrian number 121

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-51.104,-7.294,47.668
	point
	-49.526,-7.336,45.894
	point
	-42.345,-7.512,39.177
	reverse


// Pedestrian number 122

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-60.999,-7.516,28.285
	point
	-55.999,-7.483,31.047
	point
	-51.311,-7.456,33.658
	point
	-49.584,-7.501,31.834
	reverse


// Pedestrian number 123

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-50.831,-7.500,30.526
	point
	-54.714,-7.407,37.207
	point
	-58.332,-7.410,40.384
	point
	-58.565,-7.415,42.458
	reverse


// Pedestrian number 124

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-60.560,-7.511,12.597
	point
	-56.423,-7.432,6.170
	point
	-53.455,-7.318,-3.371
	reverse


// Pedestrian number 125

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-51.844,-7.322,-3.387
	point
	-55.820,-7.322,0.579
	point
	-56.034,-7.433,6.153
	point
	-57.198,-7.514,12.890
	reverse


// Pedestrian number 126

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-55.580,-7.515,12.999
	point
	-55.299,-7.499,11.588
	point
	-56.184,-7.472,9.365
	point
	-63.389,-7.513,5.222
	reverse


// Pedestrian number 127

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-52.517,-7.455,8.230
	point
	-56.082,-7.487,10.635
	point
	-59.643,-7.514,12.831
	point
	-63.236,-7.513,12.789
	reverse


// Pedestrian number 128

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-41.430,-7.497,1.052
	point
	-46.827,-7.405,-1.382
	point
	-51.218,-7.329,-3.406
	reverse


// Pedestrian number 129

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-47.373,-7.371,-3.693
	point
	-46.898,-7.399,-1.813
	point
	-46.106,-7.428,-0.110
	point
	-43.694,-7.484,2.226
	point
	-50.730,-7.495,10.010
	reverse


// Pedestrian number 130

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-33.242,-7.497,-6.208
	point
	-39.014,-7.444,-10.926
	point
	-48.124,-7.504,-18.466
	reverse


// Pedestrian number 131

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-43.811,-7.515,-19.061
	point
	-39.190,-7.442,-11.164
	point
	-37.435,-7.496,-2.985
	reverse


// Pedestrian number 132

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-34.718,-7.496,-5.634
	point
	-38.428,-7.450,-9.768
	point
	-41.061,-7.429,-12.543
	point
	-54.529,-7.487,-17.538
	reverse


// Pedestrian number 133

13				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-53.260,-7.514,-19.066
	point
	-42.754,-7.399,-10.027
	point
	-39.663,-7.436,-10.334
	point
	-35.027,-7.491,-10.809
	point
	-32.913,-7.522,-12.929
	point
	-29.286,-8.076,-13.601
	reverse


// Pedestrian number 134

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-32.983,-7.518,-14.480
	point
	-38.168,-7.455,-10.987
	point
	-49.071,-7.346,-4.045
	point
	-52.859,-7.309,-4.119
	reverse


// Pedestrian number 135

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-52.705,-7.318,-3.376
	point
	-48.303,-7.349,-0.814
	point
	-42.967,-7.496,2.450
	reverse


// Pedestrian number 136

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-56.713,-7.420,5.059
	point
	-52.750,-7.415,4.624
	point
	-47.843,-7.407,4.021
	point
	-43.073,-7.459,-0.567
	point
	-39.756,-7.498,-0.524
	reverse


// Pedestrian number 137

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-51.903,-7.449,7.526
	point
	-48.963,-7.401,0.376
	point
	-48.698,-7.358,-3.400
	reverse


// Pedestrian number 138

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-59.836,-7.511,-18.912
	point
	-60.098,-7.446,-11.054
	point
	-60.869,-7.462,0.266
	point
	-57.475,-7.414,4.578
	reverse


// Pedestrian number 139

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-57.031,-7.414,4.567
	point
	-56.314,-7.369,-0.989
	point
	-55.720,-7.357,-5.812
	point
	-57.886,-7.401,-8.092
	reverse


// Pedestrian number 140

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-58.204,-7.407,-8.703
	point
	-59.639,-7.437,-10.495
	point
	-60.513,-7.454,-12.704
	point
	-63.311,-7.512,-14.093
	point
	-63.501,-7.515,-18.966
	reverse


// Pedestrian number 141

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-62.482,-7.495,-19.002
	point
	-61.013,-7.465,-8.319
	point
	-59.883,-7.442,-2.192
	point
	-52.513,-7.442,7.088
	reverse


// Pedestrian number 142

29				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-58.160,-7.407,5.078
	point
	-61.451,-7.474,-0.256
	point
	-63.403,-7.513,-3.368
	point
	-63.243,-7.510,-9.729
	point
	-59.348,-7.431,-12.913
	reverse


// Pedestrian number 143

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-58.994,-7.424,-11.340
	point
	-60.973,-7.464,-11.872
	point
	-63.484,-7.515,-12.821
	reverse


// Pedestrian number 144

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-63.015,-7.519,-36.806
	point
	-59.915,-7.519,-45.025
	point
	-59.515,-7.519,-45.450
	point
	-59.481,-7.519,-47.978
	reverse


// Pedestrian number 145

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-59.398,-7.519,-36.736
	point
	-58.234,-7.519,-44.927
	point
	-57.871,-7.519,-45.529
	point
	-56.982,-7.519,-45.496
	point
	-55.664,-7.519,-50.380
	reverse


// Pedestrian number 146

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-60.113,-7.520,-36.786
	point
	-59.142,-7.520,-43.979
	point
	-58.523,-7.519,-44.640
	point
	-58.522,-7.519,-45.496
	reverse


// Pedestrian number 147

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-50.687,-7.520,-38.138
	point
	-58.735,-7.520,-43.861
	point
	-61.622,-7.519,-45.775
	point
	-61.775,-7.519,-50.426
	reverse


// Pedestrian number 148

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-62.586,-7.520,-36.720
	point
	-59.452,-7.519,-39.358
	point
	-54.848,-7.519,-43.296
	reverse


// Pedestrian number 149

10				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-55.855,-7.519,-36.394
	point
	-56.137,-7.519,-37.418
	point
	-58.794,-7.519,-39.086
	point
	-62.526,-7.519,-43.338
	point
	-62.983,-7.519,-50.360
	reverse


// Pedestrian number 150

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-62.577,-7.519,-50.369
	point
	-61.993,-7.519,-44.593
	point
	-59.795,-7.519,-40.512
	point
	-58.225,-7.519,-38.851
	point
	-50.174,-7.519,-36.908
	reverse


// Pedestrian number 151

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-51.025,-7.519,-44.302
	point
	-53.534,-7.519,-46.983
	point
	-56.635,-7.519,-50.415
	reverse


// Pedestrian number 152

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-52.414,-7.519,-50.384
	point
	-52.035,-7.519,-46.347
	point
	-51.515,-7.519,-36.335
	reverse


// Pedestrian number 153

29				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-53.628,-7.519,-36.296
	point
	-54.814,-7.519,-40.218
	point
	-54.505,-7.518,-42.916
	reverse


// Pedestrian number 154

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-53.784,-7.518,-43.274
	point
	-53.277,-7.518,-46.118
	point
	-52.866,-7.518,-48.348
	point
	-33.126,-7.519,-50.320
	reverse


// Pedestrian number 155

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-33.071,-7.519,-47.818
	point
	-50.995,-7.519,-47.895
	point
	-58.584,-7.519,-48.268
	reverse


// Pedestrian number 156

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-50.578,-7.519,-42.313
	point
	-55.139,-7.519,-39.885
	point
	-61.294,-7.519,-36.617
	point
	-61.947,-7.895,-33.928
	reverse


// Pedestrian number 157

1				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-53.560,-7.519,-43.104
	point
	-50.444,-7.519,-46.566
	point
	-44.618,-7.519,-46.424
	point
	-38.556,-7.519,-46.293
	point
	-33.078,-7.519,-42.177
	reverse


// Pedestrian number 158

29				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-49.931,-7.519,-44.025
	point
	-44.330,-7.519,-46.138
	point
	-40.162,-7.519,-46.097
	point
	-38.394,-7.519,-48.113
	point
	-38.367,-7.519,-50.415
	reverse


// Pedestrian number 159

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-33.093,-7.519,-46.875
	point
	-44.199,-7.519,-46.974
	point
	-45.992,-7.519,-43.602
	point
	-49.244,-7.519,-41.157
	point
	-49.295,-7.519,-35.782
	reverse


// Pedestrian number 160

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-35.921,-7.519,-36.363
	point
	-44.407,-7.519,-45.495
	point
	-49.263,-7.519,-50.370
	reverse


// Pedestrian number 161

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-46.377,-7.519,-50.382
	point
	-40.884,-7.519,-45.333
	point
	-36.874,-7.519,-41.589
	point
	-33.032,-7.520,-41.454
	reverse


// Pedestrian number 162

13				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-33.784,-7.519,-36.345
	point
	-35.836,-7.519,-40.169
	point
	-41.038,-7.519,-44.953
	point
	-43.414,-7.519,-45.213
	point
	-45.323,-7.519,-43.035
	point
	-50.181,-7.518,-42.729
	reverse


// Pedestrian number 163

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-50.184,-7.518,-40.571
	point
	-45.810,-7.518,-38.979
	point
	-44.814,-7.518,-36.265
	reverse


// Pedestrian number 164

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-20.973,-7.519,-85.150
	point
	-27.543,-7.519,-53.716
	point
	-28.237,-7.519,-45.307
	point
	-31.474,-7.518,-43.504
	reverse


// Pedestrian number 165

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-30.609,-7.518,-42.876
	point
	-28.402,-7.517,-53.502
	point
	-27.288,-7.517,-59.463
	point
	-24.162,-7.517,-62.728
	point
	-20.218,-7.517,-64.205
	reverse


// Pedestrian number 166

10				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	-20.086,-7.517,-62.330
	point
	-27.207,-7.517,-53.505
	point
	-27.230,-7.518,-48.330
	point
	-23.783,-7.518,-42.156
	point
	-23.764,-7.327,-41.030
	point
	-23.806,994.985,-37.222
	point
	-23.930,994.973,-32.750
	reverse


// Pedestrian number 167

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-23.204,-7.518,-41.012
	point
	-23.312,-7.519,-42.613
	point
	-26.761,-7.519,-52.560
	point
	-26.733,-7.519,-53.643
	point
	-20.122,-7.520,-57.445
	reverse


// Pedestrian number 168

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-20.050,-7.519,-45.149
	point
	-26.298,-7.519,-49.694
	point
	-30.564,-7.519,-52.543
	reverse


// Pedestrian number 169

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-30.543,-7.519,-51.012
	point
	-27.278,-7.519,-46.286
	point
	-24.799,-7.518,-42.736
	point
	-24.039,-7.518,-38.217
	reverse


// Pedestrian number 170

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-26.622,-7.518,-36.768
	point
	-28.453,-7.518,-44.790
	point
	-28.848,-7.519,-46.756
	point
	-30.566,-7.519,-48.150
	reverse


// Pedestrian number 171

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-20.031,-7.519,-47.180
	point
	-24.810,-7.519,-50.974
	point
	-26.251,-7.519,-51.922
	point
	-26.200,-7.519,-53.358
	point
	-25.369,-7.519,-53.243
	reverse


// Pedestrian number 172

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-25.161,-7.519,-52.380
	point
	-22.898,-7.519,-50.628
	point
	-22.215,-7.519,-45.272
	point
	-20.373,-7.518,-41.655
	point
	-20.252,-7.518,-36.904
	reverse


// Pedestrian number 173

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-22.837,-7.518,-36.797
	point
	-22.616,-7.518,-42.564
	point
	-21.798,-7.519,-45.030
	point
	-20.716,-7.519,-45.982
	point
	-20.530,-7.519,-54.972
	point
	-30.703,-7.520,-65.369
	reverse


// Pedestrian number 174

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-28.974,-7.521,-85.182
	point
	-28.232,-7.519,-57.173
	point
	-24.278,-7.519,-54.803
	point
	-20.012,-7.519,-55.515
	reverse


// Pedestrian number 175

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-20.013,-7.519,-51.668
	point
	-28.438,-7.519,-56.171
	point
	-30.282,-7.519,-59.356
	point
	-30.430,-7.521,-80.565
	point
	-26.101,-7.522,-85.304
	reverse


// Pedestrian number 176

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-24.696,-7.522,-85.206
	point
	-24.506,-7.521,-82.075
	point
	-24.856,-6.354,-74.371
	point
	-25.050,995.407,-63.965
	point
	-26.238,995.651,-62.534
	reverse


// Pedestrian number 177

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-23.990,996.543,-56.189
	point
	-24.095,995.096,-65.888
	point
	-23.952,-7.519,-82.040
	point
	-23.927,-7.519,-85.253
	reverse


// Pedestrian number 178

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-30.604,-7.519,-38.888
	point
	-26.779,-7.519,-42.663
	point
	-23.593,-7.519,-45.859
	point
	-22.379,-7.519,-85.267
	reverse


// Pedestrian number 179

5				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-19.910,-7.519,-77.177
	point
	-25.867,-7.519,-68.351
	point
	-27.582,-7.519,-59.139
	point
	-27.697,-7.519,-58.003
	point
	-27.429,-7.519,-57.431
	point
	-20.144,-7.519,-56.436
	reverse


// Pedestrian number 180

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.591,-7.518,-43.333
	point
	25.515,-7.518,-44.353
	point
	23.077,-7.517,-56.011
	reverse


// Pedestrian number 181

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	20.795,-7.517,-56.272
	point
	25.083,-7.518,-44.421
	point
	26.179,-7.518,-43.366
	reverse


// Pedestrian number 182

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	18.276,-7.518,-45.019
	point
	24.288,-7.518,-43.335
	point
	25.511,-7.518,-42.746
	point
	31.862,-7.518,-30.332
	reverse


// Pedestrian number 183

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	28.353,-7.518,-29.308
	point
	26.434,-7.518,-41.377
	point
	26.322,-7.518,-42.378
	reverse


// Pedestrian number 184

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	26.535,-7.518,-42.578
	point
	27.485,-7.518,-43.464
	point
	26.422,-7.518,-43.321
	reverse


// Pedestrian number 185

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	31.909,-7.518,-43.144
	point
	27.490,-7.518,-42.775
	point
	26.698,-7.518,-43.076
	reverse


// Pedestrian number 186

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.489,-7.518,-42.971
	point
	24.803,-7.518,-42.521
	point
	18.722,-7.518,-38.881
	reverse


// Pedestrian number 187

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	18.132,-7.518,-40.382
	point
	24.521,-7.518,-42.006
	point
	26.107,-7.518,-40.575
	point
	32.817,-7.518,-41.754
	reverse


// Pedestrian number 188

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	23.956,-7.518,-33.306
	point
	20.981,-7.518,-31.897
	point
	18.588,-7.518,-30.632
	point
	13.360,-7.518,-34.155
	reverse


// Pedestrian number 189

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	25.621,-7.518,-42.327
	point
	24.411,-7.518,-36.467
	point
	23.158,-7.518,-33.755
	point
	20.621,-7.518,-31.036
	point
	19.631,-7.518,-28.823
	point
	23.774,-7.518,-21.959
	reverse


// Pedestrian number 190

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	34.139,-7.518,-39.821
	point
	24.378,-7.518,-34.986
	point
	21.031,-7.518,-32.464
	point
	16.859,-7.518,-28.628
	point
	15.920,-7.518,-21.694
	reverse


// Pedestrian number 191

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	17.042,-7.518,-32.198
	point
	12.872,-7.518,-29.236
	point
	5.814,-7.518,-26.902
	point
	5.151,-7.518,-21.629
	reverse


// Pedestrian number 192

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	1.152,-7.518,-30.366
	point
	4.784,-7.518,-31.148
	point
	11.846,-7.518,-32.706
	point
	12.490,-7.518,-34.109
	reverse


// Pedestrian number 193

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	5.547,-7.518,-34.116
	point
	2.001,-7.518,-31.917
	point
	0.991,-7.518,-31.189
	point
	-0.006,-7.518,-31.322
	point
	-5.773,-7.518,-21.702
	reverse


// Pedestrian number 194

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-17.496,-7.519,-21.543
	point
	-8.131,-7.519,-22.452
	point
	0.613,-7.519,-27.798
	point
	5.312,-7.519,-30.514
	point
	7.078,-7.519,-34.072
	reverse


// Pedestrian number 195

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	12.655,-7.519,-21.604
	point
	6.409,-7.519,-28.864
	point
	5.509,-7.519,-30.044
	point
	0.696,-7.519,-29.769
	reverse


// Pedestrian number 196

13				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-6.148,-7.519,-34.071
	point
	-0.858,-7.519,-29.693
	point
	6.225,-7.518,-28.438
	point
	10.965,-7.518,-27.368
	point
	13.421,-7.518,-23.856
	point
	24.990,-7.518,-23.195
	reverse


// Pedestrian number 197

1				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	23.052,-7.518,-26.098
	point
	17.653,-7.518,-24.851
	point
	12.544,-7.518,-26.357
	point
	-0.898,-7.518,-24.523
	point
	-4.030,-7.519,-21.261
	point
	-3.963,-7.518,-19.964
	reverse


// Pedestrian number 198

8				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-5.373,-7.518,-19.915
	point
	-3.885,-7.521,-23.738
	point
	9.630,-7.526,-28.650
	point
	12.305,-7.525,-26.847
	point
	15.740,-7.518,-24.477
	point
	21.410,-7.518,-27.628
	reverse


// Pedestrian number 199

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	0.417,-7.518,-21.821
	point
	-8.731,-7.518,-27.208
	point
	-17.521,-7.519,-32.382
	reverse


// Pedestrian number 200

29				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-15.815,-7.519,-34.262
	point
	-13.066,-7.519,-30.842
	point
	-8.419,-7.519,-27.392
	point
	-5.505,-7.519,-23.795
	point
	-4.214,-7.516,-19.183
	point
	-2.188,-7.514,-19.098
	reverse


// Pedestrian number 201

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-8.086,-7.519,-21.680
	point
	-9.653,-7.519,-27.120
	point
	-11.173,-7.519,-34.170
	reverse


// Pedestrian number 202

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	3.127,-7.501,-18.303
	point
	-4.140,-7.504,-18.523
	point
	-9.628,-7.511,-18.975
	point
	-17.417,-7.510,-18.742
	reverse


// Pedestrian number 203

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-17.646,-7.516,-12.652
	point
	-10.993,-7.436,-13.399
	point
	3.000,-7.444,-15.138
	reverse


// Pedestrian number 204

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	14.067,-7.514,-16.036
	point
	4.160,-7.436,-14.713
	point
	-3.675,-7.374,-11.271
	point
	-10.993,-7.425,-6.161
	reverse


// Pedestrian number 205

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-9.310,-7.449,-4.170
	point
	-1.343,-7.342,-4.473
	point
	13.985,-7.513,-5.383
	reverse


// Pedestrian number 206

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	13.985,-7.513,12.278
	point
	7.508,-7.395,-4.017
	point
	-0.039,-7.328,-4.192
	point
	-4.364,-7.364,-5.932
	point
	-12.076,-7.463,-5.181
	reverse


// Pedestrian number 207

1				// Ref num
8				// Number of instructions
4				// Initial instruction

	point
	-10.832,-7.436,-5.805
	point
	-6.689,-7.377,-6.603
	point
	-3.575,-7.338,-5.090
	point
	-0.707,-7.341,-3.908
	point
	0.549,-7.329,-3.448
	point
	4.398,-7.375,1.349
	point
	13.998,-7.513,3.079
	reverse


// Pedestrian number 208

8				// Ref num
8				// Number of instructions
5				// Initial instruction

	point
	13.988,-7.513,-0.381
	point
	10.872,-7.456,-4.201
	point
	5.049,-7.350,-4.529
	point
	2.976,-7.322,-3.089
	point
	0.047,-7.330,-3.955
	point
	-1.064,-7.349,-3.580
	point
	-10.172,-7.473,-3.183
	reverse


// Pedestrian number 209

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-10.468,-7.513,-0.357
	point
	-1.793,-7.367,-2.922
	point
	-0.528,-7.345,-3.313
	point
	0.404,-7.296,-6.325
	point
	14.152,-7.516,-11.639
	reverse


// Pedestrian number 210

13				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	7.186,-7.513,-18.979
	point
	5.595,-7.448,-15.361
	point
	-0.477,-7.306,-6.498
	point
	-1.563,-7.383,-1.311
	point
	-4.057,-7.468,2.932
	point
	0.525,-7.492,9.916
	point
	1.949,-7.507,12.775
	reverse


// Pedestrian number 211

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	3.125,-7.509,12.895
	point
	10.377,-7.495,11.187
	point
	13.948,-7.512,10.171
	reverse


// Pedestrian number 212

13				// Ref num
11				// Number of instructions
2				// Initial instruction

	point
	14.022,-7.514,8.636
	point
	12.090,-7.516,13.001
	point
	11.911,-7.782,15.216
	point
	11.706,-8.186,17.716
	point
	11.796,-8.350,20.205
	point
	12.581,-8.051,24.928
	point
	12.583,-7.834,26.335
	point
	12.205,-7.530,28.127
	point
	10.960,-7.513,28.695
	point
	1.012,-7.498,29.998
	reverse


// Pedestrian number 213

5				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	8.535,-7.514,12.947
	point
	6.869,-7.453,7.823
	point
	1.635,-7.358,0.044
	point
	0.105,-7.348,-2.409
	point
	-4.666,-7.417,-1.886
	point
	-10.090,-7.480,-2.677
	reverse


// Pedestrian number 214

5				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	7.349,-7.511,12.728
	point
	3.111,-7.399,3.487
	point
	0.751,-7.369,0.058
	point
	0.201,-7.368,-0.649
	point
	2.457,-7.324,-8.483
	point
	-1.069,-7.513,-19.034
	reverse


// Pedestrian number 215

13				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	-17.586,-7.515,52.769
	point
	-16.762,-7.507,51.021
	point
	-15.106,-7.490,47.515
	point
	-11.330,-7.445,45.692
	point
	-5.049,-7.358,47.495
	point
	-2.449,-7.332,48.442
	point
	8.529,-7.509,52.916
	reverse


// Pedestrian number 216

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-17.711,-7.508,47.432
	point
	-16.952,-7.508,50.705
	point
	-16.462,-7.506,52.879
	reverse


// Pedestrian number 217

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-8.209,-7.500,39.149
	point
	2.164,-7.363,40.488
	point
	14.057,-7.514,42.363
	reverse


// Pedestrian number 218

10				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	14.125,-7.515,28.688
	point
	12.871,-7.492,38.310
	point
	2.560,-7.367,40.153
	point
	0.583,-7.373,40.707
	point
	-10.321,-7.495,41.655
	point
	-15.559,-7.494,46.804
	point
	-17.086,-7.500,47.299
	reverse


// Pedestrian number 219

1				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	-14.416,-7.499,45.455
	point
	-11.344,-7.463,45.310
	point
	1.975,-7.357,40.988
	point
	2.715,-7.361,40.702
	point
	7.620,-7.433,35.177
	point
	9.608,-7.474,31.891
	point
	13.620,-7.517,28.311
	reverse


// Pedestrian number 220

8				// Ref num
14				// Number of instructions
3				// Initial instruction

	point
	14.002,-7.513,34.779
	point
	7.445,-7.414,36.719
	point
	4.352,-7.371,40.079
	point
	-1.697,-7.327,46.793
	point
	-4.582,-7.474,52.045
	point
	-17.735,-7.517,52.155
	point
	-20.442,-7.954,52.004
	point
	-22.516,-8.166,51.894
	point
	-24.971,-8.380,51.762
	point
	-27.894,-8.226,51.694
	point
	-30.386,-7.849,50.983
	point
	-32.778,-7.526,52.261
	point
	-35.663,-7.483,52.912
	reverse


// Pedestrian number 221

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-2.230,-7.497,33.342
	point
	1.323,-7.374,39.596
	point
	1.715,-7.336,42.770
	point
	5.939,-7.373,49.508
	point
	14.093,-7.515,52.999
	reverse


// Pedestrian number 222

1				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	11.227,-7.463,52.826
	point
	5.419,-7.358,46.434
	point
	3.166,-7.339,42.723
	point
	1.581,-7.367,40.075
	point
	1.428,-7.419,35.501
	point
	-0.322,-7.490,31.992
	point
	2.767,-7.500,28.602
	reverse


// Pedestrian number 223

13				// Ref num
9				// Number of instructions
2				// Initial instruction

	point
	6.275,-7.508,28.422
	point
	2.624,-7.387,38.436
	point
	0.454,-7.350,42.689
	point
	0.415,-7.298,47.052
	point
	1.036,-7.450,51.443
	point
	-4.799,-7.505,52.832
	point
	-9.345,-7.496,52.605
	point
	-14.735,-7.471,46.694
	reverse


// Pedestrian number 224

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	10.116,-7.522,28.414
	point
	11.492,-7.501,29.677
	point
	14.110,-7.514,32.448
	reverse


// Pedestrian number 225

13				// Ref num
9				// Number of instructions
3				// Initial instruction

	point
	12.904,-7.609,27.670
	point
	12.844,-7.518,28.273
	point
	11.672,-7.505,29.361
	point
	9.444,-7.481,31.283
	point
	2.311,-7.425,35.063
	point
	1.728,-7.395,37.608
	point
	-1.607,-7.420,39.071
	point
	-6.415,-7.495,37.752
	reverse


// Pedestrian number 226

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	8.642,-7.513,28.402
	point
	10.667,-7.489,30.654
	point
	12.822,-7.491,33.204
	point
	13.772,-7.508,33.625
	point
	13.825,-7.510,51.356
	reverse


// Pedestrian number 227

5				// Ref num
8				// Number of instructions
3				// Initial instruction

	point
	14.039,-7.514,52.156
	point
	10.651,-7.452,47.773
	point
	9.361,-7.439,34.681
	point
	9.015,-7.488,30.605
	point
	8.490,-7.496,29.883
	point
	5.179,-7.492,29.732
	point
	4.565,-7.504,28.511
	reverse


// Pedestrian number 228

123				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.746,-7.341,41.191
	reverse


// Pedestrian number 229

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.741,-7.361,39.519
	reverse


// Pedestrian number 230

136				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	13.586,-7.505,52.214
	reverse


// Pedestrian number 231

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	0.922,-7.307,45.773
	reverse


// Pedestrian number 232

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.990,-7.441,34.569
	reverse


// Pedestrian number 233

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	0.926,-7.371,39.607
	reverse


// Pedestrian number 234

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.923,-7.337,42.894
	reverse


// Pedestrian number 235

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.037,-7.357,-0.199
	reverse


// Pedestrian number 236

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-0.527,-7.329,-4.696
	reverse


// Pedestrian number 237

122				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-1.768,-7.355,-3.894
	reverse


// Pedestrian number 238

104				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-0.684,-7.309,-6.638
	reverse


// Pedestrian number 239

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-0.108,-7.340,-3.322
	reverse


// Pedestrian number 240

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-11.757,-7.434,-6.265
	reverse


// Pedestrian number 241

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-9.194,-7.457,-3.495
	reverse


// Pedestrian number 242

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	0.355,-7.525,-29.875
	reverse


// Pedestrian number 243

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-0.059,-7.519,-30.690
	reverse


// Pedestrian number 244

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	0.991,-7.518,-30.620
	reverse


// Pedestrian number 245

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	4.856,-7.518,-30.919
	reverse


// Pedestrian number 246

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.146,-7.518,-28.727
	reverse


// Pedestrian number 247

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	12.195,-7.518,-26.556
	reverse


// Pedestrian number 248

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.078,-7.518,-41.883
	reverse


// Pedestrian number 249

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	25.266,-7.518,-43.335
	reverse


// Pedestrian number 250

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.834,-7.518,-43.193
	reverse


// Pedestrian number 251

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	33.535,-7.518,-30.975
	reverse


// Pedestrian number 252

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.948,-7.518,-31.358
	reverse


// Pedestrian number 253

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	36.631,-7.518,-31.704
	reverse


// Pedestrian number 254

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	38.502,-7.518,-32.090
	reverse


// Pedestrian number 255

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-24.837,-7.519,-52.519
	reverse


// Pedestrian number 256

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-25.295,-7.519,-52.046
	reverse


// Pedestrian number 257

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-25.526,-7.519,-53.524
	reverse


// Pedestrian number 258

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-25.997,-7.519,-52.105
	reverse


// Pedestrian number 259

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-24.219,-7.519,-83.994
	reverse


// Pedestrian number 260

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-24.978,-3.623,-56.130
	reverse


// Pedestrian number 261

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-27.233,-7.519,-66.633
	reverse


// Pedestrian number 262

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-25.598,-7.519,-66.504
	reverse


// Pedestrian number 263

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-24.005,-7.519,-66.379
	reverse


// Pedestrian number 264

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-22.199,-7.519,-66.237
	reverse


// Pedestrian number 265

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-28.740,-7.519,-39.089
	reverse


// Pedestrian number 266

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-26.717,-7.519,-39.089
	reverse


// Pedestrian number 267

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-23.873,-7.519,-39.089
	reverse


// Pedestrian number 268

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-21.977,-7.519,-39.089
	reverse


// Pedestrian number 269

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-50.059,-7.519,-43.291
	reverse


// Pedestrian number 270

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-50.054,-7.519,-42.242
	reverse


// Pedestrian number 271

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-50.000,-7.519,-40.870
	reverse


// Pedestrian number 272

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-49.987,-7.519,-39.774
	reverse


// Pedestrian number 273

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-49.969,-7.519,-38.327
	reverse


// Pedestrian number 274

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-60.438,-5.319,-65.403
	point
	-63.269,-5.319,-72.999
	point
	-64.485,-5.319,-77.840
	point
	-66.029,-5.319,-78.299
	reverse


// Pedestrian number 275

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-63.214,994.881,-82.938
	point
	-63.445,994.881,-81.185
	point
	-65.175,-5.319,-78.627
	point
	-66.105,-5.319,-71.662
	reverse


// Pedestrian number 276

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-66.117,-5.319,-63.310
	point
	-61.507,-5.319,-60.333
	point
	-59.382,-5.319,-57.429
	reverse


// Pedestrian number 277

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-61.144,-5.319,-60.394
	point
	-60.362,-5.319,-58.949
	point
	-57.486,-5.319,-57.824
	point
	-52.943,-5.319,-58.907
	point
	-49.808,-5.319,-57.486
	reverse


// Pedestrian number 278

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-52.623,-5.319,-57.467
	point
	-51.039,-5.319,-58.729
	point
	-50.272,-5.319,-60.211
	point
	-49.845,-5.319,-73.020
	reverse


// Pedestrian number 279

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-50.942,-5.319,-66.253
	point
	-49.287,-5.319,-61.896
	point
	-47.582,-5.319,-58.969
	point
	-38.738,-5.319,-56.087
	reverse


// Pedestrian number 280

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-39.028,-5.319,-55.866
	point
	-44.511,-5.319,-61.410
	point
	-54.503,-5.319,-72.801
	reverse


// Pedestrian number 281

12				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-53.999,-5.319,-70.056
	point
	-48.676,-5.319,-68.504
	point
	-44.945,-5.319,-62.250
	point
	-44.678,994.881,-61.904
	point
	-37.733,994.881,-62.225
	reverse


// Pedestrian number 282

12				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-40.406,-5.319,-69.793
	point
	-40.664,-5.319,-68.668
	point
	-44.323,-5.319,-63.545
	point
	-46.950,-5.319,-60.151
	point
	-47.055,-5.319,-57.561
	reverse


// Pedestrian number 283

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-48.752,-5.319,-57.414
	point
	-45.089,-5.319,-61.212
	point
	-44.475,994.881,-61.618
	point
	-37.767,994.881,-66.456
	reverse


// Pedestrian number 284

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-41.211,-5.319,-68.783
	point
	-44.510,-5.319,-63.557
	point
	-46.455,-5.319,-61.318
	point
	-50.821,-5.319,-60.304
	reverse


// Pedestrian number 285

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-43.895,-5.319,-63.287
	reverse


// Pedestrian number 286

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-43.389,-5.319,-61.342
	reverse


// Pedestrian number 287

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-44.574,-5.319,-61.043
	reverse


// Pedestrian number 288

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-44.823,-5.319,-63.653
	reverse


// Pedestrian number 289

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-29.973,-5.321,-86.105
	point
	-22.687,-5.321,-87.575
	point
	-19.886,-5.321,-88.175
	point
	-15.082,-5.321,-85.068
	point
	-2.664,-5.321,-84.839
	reverse


// Pedestrian number 290

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-29.439,-5.321,-86.864
	point
	-28.159,-5.321,-87.786
	point
	-26.863,-5.321,-88.467
	point
	1.165,-5.321,-88.338
	point
	1.445,-5.321,-88.003
	reverse


// Pedestrian number 291

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-17.543,-5.321,-88.220
	point
	-17.578,-5.321,-82.576
	point
	-17.334,-5.321,-53.504
	point
	-19.584,994.879,-48.491
	point
	-20.549,994.879,-47.300
	reverse


// Pedestrian number 292

8				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	-17.249,-5.321,-82.863
	point
	-16.898,-5.321,-59.655
	point
	-17.610,-5.321,-57.011
	point
	-17.026,-5.321,-55.206
	point
	-16.975,-5.321,-37.341
	point
	-15.924,994.879,-34.596
	point
	-15.498,994.879,-33.881
	reverse


// Pedestrian number 293

1				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-18.973,-5.321,-88.563
	point
	-19.769,-5.321,-79.246
	point
	-19.723,-5.321,-63.231
	point
	-18.935,-5.321,-60.783
	point
	-19.619,994.879,-58.848
	point
	-20.412,994.879,-56.796
	reverse


// Pedestrian number 294

133				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-6.927,-1.840,63.319
	reverse


// Pedestrian number 295

132				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-6.948,-1.840,65.806
	reverse


// Pedestrian number 296

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	1.701,-1.840,66.940
	reverse


// Pedestrian number 297

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	1.682,-1.840,65.360
	reverse


// Pedestrian number 298

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	1.655,-1.840,63.570
	reverse


// Pedestrian number 299

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	1.631,-1.840,61.978
	reverse


// Pedestrian number 300

101				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-3.340,-1.840,64.627
	reverse


// Pedestrian number 301

135				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-11.011,-1.840,64.553
	reverse


// Pedestrian number 302

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-24.212,-4.323,59.155
	reverse


// Pedestrian number 303

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-24.008,-4.323,70.911
	reverse


// Pedestrian number 304

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-23.522,-4.323,74.854
	reverse


// Pedestrian number 305

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-24.662,-4.323,50.410
	reverse


// Pedestrian number 306

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-27.930,-4.323,50.318
	reverse


// Pedestrian number 307

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-21.141,-4.323,50.311
	reverse


// Pedestrian number 308

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-43.734,-4.323,57.627
	reverse


// Pedestrian number 309

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-43.549,-4.323,60.536
	reverse


// Pedestrian number 310

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-9.252,-5.321,-87.626
	point
	-5.332,-5.321,-87.713
	point
	-2.342,-5.321,-87.746
	reverse


// Pedestrian number 311

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	2.506,-5.321,-84.058
	point
	1.971,-5.321,-84.898
	point
	-2.364,-5.321,-85.109
	reverse


// Pedestrian number 312

5				// Ref num
9				// Number of instructions
3				// Initial instruction

	point
	1.895,-5.229,-83.836
	point
	1.869,-5.229,-84.375
	point
	-3.981,-5.229,-84.487
	point
	-14.917,-5.229,-84.250
	point
	-15.965,-5.229,-80.264
	point
	-15.341,-5.229,-75.121
	point
	-16.426,-5.229,-67.839
	point
	-14.991,-5.229,-67.217
	reverse


// Pedestrian number 313

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	3.044,-5.321,-87.830
	point
	9.099,-5.321,-87.490
	point
	12.812,995.079,-88.632
	point
	14.381,995.079,-90.350
	reverse


// Pedestrian number 314

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	5.520,-5.321,-85.175
	point
	6.613,-5.321,-85.621
	point
	12.703,-5.321,-85.195
	point
	17.675,995.079,-88.060
	point
	19.680,995.079,-89.225
	reverse


// Pedestrian number 315

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	21.528,-5.321,-88.133
	point
	25.196,-5.321,-87.096
	point
	26.365,-5.321,-86.374
	point
	27.141,-5.321,-84.164
	reverse


// Pedestrian number 316

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	25.027,-5.321,-76.394
	point
	13.421,-5.321,-76.251
	point
	5.434,-5.321,-76.685
	reverse


// Pedestrian number 317

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	2.760,-5.321,-84.016
	point
	3.093,-5.321,-75.280
	point
	2.028,-5.321,-68.525
	point
	3.103,-5.321,-62.388
	reverse


// Pedestrian number 318

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	14.133,-5.321,-60.105
	point
	20.248,-5.321,-64.097
	point
	25.103,-5.321,-64.134
	point
	27.501,995.079,-64.817
	point
	38.024,995.079,-60.409
	reverse


// Pedestrian number 319

5				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-62.755,-5.321,-36.354
	point
	-65.634,-5.322,-33.243
	point
	-67.112,-5.326,-29.346
	point
	-66.405,-5.326,-27.769
	point
	-63.421,-5.321,-25.649
	point
	-63.214,-5.320,-20.691
	reverse


// Pedestrian number 320

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-66.936,-5.326,-24.033
	point
	-63.683,-5.324,-31.099
	point
	-63.056,-5.321,-35.675
	point
	-60.335,-5.321,-36.473
	reverse


// Pedestrian number 321

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-66.043,-5.328,-35.729
	point
	-65.423,-5.326,-33.213
	point
	-63.114,-5.321,-27.827
	point
	-63.105,-5.319,-22.636
	point
	-67.272,-5.322,-19.319
	reverse


// Pedestrian number 322

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-63.457,-5.325,-36.305
	point
	-63.109,-5.324,-33.925
	point
	-63.067,-5.322,-30.179
	point
	-66.351,-5.324,-26.494
	point
	-66.757,-5.321,-25.074
	reverse


// Pedestrian number 323

1				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-63.609,-5.321,-52.711
	point
	-64.193,-5.321,-35.540
	point
	-63.546,-5.321,-33.774
	point
	-63.297,-5.321,-32.618
	point
	-65.526,-5.321,-30.671
	point
	-67.101,-5.321,-29.973
	reverse


// Pedestrian number 324

1				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-63.256,-5.321,-20.408
	point
	-63.867,-5.321,-18.817
	point
	-64.157,-5.321,-15.785
	point
	-67.025,-5.321,-12.768
	point
	-67.316,-5.321,-4.971
	point
	-63.844,-5.321,-0.421
	reverse


// Pedestrian number 325

5				// Ref num
9				// Number of instructions
2				// Initial instruction

	point
	-67.593,-5.227,-30.722
	point
	-67.661,-5.227,-26.101
	point
	-67.648,-5.227,-21.513
	point
	-68.608,-5.227,-17.112
	point
	-67.693,-5.227,-6.297
	point
	-68.691,-5.227,2.903
	point
	-67.677,-5.227,15.886
	point
	-68.642,-5.227,23.389
	reverse


// Pedestrian number 326

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-67.717,-5.227,23.610
	point
	-67.837,-5.227,2.302
	point
	-68.086,-5.227,-5.329
	point
	-67.630,-5.227,-9.024
	point
	-68.674,-5.227,-11.425
	reverse


// Pedestrian number 327

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-68.605,-5.227,-28.701
	point
	-67.939,-5.227,-19.322
	point
	-67.616,-5.227,-11.352
	point
	-68.640,-5.227,-9.004
	reverse


// Pedestrian number 328

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-63.757,-5.321,-13.369
	point
	-63.832,-5.321,-2.712
	point
	-67.047,-5.321,5.641
	point
	-64.826,-5.321,11.711
	point
	-63.209,-5.321,14.099
	reverse


// Pedestrian number 329

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-63.049,-5.321,13.891
	point
	-64.504,-5.321,14.476
	point
	-66.098,-5.322,15.915
	point
	-67.220,-5.322,19.203
	reverse


// Pedestrian number 330

12				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-67.497,-5.227,19.540
	point
	-68.045,-5.227,15.781
	point
	-68.354,-5.227,11.425
	point
	-67.710,-5.227,6.526
	point
	-68.654,-5.227,5.893
	reverse


// Pedestrian number 331

8				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-63.259,-5.321,14.680
	point
	-65.113,-5.321,19.954
	point
	-66.049,-5.321,20.781
	point
	-67.096,-5.321,21.104
	point
	-67.123,-5.321,25.847
	point
	-63.848,-5.321,28.390
	reverse


// Pedestrian number 332

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-62.933,-5.321,26.891
	point
	-65.574,-5.321,21.044
	point
	-65.795,-5.321,20.681
	reverse


// Pedestrian number 333

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-67.277,-5.321,11.333
	point
	-65.744,-5.321,13.534
	point
	-63.357,-5.321,14.409
	reverse


// Pedestrian number 334

8				// Ref num
9				// Number of instructions
3				// Initial instruction

	point
	-67.265,-5.321,6.258
	point
	-67.052,-5.321,10.113
	point
	-65.838,-5.321,12.510
	point
	-64.115,-5.321,19.076
	point
	-63.358,-5.321,19.985
	point
	-63.350,-5.321,25.308
	point
	-62.263,-5.321,26.687
	point
	-61.851,-5.321,27.798
	reverse


// Pedestrian number 335

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-63.000,-5.321,27.469
	point
	-64.919,-5.321,28.366
	point
	-65.758,-5.321,31.322
	point
	-67.162,-5.321,32.037
	reverse


// Pedestrian number 336

5				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-66.089,-5.321,26.144
	point
	-65.172,-5.321,28.235
	point
	-65.123,-5.321,29.932
	point
	-63.876,-5.321,31.362
	point
	-63.816,-5.321,53.417
	point
	-60.848,-5.321,56.219
	reverse


// Pedestrian number 337

10				// Ref num
7				// Number of instructions
5				// Initial instruction

	point
	-64.153,-5.321,56.257
	point
	-65.670,-5.321,52.907
	point
	-65.550,-5.321,38.795
	point
	-63.929,-5.321,33.293
	point
	-64.871,-5.321,28.807
	point
	-65.641,-5.321,28.409
	reverse


// Pedestrian number 338

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-65.955,-5.321,27.466
	point
	-64.917,-5.321,27.719
	point
	-63.957,994.879,30.279
	point
	-63.429,994.879,30.813
	reverse


// Pedestrian number 339

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-65.729,-5.321,32.773
	point
	-64.036,-5.321,28.476
	point
	-63.337,-5.321,26.902
	reverse


// Pedestrian number 340

1				// Ref num
8				// Number of instructions
2				// Initial instruction

	point
	-65.889,-5.321,33.081
	point
	-65.747,-5.321,38.791
	point
	-67.271,-5.321,46.167
	point
	-64.013,-5.321,48.636
	point
	-64.084,-5.321,53.248
	point
	-61.602,994.879,53.652
	point
	-60.349,994.879,52.914
	reverse


// Pedestrian number 341

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-67.204,-5.321,52.943
	point
	-65.394,-5.321,55.219
	point
	-64.472,-5.321,56.341
	reverse


// Pedestrian number 342

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-67.275,-5.321,57.355
	point
	-66.376,-5.321,58.110
	point
	-65.083,-5.321,59.197
	reverse


// Pedestrian number 343

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-62.488,-5.321,63.647
	point
	-64.640,-5.321,66.265
	point
	-67.177,-5.321,68.002
	reverse


// Pedestrian number 344

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-65.729,-5.321,68.251
	point
	-64.526,-5.321,66.417
	point
	-64.098,-5.321,65.740
	point
	-63.610,-5.321,63.575
	reverse


// Pedestrian number 345

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-65.299,-5.321,60.053
	point
	-64.851,-5.321,66.001
	point
	-65.156,-5.321,72.423
	reverse


// Pedestrian number 346

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-67.277,-5.321,69.575
	point
	-64.997,-5.321,66.658
	point
	-65.021,-5.321,61.286
	point
	-67.131,-5.321,59.796
	reverse


// Pedestrian number 347

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-60.156,-5.321,56.226
	point
	-59.318,-5.321,55.131
	point
	-57.603,-5.321,53.495
	point
	-52.802,994.879,53.357
	point
	-51.771,994.879,52.813
	reverse


// Pedestrian number 348

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-60.609,-5.321,53.472
	point
	-59.315,-5.321,54.848
	point
	-57.752,-5.321,56.288
	point
	-37.928,-5.321,56.261
	point
	-30.244,-5.321,58.515
	reverse


// Pedestrian number 349

13				// Ref num
9				// Number of instructions
2				// Initial instruction

	point
	-32.629,-5.321,45.426
	point
	-32.530,-5.321,53.044
	point
	-31.045,-5.321,53.674
	point
	-29.957,-5.321,53.567
	point
	-29.595,-5.321,54.699
	point
	-28.710,-5.321,55.307
	point
	-28.708,994.879,55.600
	point
	-28.373,994.879,64.105
	reverse


// Pedestrian number 350

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-32.709,-5.321,53.210
	point
	-31.257,-5.321,54.510
	point
	-30.116,-5.321,56.034
	reverse


// Pedestrian number 351

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-32.006,-5.320,53.033
	point
	-30.888,-5.326,54.315
	point
	-30.089,-5.337,56.708
	point
	-30.115,-5.366,63.272
	point
	-29.337,-5.321,64.507
	reverse


// Pedestrian number 352

13				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-34.511,-5.321,53.220
	point
	-32.069,-5.321,53.504
	point
	-31.196,-5.321,54.334
	point
	-30.529,-5.321,55.726
	point
	-30.197,-5.321,57.549
	point
	-33.974,-5.321,65.131
	reverse


// Pedestrian number 353

1				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-42.624,-5.225,62.234
	point
	-38.595,-5.225,60.953
	point
	-38.580,-5.225,57.940
	point
	-42.793,-5.225,57.293
	reverse


// Pedestrian number 354

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-39.469,-5.227,56.526
	point
	-40.340,-5.227,58.924
	point
	-41.793,-5.227,62.607
	reverse


// Pedestrian number 355

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-30.118,-5.321,55.489
	point
	-32.677,-5.321,59.536
	point
	-34.439,-5.321,65.097
	reverse


// Pedestrian number 356

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-36.797,-5.321,63.976
	point
	-32.800,-5.321,59.235
	point
	-31.600,-5.321,56.365
	point
	-31.441,-5.321,53.440
	reverse


// Pedestrian number 357

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-33.544,-5.321,53.236
	point
	-33.004,-5.321,59.830
	point
	-31.038,-5.321,63.122
	point
	-29.519,-5.321,65.030
	reverse


// Pedestrian number 358

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-32.671,-5.321,66.095
	point
	-29.110,-5.321,73.404
	point
	-26.846,-5.321,81.534
	point
	-26.595,-5.321,81.666
	reverse


// Pedestrian number 359

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-29.228,-5.321,82.385
	point
	-28.632,-5.321,80.560
	point
	-29.201,-5.321,73.805
	point
	-30.372,-5.321,68.284
	point
	-29.497,-5.321,65.781
	reverse


// Pedestrian number 360

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-29.171,-5.227,67.387
	point
	-27.654,-5.227,75.341
	point
	-26.861,-5.227,79.165
	point
	-24.727,-5.227,80.267
	point
	-22.330,-5.227,80.296
	reverse


// Pedestrian number 361

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-25.161,-5.227,79.609
	point
	-27.530,-5.227,74.951
	point
	-28.654,-5.227,68.254
	point
	-27.420,-5.227,67.376
	reverse


// Pedestrian number 362

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-26.307,-5.321,81.134
	point
	-28.304,-5.321,84.330
	point
	-24.212,-5.321,89.533
	point
	-22.053,-5.321,90.329
	point
	-18.149,-5.321,95.426
	reverse


// Pedestrian number 363

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-19.835,-5.321,95.301
	point
	-20.051,-5.321,94.538
	point
	-26.049,-5.321,85.056
	point
	-29.223,-5.321,82.660
	reverse


// Pedestrian number 364

12				// Ref num
9				// Number of instructions
2				// Initial instruction

	point
	-29.228,-5.321,81.680
	point
	-26.296,-5.321,84.788
	point
	-26.552,-5.321,86.691
	point
	-23.672,-5.321,88.175
	point
	-22.526,-5.321,89.695
	point
	-22.675,-5.321,91.380
	point
	-20.375,-5.321,94.314
	point
	-18.779,-5.321,95.505
	reverse


// Pedestrian number 365

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-18.092,-5.321,91.998
	point
	-19.238,-5.321,93.498
	point
	-20.717,-5.321,93.991
	reverse


// Pedestrian number 366

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-20.489,-5.275,94.649
	point
	-25.584,-5.337,88.072
	point
	-24.829,-5.321,86.492
	point
	-24.774,-5.251,86.058
	reverse


// Pedestrian number 367

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-19.205,-5.321,95.505
	point
	-19.362,-5.321,94.955
	point
	-19.842,-5.321,92.160
	point
	-19.912,-5.321,82.955
	point
	-21.673,-5.321,80.825
	reverse


// Pedestrian number 368

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-23.241,-5.321,90.796
	point
	-19.985,-5.321,93.252
	point
	-16.766,-5.321,93.106
	point
	-14.600,-5.321,92.111
	point
	18.785,-5.321,92.301
	reverse


// Pedestrian number 369

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	17.697,-5.321,94.292
	point
	16.591,-5.321,91.535
	point
	15.093,-5.321,86.968
	point
	15.011,-5.321,83.324
	reverse


// Pedestrian number 370

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	15.767,-5.321,81.953
	point
	16.843,-5.321,91.742
	point
	17.991,-5.321,93.976
	reverse


// Pedestrian number 371

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	14.809,-5.321,94.873
	point
	16.324,-5.321,91.392
	point
	19.137,-5.321,87.687
	point
	19.324,-5.321,79.501
	reverse


// Pedestrian number 372

13				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	17.190,-5.321,80.916
	point
	17.206,-5.321,89.792
	point
	17.186,-5.321,92.773
	point
	15.707,-5.321,94.523
	point
	4.072,-5.321,94.721
	point
	0.778,-5.321,92.125
	reverse


// Pedestrian number 373

8				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-17.570,-5.321,91.888
	point
	-11.281,-5.321,94.568
	point
	-6.570,-5.321,94.785
	point
	-2.486,-5.321,92.723
	point
	8.424,-5.321,92.414
	point
	14.273,-5.321,94.770
	reverse


// Pedestrian number 374

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	14.537,-5.321,94.836
	point
	16.503,-5.321,85.315
	point
	17.024,-5.321,81.162
	point
	23.271,-5.321,76.654
	point
	23.165,-5.321,76.155
	reverse


// Pedestrian number 375

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	23.837,-5.321,74.500
	point
	23.446,-5.321,76.650
	point
	21.480,-5.321,79.327
	point
	18.572,-5.321,81.415
	point
	15.143,-5.321,89.847
	reverse


// Pedestrian number 376

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	15.100,-5.321,88.745
	point
	15.443,-5.321,83.625
	point
	16.417,-5.321,82.128
	point
	17.687,-5.321,81.138
	point
	17.845,-5.321,80.438
	reverse


// Pedestrian number 377

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	19.484,-5.321,81.153
	point
	16.246,-5.321,83.057
	point
	14.461,-5.321,84.167
	reverse


// Pedestrian number 378

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	15.180,-5.321,82.924
	point
	17.502,-5.321,81.903
	point
	20.065,-5.321,79.313
	point
	23.647,-5.321,77.745
	point
	27.259,-5.321,75.339
	reverse


// Pedestrian number 379

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	27.320,-5.321,75.125
	point
	26.531,-5.321,70.919
	point
	26.069,-5.321,67.801
	point
	26.249,-5.321,67.027
	reverse


// Pedestrian number 380

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	26.445,-5.321,68.218
	point
	26.327,-5.321,70.406
	point
	24.583,-5.321,72.813
	point
	24.346,-5.321,73.405
	point
	24.012,-5.321,73.752
	reverse


// Pedestrian number 381

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	24.504,-5.321,72.254
	point
	23.731,-5.321,68.581
	point
	23.160,-5.321,67.071
	point
	23.803,-5.321,64.447
	reverse


// Pedestrian number 382

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	24.430,-5.321,65.447
	point
	24.269,-5.321,67.295
	point
	24.606,-5.321,70.942
	point
	24.217,-5.321,71.649
	reverse


// Pedestrian number 383

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	23.986,-5.321,70.851
	point
	23.493,-5.321,68.431
	point
	20.684,-5.321,64.311
	point
	15.466,-5.321,61.589
	reverse


// Pedestrian number 384

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	21.950,-5.321,68.112
	point
	21.521,-5.321,66.225
	point
	20.457,-5.321,65.349
	point
	20.580,-5.321,63.694
	point
	20.066,-5.321,61.136
	reverse


// Pedestrian number 385

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	19.823,-5.321,60.474
	point
	20.217,-5.321,58.320
	point
	23.153,-5.321,54.452
	reverse


// Pedestrian number 386

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	24.245,-5.321,64.056
	point
	23.160,-5.321,58.301
	point
	23.099,-5.321,55.343
	reverse


// Pedestrian number 387

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	23.246,-5.321,64.095
	point
	22.400,-5.321,59.481
	point
	14.570,-5.321,52.842
	reverse


// Pedestrian number 388

13				// Ref num
10				// Number of instructions
3				// Initial instruction

	point
	19.940,-5.321,61.795
	point
	20.453,-5.321,60.224
	point
	20.474,-5.321,58.438
	point
	20.967,-5.321,56.106
	point
	18.139,-5.321,50.393
	point
	20.939,-5.321,40.578
	point
	23.252,-5.321,39.478
	point
	23.206,-5.321,35.477
	point
	19.179,-5.321,32.703
	reverse


// Pedestrian number 389

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	19.435,-5.321,58.108
	point
	20.217,-5.321,47.602
	point
	20.141,-5.321,40.444
	point
	18.935,-5.321,32.752
	reverse


// Pedestrian number 390

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	14.475,-5.321,33.526
	point
	20.045,-5.321,47.866
	point
	23.086,-5.321,49.934
	point
	23.480,-5.321,55.391
	reverse


// Pedestrian number 391

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	23.058,-5.321,54.271
	point
	20.529,-5.321,48.723
	point
	14.850,994.879,46.270
	point
	13.813,994.879,45.834
	reverse


// Pedestrian number 392

5				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	14.513,-5.321,47.477
	point
	22.183,-5.321,50.466
	point
	22.883,-5.321,57.121
	point
	31.941,-5.321,67.108
	point
	42.902,-5.321,67.233
	point
	43.667,-5.237,68.446
	reverse


// Pedestrian number 393

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	44.854,-5.321,65.263
	point
	42.818,-5.321,66.387
	point
	36.324,-5.321,67.060
	point
	29.246,-5.321,65.503
	point
	25.843,-5.320,63.901
	reverse


// Pedestrian number 394

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	27.190,-5.320,68.397
	point
	25.515,-5.320,64.844
	point
	24.569,-5.320,62.458
	point
	15.585,-5.316,60.478
	reverse


// Pedestrian number 395

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-62.832,-5.321,-34.284
	point
	-50.570,-5.321,-36.295
	point
	-40.265,-5.321,-36.305
	point
	-35.394,-5.321,-34.187
	reverse


// Pedestrian number 396

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-38.815,-5.321,-34.207
	point
	-36.261,-5.321,-35.795
	point
	-33.372,-5.321,-36.417
	reverse


// Pedestrian number 397

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-29.875,-5.321,-34.137
	point
	-24.733,-5.321,-34.563
	point
	-22.860,-5.321,-36.281
	point
	-19.696,-5.321,-36.363
	point
	-19.054,-5.321,-37.000
	reverse


// Pedestrian number 398

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-19.769,-5.321,-36.724
	point
	-14.729,-5.321,-34.822
	point
	-4.682,-5.321,-34.556
	reverse


// Pedestrian number 399

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-7.184,-5.321,-34.522
	point
	-2.854,-5.321,-36.298
	point
	5.089,-5.321,-36.197
	point
	8.064,-5.321,-34.441
	reverse


// Pedestrian number 400

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	6.469,994.879,-33.861
	point
	4.158,994.879,-35.841
	point
	-1.725,-5.321,-36.387
	point
	-4.141,-5.321,-38.179
	point
	-8.485,-5.321,-38.039
	reverse


// Pedestrian number 401

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-8.297,-5.321,-37.487
	point
	-6.262,-5.321,-35.711
	point
	-4.321,-5.321,-34.567
	reverse


// Pedestrian number 402

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	7.829,-5.321,-34.392
	point
	-3.488,-5.321,-34.554
	point
	-6.450,-5.321,-36.050
	point
	-8.043,-5.321,-37.742
	reverse


// Pedestrian number 403

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-8.979,-5.321,-37.738
	point
	-7.250,-5.321,-36.320
	point
	-5.920,-5.321,-36.249
	point
	-3.210,994.879,-35.084
	point
	-2.411,994.879,-33.801
	reverse


// Pedestrian number 404

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-0.098,-5.321,-37.510
	point
	8.093,-5.321,-36.303
	point
	10.453,-5.321,-34.589
	point
	15.315,-5.321,-34.479
	point
	18.834,-5.321,-31.141
	reverse


// Pedestrian number 405

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	20.271,-5.321,-29.280
	point
	19.888,-5.321,-30.734
	point
	19.306,994.879,-36.392
	point
	20.045,994.879,-38.198
	reverse


// Pedestrian number 406

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	18.455,-5.318,-37.908
	point
	22.125,-5.318,-33.694
	point
	26.139,-5.318,-30.773
	reverse


// Pedestrian number 407

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	25.323,-5.318,-30.816
	point
	20.201,-5.318,-31.584
	point
	18.956,994.882,-31.797
	point
	17.515,994.881,-31.101
	reverse


// Pedestrian number 408

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	19.191,-5.318,-30.511
	point
	19.547,-5.318,-31.202
	point
	20.197,-5.318,-34.528
	point
	16.825,-5.318,-39.124
	reverse


// Pedestrian number 409

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	17.834,-5.318,-38.178
	point
	15.619,-5.319,-38.663
	point
	12.239,-5.319,-37.985
	reverse


// Pedestrian number 410

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	14.987,-5.319,-38.812
	point
	15.389,-5.319,-36.690
	point
	17.659,-5.318,-33.339
	point
	23.930,-5.318,-33.000
	reverse


// Pedestrian number 411

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	25.837,-5.318,-30.207
	point
	25.597,-5.318,-26.569
	point
	25.542,-5.318,-21.828
	point
	24.334,-5.318,-20.187
	reverse


// Pedestrian number 412

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	24.573,-5.318,-32.403
	point
	25.252,-5.318,-30.247
	point
	29.321,-5.318,-26.787
	reverse


// Pedestrian number 413

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	30.387,-5.318,-23.891
	point
	29.530,-5.318,-25.523
	point
	26.930,-5.318,-28.595
	point
	26.450,-5.318,-29.708
	reverse


// Pedestrian number 414

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	22.352,-5.318,-27.085
	point
	27.350,-5.318,-22.083
	point
	30.442,-5.318,-18.729
	point
	32.348,-5.318,-18.695
	reverse


// Pedestrian number 415

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	30.317,-5.318,-19.338
	point
	25.267,-5.318,-14.287
	point
	24.289,-5.319,-9.813
	reverse


// Pedestrian number 416

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	24.323,-5.319,-9.044
	point
	25.308,-5.318,-9.773
	point
	25.376,-5.318,-13.778
	point
	26.428,-5.318,-16.881
	point
	30.567,-5.318,-17.575
	reverse


// Pedestrian number 417

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	29.947,-5.318,-11.529
	point
	28.919,-5.318,-10.805
	point
	27.563,-5.318,-7.753
	point
	27.472,-5.318,-3.986
	point
	28.846,-5.321,-2.872
	reverse


// Pedestrian number 418

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	31.154,-5.321,0.819
	point
	29.148,-5.321,-2.068
	point
	25.234,-5.321,-4.412
	point
	24.248,-5.321,-6.128
	reverse


// Pedestrian number 419

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	32.075,-5.321,-4.317
	point
	30.115,-5.321,-2.047
	point
	29.460,-5.321,-1.949
	point
	24.608,-5.321,1.157
	reverse


// Pedestrian number 420

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	29.668,-5.321,7.093
	point
	27.942,-5.321,12.804
	point
	26.740,-5.321,22.320
	reverse


// Pedestrian number 421

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	22.661,-5.321,18.334
	point
	25.282,-5.321,15.402
	point
	26.429,-5.321,13.389
	point
	29.001,-5.321,11.810
	reverse


// Pedestrian number 422

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	30.143,-5.321,12.123
	point
	28.223,-5.321,12.821
	point
	26.353,-5.321,13.883
	point
	23.815,-5.321,14.169
	reverse


// Pedestrian number 423

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	23.597,-5.321,14.734
	point
	27.955,-5.321,13.339
	point
	28.708,-5.321,12.945
	point
	30.983,-5.321,13.114
	reverse


// Pedestrian number 424

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	23.848,-5.321,13.315
	point
	27.510,-5.321,5.193
	point
	27.848,-5.321,1.204
	point
	29.572,-5.321,0.397
	reverse


// Pedestrian number 425

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	27.726,-5.321,0.257
	point
	25.345,-5.321,7.735
	point
	25.089,-5.321,12.943
	point
	23.960,-5.321,13.665
	point
	22.799,-5.321,17.134
	reverse


// Pedestrian number 426

5				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	30.122,-5.321,0.807
	point
	29.252,-5.321,1.061
	point
	28.126,-5.321,1.900
	point
	24.998,-5.321,2.849
	point
	24.565,-5.321,9.860
	reverse


// Pedestrian number 427

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	30.737,-5.321,11.818
	point
	39.081,-5.321,10.343
	point
	42.778,-5.321,8.905
	point
	46.674,-5.321,9.514
	reverse


// Pedestrian number 428

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	23.012,-5.321,17.544
	point
	24.418,-5.321,17.177
	point
	26.679,-5.321,16.225
	point
	29.639,-5.321,16.206
	reverse


// Pedestrian number 429

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	29.605,-5.321,17.200
	point
	21.045,-5.321,24.705
	point
	20.547,-5.321,25.721
	point
	19.429,-5.321,29.949
	point
	14.606,-5.321,29.969
	reverse


// Pedestrian number 430

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	19.368,-5.321,31.593
	point
	20.562,-5.321,29.943
	point
	23.850,-5.321,27.155
	point
	23.701,-5.321,25.978
	point
	24.473,-5.321,23.725
	reverse


// Pedestrian number 431

13				// Ref num
9				// Number of instructions
2				// Initial instruction

	point
	24.426,-5.321,27.706
	point
	20.402,-5.321,32.706
	point
	18.727,-5.321,37.187
	point
	14.572,-5.321,41.713
	point
	14.508,-5.321,54.133
	point
	8.684,-5.321,57.491
	point
	8.619,-5.321,61.659
	point
	7.648,-5.321,66.918
	reverse


// Pedestrian number 432

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	5.899,-7.519,-66.750
	point
	16.680,-7.519,-70.577
	point
	21.873,-7.519,-73.455
	point
	24.882,-7.519,-72.670
	reverse


// Pedestrian number 433

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	24.796,-7.519,-66.391
	point
	16.746,-7.519,-70.030
	point
	10.564,-7.519,-72.075
	point
	7.859,-7.519,-73.686
	point
	5.727,-7.519,-72.781
	reverse


// Pedestrian number 434

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	5.418,-7.519,-70.352
	point
	8.541,-7.519,-68.512
	point
	15.120,-7.519,-70.262
	point
	18.476,-7.519,-73.814
	reverse


// Pedestrian number 435

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	17.242,-7.519,-73.804
	point
	15.911,-7.519,-69.743
	point
	15.004,-7.519,-66.553
	point
	5.943,-7.519,-66.401
	reverse


// Pedestrian number 436

13				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	5.520,-7.519,-67.022
	point
	9.861,-7.519,-69.833
	point
	15.794,-7.519,-70.593
	point
	21.865,-7.519,-69.744
	point
	23.860,-7.519,-70.852
	point
	25.061,-7.519,-68.846
	reverse


// Pedestrian number 437

13				// Ref num
13				// Number of instructions
3				// Initial instruction

	point
	22.865,-7.519,-66.480
	point
	19.110,-7.519,-66.565
	point
	16.425,-7.519,-69.410
	point
	15.016,-7.519,-73.288
	point
	11.096,-7.519,-73.747
	point
	5.311,-7.519,-71.257
	point
	-3.358,-8.079,-72.015
	point
	-7.948,-8.268,-73.260
	point
	-14.988,-8.056,-75.298
	point
	-17.793,-7.713,-75.941
	point
	-19.953,-7.452,-75.857
	point
	-20.096,-7.519,-74.797
	reverse


// Pedestrian number 438

13				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	5.441,-7.519,-73.718
	point
	10.962,-7.519,-71.097
	point
	13.686,-7.519,-71.698
	point
	16.562,-7.519,-69.729
	point
	17.321,-7.519,-67.067
	point
	16.058,-7.519,-66.434
	reverse


// Pedestrian number 439

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	24.945,-7.519,-67.549
	point
	17.334,-7.519,-70.287
	point
	15.510,-7.519,-73.358
	point
	13.054,-7.519,-73.773
	point
	5.470,-7.519,-69.094
	reverse


// Pedestrian number 440

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	52.924,-7.518,-27.775
	point
	50.132,-7.518,-23.604
	point
	46.264,-7.517,-19.994
	reverse


// Pedestrian number 441

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	46.329,-7.517,-28.700
	point
	49.315,-7.517,-23.438
	point
	53.157,-7.518,-21.598
	reverse


// Pedestrian number 442

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	53.139,-7.518,-25.170
	point
	50.625,-7.518,-24.504
	point
	49.208,-7.517,-20.229
	point
	46.046,-7.517,-18.447
	reverse


// Pedestrian number 443

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	46.034,-7.517,-17.992
	point
	49.757,-7.518,-14.206
	point
	53.157,-7.518,-14.257
	reverse


// Pedestrian number 444

5				// Ref num
8				// Number of instructions
5				// Initial instruction

	point
	51.403,-7.518,6.279
	point
	49.130,-7.517,1.700
	point
	51.049,-7.518,-3.610
	point
	49.316,-7.517,-9.887
	point
	50.624,-7.518,-14.449
	point
	48.602,-7.517,-19.177
	point
	53.103,-7.518,-21.181
	reverse


// Pedestrian number 445

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	46.210,-7.517,-23.059
	point
	50.659,-7.518,-20.296
	point
	53.117,-7.518,-16.600
	point
	53.245,-7.518,-8.665
	reverse


// Pedestrian number 446

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	46.274,-7.517,0.701
	point
	47.056,-7.517,-8.241
	point
	52.600,-7.518,-12.577
	point
	53.234,-7.518,-17.374
	reverse


// Pedestrian number 447

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	46.129,-7.517,-16.488
	point
	50.341,-7.517,-9.524
	point
	53.204,-7.518,-1.747
	point
	53.206,-7.518,6.320
	reverse


// Pedestrian number 448

10				// Ref num
9				// Number of instructions
3				// Initial instruction

	point
	50.037,-7.517,6.360
	point
	47.838,-7.517,-0.272
	point
	46.277,-7.517,-6.074
	point
	46.553,-7.517,-11.393
	point
	50.729,-7.517,-16.592
	point
	49.625,-7.518,-23.901
	point
	49.623,994.958,-28.116
	point
	49.627,995.486,-29.192
	reverse


// Pedestrian number 449

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	46.073,-7.518,-18.954
	point
	49.941,-7.518,-23.940
	point
	49.546,-6.240,-26.257
	point
	49.454,994.963,-28.127
	point
	49.419,995.329,-28.872
	reverse


// Pedestrian number 450

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	47.358,-7.518,-29.358
	point
	49.670,-7.518,-18.594
	point
	52.091,-7.518,-15.333
	point
	52.460,-7.518,-9.082
	point
	46.163,-7.518,-3.231
	reverse


// Pedestrian number 451

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	46.160,-7.518,6.203
	point
	47.487,-7.518,-0.113
	point
	53.181,-7.518,-7.132
	reverse


// Pedestrian number 452

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	46.117,-7.518,2.696
	point
	48.939,-7.518,0.111
	point
	49.141,-7.518,-4.404
	point
	46.078,-7.518,-7.636
	reverse


// Pedestrian number 453

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	46.057,-7.518,1.236
	point
	48.616,-7.518,-2.558
	point
	53.215,-7.518,-3.983
	reverse


// Pedestrian number 454

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	52.408,-7.518,6.266
	point
	48.693,-7.518,4.736
	point
	47.163,-7.518,0.032
	point
	46.932,-7.518,-1.310
	point
	46.065,-7.518,-1.660
	reverse


// Pedestrian number 455

10				// Ref num
10				// Number of instructions
5				// Initial instruction

	point
	55.806,-7.518,-0.749
	point
	59.265,-7.518,-14.077
	point
	63.135,-7.518,-29.087
	point
	58.058,-7.518,-28.919
	point
	58.859,-7.518,-13.912
	point
	62.596,-7.518,-8.058
	point
	63.184,-7.518,-5.305
	point
	65.874,-7.518,-3.678
	point
	65.714,-7.518,-1.276
	reverse


// Pedestrian number 456

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	64.480,-7.518,-3.767
	point
	60.308,-7.518,-7.511
	point
	55.862,-7.518,-13.967
	point
	55.669,-7.518,-24.486
	reverse


// Pedestrian number 457

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	55.741,-7.518,-29.194
	point
	60.522,-7.518,-23.306
	point
	63.030,-7.518,-12.543
	point
	56.043,-7.518,-5.714
	point
	55.989,-7.518,6.330
	reverse


// Pedestrian number 458

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	55.820,-7.518,5.612
	point
	58.910,-7.518,-4.140
	point
	63.091,-7.518,-9.042
	reverse


// Pedestrian number 459

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	62.918,-7.518,6.101
	point
	59.271,-7.518,-5.065
	point
	58.269,-7.518,-13.648
	point
	55.620,-7.518,-16.906
	reverse


// Pedestrian number 460

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	55.737,-7.518,-18.559
	point
	56.489,-7.518,-22.486
	point
	58.419,-7.518,-26.556
	point
	63.168,-7.518,-28.349
	reverse


// Pedestrian number 461

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	63.041,-7.518,-26.937
	point
	57.703,-7.518,-23.443
	point
	56.012,-7.518,-18.109
	point
	55.624,-7.518,-11.978
	reverse


// Pedestrian number 462

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	55.866,-7.518,-3.734
	point
	56.255,-7.518,-17.483
	point
	56.539,-7.518,-24.095
	point
	63.118,-7.518,-27.483
	reverse


// Pedestrian number 463

5				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	59.930,-7.518,-29.258
	point
	58.952,-7.518,-20.842
	point
	58.451,-7.518,-16.359
	point
	62.245,-7.518,-10.324
	point
	62.604,-7.518,-5.108
	point
	72.232,-7.518,-2.678
	reverse


// Pedestrian number 464

5				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	72.107,-7.518,6.293
	point
	68.969,-7.518,-4.112
	point
	66.019,-7.518,-11.500
	point
	65.783,-7.518,-29.118
	point
	65.783,-7.518,-29.118
	point
	67.257,-7.518,-29.208
	reverse


// Pedestrian number 465

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	72.269,-7.518,-29.100
	point
	69.886,-7.518,-11.157
	point
	66.614,-7.518,-0.932
	point
	66.112,-7.518,6.115
	reverse


// Pedestrian number 466

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	65.844,-7.518,4.484
	point
	68.666,-7.518,-3.197
	point
	71.595,-7.518,-5.251
	point
	71.737,-7.518,-29.131
	reverse


// Pedestrian number 467

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	69.817,-7.518,-29.243
	point
	67.184,-7.518,-15.204
	point
	69.642,-7.518,-4.756
	point
	69.734,-7.518,2.078
	point
	72.359,-7.518,3.235
	reverse


// Pedestrian number 468

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	72.334,-7.518,1.144
	point
	69.032,-7.518,-2.392
	point
	66.686,-7.518,-9.179
	point
	69.835,-7.518,-14.699
	point
	68.415,-7.518,-29.214
	reverse


// Pedestrian number 469

13				// Ref num
8				// Number of instructions
4				// Initial instruction

	point
	72.443,-7.518,-26.068
	point
	68.370,-7.518,-17.751
	point
	70.592,-7.518,-11.116
	point
	68.823,-7.518,-5.947
	point
	66.184,-7.518,-2.236
	point
	68.968,-7.518,3.564
	point
	68.781,-7.518,6.275
	reverse


// Pedestrian number 470

13				// Ref num
8				// Number of instructions
4				// Initial instruction

	point
	66.812,-7.518,6.109
	point
	70.040,-7.518,4.784
	point
	71.443,-7.518,1.019
	point
	71.422,-7.518,-4.496
	point
	71.333,-7.518,-13.506
	point
	72.294,-7.518,-16.170
	point
	65.645,-7.518,-19.542
	reverse


// Pedestrian number 471

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	65.711,-7.518,-15.143
	point
	69.244,-7.518,-6.065
	point
	72.338,-7.518,-4.627
	reverse


// Pedestrian number 472

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	65.677,-7.518,-3.231
	point
	68.251,-7.518,-3.498
	point
	72.253,-7.518,-3.519
	reverse


// Pedestrian number 473

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	72.301,-7.518,-11.789
	point
	69.632,-7.518,-7.155
	point
	65.815,-7.518,-6.550
	reverse


// Pedestrian number 474

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	65.777,-7.518,3.366
	point
	67.116,-7.518,0.285
	point
	67.905,-7.518,-2.627
	point
	70.677,-7.518,-3.735
	point
	70.626,-7.518,-29.130
	reverse


// Pedestrian number 475

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	65.713,-7.518,-22.243
	point
	69.013,-7.518,-17.923
	point
	69.072,-7.518,-7.931
	point
	72.273,-7.518,-6.366
	reverse


// Pedestrian number 476

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	65.734,-7.518,1.404
	point
	66.732,-7.518,-4.387
	point
	68.763,-7.518,-10.773
	point
	67.039,-7.518,-13.523
	point
	65.672,-7.518,-13.968
	reverse


// Pedestrian number 477

13				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-66.421,-5.280,29.523
	point
	-69.853,-5.289,27.988
	point
	-76.687,-5.303,27.764
	point
	-78.416,-5.309,26.666
	point
	-79.022,-5.314,24.121
	point
	-79.491,-5.315,24.013
	reverse


// Pedestrian number 478

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-74.169,-5.296,29.036
	point
	-75.926,-5.301,28.035
	point
	-77.461,-5.305,27.920
	point
	-78.779,-5.309,26.908
	point
	-79.145,-5.321,-0.302
	reverse


// Pedestrian number 479

13				// Ref num
6				// Number of instructions
4				// Initial instruction

	point
	-78.645,-5.321,-0.356
	point
	-78.207,-5.321,7.465
	point
	-82.677,-5.321,17.214
	point
	-75.969,-5.321,24.364
	point
	-71.354,-5.321,29.652
	reverse


// Pedestrian number 480

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-67.888,-5.321,24.124
	point
	-72.055,-5.321,26.101
	point
	-76.317,-5.321,27.335
	point
	-77.033,-5.321,28.694
	reverse


// Pedestrian number 481

5				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-68.523,-5.321,29.797
	point
	-73.005,-5.321,26.013
	point
	-77.688,-5.321,25.124
	point
	-79.493,-5.321,23.675
	point
	-83.754,994.879,23.496
	point
	-85.057,994.879,23.441
	reverse


// Pedestrian number 482

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-66.770,-5.321,25.065
	point
	-69.888,-5.321,26.126
	point
	-73.859,-5.321,29.267
	reverse


// Pedestrian number 483

10				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-75.749,-5.321,11.506
	point
	-75.939,-5.321,5.116
	point
	-78.787,-5.321,-0.971
	reverse


// Pedestrian number 484

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-78.182,-5.321,11.449
	point
	-78.080,-5.321,4.468
	point
	-75.535,-5.321,2.283
	point
	-75.419,-5.321,-7.445
	point
	-79.159,-5.321,-16.101
	reverse


// Pedestrian number 485

12				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-78.436,-5.321,-17.389
	point
	-78.262,-5.321,-21.521
	point
	-78.931,-5.321,-26.431
	point
	-75.412,-5.321,-30.694
	point
	-75.437,-5.319,-53.212
	reverse


// Pedestrian number 486

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-76.683,-5.319,-53.001
	point
	-78.216,-5.319,-51.021
	point
	-78.619,994.881,-48.145
	point
	-81.604,994.881,-46.347
	reverse


// Pedestrian number 487

12				// Ref num
7				// Number of instructions
4				// Initial instruction

	point
	-78.252,-5.319,-52.205
	point
	-76.223,-5.319,-39.298
	point
	-78.207,-5.319,-33.196
	point
	-78.555,-5.319,-21.447
	point
	-75.704,-5.319,-18.061
	point
	-75.471,-5.319,-8.135
	reverse


// Pedestrian number 488

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-78.625,-5.319,-17.471
	point
	-75.852,-5.319,-23.264
	point
	-75.476,-5.319,-28.889
	point
	-78.581,994.881,-31.059
	point
	-82.538,994.881,-32.043
	reverse


// Pedestrian number 489

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-78.049,-5.319,-52.438
	point
	-77.564,-5.319,-52.640
	point
	-77.423,-5.319,-53.471
	point
	-76.873,-5.319,-53.565
	reverse


// Pedestrian number 490

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-78.793,-5.319,-50.924
	point
	-77.159,-5.319,-52.057
	point
	-72.880,-5.319,-53.122
	point
	-65.946,-5.319,-49.698
	reverse


// Pedestrian number 491

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-67.223,-5.319,-49.400
	point
	-65.405,-5.319,-50.553
	point
	-62.885,-5.319,-54.003
	point
	-62.279,-5.319,-54.180
	reverse


// Pedestrian number 492

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-67.981,-5.319,-49.737
	point
	-65.255,-5.319,-50.152
	point
	-63.844,-5.319,-51.073
	point
	-62.938,-5.319,-53.059
	reverse


// Pedestrian number 493

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-69.627,-5.319,-53.189
	point
	-65.464,-5.319,-52.523
	point
	-63.158,-5.319,-54.358
	point
	-63.061,-5.319,-55.838
	point
	-60.329,-5.319,-56.546
	reverse


// Pedestrian number 494

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-70.538,-5.319,-53.276
	point
	-75.940,-5.319,-49.291
	point
	-78.201,-5.319,-42.804
	point
	-79.270,-5.319,-41.392
	reverse


// Pedestrian number 495

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-79.445,-5.319,-41.772
	point
	-75.770,-5.319,-45.872
	point
	-78.076,-5.319,-48.281
	point
	-79.000,-5.319,-50.795
	reverse


// Pedestrian number 496

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-66.235,-5.319,-55.510
	point
	-65.369,-5.319,-60.777
	point
	-60.617,-5.319,-63.702
	reverse


// Pedestrian number 497

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-61.630,-5.319,-62.316
	point
	-63.622,-5.319,-68.668
	point
	-65.714,-5.319,-71.268
	point
	-66.090,-5.319,-77.998
	reverse


// Pedestrian number 498

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-63.548,-5.319,-81.654
	point
	-59.444,-5.319,-81.955
	point
	-55.748,-5.319,-78.555
	reverse


// Pedestrian number 499

8				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-57.497,-5.319,-79.979
	point
	-57.976,-5.319,-80.525
	point
	-63.856,-5.319,-78.904
	point
	-64.819,-5.319,-76.012
	point
	-66.106,-5.319,-75.271
	reverse


// Pedestrian number 500

8				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	24.858,-5.319,-87.398
	point
	25.172,-5.319,-86.860
	point
	26.200,-5.319,-86.166
	point
	26.981,-5.319,-85.216
	reverse


// Pedestrian number 501

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	27.303,-5.319,-82.097
	point
	27.184,-5.319,-82.938
	point
	26.687,-5.319,-86.126
	point
	25.861,-5.319,-87.241
	point
	25.150,-5.319,-87.229
	reverse


// Pedestrian number 502

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	24.956,-5.319,-76.755
	point
	25.527,-5.319,-75.934
	point
	26.390,-5.319,-73.985
	point
	28.337,-5.319,-71.959
	point
	28.548,-5.319,-70.899
	reverse


// Pedestrian number 503

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	28.683,-5.319,-70.217
	point
	28.793,-5.319,-69.975
	point
	29.999,-5.319,-68.248
	reverse


// Pedestrian number 504

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	29.734,-5.319,-72.362
	point
	28.937,-5.319,-70.341
	point
	27.990,-5.319,-67.960
	point
	28.526,-5.319,-66.478
	reverse


// Pedestrian number 505

12				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	28.138,-5.319,-71.692
	point
	30.280,-5.319,-69.233
	point
	33.220,994.881,-66.585
	point
	36.349,994.881,-62.541
	reverse


// Pedestrian number 506

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	29.043,-5.319,-73.390
	point
	30.386,-5.319,-71.112
	point
	55.871,-5.321,-30.962
	reverse


// Pedestrian number 507

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	56.099,-5.321,-31.570
	point
	55.287,-5.321,-31.130
	point
	53.734,994.879,-29.747
	point
	53.098,994.879,-24.528
	reverse


// Pedestrian number 508

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	53.084,-5.321,-30.143
	point
	53.848,-5.321,-31.335
	point
	48.371,-5.321,-36.854
	reverse


// Pedestrian number 509

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	48.069,-5.321,-35.912
	point
	53.310,-5.321,-32.193
	point
	55.542,-5.321,-31.542
	point
	63.710,-5.321,-30.848
	point
	63.873,994.879,-31.579
	point
	65.938,994.879,-40.799
	reverse


// Pedestrian number 510

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	55.647,-5.321,-30.640
	point
	50.735,-5.321,-34.912
	point
	45.990,-5.321,-43.995
	point
	42.016,-5.321,-50.526
	point
	34.511,-5.321,-54.393
	reverse


// Pedestrian number 511

8				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	34.390,-5.321,-56.176
	point
	34.058,-5.321,-63.167
	point
	31.164,-5.321,-67.235
	reverse


// Pedestrian number 512

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	31.466,-5.321,-66.247
	point
	35.386,-5.321,-59.519
	point
	40.127,994.879,-53.645
	point
	42.365,994.879,-53.196
	reverse


// Pedestrian number 513

5				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	53.506,-5.321,-29.146
	point
	55.384,-5.321,-20.657
	point
	55.248,-5.321,9.257
	reverse


// Pedestrian number 514

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	53.284,-5.321,6.696
	point
	53.602,-5.321,7.372
	point
	54.667,-5.321,8.582
	point
	54.697,-5.321,9.308
	reverse


// Pedestrian number 515

13				// Ref num
3				// Number of instructions
1				// Initial instruction

	point
	55.377,-5.321,6.541
	point
	54.038,-5.321,8.285
	reverse


// Pedestrian number 516

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	53.438,-5.321,3.073
	point
	53.670,-5.321,6.617
	point
	54.098,-5.321,7.715
	point
	57.104,-5.321,9.445
	point
	57.286,-5.321,10.561
	reverse


// Pedestrian number 517

13				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	65.263,-5.321,6.971
	point
	56.751,-5.321,8.227
	point
	54.358,-5.321,8.597
	reverse


// Pedestrian number 518

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	57.495,-5.321,11.502
	point
	58.646,-5.321,15.335
	point
	60.972,-5.321,19.388
	reverse


// Pedestrian number 519

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	63.564,-5.321,18.547
	point
	58.821,-5.321,15.240
	point
	57.186,-5.321,14.362
	reverse


// Pedestrian number 520

12				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	57.087,-5.321,12.411
	point
	58.584,-5.321,13.520
	point
	58.478,-5.321,15.979
	point
	57.343,-5.321,26.504
	reverse


// Pedestrian number 521

12				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	57.374,-5.321,10.891
	point
	58.412,-5.321,12.103
	point
	59.219,-5.321,16.491
	point
	59.381,-5.321,20.379
	point
	56.611,-5.321,26.487
	point
	54.729,-5.321,27.835
	reverse


// Pedestrian number 522

5				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	60.482,-5.321,26.075
	point
	58.112,-5.321,25.554
	point
	56.748,-5.321,26.563
	point
	53.688,-5.321,27.921
	reverse


// Pedestrian number 523

10				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	52.262,-5.321,28.109
	point
	52.501,-5.321,27.863
	point
	55.183,-5.321,27.045
	point
	57.945,-5.321,25.569
	point
	61.252,-5.321,19.936
	reverse


// Pedestrian number 524

10				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	63.981,-5.321,18.565
	point
	82.168,-5.321,8.487
	point
	92.304,-5.321,8.707
	point
	102.735,-5.321,6.773
	reverse


// Pedestrian number 525

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	95.509,-5.321,6.779
	point
	92.550,-5.321,6.743
	point
	81.540,-5.321,8.253
	point
	70.105,-5.321,9.447
	point
	66.560,-5.321,8.691
	reverse


// Pedestrian number 526

5				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	65.283,-5.321,9.873
	point
	60.845,-5.321,17.287
	point
	61.504,-5.321,20.087
	point
	58.748,-5.321,26.733
	reverse


// Pedestrian number 527

1				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	52.486,-5.321,28.215
	point
	48.149,-5.321,28.050
	point
	45.304,-5.321,25.670
	point
	43.965,-5.321,22.252
	reverse


// Pedestrian number 528

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	45.189,-5.321,21.527
	point
	50.777,-5.321,25.939
	point
	54.488,-5.321,27.878
	reverse


// Pedestrian number 529

1				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	56.158,-5.321,19.456
	point
	47.347,-5.321,25.923
	point
	42.700,-5.321,27.804
	point
	37.052,-5.321,27.909
	point
	32.177,-5.321,24.525
	reverse


// Pedestrian number 530

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	26.663,-5.321,23.994
	point
	33.642,-5.321,26.070
	point
	40.739,-5.321,26.088
	point
	42.930,-5.321,24.811
	point
	43.785,-5.321,22.043
	reverse


// Pedestrian number 531

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	44.437,-5.321,22.149
	point
	48.466,-5.321,23.600
	point
	54.742,-5.321,27.286
	point
	56.032,-5.321,27.393
	reverse


// Pedestrian number 532

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	45.348,-5.321,30.586
	point
	41.851,-5.321,28.224
	point
	38.203,-5.321,26.279
	point
	32.236,-5.321,26.180
	point
	25.738,-5.321,28.879
	point
	19.446,-5.321,29.233
	reverse


// Pedestrian number 533

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	18.503,-5.321,24.924
	point
	15.555,994.879,25.651
	point
	12.514,994.879,28.519
	reverse


// Pedestrian number 534

12				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	18.673,-5.321,29.446
	point
	14.483,994.879,27.850
	point
	2.380,994.879,28.777
	reverse


// Pedestrian number 535

12				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	15.889,-5.321,28.768
	point
	14.406,-5.321,26.228
	point
	8.575,-5.321,25.386
	point
	2.127,-5.321,28.154
	point
	0.825,-5.321,28.197
	point
	0.279,-5.321,28.521
	reverse


// Pedestrian number 536

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	0.377,-5.302,30.222
	point
	1.130,-5.303,28.512
	point
	0.200,-5.301,27.325
	point
	-0.504,-5.300,25.302
	reverse


// Pedestrian number 537

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	0.015,-5.301,25.386
	point
	4.908,-5.309,25.917
	point
	9.263,-5.317,25.984
	point
	13.935,-5.326,27.768
	point
	15.333,-5.328,28.561
	reverse


// Pedestrian number 538

8				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	14.752,-5.327,25.652
	point
	6.508,-5.312,27.965
	point
	-0.365,-5.300,27.983
	point
	-0.736,-5.300,28.471
	reverse


// Pedestrian number 539

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-50.320,-5.300,24.606
	point
	-51.655,-5.306,25.907
	point
	-55.368,994.885,26.958
	point
	-56.469,994.877,28.725
	reverse


// Pedestrian number 540

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-58.711,-5.323,27.955
	point
	-56.687,-5.318,27.328
	point
	-55.844,-5.315,26.652
	point
	-51.638,-5.302,24.614
	reverse


// Pedestrian number 541

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-50.186,-5.301,25.077
	point
	-51.756,-5.309,26.724
	point
	-55.858,-5.317,27.252
	point
	-61.594,-5.325,27.146
	point
	-64.392,-5.324,25.545
	reverse


// Pedestrian number 542

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-61.386,-5.319,25.344
	point
	-55.879,-5.316,26.870
	point
	-53.998,-5.316,27.754
	point
	-51.809,-5.313,27.826
	point
	-49.364,-5.313,28.996
	reverse


// Pedestrian number 543

13				// Ref num
7				// Number of instructions
3				// Initial instruction

	point
	-50.783,-5.303,28.709
	point
	-51.663,-5.303,27.307
	point
	-55.221,-5.303,27.468
	point
	-59.368,-5.303,27.506
	point
	-61.889,-5.303,25.549
	point
	-63.991,-5.321,25.321
	reverse


// Pedestrian number 544

13				// Ref num
6				// Number of instructions
3				// Initial instruction

	point
	-62.056,-5.321,27.990
	point
	-60.136,-5.321,27.959
	point
	-56.855,-5.321,26.823
	point
	-54.504,-5.321,24.135
	point
	-50.169,-5.321,22.469
	reverse


// Pedestrian number 545

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-50.228,-5.303,15.428
	point
	-51.919,-5.303,23.306
	point
	-57.572,994.897,26.646
	point
	-58.996,994.897,31.547
	reverse


// Pedestrian number 546

13				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-50.194,-5.303,20.605
	point
	-54.223,-5.303,22.997
	point
	-57.585,994.897,27.227
	point
	-61.831,994.897,28.483
	reverse


// Pedestrian number 547

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-20.787,-4.084,89.893
	reverse


// Pedestrian number 548

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-20.430,-4.084,86.498
	reverse


// Pedestrian number 549

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-20.405,-4.084,83.950
	reverse


// Pedestrian number 550

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-21.594,-4.084,105.913
	reverse


// Pedestrian number 551

127				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-24.167,-4.084,101.128
	reverse


// Pedestrian number 552

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-26.015,-4.084,97.570
	reverse


// Pedestrian number 553

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.533,-4.084,87.688
	reverse


// Pedestrian number 554

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-33.594,-4.084,83.924
	reverse


// Pedestrian number 555

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-57.431,-4.084,71.596
	reverse


// Pedestrian number 556

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-54.590,-4.084,79.379
	reverse


// Pedestrian number 557

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-52.134,-4.323,62.849
	reverse


// Pedestrian number 558

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-61.893,-4.323,62.868
	reverse


// Pedestrian number 559

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-62.837,-4.323,59.805
	reverse


// Pedestrian number 560

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-62.761,-4.323,57.337
	reverse


// Pedestrian number 561

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-57.754,-4.323,57.242
	reverse


// Pedestrian number 562

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-44.931,-4.323,57.165
	reverse


// Pedestrian number 563

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-54.043,-4.323,57.326
	reverse


// Pedestrian number 564

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-17.756,-5.321,66.624
	reverse


// Pedestrian number 565

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-19.673,-5.321,67.008
	reverse


// Pedestrian number 566

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.750,-5.321,63.345
	reverse


// Pedestrian number 567

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-31.472,-5.321,66.715
	reverse


// Pedestrian number 568

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.086,-6.648,77.192
	reverse


// Pedestrian number 569

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.131,-6.648,76.641
	reverse


// Pedestrian number 570

5				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-88.472,-6.648,71.888
	point
	-84.816,-6.648,62.363
	point
	-80.404,-6.648,53.669
	point
	-82.350,-6.648,40.045
	point
	-87.388,-6.648,37.988
	reverse


// Pedestrian number 571

10				// Ref num
5				// Number of instructions
3				// Initial instruction

	point
	-87.326,-6.648,36.611
	point
	-82.155,-6.648,55.293
	point
	-84.792,-6.648,61.228
	point
	-81.676,-6.648,76.953
	reverse


// Pedestrian number 572

10				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-80.805,-6.648,72.862
	point
	-84.001,-6.648,61.932
	point
	-88.127,-6.648,54.104
	point
	-87.845,-6.648,45.315
	point
	-82.525,-6.648,38.462
	reverse


// Pedestrian number 573

1				// Ref num
4				// Number of instructions
2				// Initial instruction

	point
	-82.602,-6.648,38.271
	point
	-85.419,-6.648,35.398
	point
	-87.333,-6.648,33.940
	reverse


// Pedestrian number 574

8				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-87.699,-6.648,38.541
	point
	-85.834,-6.648,33.090
	point
	-84.275,-6.648,29.767
	point
	-84.420,-6.648,21.776
	point
	-86.988,-6.648,20.497
	reverse


// Pedestrian number 575

13				// Ref num
5				// Number of instructions
2				// Initial instruction

	point
	-87.133,-6.648,21.421
	point
	-85.381,-6.648,29.681
	point
	-83.089,-6.648,35.487
	point
	-87.349,-6.648,36.295
	reverse


// Pedestrian number 576

13				// Ref num
6				// Number of instructions
2				// Initial instruction

	point
	-87.155,-6.646,14.193
	point
	-87.332,-6.637,-8.669
	point
	-83.691,-6.676,-12.830
	point
	-86.816,-6.640,-19.103
	point
	-81.575,-6.648,-42.222
	reverse


// Pedestrian number 577

10				// Ref num
7				// Number of instructions
2				// Initial instruction

	point
	-81.997,-6.648,-35.893
	point
	-85.896,-6.648,-39.279
	point
	-89.656,-6.639,-49.340
	point
	-89.787,-6.640,-52.138
	point
	-90.940,-6.647,-53.744
	point
	-93.434,-6.648,-76.236
	reverse


// Pedestrian number 578

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-64.524,-5.315,-78.231
	reverse


// Pedestrian number 579

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-66.749,-5.258,-77.614
	reverse


// Pedestrian number 580

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-66.765,-5.258,-54.409
	reverse


// Pedestrian number 581

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-29.437,-5.227,-33.421
	reverse


// Pedestrian number 582

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-21.972,-5.227,-33.140
	reverse


// Pedestrian number 583

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	49.705,-7.518,-3.879
	reverse


// Pedestrian number 584

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	49.630,-7.518,-7.149
	reverse


// Pedestrian number 585

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	49.615,-7.517,-13.054
	reverse


// Pedestrian number 586

136				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	58.883,-7.519,-16.801
	reverse


// Pedestrian number 587

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	59.103,-7.518,-10.278
	reverse


// Pedestrian number 588

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	68.827,-7.519,2.283
	reverse


// Pedestrian number 589

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	68.863,-7.519,1.838
	reverse


// Pedestrian number 590

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	68.919,-7.519,1.130
	reverse


// Pedestrian number 591

102				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	69.042,-7.519,-0.427
	reverse


// Pedestrian number 592

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	69.359,-7.519,-13.018
	reverse


// Pedestrian number 593

109				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	68.993,-7.519,-26.581
	reverse


// Pedestrian number 594

136				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-25.416,-8.399,23.574
	reverse


// Pedestrian number 595

121				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-23.585,-8.399,17.613
	reverse


// Pedestrian number 596

122				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-21.077,-8.399,19.668
	reverse


// Pedestrian number 597

129				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-19.484,-8.399,21.638
	reverse


// Pedestrian number 598

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-11.504,-5.291,39.237
	reverse


// Pedestrian number 599

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-7.449,-5.291,35.315
	reverse


// Pedestrian number 600

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-3.710,-5.291,31.557
	reverse


// Pedestrian number 601

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-0.844,-5.290,28.750
	reverse


// Pedestrian number 602

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-10.992,-3.559,36.712
	reverse


// Pedestrian number 603

134				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-20.150,-5.290,47.236
	reverse


// Pedestrian number 604

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-11.711,-5.227,57.242
	reverse


// Pedestrian number 605

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-8.217,-5.227,57.298
	reverse


// Pedestrian number 606

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	3.421,-5.227,57.251
	reverse


// Pedestrian number 607

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.859,-5.227,57.243
	reverse


// Pedestrian number 608

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-72.116,-6.650,83.616
	reverse


// Pedestrian number 609

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-65.467,-6.654,86.978
	reverse


// Pedestrian number 610

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-59.698,-6.655,89.895
	reverse


// Pedestrian number 611

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-52.827,-6.655,93.369
	reverse


// Pedestrian number 612

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-46.959,-5.319,-85.060
	reverse


// Pedestrian number 613

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-46.365,-5.319,-86.313
	reverse


// Pedestrian number 614

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-45.027,-5.319,-88.667
	reverse


// Pedestrian number 615

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-43.325,-5.319,-91.672
	reverse


// Pedestrian number 616

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-42.460,-5.319,-85.937
	reverse


// Pedestrian number 617

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-41.022,-5.319,-87.611
	reverse


// Pedestrian number 618

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-38.127,-5.319,-91.399
	reverse


// Pedestrian number 619

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-36.732,-5.319,-94.618
	reverse


// Pedestrian number 620

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-40.736,-5.319,-90.563
	reverse


// Pedestrian number 621

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-43.322,-5.319,-87.754
	reverse


// Pedestrian number 622

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-40.698,-5.319,-93.955
	reverse


// Pedestrian number 623

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.353,-5.321,-39.193
	reverse


// Pedestrian number 624

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	4.750,-5.321,-42.036
	reverse


// Pedestrian number 625

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	4.459,-5.321,-44.449
	reverse


// Pedestrian number 626

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	3.824,-5.321,-49.851
	reverse


// Pedestrian number 627

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	4.912,-5.321,-55.754
	reverse


// Pedestrian number 628

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.930,-5.321,-58.466
	reverse


// Pedestrian number 629

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.994,-5.321,-58.051
	reverse


// Pedestrian number 630

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	15.149,-5.321,-56.706
	reverse


// Pedestrian number 631

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	14.895,-5.321,-55.369
	reverse


// Pedestrian number 632

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	14.613,-5.321,-52.078
	reverse


// Pedestrian number 633

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	14.045,-5.321,-46.814
	reverse


// Pedestrian number 634

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	12.564,-5.321,-41.091
	reverse


// Pedestrian number 635

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.854,-5.321,-39.641
	reverse


// Pedestrian number 636

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.056,-5.321,-39.524
	reverse


// Pedestrian number 637

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.717,-5.321,-44.103
	reverse


// Pedestrian number 638

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	10.246,-5.321,-52.862
	reverse


// Pedestrian number 639

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.478,-5.321,-51.094
	reverse


// Pedestrian number 640

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.657,-5.321,-46.607
	reverse


// Pedestrian number 641

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.874,-5.321,-51.845
	reverse


// Pedestrian number 642

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	12.116,-5.321,-50.207
	reverse


// Pedestrian number 643

107				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.145,-5.320,-48.164
	reverse


// Pedestrian number 644

108				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	7.974,-5.320,-48.880
	reverse


// Pedestrian number 645

138				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	6.844,-5.320,-48.173
	reverse


// Pedestrian number 646

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.208,-5.320,-48.113
	reverse


// Pedestrian number 647

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	8.219,-5.320,-47.145
	reverse


// Pedestrian number 648

100				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	30.762,-5.320,-10.845
	reverse


// Pedestrian number 649

139				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.132,-5.320,-15.582
	reverse


// Pedestrian number 650

120				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.482,-5.320,-17.993
	reverse


// Pedestrian number 651

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	14.945,-5.320,-38.346
	reverse


// Pedestrian number 652

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	42.192,-5.321,-28.969
	reverse


// Pedestrian number 653

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	41.938,-5.321,-24.603
	reverse


// Pedestrian number 654

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	41.443,-5.321,-15.410
	reverse


// Pedestrian number 655

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	40.865,-5.321,-4.672
	reverse


// Pedestrian number 656

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	40.510,-5.321,-0.960
	reverse


// Pedestrian number 657

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	42.798,-5.321,10.555
	reverse


// Pedestrian number 658

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	39.883,-5.321,11.607
	reverse


// Pedestrian number 659

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	37.145,-5.321,12.596
	reverse


// Pedestrian number 660

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	33.771,-5.321,13.660
	reverse


// Pedestrian number 661

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	30.365,-5.321,14.674
	reverse


// Pedestrian number 662

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	46.354,-5.321,20.867
	reverse


// Pedestrian number 663

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	46.457,-5.321,24.476
	reverse


// Pedestrian number 664

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	49.083,-5.321,25.237
	reverse


// Pedestrian number 665

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	53.674,-5.321,24.786
	reverse


// Pedestrian number 666

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	56.268,-5.321,20.784
	reverse


// Pedestrian number 667

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	85.099,-6.647,14.635
	reverse


// Pedestrian number 668

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	79.692,-6.647,19.026
	reverse


// Pedestrian number 669

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	72.297,-6.647,23.538
	reverse


// Pedestrian number 670

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	61.919,-6.647,26.339
	reverse


// Pedestrian number 671

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	60.283,-6.635,31.332
	reverse


// Pedestrian number 672

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	64.216,-6.658,28.277
	reverse


// Pedestrian number 673

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	66.722,-6.647,24.754
	reverse


// Pedestrian number 674

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	51.859,-6.664,46.653
	reverse


// Pedestrian number 675

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	49.164,-6.657,53.771
	reverse


// Pedestrian number 676

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	37.864,-6.650,84.349
	reverse


// Pedestrian number 677

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	38.281,-6.643,85.552
	reverse


// Pedestrian number 678

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	40.688,-6.283,82.399
	reverse


// Pedestrian number 679

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	39.866,-6.594,84.312
	reverse


// Pedestrian number 680

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	35.207,-6.515,85.077
	reverse


// Pedestrian number 681

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	34.173,-6.472,89.121
	reverse


// Pedestrian number 682

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	33.047,-6.625,89.118
	reverse


// Pedestrian number 683

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	29.487,-6.628,91.921
	reverse


// Pedestrian number 684

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	27.368,-6.635,93.985
	reverse


// Pedestrian number 685

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	26.172,-6.643,92.218
	reverse


// Pedestrian number 686

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	23.887,-6.647,92.996
	reverse


// Pedestrian number 687

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	23.898,-6.244,94.469
	reverse


// Pedestrian number 688

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	24.943,-6.462,95.033
	reverse


// Pedestrian number 689

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	28.333,-6.418,90.701
	reverse


// Pedestrian number 690

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	29.571,-6.360,89.892
	reverse


// Pedestrian number 691

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-59.514,-6.563,-89.156
	reverse


// Pedestrian number 692

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-58.010,-6.638,-89.731
	reverse


// Pedestrian number 693

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-56.152,-6.534,-89.856
	reverse


// Pedestrian number 694

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-54.257,-6.393,-91.279
	reverse


// Pedestrian number 695

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-52.758,-6.659,-90.712
	reverse


// Pedestrian number 696

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-53.405,-6.598,-89.577
	reverse


// Pedestrian number 697

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-55.879,-6.651,-88.285
	reverse


// Pedestrian number 698

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-57.548,-6.652,-87.411
	reverse


// Pedestrian number 699

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-59.191,-6.547,-87.459
	reverse


// Pedestrian number 700

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-60.461,-6.503,-86.635
	reverse


// Pedestrian number 701

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-61.577,-6.219,-87.553
	reverse


// Pedestrian number 702

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-61.347,-6.561,-89.507
	reverse


// Pedestrian number 703

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-59.523,-6.656,-90.965
	reverse


// Pedestrian number 704

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-57.730,-6.669,-91.875
	reverse


// Pedestrian number 705

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-55.963,-6.527,-92.591
	reverse


// Pedestrian number 706

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-53.486,-6.352,-93.073
	reverse


// Pedestrian number 707

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-51.196,-6.417,-93.966
	reverse


// Pedestrian number 708

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-48.847,-6.625,-93.751
	reverse


// Pedestrian number 709

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-48.426,-6.529,-92.830
	reverse


// Pedestrian number 710

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-50.140,-6.663,-92.667
	reverse


// Pedestrian number 711

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-51.624,-6.529,-92.451
	reverse


// Pedestrian number 712

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.288,-6.586,-76.952
	reverse


// Pedestrian number 713

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.933,-6.656,-73.340
	reverse


// Pedestrian number 714

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.068,-6.565,-72.920
	reverse


// Pedestrian number 715

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-88.440,-6.539,-72.822
	reverse


// Pedestrian number 716

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-90.106,-6.424,-71.523
	reverse


// Pedestrian number 717

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-89.749,-6.554,-68.941
	reverse


// Pedestrian number 718

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-88.409,-6.169,-66.349
	reverse


// Pedestrian number 719

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-89.394,-6.488,-64.176
	reverse


// Pedestrian number 720

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-90.295,-6.523,-59.584
	reverse


// Pedestrian number 721

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-91.563,-6.649,-50.165
	reverse


// Pedestrian number 722

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-90.297,-6.591,-50.196
	reverse


// Pedestrian number 723

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-88.641,-6.632,-50.276
	reverse


// Pedestrian number 724

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.226,-6.645,-50.518
	reverse


// Pedestrian number 725

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.599,-6.655,-50.686
	reverse


// Pedestrian number 726

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-82.629,-6.653,-50.897
	reverse


// Pedestrian number 727

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.773,-6.651,11.190
	reverse


// Pedestrian number 728

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.485,-6.651,11.446
	reverse


// Pedestrian number 729

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.587,-6.650,12.295
	reverse


// Pedestrian number 730

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-72.465,-6.653,76.933
	reverse


// Pedestrian number 731

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-70.450,-6.652,77.732
	reverse


// Pedestrian number 732

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-69.383,-6.650,79.400
	reverse


// Pedestrian number 733

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-68.560,-6.651,80.834
	reverse


// Pedestrian number 734

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-66.480,-6.652,82.570
	reverse


// Pedestrian number 735

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-62.238,-6.652,82.442
	reverse


// Pedestrian number 736

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-59.017,-6.652,81.478
	reverse


// Pedestrian number 737

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-57.746,-6.652,84.455
	reverse


// Pedestrian number 738

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-60.614,-6.651,85.124
	reverse


// Pedestrian number 739

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-53.202,-6.652,82.558
	reverse


// Pedestrian number 740

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-53.899,-6.652,87.034
	reverse


// Pedestrian number 741

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-56.457,-6.651,87.739
	reverse


// Pedestrian number 742

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-49.935,-6.653,85.372
	reverse


// Pedestrian number 743

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-50.481,-6.652,88.214
	reverse


// Pedestrian number 744

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-51.511,-6.651,91.161
	reverse


// Pedestrian number 745

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-37.777,-6.650,89.364
	reverse


// Pedestrian number 746

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-36.278,-6.652,91.317
	reverse


// Pedestrian number 747

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-34.353,-6.655,93.827
	reverse


// Pedestrian number 748

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-32.571,-6.654,96.149
	reverse


// Pedestrian number 749

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-30.183,-6.655,99.263
	reverse


// Pedestrian number 750

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-27.891,-6.656,102.234
	reverse


// Pedestrian number 751

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-25.400,-6.655,105.427
	reverse


// Pedestrian number 752

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	38.901,-6.661,81.098
	reverse


// Pedestrian number 753

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	40.721,-6.644,80.176
	reverse


// Pedestrian number 754

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	42.869,-6.642,78.646
	reverse


// Pedestrian number 755

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	42.310,-6.470,81.780
	reverse


// Pedestrian number 756

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	79.636,-6.654,-23.120
	reverse


// Pedestrian number 757

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	78.513,-6.654,-27.506
	reverse


// Pedestrian number 758

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	81.277,-6.652,-23.901
	reverse


// Pedestrian number 759

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	61.818,-6.653,-33.921
	reverse


// Pedestrian number 760

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	62.164,-6.650,-34.876
	reverse


// Pedestrian number 761

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	48.073,-6.654,-50.393
	reverse


// Pedestrian number 762

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	42.575,-6.650,-55.010
	reverse


// Pedestrian number 763

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	43.676,-6.650,-53.818
	reverse


// Pedestrian number 764

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	45.318,-6.649,-52.566
	reverse


// Pedestrian number 765

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	28.381,-6.651,-83.497
	reverse


// Pedestrian number 766

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	29.091,-6.650,-84.604
	reverse


// Pedestrian number 767

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	29.374,-6.650,-83.059
	reverse


// Pedestrian number 768

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	29.305,-6.652,-81.924
	reverse


// Pedestrian number 769

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	28.538,-6.650,-81.373
	reverse


// Pedestrian number 770

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	28.441,-6.653,-79.414
	reverse


// Pedestrian number 771

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	29.669,-6.650,-79.629
	reverse


// Pedestrian number 772

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	29.127,-6.654,-77.944
	reverse


// Pedestrian number 773

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	28.996,-6.653,-76.319
	reverse


// Pedestrian number 774

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	30.142,-6.651,-74.818
	reverse


// Pedestrian number 775

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	30.707,-6.651,-77.602
	reverse


// Pedestrian number 776

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	31.142,-6.652,-78.826
	reverse


// Pedestrian number 777

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.596,-6.654,-80.585
	reverse


// Pedestrian number 778

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.508,-6.653,-83.005
	reverse


// Pedestrian number 779

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	31.182,-6.650,-82.572
	reverse


// Pedestrian number 780

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	31.775,-6.652,-75.839
	reverse


// Pedestrian number 781

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	32.840,-6.654,-77.051
	reverse


// Pedestrian number 782

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	31.068,-6.651,-84.295
	reverse


// Pedestrian number 783

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-24.836,-6.650,-98.390
	reverse


// Pedestrian number 784

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-22.308,-6.651,-97.834
	reverse


// Pedestrian number 785

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-20.169,-6.655,-97.409
	reverse


// Pedestrian number 786

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-17.199,-6.655,-96.822
	reverse


// Pedestrian number 787

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-14.444,-6.655,-96.282
	reverse


// Pedestrian number 788

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-12.055,-6.655,-95.826
	reverse


// Pedestrian number 789

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-9.203,-6.656,-95.280
	reverse


// Pedestrian number 790

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-5.558,-6.655,-94.576
	reverse


// Pedestrian number 791

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-1.583,-6.656,-93.798
	reverse


// Pedestrian number 792

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.066,-6.655,-93.114
	reverse


// Pedestrian number 793

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	5.774,-6.655,-92.403
	reverse


// Pedestrian number 794

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.366,-6.654,-91.916
	reverse


// Pedestrian number 795

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	12.399,-6.651,-91.332
	reverse


// Pedestrian number 796

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-24.949,-6.650,-97.831
	reverse


// Pedestrian number 797

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-22.345,-6.651,-97.252
	reverse


// Pedestrian number 798

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-20.077,-6.653,-96.761
	reverse


// Pedestrian number 799

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-16.839,-6.654,-96.116
	reverse


// Pedestrian number 800

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-13.547,-6.653,-95.460
	reverse


// Pedestrian number 801

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-10.583,-6.654,-94.877
	reverse


// Pedestrian number 802

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-5.652,-6.655,-93.940
	reverse


// Pedestrian number 803

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-1.666,-6.654,-93.148
	reverse


// Pedestrian number 804

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	2.068,-6.654,-92.370
	reverse


// Pedestrian number 805

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	5.614,-6.655,-91.638
	reverse


// Pedestrian number 806

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	9.151,-6.654,-90.969
	reverse


// Pedestrian number 807

112				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	11.987,-6.654,-90.439
	reverse


// Pedestrian number 808

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.563,-6.653,60.208
	reverse


// Pedestrian number 809

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.145,-6.652,58.883
	reverse


// Pedestrian number 810

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.851,-6.654,57.058
	reverse


// Pedestrian number 811

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.231,-6.653,54.241
	reverse


// Pedestrian number 812

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.851,-6.652,51.279
	reverse


// Pedestrian number 813

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.422,-6.651,47.838
	reverse


// Pedestrian number 814

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.857,-6.653,45.179
	reverse


// Pedestrian number 815

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.802,-6.655,43.065
	reverse


// Pedestrian number 816

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.785,-6.654,41.130
	reverse


// Pedestrian number 817

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.843,-6.652,38.861
	reverse


// Pedestrian number 818

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.569,-6.652,37.781
	reverse


// Pedestrian number 819

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.647,-6.654,36.745
	reverse


// Pedestrian number 820

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.001,-6.652,34.634
	reverse


// Pedestrian number 821

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.675,-6.653,32.817
	reverse


// Pedestrian number 822

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.429,-6.651,30.280
	reverse


// Pedestrian number 823

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.662,-6.652,28.069
	reverse


// Pedestrian number 824

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.493,-6.653,25.734
	reverse


// Pedestrian number 825

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.561,-6.653,24.132
	reverse


// Pedestrian number 826

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.877,-6.654,21.176
	reverse


// Pedestrian number 827

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.429,-6.653,19.021
	reverse


// Pedestrian number 828

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.717,-6.653,16.708
	reverse


// Pedestrian number 829

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.348,-6.651,15.332
	reverse


// Pedestrian number 830

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.837,-6.650,14.561
	reverse


// Pedestrian number 831

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.172,-6.653,9.505
	reverse


// Pedestrian number 832

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.736,-6.652,8.210
	reverse


// Pedestrian number 833

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.504,-6.651,7.658

	reverse


// Pedestrian number 834

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.567,-6.551,5.910
	reverse


// Pedestrian number 835

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.979,-6.651,4.327
	reverse


// Pedestrian number 836

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.976,-6.651,2.770
	reverse


// Pedestrian number 837

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.992,-6.653,0.917
	reverse


// Pedestrian number 838

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.769,-6.652,-1.110
	reverse


// Pedestrian number 839

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.384,-6.651,-1.973
	reverse


// Pedestrian number 840

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.406,-6.611,-3.010
	reverse


// Pedestrian number 841

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.808,-6.649,-5.299
	reverse


// Pedestrian number 842

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.936,-6.654,-6.355
	reverse


// Pedestrian number 843

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.621,-6.653,-7.265
	reverse


// Pedestrian number 844

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.850,-6.650,-8.846
	reverse


// Pedestrian number 845

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.985,-6.654,-11.685
	reverse


// Pedestrian number 846

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.021,-6.652,-14.181
	reverse


// Pedestrian number 847

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.393,-6.652,-15.801
	reverse


// Pedestrian number 848

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.666,-6.652,-17.369
	reverse


// Pedestrian number 849

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.903,-6.653,-20.273
	reverse


// Pedestrian number 850

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.592,-6.653,-23.636
	reverse


// Pedestrian number 851

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.892,-6.652,-25.497
	reverse


// Pedestrian number 852

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.736,-6.653,-26.605
	reverse


// Pedestrian number 853

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.503,-6.651,-22.797
	reverse


// Pedestrian number 854

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.925,-6.652,-18.502
	reverse


// Pedestrian number 855

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.500,-6.651,-15.976
	reverse


// Pedestrian number 856

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.183,-6.653,-9.181
	reverse


// Pedestrian number 857

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.623,-6.654,-3.780
	reverse


// Pedestrian number 858

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.345,-6.653,4.654
	reverse


// Pedestrian number 859

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.167,-6.655,13.459
	reverse


// Pedestrian number 860

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.940,-6.654,15.668
	reverse


// Pedestrian number 861

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.067,-6.652,17.555
	reverse


// Pedestrian number 862

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-86.394,-6.654,20.688
	reverse


// Pedestrian number 863

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.517,-6.652,32.284
	reverse


// Pedestrian number 864

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.027,-6.653,42.667
	reverse


// Pedestrian number 865

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.213,-6.655,44.795
	reverse


// Pedestrian number 866

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.207,-6.654,47.023
	reverse


// Pedestrian number 867

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.183,-6.655,49.609
	reverse


// Pedestrian number 868

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.106,-6.652,52.606
	reverse


// Pedestrian number 869

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.107,-6.654,54.311
	reverse


// Pedestrian number 870

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-82.390,-6.654,56.707
	reverse


// Pedestrian number 871

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-82.105,-6.652,58.836
	reverse


// Pedestrian number 872

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-82.603,-6.653,60.663
	reverse


// Pedestrian number 873

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.722,-6.653,62.216
	reverse


// Pedestrian number 874

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.398,-6.653,63.563
	reverse


// Pedestrian number 875

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-82.086,-6.654,63.057
	reverse


// Pedestrian number 876

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-81.292,-6.654,61.448
	reverse


// Pedestrian number 877

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-80.386,-6.653,59.219
	reverse


// Pedestrian number 878

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-80.058,-6.655,57.028
	reverse


// Pedestrian number 879

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-80.651,-6.653,53.908
	reverse


// Pedestrian number 880

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-81.906,-6.653,52.034
	reverse


// Pedestrian number 881

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.612,-6.652,50.692
	reverse


// Pedestrian number 882

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.507,-6.651,49.065
	reverse


// Pedestrian number 883

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-83.049,-6.653,47.841
	reverse


// Pedestrian number 884

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-82.352,-6.651,46.420
	reverse


// Pedestrian number 885

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.916,-6.654,41.046
	reverse


// Pedestrian number 886

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-85.499,-6.653,38.614
	reverse


// Pedestrian number 887

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-84.538,-6.653,35.347
	reverse


// Pedestrian number 888

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.052,-6.642,-21.316
	reverse


// Pedestrian number 889

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-87.642,-6.630,-23.277
	reverse


// Pedestrian number 890

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-88.355,-6.266,-24.862
	reverse


// Pedestrian number 891

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-90.234,-6.653,-29.525
	reverse


// Pedestrian number 892

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-90.506,-6.652,-31.544
	reverse


// Pedestrian number 893

114				// Ref num
2				// Number of instructions
1				// Initial instruction

	point
	-90.681,-6.653,-36.217
	reverse


// Pedestrian number 894

99				// Ref num
9				// Number of instructions
5				// Initial instruction

	point
	7.003,-5.227,67.883
	point
	7.239,-5.226,67.601
	point
	7.565,-5.321,67.210
	point
	8.396,-5.321,66.477
	point
	9.382,-5.321,66.040
	point
	10.137,-5.321,66.242
	point
	12.150,-5.321,67.470
	point
	14.178,-5.321,68.326
	reverse




// ****** START OF OPPONENT PATHS ******

START OF OPPONENT PATHS

207                             // Number of path nodes
   22.040,   -5.320,   65.351   // Node #0
  -37.008,   -5.321,   65.603   // Node #1
  -75.427,   -5.321,   73.963   // Node #2
  -79.761,   -6.109,   73.921   // Node #3
  -83.061,   -6.647,   72.963   // Node #4
  -84.798,   -6.648,   69.812   // Node #5
  -86.535,   -6.648,   65.168   // Node #6
  -86.742,   -6.632,  -64.115   // Node #7
  -90.144,   -6.385,  -72.337   // Node #8
  -90.257,   -6.233,  -76.200   // Node #9
  -88.189,   -6.321,  -79.246   // Node #10
  -79.520,   -5.319,  -79.799   // Node #11
  -63.879,   -5.297,  -78.975   // Node #12
  -44.532,   -5.319,  -84.923   // Node #13
  -38.867,   -5.319,  -84.903   // Node #14
  -35.761,   -5.319,  -83.658   // Node #15
  -34.463,   -5.319,  -82.387   // Node #16
  -32.449,   -5.319,  -78.651   // Node #17
  -31.668,   -5.321,   -5.168   // Node #18
  -32.068,   -8.047,   11.126   // Node #19
  -30.930,   -8.399,   15.558   // Node #20
  -28.806,   -8.399,   17.826   // Node #21
  -22.756,   -8.399,   22.317   // Node #22
  -20.274,   -8.399,   25.371   // Node #23
  -19.072,   -8.399,   27.634   // Node #24
  -19.066,   -5.321,   54.015   // Node #25
  -19.073,   -5.321,   64.891   // Node #26
  -31.802,   -5.320,  -54.324   // Node #27
  -19.065,   -5.297,   46.343   // Node #28
   21.498,   -5.320,   63.607   // Node #29
   21.416,   -5.321,   26.972   // Node #30
   25.778,   -5.321,   14.315   // Node #31
   26.793,   -5.323,  -22.725   // Node #32
   26.951,   -5.321,  -25.853   // Node #33
   29.280,   -5.321,  -27.936   // Node #34
   44.704,   -5.321,  -30.692   // Node #35
   54.103,   -5.321,  -32.261   // Node #36
   64.277,   -5.321,  -30.562   // Node #37
   72.545,   -5.321,  -30.622   // Node #38
   73.312,   -5.321,  -30.113   // Node #39
   73.752,   -5.321,  -28.936   // Node #40
   73.559,   -5.321,    7.465   // Node #41
   62.408,   -5.321,   14.431   // Node #42
   55.101,   -5.321,    6.952   // Node #43
   45.091,   -5.321,    7.718   // Node #44
   57.774,   -5.321,   20.630   // Node #45
   53.009,   -5.321,   24.597   // Node #46
   46.406,   -5.321,   56.764   // Node #47
   44.398,   -5.321,   59.559   // Node #48
   40.364,   -5.321,   62.533   // Node #49
   34.898,   -5.321,   64.374   // Node #50
   27.044,   -5.321,   65.971   // Node #51
   23.424,   -5.321,   66.224   // Node #52
  -64.779,   -5.319,  -53.358   // Node #53
  -76.793,   -5.288,  -50.976   // Node #54
  -73.523,   -5.342,   27.087   // Node #55
  -64.997,   -5.321,   27.174   // Node #56
  -51.605,   -5.303,   26.934   // Node #57
  -33.308,    2.777,   27.177   // Node #58
  -19.692,    3.525,   27.025   // Node #59
    0.139,   -5.296,   26.918   // Node #60
   15.391,   -5.321,   27.023   // Node #61
   50.596,   -5.321,   29.596   // Node #62
   60.176,   -5.321,   10.568   // Node #63
   62.060,   -5.321,   12.280   // Node #64
   26.577,   -5.321,  -76.065   // Node #65
   25.322,   -5.321,  -85.802   // Node #66
   24.291,   -5.321,  -86.664   // Node #67
   19.100,   -5.321,  -87.610   // Node #68
    4.192,   -5.321,  -86.547   // Node #69
  -18.842,   -5.321,  -86.533   // Node #70
  -32.129,   -5.321,  -88.573   // Node #71
  -76.952,   -5.288,   23.907   // Node #72
   54.414,   -5.321,    5.091   // Node #73
  -58.298,   -5.321,   27.173   // Node #74
  -52.895,   -7.405,   36.651   // Node #75
  -54.075,   -7.497,   28.621   // Node #76
  -54.620,   -7.433,    6.143   // Node #77
  -43.226,   -7.452,   -5.642   // Node #78
  -33.071,   -7.517,  -12.883   // Node #79
  -17.192,   -7.511,  -12.936   // Node #80
  -10.504,   -7.429,   -9.985   // Node #81
   -8.563,   -7.400,   -7.266   // Node #82
  -13.085,   -7.545,   -2.321   // Node #83
  -17.284,   -8.336,    3.545   // Node #84
  -19.050,   -8.278,    9.361   // Node #85
  -19.023,   -8.399,   14.984   // Node #86
  -30.493,   -8.399,   24.404   // Node #87
  -31.887,   -8.399,   27.457   // Node #88
  -31.761,   -8.281,   31.662   // Node #89
  -33.412,   -8.347,   37.458   // Node #90
  -37.168,   -7.616,   43.103   // Node #91
  -40.209,   -7.431,   44.490   // Node #92
  -43.786,   -7.388,   44.144   // Node #93
    4.178,   -5.321,  -75.119   // Node #94
    4.194,   -5.321,  -65.399   // Node #95
   26.085,   -5.321,  -65.121   // Node #96
   26.030,   -5.321,  -57.660   // Node #97
   19.064,   -5.321,  -57.453   // Node #98
   17.261,   -5.321,  -56.011   // Node #99
   16.628,   -5.321,  -37.938   // Node #100
   15.583,   -5.321,  -36.322   // Node #101
   12.958,   -5.320,  -35.670   // Node #102
  -18.814,   -5.318,  -35.518   // Node #103
  -31.440,   -5.318,  -35.526   // Node #104
  -64.498,   -5.321,  -34.996   // Node #105
  -64.662,   -5.321,  -20.476   // Node #106
  -64.743,   -5.321,   14.064   // Node #107
  -51.201,   -5.321,   14.308   // Node #108
  -19.400,   -5.321,   -4.983   // Node #109
  -18.964,   -5.321,  -19.912   // Node #110
  -17.513,   -5.321,  -85.153   // Node #111
  -18.770,   -5.321,  -82.808   // Node #112
  -31.739,   -5.321,  -19.864   // Node #113
  -61.036,   -7.174,  -15.516   // Node #114
  -61.236,   -7.519,  -37.943   // Node #115
  -55.364,   -7.517,  -45.368   // Node #116
  -50.376,   -7.517,  -47.514   // Node #117
  -32.179,   -7.519,  -44.270   // Node #118
  -19.224,   -7.581,  -43.635   // Node #119
   18.219,   -7.517,  -43.452   // Node #120
   23.905,   -7.517,  -38.677   // Node #121
   24.598,   -7.517,  -35.153   // Node #122
   19.199,   -7.519,  -30.028   // Node #123
   -1.861,   -7.517,  -26.431   // Node #124
   -4.739,   -7.519,  -22.888   // Node #125
   -4.487,   -7.497,  -18.162   // Node #126
   11.809,   -7.506,   12.121   // Node #127
   12.014,   -7.517,   28.415   // Node #128
   10.789,   -7.474,   31.875   // Node #129
  -12.941,   -7.459,   51.249   // Node #130
  -17.886,   -7.519,   51.640   // Node #131
  -38.459,   -7.408,   51.302   // Node #132
  -89.790,   -6.648,  -83.284   // Node #133
  -53.175,   -6.611,  -91.238   // Node #134
  -32.999,   -6.646, -101.795   // Node #135
  -29.400,   -6.648, -101.423   // Node #136
   27.717,   -6.648,  -88.400   // Node #137
   30.659,   -6.648,  -84.202   // Node #138
   51.468,   -6.648,  -41.647   // Node #139
   54.939,   -6.648,  -39.689   // Node #140
   75.325,   -6.648,  -33.371   // Node #141
   94.664,   -6.648,    6.165   // Node #142
   94.093,   -6.646,    9.169   // Node #143
   65.283,   -6.648,   27.254   // Node #144
   58.742,   -6.436,   34.493   // Node #145
   40.361,   -6.344,   82.670   // Node #146
   20.918,   -6.655,   96.626   // Node #147
  -81.608,   -6.648,   75.986   // Node #148
  -78.563,   -6.648,   77.113   // Node #149
   40.289,   -6.648,  -64.483   // Node #150
   39.653,   -6.648,  -61.738   // Node #151
   64.026,   -6.648,  -39.733   // Node #152
  -17.206,   -6.648,  109.330   // Node #153
  -20.312,   -6.648,  109.419   // Node #154
  -31.889,   -8.399,   26.448   // Node #155
  -48.374,   -7.332,   42.510   // Node #156
  -61.428,   -8.315,  -26.781   // Node #157
  -59.402,   -7.519,  -40.656   // Node #158
  -59.058,   -7.519,  -44.334   // Node #159
  -59.082,   -5.327,  -49.037   // Node #160
  -65.259,   -5.296,  -70.825   // Node #161
  -32.071,   -5.319, -117.418   // Node #162
  -61.663,   -5.319,  -80.697   // Node #163
  -65.212,   -5.296,  -76.177   // Node #164
  -64.136,   -5.319,  -66.680   // Node #165
  -49.118,   -5.319,  -67.064   // Node #166
  -48.655,   -5.319,  -58.113   // Node #167
  -61.549,   -5.319,  -58.145   // Node #168
  -38.326,   -5.320,  -51.691   // Node #169
  -59.689,   -5.319,  -51.900   // Node #170
  -64.732,   -5.320,  -51.252   // Node #171
  -33.233,    2.764,   14.316   // Node #172
  -17.636,    2.852,   14.407   // Node #173
    6.730,   -5.312,   14.093   // Node #174
   14.052,   -5.317,   14.051   // Node #175
   23.944,   -5.320,  -29.584   // Node #176
   18.757,   -5.320,  -34.305   // Node #177
  -65.080,   -5.321,  -28.761   // Node #178
  -65.304,   -5.321,  -32.334   // Node #179
  -60.192,   -5.321,  -35.553   // Node #180
  -65.053,   -5.317,   46.924   // Node #181
  -65.802,   -5.321,   49.382   // Node #182
  -65.849,   -5.321,   51.757   // Node #183
  -65.193,   -5.321,   53.442   // Node #184
  -64.015,   -5.321,   54.114   // Node #185
  -58.795,   -5.321,   54.737   // Node #186
  -41.078,   -5.321,   54.346   // Node #187
  -36.778,   -5.321,   55.912   // Node #188
  -34.657,   -5.321,   57.650   // Node #189
  -33.211,   -5.321,   64.985   // Node #190
  -29.883,   -5.321,   65.002   // Node #191
  -35.501,   -5.321,   65.369   // Node #192
  -28.111,   -5.321,   82.887   // Node #193
  -27.197,   -5.321,   84.773   // Node #194
  -20.551,   -5.321,   93.088   // Node #195
  -18.774,   -5.321,   94.014   // Node #196
   13.782,   -5.321,   93.997   // Node #197
   15.269,   -5.321,   93.465   // Node #198
   16.750,   -5.321,   92.096   // Node #199
   17.642,   -5.321,   90.109   // Node #200
   17.479,   -5.321,   84.675   // Node #201
   18.641,   -5.321,   81.813   // Node #202
   20.001,   -5.321,   80.021   // Node #203
   23.045,   -5.321,   77.808   // Node #204
   24.913,   -5.321,   75.702   // Node #205
   25.992,   -5.321,   72.861   // Node #206

236                                           // Number of path sections
   0,  26,   0, 255,   0, 255,    1.0,    1   // Section #0
   1,   2,   0, 255,   0, 255,    0.8,    1   // Section #1
   2,   3,   0, 255,   0, 255,    0.8,    1   // Section #2
   3,   4,   0, 255,   0, 255,    0.6,    1   // Section #3
   4,   5,   0, 255,   0, 255,    0.6,    1   // Section #4
   5,   6,   0, 255,   0, 255,    0.6,    1   // Section #5
   6,   7,   0, 255,   0, 255,    0.6,    1   // Section #6
   7,   8,   0,  50,   0,  45,    0.6,    1   // Section #7
   8,   9,   0,  35,   0,  35,    0.6,    1   // Section #8
   9,  10,   0,  30,   0,  25,    0.6,    1   // Section #9
  10,  11,   0,  25,   0,  35,    0.6,    1   // Section #10
  12, 163,   0, 255,   0, 255,    0.6,    0   // Section #11
  13,  14,   0,  35,   0,  25,    0.6,    1   // Section #12
  14,  15,   0,  25,   0,  20,    0.6,    1   // Section #13
  15,  16,   0,  20,   0,  25,    0.6,    1   // Section #14
  16,  17,   0,  35,   0,  40,    0.6,    1   // Section #15
  17,  27,   0, 100,   0, 255,    0.6,    1   // Section #16
  18,  19,   0,  45,   0,  35,    0.6,    1   // Section #17
  19,  20,   0,  30,   0,  25,    0.6,    1   // Section #18
  20,  21,   0,  30,   0,  35,    0.6,    1   // Section #19
  21,  22,   0,  50,   0,  50,    0.6,    1   // Section #20
  22,  23,   0,  35,   0,  30,    0.6,    1   // Section #21
  23,  24,   0,  30,   0,  25,    0.6,    1   // Section #22
  24,  28,   0, 255,   0, 255,    0.6,    1   // Section #23
  25,  26,   0, 255,   0,  25,    0.6,    1   // Section #24
  26, 191,   0, 255,   0, 255,    1.0,    1   // Section #25
  27, 104,   0, 255,   0, 255,    0.6,    1   // Section #26
  28,  25,   0, 255,   0, 255,    0.6,    1   // Section #27
   0,  29,   0, 255,   0, 255,    1.0,    0   // Section #28
  29,  30,   0, 255,   0, 255,    1.0,    0   // Section #29
  30,  31,   0, 255,   0, 255,    1.0,    0   // Section #30
  31,  32,   0, 255,   0, 255,    1.0,    0   // Section #31
  32,  33,   0, 255,   0, 255,    1.0,    0   // Section #32
  33,  34,   0, 255,   0, 255,    1.0,    0   // Section #33
  34,  35,   0, 255,   0, 255,    1.0,    0   // Section #34
  35,  36,   0, 255,   0, 255,    1.0,    0   // Section #35
  36,  37,   0, 255,   0, 255,    1.0,    0   // Section #36
  37,  38,   0, 255,   0, 255,    1.0,    0   // Section #37
  38,  39,   0, 255,   0, 255,    1.0,    0   // Section #38
  39,  40,   0, 255,   0, 255,    1.0,    0   // Section #39
  40,  41,   0, 255,   0, 255,    1.0,    0   // Section #40
  41,  42,   0, 255,   0, 255,    1.0,    0   // Section #41
  64,  42,   0, 255,   0, 255,    1.0,    0   // Section #42
  43,  44,   0, 255,   0, 255,    1.0,    0   // Section #43
  44,  31,   0, 255,   0, 255,    1.0,    0   // Section #44
  42,  45,   0, 255,   0, 255,    1.0,    0   // Section #45
  45,  46,   0, 255,   0, 255,    1.0,    0   // Section #46
  46,  62,   0, 255,   0, 255,    1.0,    0   // Section #47
  47,  48,   0, 255,   0, 255,    1.0,    0   // Section #48
  48,  49,   0, 255,   0, 255,    1.0,    0   // Section #49
  49,  50,   0, 255,   0, 255,    1.0,    0   // Section #50
  50,  51,   0, 255,   0, 255,    1.0,    0   // Section #51
  51,  52,   0, 255,   0, 255,    1.0,    0   // Section #52
  52,   0,   0, 255,   0, 255,    1.0,    0   // Section #53
  53, 161,   0, 255,   0, 255,    0.6,    0   // Section #54
  54, 171,   0,  35,   0, 255,    0.6,    0   // Section #55
  72,  54,   0, 255,   0,  40,    0.8,    0   // Section #56
  56,  55,   0, 255,   0,  40,    0.6,    0   // Section #57
  57,  74,   0, 255,   0, 255,    0.6,    0   // Section #58
  58,  57,   0, 255,   0, 255,    0.6,    0   // Section #59
  59,  58,   0, 255,   0, 255,    0.6,    0   // Section #60
  60,  59,  35, 255,  40, 255,    0.6,    0   // Section #61
  61,  60,   0, 255,  25, 255,    0.6,    0   // Section #62
  30,  61,   0, 255,   0, 255,    0.6,    0   // Section #63
  46,  30,   0, 255,   0, 255,    1.0,    0   // Section #64
  62,  47,   0, 255,   0, 255,    1.0,    0   // Section #65
  43,  63,   0, 255,   0, 255,    1.0,    0   // Section #66
  63,  64,   0, 255,   0, 255,    1.0,    0   // Section #67
  36,  73,   0, 255,   0, 255,    0.8,    0   // Section #68
  65,  36,   0, 255,   0, 255,    0.6,    0   // Section #69
  66,  65,   0, 255,   0, 255,    0.8,    0   // Section #70
  67,  66,   0,  30,   0,  25,    1.0,    0   // Section #71
  68,  67,   0,  40,   0,  35,    1.0,    0   // Section #72
  69,  68,   0, 255,   0,  45,    1.0,    0   // Section #73
  70,  69,   0, 255,   0, 255,    1.0,    0   // Section #74
  71,  70,   0, 255,   0, 255,    1.0,    0   // Section #75
  55,  72,   0,  30,   0,  30,    0.8,    0   // Section #76
  73,  43,   0, 255,   0, 255,    1.0,    0   // Section #77
  74,  56,   0, 255,   0, 255,    0.6,    0   // Section #78
  75,  76,   0, 255,   0, 255,    0.6,    0   // Section #79
  76,  77,   0, 255,   0, 255,    0.6,    0   // Section #80
  78,  77,   0, 255,   0, 255,    0.6,    0   // Section #81
  79,  78,   0, 255,   0, 255,    0.6,    0   // Section #82
  80,  79,   0, 255,   0, 255,    0.6,    0   // Section #83
  81,  80,   0, 255,   0, 255,    0.6,    0   // Section #84
  82,  81,   0, 255,   0, 255,    0.6,    0   // Section #85
  83,  82,   0, 255,   0, 255,    0.6,    0   // Section #86
  84,  83,   0, 255,   0, 255,    0.6,    0   // Section #87
  85,  84,   0, 255,   0, 255,    0.6,    0   // Section #88
  86,  85,   0, 255,   0, 255,    0.6,    0   // Section #89
  22,  86,   0, 255,   0, 255,    0.6,    0   // Section #90
  22,  87,   0, 255,   0, 255,    0.6,    0   // Section #91
  87, 155,   0, 255,   0, 255,    0.6,    0   // Section #92
  88,  89,   0, 255,   0, 255,    0.6,    0   // Section #93
  89,  90,   0, 255,   0, 255,    0.6,    0   // Section #94
  90,  91,   0, 255,   0, 255,    0.6,    0   // Section #95
  91,  92,   0, 255,   0, 255,    0.6,    0   // Section #96
  92,  93,   0, 255,   0, 255,    0.6,    0   // Section #97
  69,  94,   0, 255,   0, 255,    1.0,    0   // Section #98
  94,  95,   0, 255,   0, 255,    1.0,    0   // Section #99
  95,  96,   0, 255,   0, 255,    1.0,    0   // Section #100
  96,  97,   0, 255,   0, 255,    1.0,    0   // Section #101
  97,  35,   0, 255,   0, 255,    1.0,    0   // Section #102
  35,  44,   0, 255,   0, 255,    1.0,    0   // Section #103
  97,  98,   0, 255,   0, 255,    1.0,    0   // Section #104
  98,  99,   0, 255,   0, 255,    1.0,    0   // Section #105
  99, 100,   0, 255,   0, 255,    1.0,    0   // Section #106
 100, 101,   0, 255,   0, 255,    1.0,    0   // Section #107
 101, 102,   0, 255,   0, 255,    1.0,    0   // Section #108
 102, 103,   0, 255,   0, 255,    1.0,    0   // Section #109
 103, 104,   0, 255,   0, 255,    1.0,    0   // Section #110
 104, 180,   0, 255,   0,  35,    1.0,    0   // Section #111
 104, 113,   0, 255,   0, 255,    0.6,    1   // Section #112
 105, 179,   0, 255,   0, 255,    1.0,    0   // Section #113
 106, 107,   0, 255,   0, 255,    1.0,    0   // Section #114
 107, 108,   0, 255,   0, 255,    1.0,    0   // Section #115
  18, 109,   0, 255,   0, 255,    0.6,    0   // Section #116
 109, 110,   0, 255,   0, 255,    0.6,    0   // Section #117
 110, 103,   0, 255,   0, 255,    0.6,    0   // Section #118
 103, 112,   0, 255,   0, 255,    1.0,    0   // Section #119
 111,  70,   0, 255,   0, 255,    1.0,    0   // Section #120
 112, 111,   0, 255,   0, 255,    1.0,    0   // Section #121
  79,  78,   0, 255,   0, 255,    0.6,    0   // Section #122
 113, 106,   0, 255,   0, 255,    1.0,    0   // Section #123
 113, 110,   0, 255,   0, 255,    1.0,    0   // Section #124
 113,  18,   0, 255,   0, 255,    0.6,    1   // Section #125
 114, 157,   0, 255,   0, 255,    0.6,    0   // Section #126
 115, 158,   0, 255,   0, 255,    0.6,    0   // Section #127
 116, 117,   0, 255,   0, 255,    0.6,    0   // Section #128
 117, 118,   0, 255,   0, 255,    0.6,    0   // Section #129
 118, 119,   0, 255,   0, 255,    0.6,    0   // Section #130
 119, 120,   0, 255,   0, 255,    0.6,    0   // Section #131
 120, 121,   0, 255,   0, 255,    0.6,    0   // Section #132
 121, 122,   0, 255,   0, 255,    0.6,    0   // Section #133
 122, 123,   0, 255,   0, 255,    0.6,    0   // Section #134
 123, 124,   0, 255,   0, 255,    0.6,    0   // Section #135
 124, 125,   0, 255,   0, 255,    0.6,    0   // Section #136
 125, 126,   0, 255,   0, 255,    0.6,    0   // Section #137
 126, 127,   0, 255,   0, 255,    0.6,    0   // Section #138
 127, 128,   0, 255,   0, 255,    0.6,    0   // Section #139
 128, 129,   0, 255,   0, 255,    0.6,    0   // Section #140
 129, 130,   0, 255,   0, 255,    0.6,    0   // Section #141
 130, 131,   0, 255,   0, 255,    0.6,    0   // Section #142
 131, 132,   0, 255,   0, 255,    0.6,    0   // Section #143
 132, 156,   0, 255,   0, 255,    0.6,    0   // Section #144
  10, 133,   0, 255,   0, 255,    0.3,    0   // Section #145
 133, 134,   0, 255,   0, 255,    0.6,    0   // Section #146
 134, 135,   0, 255,   0, 255,    0.6,    0   // Section #147
 135, 136,   0, 255,   0, 255,    0.6,    0   // Section #148
 136, 137,   0, 255,   0, 255,    0.6,    0   // Section #149
 137, 138,   0, 255,   0, 255,    0.6,    0   // Section #150
 138, 150,   0, 255,   0, 255,    0.6,    0   // Section #151
 139, 140,   0, 255,   0, 255,    0.6,    0   // Section #152
 140, 152,   0, 255,   0, 255,    0.6,    0   // Section #153
 141, 142,   0, 255,   0, 255,    0.6,    0   // Section #154
 142, 143,   0, 255,   0, 255,    0.6,    0   // Section #155
 143, 144,   0, 255,   0, 255,    0.6,    0   // Section #156
 144, 145,   0, 255,   0, 255,    0.6,    0   // Section #157
 145, 146,   0, 255,   0, 255,    0.6,    0   // Section #158
 146, 147,   0, 255,   0, 255,    0.6,    0   // Section #159
 147, 153,   0, 255,   0, 255,    0.6,    0   // Section #160
 148,   4,   0, 255,   0, 255,    0.6,    0   // Section #161
 149, 148,   0, 255,   0, 255,    0.6,    0   // Section #162
 150, 151,   0, 255,   0, 255,    0.6,    0   // Section #163
 151, 139,   0, 255,   0, 255,    0.6,    0   // Section #164
 152, 141,   0, 255,   0, 255,    0.6,    0   // Section #165
 152,  37,   0, 255,   0, 255,    0.6,    0   // Section #166
 153, 154,   0, 255,   0, 255,    0.6,    0   // Section #167
 154, 149,   0, 255,   0, 255,    0.6,    0   // Section #168
  20, 155,   0, 255,   0, 255,    0.6,    0   // Section #169
 155,  88,   0, 255,   0, 255,    0.6,    0   // Section #170
  93, 156,   0, 255,   0, 255,    0.6,    0   // Section #171
 156,  75,   0, 255,   0, 255,    0.6,    0   // Section #172
  77, 114,   0, 255,   0, 255,    0.6,    0   // Section #173
 157, 115,   0, 255,   0, 255,    0.6,    0   // Section #174
 158, 159,   0, 255,   0, 255,    0.6,    0   // Section #175
 158, 116,   0, 255,   0, 255,    0.6,    0   // Section #176
 159, 160,   0, 255,   0, 255,    0.6,    0   // Section #177
 160, 170,   0, 255,   0, 255,    0.6,    0   // Section #178
 161, 164,   0, 255,   0, 255,    0.6,    0   // Section #179
  71,  17,   0, 255,   0, 255,    1.0,    0   // Section #180
 162,  71,   0, 255,   0, 255,    1.0,    0   // Section #181
 163,  13,   0, 255,   0,  45,    0.6,    1   // Section #182
 164,  12,   0, 255,   0,  25,    0.6,    0   // Section #183
  11,  54,   0, 255,   0, 255,    0.6,    0   // Section #184
 165, 166,   0, 255,   0, 255,    0.6,    0   // Section #185
 165, 161,   0, 255,   0, 255,    0.6,    0   // Section #186
 166, 167,   0, 255,   0, 255,    0.6,    0   // Section #187
 167, 168,   0, 255,   0, 255,    0.6,    0   // Section #188
 168, 165,   0, 255,   0, 255,    0.6,    0   // Section #189
  27, 169,   0, 255,   0, 255,    0.6,    0   // Section #190
 169, 170,   0, 255,   0, 255,    0.6,    0   // Section #191
 170, 168,   0, 255,   0, 255,    0.6,    0   // Section #192
 171, 105,   0, 255,   0, 255,    1.0,    0   // Section #193
 171,  53,   0, 255,   0,  25,    0.6,    0   // Section #194
  82, 126,   0, 255,   0, 255,    0.6,    0   // Section #195
 108, 172,   0, 255,   0, 255,    1.0,    0   // Section #196
 172, 173,   0, 255,   0, 255,    1.0,    0   // Section #197
 173, 174,   0, 255,   0, 255,    1.0,    0   // Section #198
 174, 175,   0, 255,   0, 255,    1.0,    0   // Section #199
  32, 176,   0, 255,   0, 255,    1.0,    0   // Section #200
 176, 177,   0, 255,   0, 255,    1.0,    0   // Section #201
 177, 102,   0, 255,   0, 255,    1.0,    0   // Section #202
 178, 106,   0, 255,   0, 255,    1.0,    0   // Section #203
 179, 178,   0, 255,   0, 255,    1.0,    0   // Section #204
 180, 105,   0,  20,   0,  15,    0.9,    0   // Section #205
 107, 181,   0, 255,   0, 255,    1.0,    0   // Section #206
 181, 182,   0, 255,   0, 255,    1.0,    0   // Section #207
 182, 183,   0, 255,   0, 255,    1.0,    0   // Section #208
 183, 184,   0, 255,   0, 255,    1.0,    0   // Section #209
 184, 185,   0, 255,   0, 255,    1.0,    0   // Section #210
 185, 186,   0, 255,   0, 255,    1.0,    0   // Section #211
 186, 187,   0, 255,   0, 255,    1.0,    0   // Section #212
 187, 188,   0, 255,   0, 255,    1.0,    0   // Section #213
 188, 189,   0, 255,   0, 255,    1.0,    0   // Section #214
 189, 190,   0, 255,   0, 255,    1.0,    0   // Section #215
 191, 190,   0, 255,   0, 255,    1.0,    1   // Section #216
 190, 192,   0, 255,   0, 255,    1.0,    1   // Section #217
 192,   1,   0, 255,   0, 255,    1.0,    1   // Section #218
 191, 193,   0, 255,   0, 255,    1.0,    0   // Section #219
 193, 194,   0, 255,   0, 255,    1.0,    0   // Section #220
 194, 195,   0, 255,   0, 255,    1.0,    0   // Section #221
 195, 196,   0, 255,   0, 255,    1.0,    0   // Section #222
 196, 197,   0, 255,   0, 255,    1.0,    0   // Section #223
 197, 198,   0, 255,   0, 255,    1.0,    0   // Section #224
 198, 199,   0, 255,   0, 255,    1.0,    0   // Section #225
 199, 200,   0, 255,   0, 255,    1.0,    0   // Section #226
 200, 201,   0, 255,   0, 255,    1.0,    0   // Section #227
 201, 202,   0, 255,   0, 255,    1.0,    0   // Section #228
 202, 203,   0, 255,   0, 255,    1.0,    0   // Section #229
 203, 204,   0, 255,   0, 255,    1.0,    0   // Section #230
 204, 205,   0, 255,   0, 255,    1.0,    0   // Section #231
 205, 206,   0, 255,   0, 255,    1.0,    0   // Section #232
 206,  52,   0, 255,   0, 255,    1.0,    0   // Section #233
  11, 163,   0, 255,   0, 255,    0.6,    1   // Section #234
  26, 196,   0, 255,   0, 255,    1.0,    0   // Section #235

3                                                             // Number of cop start points
   44.861,   -5.321,   39.954,    0.000,    0.000,    0.000   // Cop start point #0
   50.235,   -7.518,    1.442,    0.000,    0.000,    0.000   // Cop start point #1
  -53.529,   -7.385,   39.013,    0.000,    0.000,    0.000   // Cop start point #2

END OF OPPONENT PATHS

8										// number of material modifiers

// default material
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
1.0										// sparkiness
1										// room for expansion
ROAD1.MAT							// skid mark material

//	material '0'
1.2										// car wall friction
1.2										// tyre road friction
1										// down force
2										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
2										// room for expansion
SAND1.MAT										// room for expansion

//	material '1'
1										// car wall friction
1										// tyre road friction
1.0										// down force
2										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
5										// room for expansion
MUD1.MAT										// room for expansion

//	material '2'
1										// car wall friction
1										// tyre road friction
1.0										// down force
1.5										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
2										// room for expansion
SAND2.MAT										// room for expansion

//	material '3'
1										// car wall friction
1										// tyre road friction
1.0										// down force
2										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
4										// room for expansion
MUD1.MAT										// room for expansion

//	material '4'
0.5										// car wall friction
0.5										// tyre road friction
0.40										// down force
1.0										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
1										// sparkiness
1										// room for expansion
none									// room for expansion

//	material '5'
1										// car wall friction
1										// tyre road friction
1.0										// down force
2										// bumpiness
-1										// tyre sound index
0										// crash sound index
0										// scrape noise index
0.0										// sparkiness
1										// room for expansion
SAND1.MAT										// room for expansion

//	material '6'
1.0										// car wall friction
1.0										// tyre road friction
1.0										// down force
0.0										// bumpiness
0										// tyre sound index
0										// crash sound index
0										// scrape noise index
9.0										// sparkiness
1										// room for expansion
none									// room for expansion

// Non CarObjects
6										// number of non car objects

GASPUMP.TXT
GREENCAR.TXT
WRECK.TXT
PALM2.TXT
PHONE.TXT
CONE.TXT

4										// number of dust shade tables

228, 199, 83								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"

128, 145, 64								// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"

92, 51, 34							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"

92, 71, 61							// r g b values
0.25, 0.5, 0.75							// quarter, half and three quarter "strength"


12										// Number of network start points

-18.855,-5.321,113.912							//1
0													

-11.990,-5.321,65.026							//2						
89									

-19.005,-5.321,53.855							//3						
182									

-11.583,-5.318,14.136							//4						
90									

-31.702,-5.321,-20.684							//5						
180									

-59.929,-5.321,26.975							//6						
270									

-76.975,-5.321,16.893							//7						
0									

-54.008,-5.320,-51.708							//8						
270									

-32.053,-5.320,-115.423							//9						
180									

16.997,-5.320,-44.870							//10						
0									

100.186,-5.321,7.594							//11						
90									

25.772,-5.320,71.808							//12						
16									

1										// number of splash files
SPLSHBLU.PIX 								//  name of pixelmapfile for splashes

1

DEZRACE1.TXT
